1. 双目摄像头改成树莓派连接座定义的。

Modify the camera interface’s pin definitions to align with the Raspberry Pi's interface

2. 替换部分器件来通过FCC/CE认证

Replacing certain components to comply with FCC/CE certification requirements​







