VERSION:285606329

2,IIii,[ wlan_ant_share.c : 169 ] COEX_MWS_ANT_DIVERSITY: chnmsk completed Rx:0x%x, Tx:0x%x, Cal:%d, ReqId:%d 
1,ii,[ wlan_ant_share.c : 183 ] COEX_MWS_ANT_DIVERSITY: [Warr] chnmsk completed but ReqId:%d not matched with RespId:%d 
0,iIIIiii,[ wlan_ant_share.c : 125 ] COEX_MWS_ANT_DIVERSITY: Chainmask Req ret(%d)::Rx:0x%x, Tx:0x%x, RxNSS:0x%x, SMPS_Diff:%d, ReqId:%d, Cal:%d 
6,iiIi,[ wlan_bwa.c : 184 ] WLAN_BWA_UPDATE_VDEV_BW: phy_mode=%d, opmode=%d, Requested operating voltage corner=0x%x vdev_bw %d 
5,ii,[ wlan_bwa.c : 256 ] WLAN_BWA_GET_VDEV_BW: vdev_id=%d, vdev_bw=%d [>=BW_CNT returned] 
4,ii,[ wlan_bwa.c : 140 ] WLAN_BWA_SET_PMAC_BW: mac_id=%d, pmac_bw=%d 
3,ii,[ wlan_bwa.c : 149 ] WLAN_BWA_SET_PMAC_BW: mac_id=%d, pmac_bw=%d [!WAL_EOK returned] 
9,I,[ wlan_chainmask_proxy.c : 27 ] Chainmask_Proxy_CHM_NOTIF: event_type = 0x%x 
8,Iiii,[ wlan_chainmask_proxy.c : 131 ] Chainmask_Proxy_Set_Antenna_Mode:  mac_id_map = 0x%x, mac_id = %d, num_tx_chains = %d, num_rx_chains = %d 
7,IIii,[ wlan_chainmask_proxy.c : 161 ] Chainmask_Proxy_Set_Chainmask: band_map = 0x%x, mac_id_map = 0x%x, chainmask = %d, Tx_Rx = %d (Tx = 0, Rx = 1) 
24,i,[ wlan_swbmiss_offload.c : 531 ] wlan_bmiss_update_hwbmiss = %d 
23,iiiiiiii,[ wlan_swbmiss_offload.c : 681 ] SWBMISS_NULL_SEND_CMPLT: vdev_id=%d, isQosNullSuccess=%d, isFinalBmiss=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, fbmiss_evnt_posted=%d, vbmiss->connected = %d, cons_bmiss_count = %d  
22,ii,[ wlan_swbmiss_offload.c : 550 ] SWBMISS_BCON_RECVED: vdev_id=%d, IS_HWBMISS=%d 
21,iiiiiii,[ wlan_swbmiss_offload.c : 990 ] SWBMISS_TIMER_FN: vdev_id=%d, curr_bmiss_bcnt=%d, pre_bmiss_detected=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, b_timeout=%d, cons_bmiss_count = %d  
20,i,[ wlan_swbmiss_offload.c : 419 ] wlan_swbmiss_check_if_bmiss_enabled: vdev id=%d, bmiss timer isn't armed, restart it. 
19,iIii,[ wlan_swbmiss_offload.c : 1166 ] SWBMISS_DELIVER_EVT: vdev_id=%d, evt_type=0x%x, bcn_rssi_avg=%d, bcn_rssi_last=%d 
18,iiIiI,[ wlan_swbmiss_offload.c : 499 ] SWBMISS_DISABLED: vdev_id=%d, swbmiss_module_id=%d, bmiss_disable_bitmap=0x%x, curr_bmiss_bcnt=%d, cur_disable_bitmask=0x%x 
17,iiIii,[ wlan_swbmiss_offload.c : 455 ] SWBMISS_ENABLED: vdev_id=%d, swbmiss_module_id=%d, bmiss_disable_bitmap=0x%x, curr_bmiss_bcnt=%d, final_bmiss_detected=%d 
16,i,[ wlan_swbmiss_offload.c : 374 ] SWBMISS_RESYNC_ALL_VDEV: mac_id=%d 
15,ii,[ wlan_swbmiss_offload.c : 399 ] SWBMISS_RESYNC_ALL_VDEV: vdev id=%d HWBMISS %d 
14,i,[ wlan_swbmiss_offload.c : 321 ] SWBMISS_SWITCH_2_HWBMISS: vdev_id=%d 
13,ii,[ wlan_swbmiss_offload.c : 611 ] SWBMISS_TIMER_SET: vdev_id=%d, timeout_val=%d 
12,i,[ wlan_swbmiss_offload.c : 1203 ] wlan_swbmiss_update_bcn_stats mode %d 
11,i,[ wlan_swbmiss_offload.c : 332 ] *wlan_vdev_reset_beacon_stats vdev id %d 
10,ii,[ wlan_swbmiss_offload.c : 752 ] wlan_vdev_swbcn_evt_handler vdev id %d HWBMISS %d 
30,,[ wlan_hwbmiss_offload.c : 188 ] PMR error detected, disabling HWBMISS 
29,i,[ wlan_hwbmiss_offload.c : 103 ] HWBMISS_DISABLED: vdev_id=%d 
28,,[ wlan_hwbmiss_offload.c : 54 ] HWBMISS_ENABLED: [final_bmiss_detected=1] 
27,iiiiiiIi,[ wlan_hwbmiss_offload.c : 92 ] HWBMISS_ENABLED: vdev_id=%d, pre_bmiss_detected=%d, first_bmiss_detected=%d, final_bmiss_detected=%d, curr_bmiss_bcnt=%d, curr_listen_interval=%d, last_hwbmiss_enable_ts = 0x%x, cons_bmiss_count = %d  
26,iIIIII,[ wlan_hwbmiss_offload.c : 159 ] HWBMISS_SWITCH_2_SWBMISS: vdev_id=%d, hwbmiss_bcnt=%u, curr_ts = 0x%x %x , last_hwbmiss_enable_ts = 0x%x %x  
25,iiiiI,[ wlan_hwbmiss_offload.c : 167 ] HWBMISS_SWITCH_2_SWBMISS: cons_bmiss_count = %d, bmiss_threshold = %d curr_listen_interval = %d , bmiss_since_last_hwbmiss_enable = %d BI = 0x%x 
120,ii,[ wlan_dev.c : 5932 ] cbc calibration 0 data_ptr1:%d cbc_ena:%d 
119,,[ wlan_dev.c : 5936 ] cbc  calibration 1 
118,i,[ wlan_dev.c : 7248 ] ####5G CTL Subband feature enable, Sub band flag= %d #### 
117,i,[ wlan_dev.c : 7256 ] ####6G CTL Subband feature enable, Sub band flag= %d #### 
116,,[ wlan_dev.c : 7383 ] WMI_REQUEST_LINK_STATS_CMDID, ftm mode 
115,,[ wlan_dev.c : 7595 ] WMI_PDEV_SET_WMM_PARAMS_CMDID DEPRECATED - use VDEV level command instead 
114,,[ wlan_dev.c : 7646 ] wlan_pdev_set_param: Param WMI_PDEV_GREEN_AP_PS_ENABLE_CMDID is not handled 
113,,[ wlan_dev.c : 7798 ] wlan_pdev_resume_cmd: NOT expected to receive during wifi on 
112,i,[ wlan_dev.c : 7811 ] wlan_pdev_resume_cmd: NOT expected to receive during wifi on, mac id=%d 
111,,[ wlan_dev.c : 7958 ] WMI_REQUEST_LINK_STATS_CMDID, ftm mode 
110,,[ wlan_dev.c : 8001 ] WMI_START_LINK_STATS_CMDID, ftm mode 
109,,[ wlan_dev.c : 8014 ] WMI_CLEAR_LINK_STATS_CMDID, ftm mode 
108,iII,[ wlan_dev.c : 8161 ] WMI_LRO_CONFIG_CMDID 1 mac=%d en=%x flags=%x 
107,iii,[ wlan_dev.c : 8561 ] WMI_PDEV_SET_RAP_CONFIG_CMDID: pdev_id=%d, type=%d, sta_ps_detection_enabled=%d 
106,i,[ wlan_dev.c : 8567 ] WMI_PDEV_SET_RAP_CONFIG_CMDID: num_of_rap=%d 
105,IIII,[ wlan_dev.c : 8764 ] WMI_GPIO_CONFIG_CMDID: %x %x %x %x 
104,II,[ wlan_dev.c : 8834 ] WMI_GPIO_OUTPUT_CMDID: %x %x 
103,ii,[ wlan_dev.c : 3364 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   header length (%d) > %d 
102,ii,[ wlan_dev.c : 3374 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   data length (%d) > %d 
101,ii,[ wlan_dev.c : 3384 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   mac address length (%d) > %d 
100,ii,[ wlan_dev.c : 3395 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   capability length (%d) > %d 
99,ii,[ wlan_dev.c : 3415 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   total_length (%d) > %d 
98,ii,[ wlan_dev.c : 3451 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                    total_num_configured_element (%d) > %d 
97,ii,[ wlan_dev.c : 3462 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                    num_vendor_oui_ext (%d) > %d 
96,ii,[ wlan_dev.c : 3481 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                     total_num_of_configured_oui (%d) < %d 
95,ii,[ wlan_dev.c : 3493 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   num_of_oui_read %d and index of buf_data %d should be equal 
94,,[ wlan_dev.c : 3502 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                   oui_cmd_buff_length validation failed 
93,ii,[ wlan_dev.c : 3575 ] WMI_PDEV_CONFIG_VENDOR_OUI_ACTION_CMDID Error:                        curr_data_index (%d) > next_data_index %d 
92,iiii,[ wlan_dev.c : 2724 ] To serve %d peers %d TIDs is enough (TQM TIDs = %d, TQM BYPASS TIDs = %d) 
91,iiii,[ wlan_dev.c : 2731 ] To serve %d peers %d TIDs required (TQM TIDs = %d, TQM BYPASS TIDs = %d) 
90,iiiiii,[ wlan_dev.c : 10042 ] CCA_BUSY_MONITOR_CHECK_RECORD: mac_id = %d chan_mhz = %d, time_diff_us =%d, cca_busy_percent = %d,time_diff_us_thr = %d, cca_busy_perc_thr = %d 
89,ii,[ wlan_dev.c : 6364 ] wlan_dev_set_pcl not match pcl_cnt=%d,supp_chan_cnt=%d 
88,iii,[ wlan_dev.c : 6390 ] wlan_dev_set_pcl: cur_category %d: num_chans_in_category %d -> cur_idx %d 
87,i,[ wlan_dev.c : 6398 ] wlan_dev_set_pcl: num_chans=%d 
86,ii,[ wlan_dev.c : 9158 ] wlan_dev_unit_test: cmd = PDEV_SET_HW_MODE, hw_mode = %d, ret_status = %d 
85,i,[ wlan_dev.c : 9190 ] unit_test: sleep for %d ms 
84,I,[ wlan_dev.c : 9199 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_ABG_MODE_TX_CHAIN_NUM, value = 0x%x 
83,I,[ wlan_dev.c : 9212 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK, value=0x%x 
82,I,[ wlan_dev.c : 9221 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK, value=0x%x 
81,I,[ wlan_dev.c : 9231 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK_2G, value=0x%x 
80,I,[ wlan_dev.c : 9241 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK_2G, value=0x%x 
79,I,[ wlan_dev.c : 9251 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_TX_CHAIN_MASK_5G, value=0x%x 
78,I,[ wlan_dev.c : 9261 ] wlan_dev_unit_test: cmd = WMI_PDEV_PARAM_RX_CHAIN_MASK_5G, value=0x%x 
77,ii,[ wlan_dev.c : 9271 ] wlan_dev_unit_test: cca_busy_detector_config time_diff_threshold = %d us, cca_busy_percent_threshold = %d 
76,I,[ wlan_dev.c : 9345 ] error on wlan_log_save_module_level: mod_id=%u 
75,i,[ wlan_dev.c : 5214 ] wlan_get_beacon_reception_stats_process: vdev id %d  
74,i,[ wlan_dev.c : 5224 ] wlan_get_beacon_reception_stats_process: bcn_cnt %d  
73,I,[ wlan_dev.c : 5378 ] wlan_get_chip_power_stats: stats_capture->num_debug_register 0x%x 
72,iiii,[ wlan_dev.c : 423 ] GreenAP Curr Chainmask: %d/%d, Phy_mode: %d, bw[20/40/80/160]: %d 
71,iiiii,[ wlan_dev.c : 425 ] GreenAP saved tx/rx chainmask: %d/%d, phymode: %d, freq1: %d, valid flag: %d 
70,iii,[ wlan_dev.c : 427 ] GreenAP cur_channel mhz: %d, freq1: %d, freq2: %d 
69,Ii,[ wlan_dev.c : 10431 ] wlan_oem_phy_reg_dump_cmd: register data to dump, ptr%x, size%d 
68,,[ wlan_dev.c : 10439 ] wlan_oem_phy_reg_dump_cmd: Data is exceeding the maximum allowable limit 
67,iiii,[ wlan_dev.c : 10460 ] wlan_oem_phy_reg_dump_cmd: buff_size %d, event_size %d max: %d, no of bytes to be sent in the alloc event: %d 
66,ii,[ wlan_dev.c : 10465 ] wlan_oem_phy_reg_dump_cmd: max event size exceeded %d, max_limit %d 
65,i,[ wlan_dev.c : 10471 ] wlan_oem_phy_reg_dump_cmd: memory allocation failed, %d 
64,IIi,[ wlan_dev.c : 9730 ] wlan_pdev_get_hw_mode_transition_event: old_hw_idx=0x%x, new_hw_idx=0x%x, vdev_num=%d 
63,ii,[ wlan_dev.c : 10295 ] wlan_pdev_handle_get_channel_ani_cmd max_channel_limit %d, received_count %d 
62,i,[ wlan_dev.c : 10307 ] wlan_pdev_handle_get_channel_ani_cmd memory allocation failed, %d 
61,iii,[ wlan_dev.c : 10339 ] wlan_pdev_handle_get_channel_ani_cmd freq:%d, mac_id:%d, ani:%d 
60,i,[ wlan_dev.c : 10343 ] wlan_pdev_handle_get_channel_ani_cmd unsupported freq:%d 
59,iiiI,[ wlan_dev.c : 6812 ] pdev_id = %d: DMA %d push config status %d event %p 
58,ii,[ wlan_dev.c : 442 ] GreenAP wlan_pdev_set_greenap_cmd enable: %d, zero_client:%d 
57,I,[ wlan_dev.c : 6446 ] wlan_pdev_set_hw_mode: HW_Mode_Idx = 0x%x 
56,I,[ wlan_dev.c : 6471 ] wlan_pdev_set_hw_mode: DBSMGR_Ret_Status = 0x%x 
55,,[ wlan_dev.c : 6616 ] wlan_pdev_set_hw_mode_resp_event: WMI Event Alloc Failed!!! 
54,II,[ wlan_dev.c : 6656 ] wlan_pdev_set_hw_mode_resp_event: status=0x%x, cfg_hw_mode_idx=0x%x 
53,,[ wlan_dev.c : 6525 ] WMI_PDEV_SET_MAC_CONFIG_RESP_EVENT: WMI Event Alloc Failed!!! 
52,I,[ wlan_dev.c : 6542 ] WMI_PDEV_SET_MAC_CONFIG_RESP_EVENT: status=0x%x 
51,I,[ wlan_dev.c : 3693 ] wlan_pdev_set_param: Param WMI_PDEV_PARAM_TX_CHAIN_MASK 0x%x 
50,I,[ wlan_dev.c : 3745 ] wlan_pdev_set_param: Param WMI_PDEV_PARAM_RX_CHAIN_MASK 0x%x 
49,I,[ wlan_dev.c : 3771 ] wlan_pdev_set_param: WMI_PDEV_PARAM_TX_CHAIN_MASK_2G 0x%x 
48,I,[ wlan_dev.c : 3794 ] wlan_pdev_set_param: WMI_PDEV_PARAM_RX_CHAIN_MASK_2G 0x%x 
47,I,[ wlan_dev.c : 3817 ] wlan_pdev_set_param: WMI_PDEV_PARAM_TX_CHAIN_MASK_5G 0x%x 
46,I,[ wlan_dev.c : 3840 ] wlan_pdev_set_param: WMI_PDEV_PARAM_RX_CHAIN_MASK_5G 0x%x 
45,,[ wlan_dev.c : 4361 ] WMI_PDEV_PARAM_POWER_GATING_SLEEP setting 
44,,[ wlan_dev.c : 4637 ] PDEV_PARAM_RX_FILTER not supported 
43,I,[ wlan_dev.c : 4814 ] PDEV_PARAM_IOT_PATTERN=%08x 
42,,[ wlan_dev.c : 4929 ] PDEV_PARAM_GCMP_SUPPORT_ENABLE not handled in FW 
41,III,[ wlan_dev.c : 10718 ]  wlan_pdev_tsf_auto_report return detla too small, pdev_%x, delta(%x/%x) 
40,III,[ wlan_dev.c : 10729 ]  wlan_pdev_tsf_auto_report return in wow, pdev_%x, delta(%x/%x) 
39,,[ wlan_dev.c : 10750 ]  wlan_pdev_tsf_auto_report: no memory 
38,iiIIIIII,[ wlan_dev.c : 10783 ]  wlan_pdev_tsf_auto_report: vdev_id = %d, mac_id = %d, tsf_low = 0x%x(%u), qtimer_low=0x%x(%u),cur_delta_0x%x(%u) 
37,,[ wlan_dev.c : 7022 ] WMI_PDEV_UPDATE_PKT_ROUTING_CMDID SOC level command not valid
 
36,ii,[ wlan_dev.c : 3161 ] wlan_resync_imps: IMPS_ENABLED=%d, VDEV_UP_COUNT=%d 
35,,[ wlan_dev.c : 10113 ] DISPLAY_TPC_STATS:  Alloc tpc_configs_reg_event_buf failed
 
34,,[ wlan_dev.c : 10137 ] DISPLAY_TPC_STATS:  Alloc tgt_pwrs_event_buf failed
 
33,,[ wlan_dev.c : 10165 ] DISPLAY_TPC_STATS:  Alloc tgt_pwrs_set2_event_buf failed
 
32,,[ wlan_dev.c : 10194 ] DISPLAY_TPC_STATS:  Alloc ctl_event_buf failed
 
31,,[ wlan_dev.c : 10203 ] DISPLAY_TPC_STATS:  Allocation complete! 
179,,[ wlan_peer.c : 5717 ] Invalid sta_fixed_rate: Found CCK rate in 5G
 
178,IIIIIIII,[ wlan_peer.c : 5829 ] WMI_PEER_PARAM_DISABLE_AGGRESSIVE_TX:peer %x value %x mac_address %x:%x:%x:%x:%x:%x 
177,IIi,[ wlan_peer.c : 6286 ] Invalid CHAN_WIDTH_SWITCH: mac_addr31to0 = 0x%x, mac_addr47to32 = 0x%x, phy_mode %d 
176,,[ wlan_peer.c : 5734 ] Invalid sta_fixed_rate: Found CCK rate in 5G
 
175,iiIIiiII,[ wlan_peer.c : 4998 ] WLAN_PEER_ASSOC_REQ peer %d peer_assoc_evt %d, ni_flags 0x%x, valid_tx_chainmask 0x%x, peer_nss %d, phymode %d, ni_vht_mcs_set 0x%x, ni_legacy_rate_set 0x%x, 
174,ii,[ wlan_peer.c : 5018 ] WLAN_PEER_CHANGE_BW peerid %d  bw %d 
173,iii,[ wlan_peer.c : 5068 ] WLAN_PEER_CHANGE_NSS peer %d  peer_nss %d ul_nss %d 
172,ii,[ wlan_peer.c : 5101 ] WLAN_PEER_CHANGE_PHY_MODE peer %d  bw %d 
171,iIIiiII,[ wlan_peer.c : 5129 ] WLAN_PEER_CHANGE_CHAN_WIDTH peer %d ni_flags 0x%x, valid_tx_chainmask 0x%x, peer_nss %d, phymode %d, ni_vht_mcs_set 0x%x, ni_legacy_rate_set 0x%x, 
170,iIIIi,[ wlan_peer.c : 644 ] wal peer allocaton status = %d vdev_id_8/mac_id_8 = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d 
169,iIIIi,[ wlan_peer.c : 666 ] wal peer allocaton status = %d vdev_id_8/mac_id_8 = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x peer_type = %d 
168,,[ wlan_peer.c : 259 ] wlan_find_peer: NULL vdev 
167,iIIi,[ wlan_peer.c : 869 ] VDEV EVT:RESOURCE_PEER_FREE vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
166,iI,[ wlan_peer.c : 954 ] VDEV EVT PEER: wlan_free_peer del_resp=%d, wal_peer:0x%x 
165,iI,[ wlan_peer.c : 2567 ] HE160NSS : 160_mcs_nss_set %d, 160_mcs_nss_map %x 
164,II,[ wlan_peer.c : 6737 ] Deauth frame is not sent because of different RT thread addr1 0x%x addr2 = 0x%x 
163,I,[ wlan_peer.c : 4951 ] wlan_peer_mask_cck_rates_internal:wlan_peer 0x%x 
162,,[ wlan_peer.c : 2805 ] rc_node_update: ABORT 
161,III,[ wlan_peer.c : 2484 ] Assoc OMI: NSS=0x%x BW=0x%x er_su_disable=0x%x 
160,iiIIii,[ wlan_peer.c : 1701 ] peer_update status=%d,vdevid=%d,macaddr=0x%8x0x%4x peer_type=%d,req_peer_type=%d
 
159,IIII,[ wlan_peer.c : 4630 ] wal_vdev non_data_rc:0x%x bcast_data_rc:0x%x mcast_data_rc:0x%x beacon_rc:0x%x 
 
158,I,[ wlan_peer.c : 4652 ] wal_peer: %x, wlan_peer_vdev_restart_done: tearing down tx_ba and rx_ba 
157,II,[ wlan_peer.c : 4667 ] update non data1, peer:0x%x, rc:0x%x 
156,II,[ wlan_peer.c : 4676 ] update ofdm non data1, peer:0x%x, rc:0x%x 
155,II,[ wlan_peer.c : 4704 ] update rts_rix, peer:0x%x, rts_rix:0x%x 
154,i,[ wlan_peer.c : 5195 ] WMI_PEER_UNMAP_RESPONSE_CMDID: %d 
153,ii,[ wlan_peer.c : 5202 ] peer_id[%d]: %d 
152,I,[ wlan_peer.c : 2244 ] wlan_set_peer_he_txbf_cap:ax_txbf_caps.suax_max_nc=%x 
151,I,[ wlan_peer.c : 1422 ] wlan_set_peer_vht_txbf_cap vht_caps: %x 
150,III,[ wlan_peer.c : 1453 ] Nr=%x Nrx=%x, Nc=%x
 
149,IIII,[ wlan_peer.c : 1527 ] Nr=%x Nc=%x peer_nss=%x Ntx=%x 
148,iIIiii,[ wlan_peer.c : 468 ] RESOURCE_PEER_ALLOC error vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d, peer_type = %d, delete_in_process:%d 
147,I,[ wlan_peer.c : 3932 ] wlan_vdev_change_minimum_allowed_mcs: minimum_allowed_mcs 0x=%x 
146,,[ wlan_peer.c : 3090 ] PEER_ASSOC null vdev 
145,,[ wlan_peer.c : 3095 ] PEER_ASSOC null vdev->bss 
144,,[ wlan_peer.c : 3106 ] PEER_ASSOC null peer 
143,,[ wlan_peer.c : 3108 ] PEER_ASSOC null wal_peer 
142,IIiIIIii,[ wlan_peer.c : 3264 ] PEER_ASSOC cmd for mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x, num_peer_ht_rates=%d, ni_flags=0x%x phymode=0x%x nss=0x%x mpdudensity=%d max_mpdu=%d 
141,iI,[ wlan_peer.c : 3524 ] P2P: PEER_ASSOC: Update legacy RTS consecutive failure threshold = %d for OUI=0x%x 
140,IIIII,[ wlan_peer.c : 3022 ] PEER_ASSOC ni_legacy_rate_set= 0x%x ht_caps=0x%x vht_caps=0x%x vht_mcs_set=0x%x ht_mcs_set= 0x%x 
139,I,[ wlan_peer.c : 3041 ] Peer_assoc:peer_he_cap_phy = 0x%x 
138,II,[ wlan_peer.c : 3047 ] Peer_assoc: he_ops=0x%x he_cap_info_internal=0x%x 
137,IIIII,[ wlan_peer.c : 4190 ] wlan_vdev_dispatch_peer_change_bw:prev_ni_flags=%x new_ni_flags=%x new_bw = %x ht_caps = %x vht_caps = %x 
136,iII,[ wlan_peer.c : 1740 ] peer create cmd ingored vdev_id =%d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
 
135,II,[ wlan_peer.c : 1848 ] peer create command for mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
 
134,iII,[ wlan_peer.c : 1982 ] peer delete command for vdev_id %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
133,,[ wlan_peer.c : 1995 ] PEER_DELETE null vdev 
132,,[ wlan_peer.c : 2027 ] PEER_DELETE peer not exist, still generating PEER_DELETE_RESP_EVENTID 
131,IIII,[ wlan_peer.c : 4595 ] wlan_vdev_dispatch_peer_mask_cck_rates is-2g:0x%x rc_node:0x%x legacy_rate:0x%x  is_cck_rate_mask 0x%x 
130,,[ wlan_peer.c : 3896 ] RATE_DBG wlan_vdev_migrate_rate_reset peer_params NULL: peer_id 
129,,[ wlan_peer.c : 3901 ] RATE_DBG wlan_vdev_migrate_rate_reset: peer_id 
128,I,[ wlan_peer.c : 3861 ] wlan_vdev_peer_autorate_reset: user_start_rate 0x=%x 
127,I,[ wlan_peer.c : 4056 ] wlan_vdev_peer_change_bw_internal: new_bw = %x 
126,iI,[ wlan_peer.c : 3996 ] wlan_vdev_peer_change_phymode_internal: peerid %d phymode = %x 
125,I,[ wlan_peer.c : 4931 ] wlan_vdev_peer_mimo_ps_internal: valid_tx_chainmask 0x=%x 
124,II,[ wlan_peer.c : 4261 ] TXBF_UPDATE_PEER_PARAMS peer_nss = %u, nc_idx = %u. 
123,II,[ wlan_peer.c : 4270 ] TXBF_UPDATE_PEER_PARAMS peer_nss_160 = %u, nc_idx_160 = %u. 
122,,[ wlan_peer.c : 781 ] WMI_EVENT_ALLOC_FAILURE: WMI_PEER_DELETE_RESP_EVENTID buffer failure 
121,iiII,[ wlan_peer.c : 797 ] VDEV EVT:WMI_PEER_DELETE_RESP_EVENTID send vdevId=%d time=%d peer_macaddr31to0 =0x%x peer_macaddr47to32 =0x%x 
197,IIIII,[ wlan_mgmt_local_txrx.c : 2239 ] _wlan_local_send_peer_change_omi()invalid rx=0x%x bw=0x%x ulmu=0x%x tx=0x%x ulmu_data=0x%x
 
196,I,[ wlan_mgmt_local_txrx.c : 2254 ] _wlan_local_send_peer_change_omi()newOMI=0x%x 
195,III,[ wlan_mgmt_local_txrx.c : 1624 ] mac id mismatch:rx:%x vdev:%x, frame: %x
 
194,III,[ wlan_mgmt_local_txrx.c : 1768 ] mac id mismatch:rx:%x vdev:%x, frame: %x
 
193,IIIIIiII,[ wlan_mgmt_local_txrx.c : 530 ] MGMT_TXRX_SENT_FROM_LOCAL: macidh8/tid8/ptype16:0x%08x, cbflags=0x%08x, peerflag=0x%x,addr=0x%08x 0x%04x cur_chan=%d ppdu_H32=0x%x ppdu_L32=0x%x 
192,ii,[ wlan_mgmt_local_txrx.c : 637 ] MGMT_TXRX_SENT_FROM_LOCAL: send failure:%d, flags:%d 
191,I,[ wlan_mgmt_local_txrx.c : 2095 ] LOCAL MGMT DEAUTH-DISASSOC tx compl. status 0x%x 
190,IiI,[ wlan_mgmt_local_txrx.c : 908 ] _wlan_mgmt_local_send_nullfunc() get nullfunc failed: peer = %p peer_type = %d cb_flags: 0x%x 
189,IIIII,[ wlan_mgmt_local_txrx.c : 671 ] OMI: wlan_mgmt_txrx_send_omi rx_nss: 0x%lx, bw: 0x%lx, ulmu_disable: 0x%lx, ulmu_data_disable: 0x%lx, tx_nss: 0x%lx
 
188,IIIIIIII,[ wlan_mgmt_local_txrx.c : 1426 ] FORWARD_TO_HOST: mgmt pkt, Ch_VdevActCnt_ToHost=0x%08x MacId_Type_Subtype=0x%06x Seq=%04d(0x%03x) Addr2=0x%04x 0x%08x RssiComb_Ch0_Ch1=0x%06x monMode_emaSupp_compList=0x%06x 
187,IIiIIi,[ wlan_mgmt_local_txrx.c : 1455 ] FORWARD_TO_HOST: not mgmt pkt, Ch_VdevActCnt_ToHost=0x%08x MacId_Type_Subtype=0x%06x Seq=%d(0x%x) RssiComb_Ch0_Ch1=0x%06x sta_mon_mode=%d 
186,i,[ wlan_mgmt_local_txrx.c : 659 ] wlan_mgmt_txrx_omi_req_completion: set mu  as %d
 
185,II,[ wlan_mgmt_local_txrx.c : 717 ] setUnitTestCmd 13 9 1 %x %x - couldn't find peer! 
184,,[ wlan_mgmt_local_txrx.c : 732 ] Invalid input for OMI unit test.
 
183,,[ wlan_mgmt_local_txrx.c : 786 ] Invalid input for muedca unit test to set mu wmm params.
 
182,,[ wlan_mgmt_local_txrx.c : 818 ] Invalid input for muedca unit test to emulate trigger frm.
 
181,I,[ wlan_mgmt_local_txrx.c : 828 ] Unit test: mu edca enable = %lu
 
180,IIIIiI,[ wlan_mgmt_local_txrx.c : 728 ] OMI: Unit test with rx_nss = 0x%lx, bw = 0x%lx, ulmu disable = 0x%lx, tx_nss = 0x%lx, er_su disable %d, ulmu_data_disable = 0x%lx
 
214,IIi,[ wlan_mgmt_txrx.c : 396 ] _wlan_mgmt_rx_frame_handler Droping frame from non associated Peer type=0x%x subtype=0x%x bNull=%d 
213,IIii,[ wlan_mgmt_txrx.c : 1496 ] MGMT_TX_WMI_FROM_HOST is_home_8/is_curr_8=0x%x mode_8/submode_8=0x%x pmac->mac_id=%d e_mac_id=%d 
212,IIIi,[ wlan_mgmt_txrx.c : 1577 ] MGMT_TX_WMI_FROM_HOST subtype=0x%02x addr=0x%04x%08x chanfreq=%d 
211,iiIiIIiI,[ wlan_mgmt_txrx.c : 1582 ] MGMT_TX_WMI_FROM_HOST check_tag=%d tx_param_valid=%d cmd_ch=0x%x frame_len=%d tx_flags=0x%x desc_id=0x%x tid_num=%d ppdu_info=0x%x 
210,ii,[ wlan_mgmt_txrx.c : 2284 ] MGMT_TX_WMI_FROM_HOST register %d %d 
209,ii,[ wlan_mgmt_txrx.c : 2289 ] MGMT_TX_WMI_FROM_HOST register %d %d 
208,iii,[ wlan_mgmt_txrx.c : 2022 ] WMI TX comp hold,idx:%d, desc id=%d,comp=%d 
207,I,[ wlan_mgmt_txrx.c : 1725 ] WMI TX comp send bundle: bundle_evt_size:0x%x 
206,iii,[ wlan_mgmt_txrx.c : 1790 ] WMI TX comp send bundle, num:%d, desc id=%d comp=%d 
205,,[ wlan_mgmt_txrx.c : 1857 ] MGMT_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
204,,[ wlan_mgmt_txrx.c : 1863 ] MGMT_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
203,IIii,[ wlan_mgmt_txrx.c : 1907 ] MGMT_TX_WMI_FROM_HOST_COMP desc_id=0x%x tx_status=0x%x ppdu_id:%d ack_rssi=%d 
202,I,[ wlan_mgmt_txrx.c : 995 ] WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
201,I,[ wlan_mgmt_txrx.c : 908 ] WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
200,,[ wlan_mgmt_txrx.c : 1805 ] OFFCHAN_DATA_TX_WMI_TXCOMP_SEND_EVT PKT NULL 
199,II,[ wlan_mgmt_txrx.c : 1821 ] MGMT_TX_WMI_FROM_HOST_COMP desc_id=0x%x tx_status=0x%x 
198,IIIII,[ wlan_mgmt_txrx.c : 1348 ] MGMT_TX_WMI_FROM_HOST: dword0=0x%x dword1=0x%x, subtype:%x, ppdu_info:0x%x multiplier:0x%x 
251,iii,[ offload_mgr.c : 1969 ] OFLD drop wmi evt, id=%d, len:%d status:%d 
250,ii,[ offload_mgr.c : 342 ] OFLD dereg data name=%d vdev id=%d, vdev mask 
249,ii,[ offload_mgr.c : 384 ] OFLD dereg htt name=%d ref_cnt=%d 
248,ii,[ offload_mgr.c : 322 ] OFLD dereg nondata name=%d ref_cnt=%d 
247,ii,[ offload_mgr.c : 363 ] OFLD dereg wmi name=%d ref_cnt=%d 
246,,[ offload_mgr.c : 1251 ] drop data in wow awake 
245,I,[ offload_mgr.c : 1270 ] OFLD remote data hdlr dropping frame as L2_valid :%x 
244,,[ offload_mgr.c : 1279 ] OFLD remote data hdlr drop loop back frame! 
243,II,[ offload_mgr.c : 1286 ] OFLD remote data hdlr ds2ds, id:%x, mode:%x 
242,II,[ offload_mgr.c : 1293 ] OFLD remote data hdlr nonds, id:%x, mode:%x 
241,iiii,[ offload_mgr.c : 1302 ] OFLD remote data hdlr pktlen=%d, dataT=%d addrT=%d vdevId=%d 
240,iii,[ offload_mgr.c : 1365 ] OFLD enhanced data hdlr ofld id=%d status=%d, wow data state:%d 
239,I,[ offload_mgr.c : 2021 ] evt store:%x 
238,III,[ offload_mgr.c : 1754 ] _ofld_non_data_hdlr: peer = 0x%x addr1 0x%x addr2 = 0x%x 
237,II,[ offload_mgr.c : 1852 ] _ofld_nondata_hdlr: status_h8/sub_sts_8/ofld_id_16:0x%x frmtyp = 0x%x 
236,II,[ offload_mgr.c : 1939 ] _ofld_nondata_hdlr: status = 0x%x frmtyp = 0x%x 
235,ii,[ offload_mgr.c : 1415 ] OFLD proto data hdlr ret_Status=%d curr_wow=%d 
234,III,[ offload_mgr.c : 211 ] OFLD reg data name=0x%x, vdevid:0x%x, vdev_bitmap:0x%x 
233,ii,[ offload_mgr.c : 230 ] OFLD reg data vdev id=%d, max_len =%d 
232,II,[ offload_mgr.c : 286 ] OFLD reg HTT name=0x%x, refcnt:0x%x 
231,II,[ offload_mgr.c : 170 ] OFLD reg nondata name=0x%x, refcnt:0x%x 
230,II,[ offload_mgr.c : 248 ] OFLD reg wmi name=0x%x, refcnt:0x%x 
229,,[ offload_mgr.c : 1083 ] OFLD status hdlr: unable to handle this in status buf! HIF CPY 
228,iiii,[ offload_mgr.c : 1088 ] OFLD status hdlr pktlen=%d, dataT=%d addrT=%d vdevId=%d 
227,iiiI,[ offload_mgr.c : 1201 ] OFLD status hdlr ofld id=%d status=%d, route_type=%d, status_buf_flags:0x%x 
226,ii,[ offload_mgr.c : 2142 ] OFLD wmi evt flush evt_id=%d, evt_len=%d 
225,ii,[ offload_mgr.c : 2111 ] OFLD wmi evt store evt_id=%d, evt_len=%d 
224,,[ offload_mgr.c : 2116 ] ofld wmi evt store failure - no memory 
223,Iiiii,[ offload_mgr.c : 650 ] OFLD data parse 11c_snap_hdr_t exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d,dsDir:%d 
222,Iiii,[ offload_mgr.c : 697 ] OFLD data parse llc_snap_hdr_t exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
221,i,[ offload_mgr.c : 713 ] Unknown RX Decap mode %d 
220,Iiii,[ offload_mgr.c : 767 ] OFLD data parse IP_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
219,Iiii,[ offload_mgr.c : 783 ] OFLD data parse IP6_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
218,Iiii,[ offload_mgr.c : 815 ] OFLD data parse TCP_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
217,Iiii,[ offload_mgr.c : 828 ] OFLD data parse UDP_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
216,Iiii,[ offload_mgr.c : 840 ] OFLD data parse ICMPV6_HDR exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
215,Iiii,[ offload_mgr.c : 680 ] OFLD data parse ether_header exceeds frame length pktbuf:%x,rx_mode:%d,buf_len:%d,offset:%d 
262,,[ channel_mgr.c : 103 ] chan mgr pause complete timeout!!! 
261,ii,[ channel_mgr.c : 115 ] CHAN_MANAGER_SM_EVENT: %d < %d
 
260,II,[ channel_mgr.c : 304 ] CHAN_MGR_CTS2S_TX_COMP: status = 0x%x ch_handle = 0x%x 
259,II,[ channel_mgr.c : 271 ] CHAN_MGR_PAUSE_CMPL_CB: status = 0x%x curr_time = 0x%x 
258,iIIiI,[ channel_mgr.c : 208 ] CHAN_MGR_VDEV_PAUSE: chan = %d link = 0x%x flg = 0x%x max_sw_time = %d curr_time = 0x%x 
257,III,[ channel_mgr.c : 175 ] CHAN_MANAGER_SM_EVENT_DATA: chan = 0x%x sec_chan = 0x%x sw_time = 0x%x 
256,iiIIIIi,[ channel_mgr.c : 475 ] CHAN_MGR_TRIGGER_CHANNEL_CHANGE: pri_ch = %d, chan_change_dur = %d,is_chm_valid = 0x%x tx_chm = 0x%x, rx_chm = 0x%x, selfgen_chm = 0x%x, pf_cnt = %d 
255,iiIIIIi,[ channel_mgr.c : 597 ] CHAN_MGR_TRIGGER_CHANNEL_CHANGE: sec_ch = %d, chan_change_dur = %d,is_chm_valid = 0x%x tx_chm = 0x%x, rx_chm = 0x%x, selfgen_chm = 0x%x, pf_cnt = %d 
254,iiiii,[ channel_mgr.c : 850 ] CHAN_MGR_TRIGGER_HW_MODE_CHANGE: Cur_HW_Mode = %d, Next_HW_Mode = %d,pri_ch = %d, sec_ch = %d, HW_Mode_Switch_Dur = %d 
253,IIII,[ channel_mgr.c : 919 ] RESMGR_DELIVER_EVT: type = 0x%x, old_hw_mode = 0x%x, new_hw_mode = 0x%x, band_to_mac = 0x%x 
252,iII,[ channel_mgr.c : 242 ] CHAN_MGR_VDEV_UNPAUSE:chan =%d link =0x%x curr_time = 0x%x 
267,ii,[ channel_mgr_sm.c : 134 ] CHAN_MANAGER_SM: %d => %d 
266,III,[ channel_mgr_sm.c : 132 ] RESMGR_CHMGR_SEND_CTS2SELF: cur_vc = 0x%x link = 0x%x status = 0x%x 
265,ii,[ channel_mgr_sm.c : 115 ] CHAN_MANAGER_SM_EVENT: %d < %d
 
264,ii,[ channel_mgr_sm.c : 205 ] CHAN_MGR_PAUSE: PF %d, time %d 
263,ii,[ channel_mgr_sm.c : 261 ] CHAN_MGR_UNPAUSE: PF %d, time %d 
277,II,[ resmgr.c : 100 ] RESMGR_OCS_INVALID_QUOTA Different MAC: chan0 = 0x%x chan1 = 0x%x 
276,II,[ resmgr.c : 153 ] RESMGR_OCS_INVALID_LATENCY Different MAC: chan0 = 0x%x chan1 = 0x%x 
275,II,[ resmgr.c : 562 ] RESMGR_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x not found!!! 
274,II,[ resmgr.c : 568 ] RESMGR_DEREG_EVT_HDLR:  handler = 0x%x arg = 0x%x deregistered 
273,II,[ resmgr.c : 526 ] RESMGR_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x exists!!! 
272,II,[ resmgr.c : 534 ] RESMGR_REG_EVT_HDLR: handler = 0x%x arg = 0x%x no memory!!! 
271,II,[ resmgr.c : 544 ] RESMGR_REG_EVT_HDLR:  handler = 0x%x arg = 0x%x registered 
270,III,[ resmgr.c : 364 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
269,III,[ resmgr.c : 386 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
268,III,[ resmgr.c : 372 ] RESMGR_OCS_REQ_QUOTA_STATS  arg = 0x%x chan_mhz = 0x%x req_chan_time/latency = 0x%x 
283,i,[ resmgr_ocm.c : 351 ] RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d 
282,I,[ resmgr_ocm.c : 511 ] OCM_Migrate: migrate_mode = 0x%x 
281,II,[ resmgr_ocm.c : 568 ] OCM_Resume: ocs_cfg = 0x%x, Pause_OCS = 0x%x 
280,II,[ resmgr_ocm.c : 440 ] OCM_Suspend: Pause_Pending = 0x%x, Pause_OCS = 0x%x 
279,ii,[ resmgr_ocm.c : 645 ] resmgr_ocm_update_ocs_min_cat_dur: ocs_ins = %d, min_cat_dur = %d 
278,,[ resmgr_ocm.c : 283 ] RESMGR_OCS_CHAN_CHANGE_PROGRESS FAILURE 
287,iiii,[ resmgr_dyn_sch.c : 184 ] RESMGR_DYN_SCH_TOT_UTIL_PER  chan0_mhz = %d chan0_util_percentage = %d chan1_mhz = %d chan1_util_percentage = %d 
286,iiii,[ resmgr_dyn_sch.c : 250 ] RESMGR_DYN_SCH_HOME_CH_QUOTA  chan0_mhz = %d ch0_new_quota = %d chan1_mhz = %d ch1_new_quota = %d 
285,II,[ resmgr_dyn_sch.c : 357 ] RESMGR_DYN_SCH_ENABLE  enable = 0x%x fw_disable_bmap = 0x%x 
284,i,[ resmgr_dyn_sch.c : 88 ] RESMGR_DYN_SCH_ACTIVE  is_active = %d 
318,IIiii,[ resmgr_ocs.c : 4704 ] RESMGR_OCS_CHREQ_CREATE: req_id = 0x%x chan_req_addr = 0x%x chan_mhz = %d, sec_chan_mhz = %d prioirty = %d  
317,IiiIiI,[ resmgr_ocs.c : 4710 ] RESMGR_OCS_CHREQ_CREATE: start_tsf = 0x%x duration_usec = %d interval = %d dtim_start_tsf = 0x%x dtim_period = %d end_tsf = 0x%x 
316,IiI,[ resmgr_ocs.c : 4735 ] CHREQ_DELETE: chreq=0x%x chan=%d req_id(1)|state(1)|sec_chan(2)=0x%08x 
315,III,[ resmgr_ocs.c : 5101 ] CHREQ_START: chreq=0x%x chan(2)|sec_chan(2)=0x%08x req_id(1)|prio(1)|freq2(2)=0x%08x 
314,IiiIiI,[ resmgr_ocs.c : 5106 ] CHREQ_START: start_tsf=0x%x dur_usec=%d interval=%d dtim_start_tsf=0x%x dtim_period=%d end_tsf=0x%x 
313,IiI,[ resmgr_ocs.c : 5168 ] CHREQ_STOP: chreq=0x%x chan=%d req_id(1)|state(1)|sec_chan(2)=0x%08x 
312,IIIiiIII,[ resmgr_ocs.c : 4915 ] CHREQ_UPDATE: chreq=0x%x chan(2)|sec_chan(2)=0x%08x start_tsf=0x%x dur_usec=%d interval=%d req_id(1)|prio(1)|dtim_period(2)=0x%08x dtim_start_tsf=0x%x end_tsf=0x%x  
311,i,[ resmgr_ocs.c : 4547 ] RESMGR_OCS_ALLOCRAM_SIZE  size_in_bytes = %d 
310,i,[ resmgr_ocs.c : 2920 ] RESMGR_OCS_WIN_CAT_DUR  duration = %d 
309,IIIIiIII,[ resmgr_ocs.c : 574 ] CHREQ_UPDATE chreq=0x%x chan(2)|sec_chan(2)=0x%08x start_tsf=0x%x dur_usec=0x%x interval=%d req_id(1)|prio(1)|purge(1)|dtim_period(1)=0x%08x dtim_start_tsf=0x%x, end_tsf=0x%x 
308,,[ resmgr_ocs.c : 4479 ] RESMGR_OCS_CH_SWITCH_REQ 
307,II,[ resmgr_ocs.c : 3641 ] RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
306,IIi,[ resmgr_ocs.c : 3682 ] RESMGR_OCS_CHREQ_TERMINATE: req_id = 0x%x cur_ch_req = 0x%x state = %d 
305,IIIII,[ resmgr_ocs.c : 4391 ] RESMGR_OCS_RESOURCES  req_id = 0x%x ch_req_addr = 0x%x ch_alloc_addr = 0x%x state = 0x%x priority = 0x%x 
304,iii,[ resmgr_ocs.c : 4394 ] RESMGR_OCS_RESOURCES chan_mhz = %d sec_chan_mhz = %d, band_center_freq2 = %d 
303,II,[ resmgr_ocs.c : 135 ] CHREQ_GRANT cur_time=0x%x chreq=0x%x 
302,II,[ resmgr_ocs.c : 721 ] RESMGR_OCS_CHREQ_COMPLETE  curr_time = 0x%x ch_req_addr = 0x%x 
301,i,[ resmgr_ocs.c : 5204 ] RESMGR_OCS_CHANNEL_SWITCHED  status = %d 
300,i,[ resmgr_ocs.c : 5353 ] RESMGR_OCS_NEXT_SCH_INTERVAL = %d 
299,ii,[ resmgr_ocs.c : 5008 ] RESMGR_OCS_RECAL_QUOTAS  num_home_chans = %d tracking_interval = %d 
298,ii,[ resmgr_ocs.c : 5055 ] RESMGR_OCS_RECAL_QUOTAS  chan_mhz = %d latency = %d 
297,iii,[ resmgr_ocs.c : 5062 ] RESMGR_OCS_ALLOCATED_QUOTA_STATS  chan_mhz = %d req_chan_time_percentage = %d chan_time_quota = %d 
296,i,[ resmgr_ocs.c : 3038 ] RESMGR_OCS_RECOMPUTE_SCHEDULE: ocs_ins = %d 
295,i,[ resmgr_ocs.c : 3044 ] RESMGR_OCS %d has been paused 
294,I,[ resmgr_ocs.c : 385 ] RESMGR_OCS_CURR_CAT_WINDOW: Channel change pending, flags = 0x%x 
293,iII,[ resmgr_ocs.c : 3863 ] OCS_INVOKED: ins=%d last_entry=0x%x cur_time=0x%x 
292,I,[ resmgr_ocs.c : 4000 ] RESMGR_OCS_TSF_TIMEOUT_US defer_sch_time = %x 
291,I,[ resmgr_ocs.c : 4069 ] RESMGR_OCS_TSF_TIMEOUT_US next_tsftime = %x 
290,I,[ resmgr_ocs.c : 4081 ] RESMGR_OCS_NEXT_TSFTIME  next_tsf_time = 0x%x 
289,iii,[ resmgr_ocs.c : 4112 ] RESMGR_OCS_TSF_TIMEOUT_US wake up latency = %d, wlan_chan_num = %d, wlan_cb_num = %d 
288,i,[ resmgr_ocs.c : 4125 ] TSF_TIMEOUT_US  timeout_us=%d 
323,,[ resmgr_vcm.c : 48 ] RESMGR_CREATE_LINK failed due to invalid channel param 
322,IIiiii,[ resmgr_vcm.c : 140 ] RESMGR_LINK_CREATE link_pointer = 0x%x link_flags = 0x%x ch_mhz = %d phy_mode = %d band_center_freq1 = %d band_center_freq2 = %d 
321,I,[ resmgr_vcm.c : 153 ] RESMGR_LINK_DELETE  Link Pointer = 0x%x 
320,,[ resmgr_vcm.c : 268 ] RESMGR_UPDATE_LINK failed due to invalid channel param 
319,I,[ resmgr_vcm.c : 820 ] VCM_Init:  VC Pool Size = 0x%x 
333,iII,[ virtual_channel.c : 397 ] RESMGR_VC_UPDATE_HOME_CHAN_INFO: mac_id = %d virtual_chan_count = 0x%x home_chan_count = 0x%x 
332,iiIIiiII,[ virtual_channel.c : 474 ] RESMGR_ADD_LINK ch_mhz = %d phy_mode = %d link_flags = 0x%x link_valid_attr = 0x%x no_160_link_cnt = %d 160_link_cnt = %d vc = 0x%x link = 0x%x 
331,iIIIIi,[ virtual_channel.c : 276 ] RESMGR_VC_INIT_VIR_CHAN: chan_mhz = %d, mac_id = 0x%x, band = 0x%x, tx_chm = 0x%x, rx_chm = 0x%x, rx_nss = %d 
330,i,[ virtual_channel.c : 314 ] RESMGR_VC_INIT_HOME_CHAN: chan_mhz = %d 
329,iI,[ virtual_channel.c : 610 ] RESMGR_OCS_REQ_QUOTA_STATS chan_mhz = %d req_chan_time/latency = 0x%x 
328,iiiiII,[ virtual_channel.c : 793 ] RESMGR_VC_REGISTER_LINK: chan_mhz = %d link_count = %d ephemeral_link_count = %d is_home_chan = %d link_flags = 0x%x link_valid_attr = 0x%x 
327,iiIIii,[ virtual_channel.c : 511 ] RESMGR_RMV_LINK ch_mhz = %d phy_mode = %d link_flags = 0x%x link_valid_attr = 0x%x no_160_link_cnt = %d 160_link_cnt = %d 
326,III,[ virtual_channel.c : 990 ] !cts2s_sent: 0x%x 0x%x 0x%x 
325,iiii,[ virtual_channel.c : 815 ] RESMGR_VC_UNREGISTER_LINK: chan_mhz = %d link_count = %d ephemeral_link_count = %d is_home_chan = %d 
324,i,[ virtual_channel.c : 671 ] RESMGR_VC_UPDATE_CUR_VC  chan_mhz = %d 
339,ii,[ virtual_channel_arbiter.c : 689 ] VC_HW_CHM_UPDATE rx_chm = %d, tx_chm = %d 
338,iiii,[ virtual_channel_arbiter.c : 695 ] VC_NSS_SELFGEN_CHM_UPDATE nss1_tx_chm = %d, nss2_tx_chm = %d, nss3_tx_chm = %d, selfgen_chm = %d 
337,iiii,[ virtual_channel_arbiter.c : 701 ] VC_ABG_CHM_UPDATE nss_11b = %d, nss_ofdm = %d, selfgen_11b = %d, selfgen_ofdm = %d 
336,ii,[ virtual_channel_arbiter.c : 600 ] wlan_virtual_chan_apply_vc_chainmask  rx = %d tx = %d 
335,iiiiiI,[ virtual_channel_arbiter.c : 1130 ] RESMGR_VC_ARBITRATE_ATTRIBUTES arbitrated silent_num_chains = %d, num_tx_chains = %d, num_rx_chains = %d, num_tx_chains_b = %d, num_tx_chains_ag = %d, pref_chainmask = 0x%x 
334,iii,[ virtual_channel_arbiter.c : 1186 ] VC_ARB_SMPS: mhz = %d, smps_supp = %d, dyn_smps = %d 
366,iIii,[ resmgr_dbsmgr.c : 1495 ] DBSMGR: Notify HW Mode, fake_hw_mode_change = %d, HW_Mode_Pending_Bitmask = 0x%x, Cur_HW_Mode = %d, cur_dbs_cfg = %d 
365,iI,[ resmgr_dbsmgr.c : 1506 ] DBSMGR: Notify fake HW Mode, reason = %d, handler = 0x%p 
364,iI,[ resmgr_dbsmgr.c : 1576 ] DBSMGR: Notify HW Mode, requestor = %d, cb = 0x%p 
363,,[ resmgr_dbsmgr.c : 1218 ] DBSMGR_UPDATE_ALLOWED_SCAN_POLICY: Scan Disallowed due to CAC in Progress 
362,I,[ resmgr_dbsmgr.c : 1781 ] DBSMGR_CHM_NOTIF: event_type = 0x%x 
361,,[ resmgr_dbsmgr.c : 1849 ] DBSMGR: use custom DBS tx chain mask 
360,ii,[ resmgr_dbsmgr.c : 321 ] DBSMGR_SM_EVENT: %d < %d 
359,iiiII,[ resmgr_dbsmgr.c : 421 ] DBSMGR: dbsmgr_set_hw_mode requestor = %d, hw_mode_switch_aborted = %d,fake_hw_mode_change_ongoing = %d, set_hw_mode_pending_bitmask = 0x%x, handler=0x%p 
358,iiii,[ resmgr_dbsmgr.c : 474 ] DBSMGR: dbsmgr_set_hw_mode final_hw_mode = %d, cur_hw_mode = %d cur_dbs_cfg = %d next_hw_mode = %d 
357,iii,[ resmgr_dbsmgr.c : 538 ] DBSMGR: dbsmgr_set_hw_mode Start SM DBSMGR_EVENT_HW_MODE_CHANGE_REQUESTcur_hw_mode = %d cur_dbs_cfg_state = %d next_hw_mode = %d 
356,iiiii,[ resmgr_dbsmgr.c : 171 ] DBSMGR: use_default_tx_chain:%d, use_default_tx_chain_next_time:%d, requestor:%d, is_2g_vdev_active:%d, is_5g_vdev_active:%d 
355,i,[ resmgr_dbsmgr.c : 1977 ] DBSMGR: cancel fake hw mode change, reason = %d 
354,ii,[ resmgr_dbsmgr.c : 1685 ] DBSMGR_Change_Scan_State: Cur_Scan_State = %d, New_Scan_State = %d 
353,II,[ resmgr_dbsmgr.c : 1436 ] DBSMGR: LFR Set HW Mode, Cur_HW_Mode = 0x%x, New_HW_Mode Requested = 0x%x 
352,IIIiiiiI,[ resmgr_dbsmgr.c : 2408 ] DBSMGR_RECOMPUTE_SCAN_POLICY: policy_priority_bitmap = 0x%x (policy_allow = 0x%x), unwanted_policy_bitmap = 0x%x, vdev_index = %d, chan_index = %d, is_reliable_scan = %d, hw_mode = %d, conc_scan_cfg = 0x%x 
351,II,[ resmgr_dbsmgr.c : 638 ] DBS_MGR_UNREG_SCAN_POLICY_HDL: handler = 0x%x arg = 0x%x not found 
350,II,[ resmgr_dbsmgr.c : 644 ] DBS_MGR_UNREG_SCAN_POLICY_HDL handler = 0x%x arg = 0x%x 
349,II,[ resmgr_dbsmgr.c : 593 ] DBS_MGR_REG_SCAN_POLICY_HDL: handler = 0x%x arg = 0x%x Exists!! 
348,,[ resmgr_dbsmgr.c : 601 ] DBS_MGR_REG_SCAN_POLICY_HDL: Pool Empty!! 
347,II,[ resmgr_dbsmgr.c : 611 ] DBS_MGR_REG_SCAN_POLICY_HDL:  handler = 0x%x arg = 0x%x 
346,iI,[ resmgr_dbsmgr.c : 1897 ] DBSMGR: connection_in_progress=%d, conn_in_progress_bitmap=0x%x 
345,i,[ resmgr_dbsmgr.c : 2796 ] dbsmgr etm log is enable: %d
 
344,i,[ resmgr_dbsmgr.c : 1945 ] DBSMGR: set fake hw mode, reason = %d 
343,,[ resmgr_dbsmgr.c : 1951 ] DBSMGR: set fake hw mode fail, no buffer 
342,,[ resmgr_dbsmgr.c : 2784 ] DBSMGR: resmgr_dbsmgr_set_vdev_stop 
341,IIi,[ resmgr_dbsmgr.c : 1358 ] DBSMGR: Policy Mgr Set HW Mode, Cur_HW_Mode = 0x%x, New_HW_Mode Requested = 0x%x, roam_in_progress = %d 
340,IIIi,[ resmgr_dbsmgr.c : 1637 ] DBSMGR_UPDATE_MAC_CFG: conc_scan_cfg = 0x%x, fw_mode_cfg = 0x%x, hw_mode_pending = 0x%x, cur_hw_mode = %d 
373,ii,[ resmgr_dbsmgr_sm.c : 351 ] DBSMGR_SM:  %d => %d 
372,iiii,[ resmgr_dbsmgr_sm.c : 935 ] DBSMGR HW Mode change after Calibration: cur_hw_mode = %d, mac0_channel_mhz = %d, mac1_channel_mhz = %d, Loopback_Calibration_Dur = %d 
371,iii,[ resmgr_dbsmgr_sm.c : 566 ] DBSMGR_HW_Mode_Switch_Complete: Prev_HW_Mode = %d, Cur_HW_Mode = %d, HW_Mode_Switch_Dur = %d 
370,ii,[ resmgr_dbsmgr_sm.c : 607 ] DBSMGR: need_change_hw_mode:%d, need_change_tx_chain_mask:%d 
369,ii,[ resmgr_dbsmgr_sm.c : 321 ] DBSMGR_SM_EVENT: %d < %d 
368,i,[ resmgr_dbsmgr_sm.c : 1020 ] switch hw mode complete: PAGE_FAULT_COUNTER: %d
 
367,i,[ resmgr_dbsmgr_sm.c : 1058 ] switch hw mode start: PAGE_FAULT_COUNTER: %d
 
406,iIIii,[ resmgr_chainmask_mgr.c : 1507 ] RESMGR_CHMMGR_CALC_PERVC_T1_CHM: chan_mhz = %d, tx_chainmask = 0x%x, rx_chainmask = 0x%x, hw_chm_changed = %d, chm_change_state = %d 
405,iIIIi,[ resmgr_chainmask_mgr.c : 1544 ] RESMGR_CHMMGR_CALC_PERVC_T2_CHM: chan_mhz = %d, nss1_chainmask = 0x%x, nss1_chainmask = 0x%x, selfgen_chainmask = 0x%x, tx_chm_changed = %d 
404,IIII,[ resmgr_chainmask_mgr.c : 1551 ] RESMGR_CHMMGR_CALC_ABG_CHM: 11b_nss_tx = 0x%x, ofdm_nss_tx = 0x%x, 11b_selfgen = 0x%x, ofdm_selfgen = 0x%x 
403,iiIi,[ resmgr_chainmask_mgr.c : 1817 ] RESMGR_CHMMGR_SMPS_CB: mac_id = %d, vc_mhz = %d, smps_pending_bitmask = 0x%x, smps_status = %d 
402,III,[ resmgr_chainmask_mgr.c : 463 ] RESMGR_CHMMGR_CHAINMASK_CHANGE_REQ: cli_type = 0x%x, client_id = 0x%x, req_id = 0x%x 
401,Ii,[ resmgr_chainmask_mgr.c : 1700 ] RESMGR_CHMMGR_INITIATE_VC_OPS: state = 0x%x, chm_ctx->hw_mode_change_pending = %d 
400,I,[ resmgr_chainmask_mgr.c : 1764 ] SMPS operation failed. status = 0x%x 
399,ii,[ resmgr_chainmask_mgr.c : 1737 ] RESMGR_CHMMGR_INITIATE_VC_OPS: mac_id = %d, cur_vc_mhz = %d 
398,iIIi,[ resmgr_chainmask_mgr.c : 1747 ] RESMGR_CHMMGR_NOTIF_SMPS: vc_mhz = %d, new_chainmask = 0x%x, bandwidth = 0x%x, finish_timeout_ms = %d 
397,,[ resmgr_chainmask_mgr.c : 1908 ] RESMGR_CHMMGR_WAL_OPS: HW mode mismatch between DBS_req_hw_mode and soc_hw_mode 
396,iiii,[ resmgr_chainmask_mgr.c : 1923 ] RESMGR_CHMMGR_WAL_OPS: mac_id = %d, cur_mhz = %d,hw_chm_changed = %d, tx_chm_changed = %d 
395,IIIII,[ resmgr_chainmask_mgr.c : 1948 ] RESMGR_CHMMGR_WAL_OPS: tx_chainmask = 0x%x, rx_chainmask = 0x%xnss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chainmask = 0x%x 
394,IIII,[ resmgr_chainmask_mgr.c : 1955 ] RESMGR_CHMMGR_WAL_OPS: 11b_nss_tx = 0x%x, ofdm_nss_tx = 0x%x, 11b_selfgen = 0x%x, ofdm_selfgen = 0x%x 
393,ii,[ resmgr_chainmask_mgr.c : 2012 ] RESMGR_CHMMGR_NOTIFY_ALL_T1_CLIENTS: Client_ID = %d, Resp_ID = %d  
392,i,[ resmgr_chainmask_mgr.c : 2024 ] RESMGR_CHMMGR_NOTIFY_INITIAL_HW_CHM_T2_CLIENTS: Client_ID = %d 
391,ii,[ resmgr_chainmask_mgr.c : 2037 ] RESMGR_CHMMGR_NOTIFY_T1_REQESTER: cli_id = %d, req_id = %d 
390,ii,[ resmgr_chainmask_mgr.c : 2063 ] RESMGR_CHMMGR_NOTIFY_ALL_T2_CLIENTS: Client_ID = %d, Resp_ID = %d 
389,ii,[ resmgr_chainmask_mgr.c : 2076 ] RESMGR_CHMMGR_NOTIFY_T2_REQESTER: cli_id = %d, req_id = %d 
388,,[ resmgr_chainmask_mgr.c : 553 ] RESMGR_CHMMGR_NOTIFY_INIT_CHM 
387,IIiII,[ resmgr_chainmask_mgr.c : 623 ] RESMGR_CHMMGR_NOTIF_VDEV_UP: chan_mhz = 0x%x, hw_rx_chm = 0x%x, rx_nss = %d, new_rx_chm = 0x%x, bandwidth = 0x%x 
386,i,[ resmgr_chainmask_mgr.c : 2108 ] RESMGR_CHMMGR_POST_PROCESS: error_code = %d 
385,iiIIi,[ resmgr_chainmask_mgr.c : 2178 ] RESMGR_CHMMGR_DB_UPDATE: mac = %d, band = %d, tx_chm = 0x%x, rx_chm = 0x%x RX_NSS = %d 
384,IIII,[ resmgr_chainmask_mgr.c : 2185 ] RESMGR_CHMMGR_DB_UPDATE: nss1_tx_chm = 0x%x, nss2_tx_chm = 0x%x, selfgen_chm = 0x%x, bandwidth = 0x%x 
383,I,[ resmgr_chainmask_mgr.c : 799 ] RESMGR_CHMMGR_PROCESS_CHM_CHANGE_REQ: chm_state = 0x%x 
382,Ii,[ resmgr_chainmask_mgr.c : 1870 ] RESMGR_CHMMGR_PROTO_CHANGES_COMP: chm_ctx_state = 0x%x, hw_mode_pending = %d 
381,iii,[ resmgr_chainmask_mgr.c : 345 ] RESMGR_CHMMGR_REGISTER: client_id = %d, cli_type = %d, client_idx = %d 
380,iiI,[ resmgr_chainmask_mgr.c : 1037 ] RESMGR_CHMMGR_RESOLVE_BANDWIDTH: band = %d, mac = %d, max_bandwidth = 0x%x 
379,iiiIIiI,[ resmgr_chainmask_mgr.c : 1129 ] RESMGR_CHMMGR_RESOLVE_T1: mac_id = %d, band = %d, t1_cli_id = %d, tx_chainmask = 0x%x, rx_chainmask = 0x%x, res_rx_nss = %d, disable_ul_mu = 0x%x 
378,iiIII,[ resmgr_chainmask_mgr.c : 1222 ] RESMGR_CHMMGR_RESOLVE_T2: band = %d, mac = %d, nss1_tx_chainmask = 0x%x, nss2_tx_chainmask = 0x%x, selfgen_chainmask = 0x%x 
377,I,[ resmgr_chainmask_mgr.c : 2265 ] RESMGR_CHMMGR_SCHEDULE: chm_state = 0x%x 
376,i,[ resmgr_chainmask_mgr.c : 2805 ] RESMGR_CHMMGR_SEND_HW_MODE_PRE_NOTIF: event.resp_id = %d 
375,i,[ resmgr_chainmask_mgr.c : 2321 ] RESMGR_CHMMGR_SMPS_OP_COMPLETE_TIMEOUT: smps_pending_bitmask = %d 
374,iii,[ resmgr_chainmask_mgr.c : 388 ] RESMGR_CHMMGR_UNREGISTER: client_id = %d, cli_type = %d, client_idx = %d 
408,IIIi,[ resmgr_concurrency_mgr.c : 259 ] _resmgr_concurrency_mgr_is_low_freq_vdev_chreq_apply:  active_sta_vdev_num = 0x%x, active_vdev_num = 0x%x, resmgr_nan_discovery_enable = 0x%x, result = %d 
407,I,[ resmgr_concurrency_mgr.c : 338 ] resmgr_concurrency_mgr_notify:  module = 0x%x 
426,iiiiiii,[ wlan_scan.c : 1341 ] SCAN_ENG_CALC_CHAN num_2g = %d num_5g_active = %d (num_5g_low_act_ch = %d) num_5g_passive = %d double_passive_chan_scan = %d num_6g_ch = %d num_extra_6g_ch = %d 
425,IIII,[ wlan_scan.c : 1369 ] SCAN_ENG_SPOOFED_MAC_ADDR full_mac_addr = %08x%04x partial_mac_addr = %08x%04x 
424,IIIIIiii,[ wlan_scan.c : 772 ] SCAN_ENG_START scan_id = 0x%x eng_id(3)|req_type(3) = %06d num_chans_[req(3)|granted_2g(3)|granted_5g(3)] = %09d num_[ssid(3)|bssid(3)] = %06d flags = 0x%x vdev_freq = %d cur_ch_idx_2g|5g = %d %d 
423,iiiiii,[ wlan_scan.c : 784 ] SCAN_ENG_PARAM_1 dwell_time_active = %d dwell_time_active_2g = %d msec dwell_time_passive = %d msec min_rest_time = %d msec max_rest_time = %d msec max_scan_time = %d msec 
422,iiiiiii,[ wlan_scan.c : 795 ] SCAN_ENG_PARAM_2 idle_time = %d msec repeat_probe_time = %d msec probe_spacing_time = %d msec probe_delay = %d msec burst_duration = %d msec max_num_probes(2g|5g) = %d cancel_probe_req_defer = %d 
421,iiii,[ wlan_scan.c : 1500 ] SCAN_ADJUST_PARAM active=%d active_2g=%d passive=%d rest=%d 
420,IIIIIii,[ wlan_scan.c : 204 ] CHANNEL_CONGESTION_PRINTS cycle_cnt = %10u, busy = %10u, tx = %10u, rx = %10u, mr_rx = %10u, chan_freq= %d send_stats:%d 
419,iiiiiiii,[ wlan_scan.c : 990 ] SCAN_ENG_CALC_CHAN num_6g_active = %d num_6g_passive = %d num_items_in_cache = %d scan_all_psc_chan = %d scan_all_non_psc_chan = %d match_hint = %d skip_non_rnr_chan = %d client_priority = %d 
418,iIIiii,[ wlan_scan.c : 1711 ] SCAN_ENG_CANCEL scanhandler_id = %d scan_id = 0x%x requestor= 0x%x stop_mode = %d scan_in_progress = %d cancel_in_progress = %d 
417,iiiII,[ wlan_scan.c : 85 ] AUTO_CHAN_EVT_HDNLR CURR_CHAN_STATS_ERROR error_code = %d (1:scan_handle NULL, 2:chan_freq 0) scan_id = %d evt_mac_id = %d type = 0x%x freq = 0x%x 
416,iIIii,[ wlan_scan.c : 1994 ] SCAN_PASSIVE_TO_ACTIVE mhz=%d cur=%08x end=%08x remaining=%d usec active dwell=%d msec 
415,iIii,[ wlan_scan.c : 2016 ] SCAN_BCN_RECVD mhz=%d at %08x is_scan_in_progress=%d (0 ignored) send_probe_req_on_DFS_ch=%d (1 ignored) 
414,ii,[ wlan_scan.c : 1769 ] SCAN_SET_CHANLIST_FAILED support_chan %d num_scan_chans %d 
413,iiiIIii,[ wlan_scan.c : 1875 ] SCAN_SET_CHAN_LIST idx = %d, mhz = %d, is_passive = %d ch_info = 0x%x reg_info_1 = 0x%x max_bd = %d  is_nan_disabled = %d 
412,ii,[ wlan_scan.c : 2372 ] SCAN_SM_SKIP_NON_RNR_CH freq = %d chan_index = %d 
411,IIIi,[ wlan_scan.c : 1539 ] SCAN_ENG_START_IN_PROGRESS = 1 scan_id = 0x%x requestor = 0x%x req_sub_id = 0x%x priority = %d -> return EBUSY 
410,I,[ wlan_scan.c : 1662 ] SCAN_SM_START_COMMAND_FAILED cur_sch_scan_req = NULL handle = 0x%x 
409,iI,[ wlan_scan.c : 648 ] SCAN_ENG_MAX_SCAN_TIMEOUT scanhandle_id = %d scan_id = 0x%x 
461,I,[ wlan_scan_sch.c : 2905 ] SCAN_SCH_CSA_FAILED status = 0x%x 
460,III,[ wlan_scan_sch.c : 3172 ] SCAN_SCH_RESUME requestor_id = 0x%x suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
459,iIIi,[ wlan_scan_sch.c : 194 ] SCAN_SCH_SUPPRESS_REQ req_mod_id=%d sch_class = 0x%x id = 0x%x is_disable_scan = %d 
458,III,[ wlan_scan_sch.c : 3146 ] SCAN_SCH_SUSPEND requestor_id = 0x%x suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
457,IIiiIIii,[ wlan_scan_sch.c : 1375 ] SCAN_INTERN_EVT evt_type=%x(1:start 2:compl 4:bss 8:frn_ch 10:deq 20:preempt 40:start_fail 80:restart 100:frn_ch_exit 200:susp 400:resume) scan_id=0x%x vdev_id=%d freq=%d req_sub_id=0x%x to_host(8b)|reason(8b)=0x%x abs_pri=%d dwell=%d 
456,Iiiii,[ wlan_scan_sch.c : 1429 ] SCAN_INTERN_EVT (FOREIGN_CHANNEL) scan_id = 0x%x ch_freq = %d bss_ch_freq = %d passive/active = %d dwell_time = %d 
455,IIi,[ wlan_scan_sch.c : 1442 ] SCAN_INTERN_EVT (PREEMPTED) scan_id = 0x%x preempted_by (scan_id) = 0x%x reason = %d 
454,ii,[ wlan_scan_sch.c : 1464 ] SCAN_INTERN_EVT evt_type: %d(1:start 2:complete) PAGE_FAULT_COUNTER: %d
 
453,IIIIIIII,[ wlan_scan_sch.c : 2096 ] SCAN_SCH_WMI_START 6ghz_ch 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
452,iiiiii,[ wlan_scan_sch.c : 2124 ] SCAN_SCH_WMI_START_SCAN num_ssid from %d to %d, num_bssid from %d to %d, num_chan = %d ie_len = %d 
451,IIIIII,[ wlan_scan_sch.c : 2131 ] SCAN_SCH_WMI_START_SCAN bssid = %02x:%02x:%02x:%02x:%02x:%02x 
450,Iiiiii,[ wlan_scan_sch.c : 2178 ] SCAN_SCH_WMI_START s_ssid_bssid_cache = 0x%x num_hint_freq_short_ssid_list = %d num_hint_freq_bssid_list = %d dtime_act = %d dtime_pas = %d min_dtime=%d 
449,iI,[ wlan_scan_sch.c : 2261 ] SCAN_START_COMMAND_FAILED err_ret_code = %d(1:normal 2:NOL) status = 0x%x 
448,I,[ wlan_scan_sch.c : 2286 ] SCAN_SCH_STOP_COMMAND_FAILED status = 0x%x 
447,iiiI,[ wlan_scan_sch.c : 3467 ] SCAN_WLM_NOTIF lvl = %d actv_time = %d pass_time = %d flags = 0x%x 
446,II,[ wlan_scan_sch.c : 644 ] SCAN_SCH_SUSPENDED suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
445,i,[ wlan_scan_sch.c : 671 ] SCAN_SCH_START_NEW_REQ_FAILED error_code=%d 
444,,[ wlan_scan_sch.c : 674 ] SCAN_DETERM_HIGH_PRI cur scan not completed 
443,,[ wlan_scan_sch.c : 1886 ] SCAN_OEM_SET_PARAM tlv error 
442,,[ wlan_scan_sch.c : 1906 ] SCAN_OEM_SET_PARAM tlv wrong config type 
441,iI,[ wlan_scan_sch.c : 984 ] SCAN_SCH_START_PARAM_INVALID scan_id=0x%d param=0x%x 
440,IIIiiiii,[ wlan_scan_sch.c : 1175 ] SCAN_SCH_START scan_id = 0x%x requestor_id = 0x%x req_sub_id = 0x%x requested_priority = %d absolute_priority = %d actv_time_5g = %d actv_time_2g = %d pass_time = %d 
439,iiIIii,[ wlan_scan_sch.c : 1222 ] SCAN_SCH_START_FAIL err_code = %d(1:misc 2:vdev_invalid 3:no_mem_new_req 4:chunk_copy_fail) scan_id = 0x%d requestor_id = 0x%x req_sub_id = 0x%x requested_priority = %d ie_len = %d 
438,I,[ wlan_scan_sch.c : 1801 ] SCAN_EVENT_SEND_FAILED 0x%x 
437,IiiIi,[ wlan_scan_sch.c : 1539 ] SCAN_EVENT_SEND_FAILED scan_id = 0x%x vdev_id = %d ch_freq = %d req_sub_id = 0x%x reason = %d 
436,IIii,[ wlan_scan_sch.c : 317 ] SCAN_SCH_CANCEL scan_id = 0x%x requestor_id = 0x%x vdev_id = %d req_type = %d 
435,,[ wlan_scan_sch.c : 369 ] SCAN_SCH_CANCEL already in progress 
434,,[ wlan_scan_sch.c : 375 ] SCAN_SCH_CANCEL no match found 
433,iiiiiii,[ wlan_scan_sch.c : 915 ] SCAN_SCH_SPLIT_PASSIVE_CH num_ch_2g = %d num_ch_5g_active = %d num_ch_5g_passive = %d (start_ch_idx = %d end_ch_idx = %d) num_ch_6g = %d total_num_ch = %d 
432,II,[ wlan_scan_sch.c : 570 ] SCAN_SCH_SUSPEND_NEXT_SCAN suspend_bitmap_63_32 = 0x%x, suspend_bitmap_31_0 = 0x%x 
431,IIIIIII,[ wlan_scan_sch.c : 603 ] SCAN_SCH_SUPPRESS_MATCH scan_id = 0x%x, requestor = 0x%x, vdev_id = 0x%x, suppress_vdev_id_bitmap = 0x%x suppress_mod_bitmap[0:2] 0x%x 0x%x 0x%x 
430,II,[ wlan_scan_sch.c : 1268 ] SCAN_SCH_ENGINE_STOP_DUE_TO_TIMEOUT  evt_scan_id = 0x%x evt_reason = 0x%x 
429,i,[ wlan_scan_sch.c : 1648 ] SCAN_SCH_NEXT_SCAN_FAILED error_code=%d 
428,i,[ wlan_scan_sch.c : 1332 ] SCAN_EVENT_COMPLETED really cancelled scan_id %d 
427,i,[ wlan_scan_sch.c : 3564 ] SCAN etm log is enable: %d
 
490,,[ wlan_scan_sm.c : 1404 ] SCAN_SM_REQ_NEXT_CH_AGILE agile scan totally complete 
489,iiiii,[ wlan_scan_sm.c : 2895 ] SCAN_SM_REQ_NEXT_CHAN_ASYNC_CMPLT band_2g_num_chan_indices = %d band_2g_cur_chan_index = %d band_5g_low_num_chan_indices = %d band_5g_cur_chan_index = %d comp_pending_5g_low_band = %d 
488,iiii,[ wlan_scan_sm.c : 2902 ] SCAN_SM_REQ_NEXT_CHAN_ASYNC_CMPLT2 comp_pending_5g_dbs_active_ch = %d band_5g_low_num_active_chan_indices = %d chan_list_mode = %d comp_pending_bitmask = %d 
487,I,[ wlan_scan_sm.c : 2952 ] SCAN_SM_REQ_NEXT_CHAN_ASYNC_CMPLT scanhandler_id = 0x%x 
486,,[ wlan_scan_sm.c : 3122 ] SCAN_NEXT_CH_ERROR n_chan is not assigned 
485,iii,[ wlan_scan_sm.c : 88 ] SCAN_SM_TRANSITIONS_MAC_%d %d => %d 
484,iii,[ wlan_scan_sm.c : 73 ] SCAN_SM_DISPATCH_MAC_%d %d < %d 
483,iii,[ wlan_scan_sm.c : 755 ] SCAN_SM_MSPS_GET_CH_IDX freq = %d cur_ch_idx = %d split_pass_ch_idx = %d 
482,Iii,[ wlan_scan_sm.c : 6751 ] SCAN_OCE_CCA_TIMEOUT cancel probe delay for scan_id:0x%x scanhdl_id:%d scan_policy:%d as CU < 50 percent 
481,Iiiii,[ wlan_scan_sm.c : 6776 ] SCAN_OCE_CCA_TIMEOUT cancel probe delay for scan_id:0x%x scanhdl_id:%d scan_policy:%d num_timeslots:%d, continous_free:%d 
480,Iiii,[ wlan_scan_sm.c : 6804 ] SCAN_SM_OCS_TIMEOUT scan_id 0x%x, requestor = %d, curr_index = %d, curr_policy = %d 
479,IIIIiiii,[ wlan_scan_sm.c : 989 ] SCAN_SM_REQ_NEXT_CHAN scan_id=0x%x cur_policy(8)|hdl_id(8)=0x%x 2g_idx(16)|tot(16)=0x%x 5g_idx(8)|tot(E8_H8_L8)=0x%x dwell=%dms dur=%dus freq_pri=%d freq_sec=%d 
478,iii,[ wlan_scan_sm.c : 898 ] SCAN_NOA_DWELL_TIME_OFFSET cur_policy=%d round_up_offset=%d scan_pre_foreign_chan_exit_time=%d 
477,Ii,[ wlan_scan_sm.c : 6912 ] SCAN_SM_CANCEL scan_stop = 0x%x scan_timeout = %d 
476,i,[ wlan_scan_sm.c : 3300 ] SCAN_SM_REQ_NEXT_CHAN !error! not implemented scan policy: %d 
475,ii,[ wlan_scan_sm.c : 4889 ] SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 6g_freq = %d 
474,iIiIIII,[ wlan_scan_sm.c : 4928 ] SEND_PROBE_ON_6GHZ_CH freq = %d short_ssid = 0x%x (cur_20TU_idx = %d add_flags_save = 0x%x add_flags = 0x%x chainmask = 0x%x ppdu_info = 0x%x) 
473,iIIiIIII,[ wlan_scan_sm.c : 4938 ] SEND_PROBE_ON_6GHZ_CH freq = %d bssid = %08x%04x (cur_20TU_idx = %d add_flags_save = 0x%x add_flags = 0x%x chainmask = 0x%x ppdu_info = 0x%x) 
472,i,[ wlan_scan_sm.c : 5030 ] SCAN_SEND_PROBE_REQ_6G_MGR err_ret = %d 
471,IiiI,[ wlan_scan_sm.c : 5911 ] SCAN_SEND_PROBE_REQ_2G_RET scan_id = 0x%x freq = %d cur_index = %d flags = 0x%02x 
470,IiiI,[ wlan_scan_sm.c : 5924 ] SCAN_SEND_PROBE_REQ_5G_RET scan_id = 0x%x freq = %d cur_index = %d flags = 0x%02x 
469,IIIiiiii,[ wlan_scan_sm.c : 6070 ] SCAN_SEND_PROBE_REQ_INFO scan_id = 0x%x band_2G_info = 0x%x band_5G_info = 0x%x probe_time = %d last_ssid_idx = %d last_bssid_idx = %d last_sent_probes = %d increase_probe_cnt:%d 
468,iI,[ wlan_scan_sm.c : 6076 ] SCAN_SEND_PROBE_REQ_RET err_ret = %d scan_id = 0x%x 
467,i,[ wlan_scan_sm.c : 5583 ] SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 
466,iii,[ wlan_scan_sm.c : 5247 ] SCAN_SM_PROBE_REQ_FRAME_GEN_FAILED scanhandler_id = %d 5g_freq = %d 2g_freq = %d 
465,iiiii,[ wlan_scan_sm.c : 386 ] SCAN_SM_BSSCH_ENTRY scanhandler_id = %d is_passive_ch_split = %d band_5g_cur_chan_index = %d freq = %d min_rest_time = %d 
464,iii,[ wlan_scan_sm.c : 4309 ] SCAN_SM_FOREIGN_CH actual_probe_delay = %d, scan_sch_handle->cancel_probe_req_defer = %d, params.cancel_probe_req_defer = %d 
463,iiii,[ wlan_scan_sm.c : 4332 ] SCAN_SM_LEGACY_MAC_CHANGE scanhandler_id = %d, last_legacy_macid = %d req_mac_id = %d, index = %d 
462,i,[ wlan_scan_sm.c : 6459 ] SCAN_SM_FOREIGN_CHAN_EVENT !error! not implemented scan policy: %d 
515,iiii,[ wlan_scan_mgr.c : 486 ] SCAN_MGR_PDEV_SUSPEND_RESUME_CHANGE_EVT pdev_id = %d requestor = %d reason %d state = %d 
514,IIII,[ wlan_scan_mgr.c : 457 ] SCAN_POLICY_EVENT current_allowed_policy = 0x%x new_allowed_policy = 0x%x current_scan_req = 0x%x suppress_mode_bitmap = 0x%x 
513,Iiiii,[ wlan_scan_mgr.c : 91 ] SCAN_MGR_STATE_CHANGE scan_id = 0x%x num_ssid = %d num_bssid = %d num_chan = %d new_scan_state = %d (0:completed 1:legacy 2:sync_DBS 3:async_DBS 4:agile 5:agile_DFS_2g 6:agile_DFS_5g) 
512,,[ wlan_scan_mgr.c : 1549 ] SCAN_MGR_CH_MODE_CHANGE scan cancelled 
511,iiiii,[ wlan_scan_mgr.c : 1615 ] SCAN_MGR_CHECK_PARAMS_CHANNELS params->num_chan=%d params->chan_list[0]=%d has_2g_chan=%d has_5g_chan_active=%d has_5g_chan_passive=%d 
510,ii,[ wlan_scan_mgr.c : 1962 ] SCAN_MGR_CLIENT_SCAN_SELECTION ret_selection = %d (param_selection = %d) 
509,iiiii,[ wlan_scan_mgr.c : 1915 ] wlan_scan_mgr_compute_client_scan_policy_by_duty_cycle  module_id = %d cur_num_dbs = %d cur_num_legacy = %dmax_num_dbs=%d max_num_legacy = %d 
508,iii,[ wlan_scan_mgr.c : 2002 ] SCAN_MGR_DBS_SCAN_DUTY_CYCLE_PARAM module_id = %d max_num_dbs_scans = %d max_num_legacy = %d  
507,i,[ wlan_scan_mgr.c : 2011 ] SCAN_MGR_DBS_SCAN_DUTY_CYCLE_PARAM_FAIL err_code = %d(1:num_clients_zero 2:scanhandle_null) 
506,iI,[ wlan_scan_mgr.c : 155 ] SCAN_MGR_EVENT_FAIL: Invalid input - scan_handler_id = %d, current_scan_sch_req = 0x%x 
505,IIIiiii,[ wlan_scan_mgr.c : 193 ] SCAN_MGR_EVENT_PREEMP_SUSP engid_policy_susp_preempt = 0x%08x 2g_idx(8)|tot(8)|5g_idx(8) = 0x%x 5g_E8_H8_L8_LA8 = 0x%x cancel_pending_bitmask = %d comp_pending_bitmask = %d comp_pending_5g_LB = %d comp_pending_5g_LB_act_ch = %d 
504,IIiiiiiIi,[ wlan_scan_mgr.c : 331 ] SCAN_MGR_EVENT_PREEMPTED scan_id = 0x%x cur_chan_index = 0x%x  mac_id = %d 2g_next_idx = %d 2g_curr = %d 5g_next_idx = %d 5g_curr = %d reason = 0x%x cur_scan_policy = %d 
503,IIIi,[ wlan_scan_mgr.c : 337 ] SCAN_MGR_EVENT_SUSPENDED scan_id = 0x%x cur_chan_index = 0x%x reason = 0x%x cur_scan_policy = %d 
502,i,[ wlan_scan_mgr.c : 343 ] SCAN_MGR_EVENT_PREEMPTED or SCAN_MGR_EVENT_SUSPENDED drop_event = %d 
501,IiiIi,[ wlan_scan_mgr.c : 356 ] SCAN_MGR_EVENT_ASYNC_COMPLETE scan_handler_id = 0x%x band_5g_cur_chan_index = %d band_2g_cur_chan_index = %d comp_pending_bitmask = 0x%x comp_pending_5g_LB_act_ch = %d 
500,Iiiii,[ wlan_scan_mgr.c : 413 ] SCAN_MGR_EVENT_COMPLETED scan_id = 0x%x num_ssid = %d num_bssid = %d num_chan = %d is_drop = %d 
499,Ii,[ wlan_scan_mgr.c : 1712 ] SCAN_MGR_SCAN_POLICY_RECOMPUTE_START suppress mode bitmap = 0x%x is_scan_start = %d 
498,iiii,[ wlan_scan_mgr.c : 1766 ] SCAN_MGR_SCAN_POLICY_RECOMPUTE invalid chan index vdev_index=%d has_2g_chan=%d passive_5g=%d has_5g_chan_active=%d 
497,iiiiiiI,[ wlan_scan_mgr.c : 1817 ] SCAN_MGR_SCAN_POLICY_RECOMPUTE_END vdev_index = %d, chan_index = %d, policy_sel = %d, new_scan_policy = %d, cur_scan_policy = %d, scan_policy_max = %d, suppress mode bitmap = 0x%x 
496,IIii,[ wlan_scan_mgr.c : 1078 ] SCAN_MGR_CANCEL scan_id = 0x%x requstor = 0x%x stop_mode = %d scan_eng_start_pending = %d 
495,II,[ wlan_scan_mgr.c : 1181 ] SCAN_MGR_CANCEL comp_pending=0x%x cancel_pending=0x%x 
494,Iii,[ wlan_scan_mgr.c : 1029 ] SCAN_MGR_SCAN_START scan_id = 0x%x  cur_scan_policy = %d scan_cfg_state = %d 
493,Ii,[ wlan_scan_mgr.c : 1043 ] SCAN_MGR_SCAN_START_NON_DBS scan_id = 0x%x  cur_scan_policy = %d  
492,i,[ wlan_scan_mgr.c : 1241 ] SCAN_SCH_NEXT_SCAN_FAILED after setting new channel lists, error_code=%d 
491,iiiiiiii,[ wlan_scan_mgr.c : 714 ] SCAN_MGR_RESUME_EVENT 2g cur_chan = %d, 2g next_chan = %d, 5g cur_chan = %d, 5g next_chan = %d, band_5g_low(high)_num_chan_indices = %d(%d), band_5g_low(high)_num_chan_indices = %d(%d) 
516,i,[ wlan_scan_unit_test.c : 65 ] SCAN_NUM_SUPP_CHAN_LIST %d 
521,i,[ wlan_scan_oce.c : 103 ] wlan_scan_is_oce_probe_deferral_needed result ​%d 
520,I,[ wlan_scan_oce.c : 211 ] wlan_scan_process_scan_results: Set OCE bit for chan freq-0x%x 
519,I,[ wlan_scan_oce.c : 220 ] wlan_scan_process_scan_results: Clear OCE bit for chan freq-0x%x 
518,i,[ wlan_scan_oce.c : 340 ] Current scan OCE FD bssids are > %d hence discarding 
517,i,[ wlan_scan_oce.c : 349 ] Current scan OCE bssids are > %d hence discarding 
525,i,[ wlan_scan_6g_discv.c : 765 ] SCAN_FILSD_HANDLER_ERROR err_code = %d 
524,iiI,[ wlan_scan_6g_discv.c : 803 ] SCAN_FILSD_PARSER_ERROR rx_freq = %d len = %d ret = 0x%x 
523,IiiIII,[ wlan_scan_6g_discv.c : 167 ] SCAN_RNR_CACHE_TBL_ACT act_target_reason_attrib = 0x%08x num_items_in_cache = %d freq = %d s_ssid = 0x%08x bssid = %08x%04x 
522,i,[ wlan_scan_6g_discv.c : 411 ] SCAN_RNR_HANDLER ret_code = %d 
531,ii,[ wlan_scan_mbssid.c : 313 ] SCAN_EMA_MBSSID BSSID index %d exceed max supported number %d 
530,iIIIIii,[ wlan_scan_mbssid.c : 353 ] SCAN_EMA_MBSSID ec=%d SA=%02x:%02x:%02x known_bssid_bitmap=0x%x rcvd_bssid_cnt=%d probe_done=%d 
529,iIII,[ wlan_scan_mbssid.c : 356 ] SCAN_EMA_MBSSID ec=%d SA=%02x:%02x:%02x 
528,iIIiiiI,[ wlan_scan_mbssid.c : 122 ] SCAN_EMA_MBSSID SEND_PROBE_ON_6GHZ_CH freq = %d bssid = %08x%04x (cur_20TU_idx = %d max_bssid_ind = %d known_bssid_len = %d known_bssid_bmp = 0x%x) 
527,III,[ wlan_scan_mbssid.c : 128 ] SCAN_EMA_MBSSID Failed to send probe request to %02x:%02x:%02x 
526,,[ wlan_scan_mbssid.c : 131 ] SCAN_EMA_MBSSID No mgmt buffer 
537,iii,[ wlan_thermal_unit_test.c : 86 ] WLAN_THERMAL_TSENS_TEMP_1 temp_req = %d, sensor_id = %d, temp = %d 
536,iiiiiiii,[ wlan_thermal_unit_test.c : 96 ] WLAN_THERMAL_TSENS_TEMP_2 sensor[1-8] %d %d %d %d %d %d %d %d 
535,ii,[ wlan_thermal_unit_test.c : 373 ] wlan_thermal_unit_test %d %d 
534,ii,[ wlan_thermal_unit_test.c : 48 ] WLAN_THERMAL_TSENS_INVALID_CONFIG vdev_id = %d, num_args = %d 
533,iiiiii,[ wlan_thermal_unit_test.c : 52 ] WLAN_THERMAL_TSENS_RECONFIG num_args = %d, Temp1|2 degC = %d %d, kp|ki|kd = %d %d %d 
532,ii,[ wlan_thermal_unit_test.c : 180 ] WLAN_TSENS_CLIENT_UPDATE ret = %d pdev_id = %d 
633,,[ wlan_vdev.c : 481 ] vdev connecting client is registered in non wow mode 
632,I,[ wlan_vdev.c : 505 ] allow during connecting, subtype:%x 
631,iiI,[ wlan_vdev.c : 579 ] set_restore_mac_addr status = %d, freq = %d, evh = 0x%x 
630,ii,[ wlan_vdev.c : 6667 ] VDEV_MGR_STA_PS_EVENT: vdev_id=%d, event_type=%d 
629,ii,[ wlan_vdev.c : 1538 ] VDEV EVT:RT thread handle vdev_stop_down_del cmd:%d, vdev_id:%d 
628,iii,[ wlan_vdev.c : 1467 ] VDEV EVT:DATA offload thread handle vdev_stop_down_del msg cmd = %d, vdev_id = %d, vdev_mode = %d 
627,iii,[ wlan_vdev.c : 1373 ] VDEV EVT:RT thread handle vdev_stop_down_del msg cmd = %d, vdev_id = %d, vdev_mode = %d 
626,,[ wlan_vdev.c : 10755 ]  SET GTX PARAM from WMI is not supported  
625,II,[ wlan_vdev.c : 7242 ] VDEV_STOP_ABORT_TX try_to_abort, hwq=0x%x, swq=0x%x 
624,II,[ wlan_vdev.c : 7249 ] VDEV_STOP_ABORT_TX abort_fails, hwq=0x%x, swq=0x%x 
623,II,[ wlan_vdev.c : 7253 ] VDEV_STOP_ABORT_TX abort_succeeds, hwq=0x%x, swq=0x%x 
622,II,[ wlan_vdev.c : 7260 ] VDEV_STOP_ABORT_TX after_abort, hwq=0x%x, swq=0x%x 
621,iii,[ wlan_vdev.c : 7280 ] VDEV_STOP_EVT VDEV ID = %d HW Q depth= %d, SW Q depth = %d 
620,ii,[ wlan_vdev.c : 7372 ] WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d 
619,iii,[ wlan_vdev.c : 1017 ] VDEV EVT: vdev create id=%d, mode=%d submode=%d 
618,ii,[ wlan_vdev.c : 1991 ] VDEV EVT: vdev delete id=%d, mode=%d 
617,i,[ wlan_vdev.c : 1580 ] wlan_beacon_tx: vdev id = %d vdev delete return becasue bcn ctxt is not free yet 
616,iiIIi,[ wlan_vdev.c : 1611 ] VDEV EVT peer not cleared idx=%d vdev_id = %d mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x usage_count = %d 
615,iii,[ wlan_vdev.c : 1654 ] VDEV EVT: WMI_VDEV_DELETE_RESP_EVENTID vdevId=%d vdev_type: %d vdev_subtype: %d 
614,iiiiiii,[ wlan_vdev.c : 10269 ] VDEV_CHAINMASK_CONFIG_1 vdev_id=%d num_tx_chains_2g = %d, num_rx_chains_2g = %d, tx_nss_2g = %d, rx_nss_2g = %d, num_tx_chains_b = %d, num_tx_chains_g = %d 
613,iiiii,[ wlan_vdev.c : 10272 ] VDEV_CHAINMASK_CONFIG_2 num_tx_chains_5g = %d, num_rx_chains_5g = %d, tx_nss_5g = %d, rx_nss_5g = %d, num_tx_chains_a = %d 
612,iiii,[ wlan_vdev.c : 10275 ] VDEV_CHAINMASK_CONFIG_3 disable_tx_mrc_2g = %d, disable_rx_mrc_2g = %d, disable_tx_mrc_5g = %d, disable_rx_mrc_5g = %d 
611,iiiii,[ wlan_vdev.c : 10023 ] Error: vdev id %d, aggregation type %d, ac %d, max num frames %d, enable_bitmap %d 
 
610,iiiiii,[ wlan_vdev.c : 10030 ] vdev id %d, aggregation type %d, ac %d, max num frames %d, enable_bitmap %d rx_size %d
 
609,iiiiii,[ wlan_vdev.c : 10107 ] vdev id %d, ac %d, software retry type %d, software retry threshold %d, pdev->agg_retry_th %d, pdev->non_agg_retry_th %d 
608,i,[ wlan_vdev.c : 8843 ] WMI_VDEV_GET_ARP_STAT_CMDID: vdev_id = %d event alloc failed 
607,,[ wlan_vdev.c : 8554 ] BIGDATA ERR: vdev NULL or FREE 
606,i,[ wlan_vdev.c : 8705 ] WMI_VDEV_GET_KEEPALIVE_CMDID: vdev_id = %d event alloc failed 
605,iiiii,[ wlan_vdev.c : 7933 ] 11w PMF vdevId=%d key_ix=%d cipher=%d is_group_key_valid %d group_key_ix %d 
604,iIIi,[ wlan_vdev.c : 8046 ] VDEV_INSTALL_KEY_FAIL vdev_id %d mac_addr %04x:%08x status %d 
603,iI,[ wlan_vdev.c : 8131 ] WAL_DBGID_SET_M4_SENT_MANUALLY  VDEV ID = %d, peer = 0x%x 
602,i,[ wlan_vdev.c : 9752 ] LIMIT_OFFCHAN_ERROR client_id=%d 
601,i,[ wlan_vdev.c : 9762 ] LIMIT_OFFCHAN_ERROR vdev_id=%d 
600,i,[ wlan_vdev.c : 8944 ] dispatch_request_stats_ext_cmd invalid vdev id =%d 
599,i,[ wlan_vdev.c : 8948 ] dispatch_request_stats_ext_cmd vdev id =%d 
598,Iiii,[ wlan_vdev.c : 9427 ] dispatch_set_ie_cmd: ie_id = 0x%x, id_len = %d, source=%d, band=%d 
597,Iii,[ wlan_vdev.c : 9445 ] vdev_set_scan_default_ie status = 0x%x vdev_id=%d prunned_ie_len=%d 
596,iII,[ wlan_vdev.c : 8661 ] KA: cmd handler() -> start timer vdev_id = %d keepalive_interval = 0x%x keepalive_method = 0x%x 
595,i,[ wlan_vdev.c : 7756 ] Invalid VDEV in WMI_VDEV_SET_WMM_PARAMS_CMDID, VDEV ID = %d 
594,i,[ wlan_vdev.c : 7763 ] Invalid WAL VDEV in WMI_VDEV_SET_WMM_PARAMS_CMDID, VDEV ID = %d 
593,i,[ wlan_vdev.c : 7784 ] WMI_VDEV_SET_WMM_PARAMS_CMDID type=%d 
592,IIII,[ wlan_vdev.c : 7797 ] WMI_VDEV_SET_WMM_PARAMS_CMDID ac[31-16]/acm[15-0] = 0x%x cw_min = 0x%x cw_max = 0x%x txop_limit[31-16]/aifs[15-0] = 0x%x 
591,I,[ wlan_vdev.c : 7563 ] Rejecting vdev_start Roaming in progress  vdev_id= 0x%x  
590,I,[ wlan_vdev.c : 7572 ] Rejecting vdev_start BSS Peer not created  vdev_id= 0x%x  
589,I,[ wlan_vdev.c : 7580 ] Rejecting vdev_start Home channel not in supported band vdev_id= 0x%x  
588,III,[ wlan_vdev.c : 7601 ] Rejecting vdev_start request from requestor_id = 0x%x. start_delay_us = 0x%x, max_start_delay_us=0x%x 
587,iI,[ wlan_vdev.c : 7614 ] Rejecting vdev_start request for vdev_id = %d from requestor_id = 0x%x. STA + STA not supported 
586,IIIIIii,[ wlan_vdev.c : 8435 ] WLAN_DISPATCH_VDEV_UP vdev_flags:0x%x vdev_bssid:%x_%x trans_bssid:%x_%x profile_idx:%d profile_num:%d 
585,,[ wlan_vdev.c : 8471 ] WLAN_DISPATCH_VDEV_UP !!!host sends wrong MBSSID param!!! 
584,iii,[ wlan_vdev.c : 8202 ] WMI_CMD_PARAMS AC = %d Med-Time usec = %d DwnGrd_Type = %d 
583,ii,[ wlan_vdev.c : 8908 ] dispatch_wmm_delts_cmd: ac = %d vdev id = %d 
582,,[ wlan_vdev.c : 8928 ] dispatch_wmm_delts_cmd: end 
581,Ii,[ wlan_vdev.c : 681 ] VDEV_MGR loopback cal  vdev_id = 0x%x cur_policy_mgr_hw_mode = %d 
580,Iii,[ wlan_vdev.c : 751 ] VDEV_MGR loopback cal  vdev_id = 0x%x cal_time = %d do_noa = %d 
579,ii,[ wlan_vdev.c : 4613 ] VDEV EVT: vdev down id=%d, mode=%d 
578,ii,[ wlan_vdev.c : 9387 ] vdev_extract_mandatory_ies: id=%d, len=%d 
577,Ii,[ wlan_vdev.c : 9301 ] vdev_extract_optional_vendor_ies: oui=0x%x, len=%d 
576,I,[ wlan_vdev.c : 6942 ] VDEV free error, peer addr:0x%x, mac:0x8x 0x8x 
575,iiiiiii,[ wlan_vdev.c : 10198 ] wlan_vdev_get_chain_config vdev_id = %d, conn_tx_nss=%d, conn_rx_nss = %d, num_tx_chains = %d, num_rx_chains = %d, num_tx_chains_b = %d, num_tx_chains_ag = %d 
574,II,[ wlan_vdev.c : 7442 ] wlan_vdev_get_vdev_start_delay_us cur_one_shot_end_time = 0x%x. cur_wal_time = 0x%x 
573,iii,[ wlan_vdev.c : 10627 ] VDEV_SET_PARAM_TPC_POWER psd_power=%d, eirp_power=%d, num_pwr_levels=%d 
572,iiiii,[ wlan_vdev.c : 10596 ] wlan_vdev_handle_wfa_config_cmd override_rsnxe=%d, ignore_csa=%d, deauth_on_saquery_timeout=%d override_oci_chan frame_types=%d, override_oci_chan=%d 
571,iIii,[ wlan_vdev.c : 9713 ] LIMIT_OFFCHAN_ARBITER client=%d flag=0x%x max_offchan_time=%d rest_time=%d 
570,Iii,[ wlan_vdev.c : 9735 ] LIMIT_OFFCHAN_ARBITER_RESULT flag=0x%x max_offchan_time=%d rest_time=%d 
569,II,[ wlan_vdev.c : 2433 ] wlan_vdev_migrate vdev_id[31-16]/from_mac[15-8]/to_mac[7-0] 0x%x, is_up[24]/is_active[16]/mode[15-8]/submode[7-0] 0x%x 
568,,[ wlan_vdev.c : 7471 ] WMI_EVENT_ALLOC_FAILURE: VDEV_REJECT_VDEV_START_REQ_RESP_EVENTID buffer failure 
567,iIi,[ wlan_vdev.c : 9620 ] WMI RSSI threshold met: vdev %d evt_type 0x%x cur_rssi %d 
566,ii,[ wlan_vdev.c : 9141 ] vdev_set_mandatory_ie: ie_id=%d, id_len=%d 
565,i,[ wlan_vdev.c : 9252 ] vdev_set_mandatory_ie: not handled ie_id=%d 
564,iii,[ wlan_vdev.c : 9037 ] vdev_set_mandatory_ie_by_band: ie_id=%d, band=%d, id_len=%d 
563,iI,[ wlan_vdev.c : 11321 ] wlan_vdev_set_max_pause_delay_us vdev_id=%d max_pause_delay_us = 0x%x 
562,ii,[ wlan_vdev.c : 5505 ] WMI_CMD_PARAMS VdevId/AC/Arg1 = %d Cmd/Med-Time/Action/Arg2 = %d 
561,iII,[ wlan_vdev.c : 5510 ] vdev_id: %d vdev_set_param: id: 0x%x param_value: 0x%x 
560,iII,[ wlan_vdev.c : 6039 ] WLAN_VDEV_SET_PARAM_FAIL3 paramid:%d vdevp:0x%x vdevp->bss:0x%x 
559,iii,[ wlan_vdev.c : 6262 ] WMI_VDEV_PARAM_DISABLE_NOA_P2P_GO ic_mode:%d ic_subopmode:%d param:%d  
558,ii,[ wlan_vdev.c : 6283 ] WMI_VDEV_PARAM_SMPS_INTOLERANT: vdev_id:%d, param:%d 
557,iii,[ wlan_vdev.c : 6382 ] WMI_VDEV_PARAM_ABG_MODE_TX_CHAIN_NUM: vdev_id = %d, tx_chains_num_11b = %d, tx_chains_num_11ag = %d 
556,I,[ wlan_vdev.c : 6472 ] Setting CABQ to %x 
555,,[ wlan_vdev.c : 6520 ] Err: WMI_VDEV_PARAM_NTH_BEACON_TO_HOST command came for non STA vdev 
554,IiiiiiI,[ wlan_vdev.c : 3305 ] VDEV_START: vdev_id[31-24]/mode[23-16]/mode[15-8]/mac_id[7-0] = 0x%x chan_mhz = %d  phy_mode=%d band_center_freq1=%d band_center_freq2=%d ldpc_rx_enabled=%d vdev_flags:0x%x 
553,IiI,[ wlan_vdev.c : 3496 ] VDEV_MGR_HP_START_TIME  vdev_id = 0x%x chan_mhz = %d start_tsf = 0x%x 
552,iIIII,[ wlan_vdev.c : 8243 ] wlan_vdev_tsf_report: vdev_id = %d, tsf_low = 0x%x, tsf_high = 0x%x, qtimer_low=0x%x, qtimer_high=0x%x 
551,iI,[ wlan_vdev.c : 8264 ] wlan_vdev_tsf_tstamp_action:vdev_id = %d, action = 0x%x 
550,ii,[ wlan_vdev.c : 8272 ] wlan_vdev_tsf_tstamp_action: vdev_id = %d, vdev_ifUp = %d 
549,iII,[ wlan_vdev.c : 10291 ] VDEV_TX_DIVERSITY_CHAINMASK_UPDATE vdev_id=%d cur_chm = 0x%x, new_chm = 0x%x 
548,iI,[ wlan_vdev.c : 11176 ] wlan_vdev_unit_test: vdev_id = %d, cmd = WMI_VDEV_PARAM_ABG_MODE_TX_CHAIN_NUM, value = 0x%x 
547,ii,[ wlan_vdev.c : 4176 ] VDEV_MGR_VDEV_UP id=%d, mode=%d 
546,i,[ wlan_vdev.c : 4362 ] VDEV RESMGR_LINK_ATTR_SMPS_VALID Peer_flags:%d 
545,i,[ wlan_vdev.c : 4410 ] VDEV RESMGR_LINK_ATTR_SMPS_VALID VHT mode:%d 
544,iII,[ wlan_vdev.c : 4478 ] KA: wlan_vdev_up() -> start timer vdev_id = %d keepalive_interval = 0x%x keepalive_method = 0x%x 
543,iI,[ wlan_vdev.c : 5432 ] VDEV_OCE_FLAGS vdev_id %d flags 0x%x 
542,i,[ wlan_vdev.c : 2739 ] wlan_vdevs_migrate, vdevs_migrate_duration = %d us 
541,i,[ wlan_vdev.c : 2744 ] wlan_vdevs_migrate, PAGE_FAULT_COUNTER: %d 
540,iIii,[ wlan_vdev.c : 9652 ] WMI RSSI breach config: vdev %d enabled_bitmap 0x%x high_rssi %ddBm low_rssi %ddBm 
539,iii,[ wlan_vdev.c : 6976 ] WAL Peer event vdevp %d is_free %d, is_vdev_stopping %d 
538,iii,[ wlan_vdev.c : 6984 ] WAL Peer event Vdev ID = %d HW Q depth= %d, SW Q depth = %d 
674,iii,[ wlan_vdev_misc.c : 1250 ] VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
673,iiI,[ wlan_vdev_misc.c : 1297 ] VDEV_MGR_MY_BEACON_BAD_IE id=%d,len=%d,status=0x%x 
672,iII,[ wlan_vdev_misc.c : 645 ] action bitmask of %dth OUI is %x and oui matched is %x 
671,iii,[ wlan_vdev_misc.c : 678 ] %d byte fail to match for data.                                        actual_data %d, configured data %d 
670,iii,[ wlan_vdev_misc.c : 713 ] %d byte fail to match for mac address.                                actual_mac = %d, Configured mac = %d 
669,II,[ wlan_vdev_misc.c : 742 ] Capability mismatch %x != (%x) 
668,I,[ wlan_vdev_misc.c : 762 ] oui_action_matched %x 
667,i,[ wlan_vdev_misc.c : 798 ] number_of_configured_oui = %d 
666,iii,[ wlan_vdev_misc.c : 902 ] VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
665,III,[ wlan_vdev_misc.c : 913 ] VENDOR SPECIFIC IE :%02x, %02x, %02x 
664,iii,[ wlan_vdev_misc.c : 832 ] VDEV_MGR_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
663,iiI,[ wlan_vdev_misc.c : 861 ] VDEV_MGR_MY_BEACON_BAD_IE id=%d,len=%d,status=0x%x 
662,IIIIII,[ wlan_vdev_misc.c : 1059 ] VENDOR SPECIFIC IE :%u, %u, %02x, %02x, %02x, %02x 
661,i,[ wlan_vdev_misc.c : 1341 ] SSID LEN ERROR, ssid_len = %d 
660,IIIIIIII,[ wlan_vdev_misc.c : 1370 ] NAV_WAR, ssid=%x %x %x %x %x %x %x, detect=%x 
659,ii,[ wlan_vdev_misc.c : 3395 ] User configured fils discovery period (%d) is more than max supported value (%d). Capping fd period to max supported 
658,ii,[ wlan_vdev_misc.c : 2963 ] wlan_vdev_fill_vdev_mac_entry: vdev_id=%d, pdev_id=%d 
657,,[ wlan_vdev_misc.c : 1018 ] 2xLTF not supported 
656,I,[ wlan_vdev_misc.c : 3113 ] wlan_vdev_get_migrate_active_vdev_list  vdev_id_list=0x%x 
655,I,[ wlan_vdev_misc.c : 1851 ] Received IBSS Beacon peer = 0x%x send_to_host =  
654,iIIIiiiii,[ wlan_vdev_misc.c : 1574 ] VDEV_MGR_MY_BEACON_RECEIVED: vdev_id = %d curr_time = 0x%x  curr_vdev_tsf = 0x%x seq = %u rssi = %d rssi_ch0 = %d rssi_ch1 = %d bss_ch = %d recv_ch = %d 
653,II,[ wlan_vdev_misc.c : 1663 ] wlan_vdev_handle_own_beacon: RAP: current AP bssid=0x%x 0x%x 
652,i,[ wlan_vdev_misc.c : 3897 ] wlan_vdev_is_mcc_vdev_connect_in_progress result %d 
651,IIIIi,[ wlan_vdev_misc.c : 2225 ] OMI: Error peernss = 0x%lx OMI nss = 0x%lx bssBw= %1x OMI Bw= %1x peerMaxBw = %d
 
650,i,[ wlan_vdev_misc.c : 2434 ] wlan_vdev_reconfig: wlan_vdev vdev_id = %d is not up 
649,iii,[ wlan_vdev_misc.c : 2352 ] wlan_vdev_reg_unreg_p2p_dev_mac_addr: vdev_id = %d, is_reg_mac_addr = %d, mac_addr_registered = %d 
648,IIIII,[ wlan_vdev_misc.c : 1174 ] set_ignore_check_for_OUI :: VENDOR SPECIFIC IE :%u, %u, %02x, %02x, %02x 
647,i,[ wlan_vdev_misc.c : 3515 ] FILS_DISCOVERY Started on vdev_id = %d 
646,i,[ wlan_vdev_misc.c : 3528 ] FILS_DISCOVERY Stopped on vdev_id = %d 
645,IIIIIII,[ wlan_vdev_misc.c : 2076 ] tx_bytes = 0x%x rx_bytes = 0x%x mpdu_enqueue = 0x%x mpdu_requeued = 0x%x rx_mcs = 0x%x tx_mcs = 0x%x, mpdu_missed = 0x%x 
644,iiii,[ wlan_vdev_misc.c : 1482 ] MU EDCA BEACON: ignoring edca update qos_present=%d                 mu_edca_present=%d bcn_update_cnt=%d vdev_update_cnt=%d 
643,i,[ wlan_vdev_misc.c : 332 ] STA_KICKOUT: Reason=%d 
642,,[ wlan_vdev_misc.c : 3552 ] wal_wlm_notif input error 
641,,[ wlan_vdev_misc.c : 3558 ] wal_wlm_notif enable 1nss 
640,i,[ wlan_vdev_misc.c : 3562 ] wal_wlm_notif back to %d stream 
639,,[ wlan_vdev_misc.c : 3577 ] wal_wlm_notif rts/cts already enabled for all try 
638,iII,[ wlan_vdev_misc.c : 3585 ] wal_wlm_notif vdev_id %d change rts profile from 0x%x to 0x%x 
637,iI,[ wlan_vdev_misc.c : 3591 ] wal_wlm_notif vdev_id %d back to default rts policy 0x%x 
636,,[ wlan_vdev_misc.c : 3598 ] wal_wlm_notif secondary rate already disabled 
635,iII,[ wlan_vdev_misc.c : 3605 ] wal_wlm_notif pdev_id %d change secondary rate from 0x%x to 0x%x 
634,I,[ wlan_vdev_misc.c : 3611 ] wal_wlm_notif pdev_id back to default secondary rate policy 0x%x 
682,iIIII,[ wlan_vdev_keepalive.c : 752 ] KA: VDEV_MGR_AP_KEEPALIVE_INACTIVE  vdev_id = %d cur_txrx_ref_time = 0x%x last_txrx_time = 0x%xlast_tx_time = 0x%x last_rx_time = 0x%x 
681,IIi,[ wlan_vdev_keepalive.c : 763 ] KA: wlan_vdev_keepalive_ready_to_send cur_txrx_ref_time = 0x%x last_txrx_time = 0x%x inactive_time_ms = %d 
680,,[ wlan_vdev_keepalive.c : 156 ] AP_KEEPALIVE_REMOTE_PEER_FAKE_SLEEP_ENTER 
679,IIII,[ wlan_vdev_keepalive.c : 369 ] VDEV_MGR_AP_KEEPALIVE_INACTIVE  vdev_id = 0x%x assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
678,iIII,[ wlan_vdev_keepalive.c : 375 ] VDEV_MGR_AP_KEEPALIVE_UNRESPONSIVE  vdev_id = %d assoc_id = 0x%x inact_gen = 0x%x n_buffered_mpdu = 0x%x 
677,i,[ wlan_vdev_keepalive.c : 833 ] VDEV_MGR_FIRST_BMISS_DETECTED: vdev_id = %d 
676,i,[ wlan_vdev_keepalive.c : 843 ] VDEV_MGR_FINAL_BMISS_DETECTED: vdev_id = %d 
675,i,[ wlan_vdev_keepalive.c : 875 ] VDEV_MGR_BCN_IN_SYNC: vdev_id = %d  
714,iIIII,[ wlan_vdev_schedule.c : 618 ] VDEV_MGR_AP_TBTT_CONFIG: vdev_id =%d, chan_mhz = 0x%x, tbtt_link_type = 0x%x, ni_intval = 0x%x, tbtt_offset = 0x%x 
713,iII,[ wlan_vdev_schedule.c : 690 ] Corr_sta_tbtt_drift: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x 
712,iI,[ wlan_vdev_schedule.c : 1661 ] VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: vdev_id = %d, go_chan_quota_per_bi = 0x%x 
711,IIII,[ wlan_vdev_schedule.c : 1668 ] VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: curr_tsf = 0x%x, next_tbtt = 0x%x, go_time_to_tbtt = 0x%x, sta1_time_to_tbtt = 0x%x 
710,II,[ wlan_vdev_schedule.c : 1683 ] VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: tbtt_diff1 = 0x%x, tbtt_diff1 = 0x%x 
709,III,[ wlan_vdev_schedule.c : 1708 ] VDEV_MGR_OFF_CHAN_GO_CH_REQ_SETUP: tbtt_pre_slop = 0x%x, tbtt_post_slop = 0x%x, go_quota_remain = 0x%x 
708,iII,[ wlan_vdev_schedule.c : 1746 ] VDEV_MGR_HP_START_TIME: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x 
707,iIIi,[ wlan_vdev_schedule.c : 3173 ] VDEV_MGR AP Connection protection critical channel request: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x, duration = %d 
706,iIIi,[ wlan_vdev_schedule.c : 3108 ] VDEV_MGR SWBA  protection critical channel request: vdev_id = %d, chan_mhz = 0x%x, start_tsf = 0x%x, duration = %d 
705,,[ wlan_vdev_schedule.c : 1800 ] vdev_bmiss_crit_ch_req_cb: ch_req granted 
704,,[ wlan_vdev_schedule.c : 1840 ] vdev_bmiss_crit_ch_req_cb: ch_req completed without receiving beacon 
703,i,[ wlan_vdev_schedule.c : 2511 ] VDEV_MGR_FIRST_BCN_RECEIVED: vdev_id = %d 
702,i,[ wlan_vdev_schedule.c : 2516 ] VDEV_MGR_PEER_AUTHORIZED: vdev_id = %d 
701,i,[ wlan_vdev_schedule.c : 2534 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_STOP: vdev_id = %d 
700,i,[ wlan_vdev_schedule.c : 2546 ] WLAN_VDEV_DPD_CAL_START vdev_id:%d 
699,iI,[ wlan_vdev_schedule.c : 2383 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE without VDEV UP: vdev_id = %d, ch_req_flag = 0x%x 
698,i,[ wlan_vdev_schedule.c : 2420 ] VDEV_MGR_VDEV_START_OCS_HP_REQ_COMPLETE: vdev_id = %d 
697,ii,[ wlan_vdev_schedule.c : 2114 ] WLAN_VDEV_DPD_CAL_DONE vdev_id:%d ch:%d 
696,iiI,[ wlan_vdev_schedule.c : 2242 ] multi_vdev response: vdev_id=%d, num_multi_vdev_restart_compl=%d, multi_vdev_restart_bitmap=0x%x 
695,ii,[ wlan_vdev_schedule.c : 2063 ] WMI_EVENT_ALLOC_FAILURE: vdev_id = %d, opmode = %d, evt_id = WMI_PDEV_MULTIPLE_VDEV_RESTART_RESP_EVENTID 
694,i,[ wlan_vdev_schedule.c : 2088 ] multi_vdev WMI_EVENT_SEND: pdev_id = %d, event = WMI_PDEV_MULTIPLE_VDEV_RESTART_RESP_EVENTID 
693,ii,[ wlan_vdev_schedule.c : 1984 ] WMI_EVENT_ALLOC_FAILURE: vdev_id = %d, opmode = %d, evt_id = WMI_VDEV_START_RESP_EVENTID 
692,ii,[ wlan_vdev_schedule.c : 2037 ] WMI_EVENT_SEND: vdev_id = %d, opmode = %d, event = WMI_VDEV_START_RESP_EVENTID 
691,iII,[ wlan_vdev_schedule.c : 3403 ] wlan_vdev_sta_concurrency_event_handler: vdev_id = %d, next_state  = 0x%x, cur_state = 0x%x 
690,,[ wlan_vdev_schedule.c : 3040 ] VDEV_MGR_FIRST_BMISS_DETECTED: Post Critical ch_req 
689,iIII,[ wlan_vdev_schedule.c : 1425 ] VDEV_MGR_AP_TBTT_CONFIG: vdev_id = %d, chan_mhz = 0x%x, tbtt_link_type = 0x%x, ap_tbtt_offset = 0x%x 
688,i,[ wlan_vdev_schedule.c : 2678 ] wlan_vdev_up_ch_req_setup noA_disableEnable_P2pgo:%d  
687,iI,[ wlan_vdev_schedule.c : 2823 ] VDEV_MGR_LOWPOWER_HP_CHREQ_ENABLED: vdev_id = %d, chan_mhz  = 0x%x 
686,iII,[ wlan_vdev_schedule.c : 2906 ] VDEV_MGR_HP_START_TIME: vdev_id = %d, chan_mhz  = 0x%x, start_tsf = 0x%x 
685,iI,[ wlan_vdev_schedule.c : 2941 ] VDEV_MGR_LOWPOWER_LP_CHREQ_ENABLED: vdev_id = %d, factor = 0x%x 
684,iI,[ wlan_vdev_schedule.c : 2947 ] VDEV_MGR_LOWPOWER_LP_CHREQ_ENABLED: vdev_id = %d, factor = 0x%x 
683,iII,[ wlan_vdev_schedule.c : 2965 ] VDEV_MGR_OCS_HP_LP_REQ_POSTED: vdev_id = %d, hp_ch_req = 0x%x, lp_ch_req = 0x%x 
730,iI,[ wlan_vdev_pause.c : 499 ] VDEV Unpause Failure: VDEV ID = %d pause_bitmap = 0x%x in Unpause complete 
729,ii,[ wlan_vdev_pause.c : 1275 ] Disable leaky AP CTS2S: vdev_id = %d pause_delay_us = %d  
728,I,[ wlan_vdev_pause.c : 1278 ] enable_null_leaky_ap_pause=0x%x 
727,III,[ wlan_vdev_pause.c : 133 ] force leak ap check oui:%x, latency level:%x, a2dp:%x 
726,III,[ wlan_vdev_pause.c : 147 ] force leak ap check oui:%x, latency level:%x, a2dp:%x 
725,I,[ wlan_vdev_pause.c : 609 ] vdev->bcn_tx_paused_wlan_vdev_pause_1=0x%x 
724,,[ wlan_vdev_pause.c : 627 ] VDEV_PAUSE_FAIL ifPaused set with pause_bitmap = 0 in _wlan_vdev_pause 
723,IiiiI,[ wlan_vdev_pause.c : 693 ] VDEV_MGR_VDEV_PAUSE: enable_null_leaky_ap_pause=0x%x no_null_to_ap_for_roaming=%d leakyAp_cts2s_enable=%d pause_delay_us=%d req from mod_id = %x 
722,iiiii,[ wlan_vdev_pause.c : 272 ] VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = LEAKY AP DETECTED data_null_tx_delay = %d actual_leak_window = %d pause_delay_us = %d consec_detect_leaky_ap_cnt = %d 
721,iiiii,[ wlan_vdev_pause.c : 407 ] VDEV_MGR_VDEV_PAUSE_DELAY_UPDATE: vdev_id = %d avg_data_null_tx_delay = %d avg_rx_leak_window = %d pause_delay_us = %d is_bt_connected = %d 
720,iiiii,[ wlan_vdev_pause.c : 327 ] VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = FAILURE data_null_tx_delay = %d avg_data_null_tx_delay = %d actual_leak_window = %d avg_rx_leak_window = %d 
719,iiiii,[ wlan_vdev_pause.c : 350 ] VDEV_MGR_VDEV_PAUSE_COMP: vdev_id = %d pause_status = SUCCESS data_null_tx_delay = %d avg_data_null_tx_delay = %d actual_leak_window = %d avg_rx_leak_window = %d 
718,i,[ wlan_vdev_pause.c : 1286 ] no_null_to_ap_for_roaming=%d 
717,I,[ wlan_vdev_pause.c : 877 ] VDEV_UNPAUSE_FAIL: ifPaused not set with pause_bitmap = 0x%x in _wlan_vdev_unpause 
716,,[ wlan_vdev_pause.c : 918 ] VDEV_MGR_VDEV_PAUSE unpause non_protocol_unpaused 
715,,[ wlan_vdev_pause.c : 984 ] VDEV_MGR_VDEV_PAUSE csa_roaming_ongoing and no host unpause 
735,,[ wlan_vdev_unit_test.c : 86 ] wlan_vdev_config_test: vdev is NULL 
734,iiii,[ wlan_vdev_unit_test.c : 157 ] wlan_vdev_unit_test: vdev_id = %d, custom_sw_retry_th_cmd, ac %d sw_retry_type = %d sw_retry_th = %d 
733,I,[ wlan_vdev_unit_test.c : 232 ] wlan_vdev_unit_test: g_wmi_cmd_enable_pf_log = 0x%x 
732,iiiii,[ wlan_vdev_unit_test.c : 100 ] wlan_vdev_config_test: vdev_id = %d, test_cmd = %d, args[1] = %d, args[2] = %d, num_args = %d  
731,iii,[ wlan_vdev_unit_test.c : 135 ] wlan_vdev_unit_test: vdev_id = %d, custom_aggr_size_cmd, subfram %d ac = %d 
746,II,[ wlan_coex_main.c : 1685 ] COEX_BT_ACTIVITY: prof_bitmap(0x%x), scan_bitmap(0x%x) 
745,Iii,[ wlan_coex_main.c : 518 ] WLAN_COEX_LEAKYAP_NULL: found(%u) vdev_id = %d, enable_null_pause = %d 
744,iI,[ wlan_coex_main.c : 956 ] WLAN_COEX_MCS_RATE: status(%d) mcs(%u) 
743,iI,[ wlan_coex_main.c : 1702 ] COEX_GENERIC_ERROR: Set TDM Guard Period to %d, Error (0x%x) 
742,,[ wlan_coex_main.c : 410 ] WLAN_COEX_LEAKYAP: Enable NULL for Leaky Ap for scan + a2dp/ble scan! 
741,,[ wlan_coex_main.c : 442 ] WLAN_COEX_LEAKYAP: Disable NULL for Leaky AP Pause due to Scan Stop ! 
740,I,[ wlan_coex_main.c : 911 ] WLAN_COEX_SET_SWBMISS: wlan_vdev_t is NULL, enable: %u 
739,I,[ wlan_coex_main.c : 1034 ] WLAN_COEX_VDEV_CREATE: Error(0x%x) 
738,iIIII,[ wlan_coex_main.c : 301 ] WLAN_COEX_VDEV_PAUSE: status(%d) max_time(%u) pause(%u) softAp(%u) opmode(%u) 
737,IiIii,[ wlan_coex_main.c : 199 ] WLAN_COEX_TXRX_CB: frameType 0x%x vdev %d txSt 0x%x flush %d consFlshCnt %d 
736,ii,[ wlan_coex_main.c : 1715 ] WLAN_COEX_SLEEP: Received WOW Entered/Exit event from OffloadMgr %d,                                                        pCOEX->is_wow_entered = %d 
748,i,[ wlan_coex_mws.c : 108 ] COEX_MWS_OTHER: evh is NULL, WMI_WLAN_FREQ_AVOID_EVENTID NOT send : Retry counter=%d 
747,i,[ wlan_coex_mws.c : 148 ] COEX_MWS_OTHER: WMI_WLAN_FREQ_AVOID_EVENTID send : Retry counter=%d 
749,II,[ wlan_coex_11ax.c : 86 ] COEX_BT_ACTIVITY: is_bt_on %u  mac_2g %u 
763,IIIII,[ wlan_coex_ps.c : 132 ] COEX_PSP_STAT_1: Resp0(%u) Resp1(%u) Resp2(%u) Resp3(%u) Resp4(%u) 
762,IIIII,[ wlan_coex_ps.c : 135 ] COEX_PSP_STAT_2: DP(%u) Max(%u) RespIdx(%u) ValidDps(%u) PsPAvg(%u) 
761,I,[ wlan_coex_ps.c : 560 ] COEX_PSP_ERROR: COEX_PSP_ERROR_VDEV_NULL Stimulus(%u) 
760,iiIiI,[ wlan_coex_ps.c : 697 ] COEX_PSP_RX_STATUS_STATE_1: ExpTS(%d) ActTS(%d) IsOverRun(%u) RespOverUnderRunTime(%d) ApResponseRxDuration(%u) 
759,,[ wlan_coex_ps.c : 740 ] COEX_PSP_SEND_PSPOLL: 0 
758,IIII,[ wlan_coex_ps.c : 766 ] COEX_PSP_NONWLAN_INTERVAL: BaseIntrvl(%u) NonWlanIdleTime(%u) PsPollSpecInterval(%u) ApResponseTimeout(%u) 
757,IIIIIII,[ wlan_coex_ps.c : 801 ] COEX_PSP_MGR: Error(0x%x) Stimulus (%u) State(0x%x), Avg(%u) EstimationOverun(%u) SpecCount(%u) MoreData(%u) 
756,II,[ wlan_coex_ps.c : 474 ] COEX_PSP_SEND_PSPOLL: State(0x%x) PSPNum(%u) 
755,,[ wlan_coex_ps.c : 520 ] COEX_PSP_SEND_PSPOLL: 0 
754,IiIiI,[ wlan_coex_ps.c : 525 ] COEX_PSP_READY_STATE: T2NonWlan(%u) EndTS(%d) MoreData(%u) ExpTS(%d) NonWlanIdleTime(%u) 
753,,[ wlan_coex_ps.c : 528 ] COEX_PSP_SEND_PSPOLL: 0 
752,IIIIII,[ wlan_coex_ps.c : 510 ] COEX_PSP_SPEC_POLL: En(%u) Count(%u) TS(%u) AllowSpecPsPollTx(%u) Delta(%u) Intrvl(%u) 
751,III,[ wlan_coex_ps.c : 88 ] COEX_PSP_SEND_PSPOLL: status(0x%x) PsPollState(0x%x) PsPollNum(%u) 
750,IIII,[ wlan_coex_ps.c : 59 ] WLAN_COEX_SLEEP: status(%u) enable(%u) mac(%u) reason(%u) 
779,,[ wlan_coex_ocs.c : 821 ] COEX_GENERIC_ERROR: Defer the Disable NULL for Leaky AP Pause due to A2DP Stop during Scan to SCAN_COMPLETE ! 
778,,[ wlan_coex_ocs.c : 865 ] COEX_GENERIC_ERROR: Enable NULL for Leaky AP Pause due to A2DP Start during Scan ! 
777,IIIiIi,[ wlan_coex_ocs.c : 928 ] WLAN_COEX_OCS_MGR: Stimulus(%u) Status(%u) State(0x%x) ExpBtStartTime(%d) now(%u) delta(%d) 
776,,[ wlan_coex_ocs.c : 1229 ] COEX_GENERIC_ERROR: Enable NULL for Leaky AP Pause due to A2DP Start during Scan ! 
775,IIIiIi,[ wlan_coex_ocs.c : 1281 ] WLAN_COEX_LL_OCS_MGR: Stimulus(%u) Status(%u) State(0x%x) ExpBtStartTime(%d) now(%u) delta(%d) 
774,IIIIi,[ wlan_coex_ocs.c : 1298 ] WLAN_COEX_LL_OCS_RECOMP: State(0x%x) A2dpCrit(%u), ExpBtStartTime(%u), now (%u) delta(%d)  
773,IIIIIii,[ wlan_coex_ocs.c : 1135 ] WLAN_COEX_OCS_RECOMP: State(0x%x) A2dpCrit(%u), ExpBtStartTime(%u), ExpBtStartTimeUT(%u), now (%u) delta(%d) delta_ut(%d) 
772,iI,[ wlan_coex_ocs.c : 246 ] WLAN_OCS_RESTART: rc(%d) vdev_id(%u) 
771,,[ wlan_coex_ocs.c : 936 ] COEX_SYNC_OCS_GRANTTIMER: ocs grant delayed timer fired 
770,IiIIi,[ wlan_coex_ocs.c : 383 ] WLAN_OCS_REQ: Error(0x%x), status(%d) ocs_req_state(0x%x) bt_req(0x%x) priority(%d) 
769,IIIi,[ wlan_coex_ocs.c : 463 ] WLAN_OCS_REQ: OCS Start: COEX_OCS_START_ERROR (0x%x), ocs_req_state(0x%x) bt_req(0x%x) priority(%d) 
768,,[ wlan_coex_ocs.c : 956 ] COEX_SYNC_OCS_LEAKY: Defer the Disable NULL for Leaky AP Pause due to A2DP Stop during Scan to SCAN_COMPLETE ! 
767,IIIIIii,[ wlan_coex_ocs.c : 1066 ] WLAN_COEX_SYNC_OCS_MGR: stimulus(%u) status(%u) state(0x%x) exp_bt_start(0x%x) now(0x%x) delta(%d) timer_dur(%d) 
766,IIII,[ wlan_coex_ocs.c : 1110 ] COEX_SYNC_OCS_RECOMP: status(%u) state(%u) bt_start_tsf(0x%x) dur(%u) 
765,IiIIi,[ wlan_coex_ocs.c : 758 ] WLAN_OCS_UPDATE: Error(0x%x) status(%d) ocs_req_state(0x%x) bt_req(0x%x) priority(%d) 
764,IIi,[ wlan_coex_ocs.c : 526 ] WLAN_COEX_BTREQ: One Shot  0x%x 0x%x priority(%d) 
780,i,[ wlan_coex_test.c : 317 ] Automation Code %d 
781,I,[ wlan_coex_gnss.c : 56 ] WLAN_COEX_GNSS: demod_cmd(%u) 
791,,[ wlan_coex_sar.c : 179 ] COEX_GENERIC_ERROR: [SAR][Error] cannot get SAR limits from FW to send to host 
790,,[ wlan_coex_sar.c : 183 ] COEX_GENERIC_ERROR: [SAR][Error] cannot get correct number of SAR limits from FW to send to host 
789,,[ wlan_coex_sar.c : 193 ] COEX_MWS_OTHER: [SAR] deprecated SAR limit command was triggered 
788,III,[ wlan_coex_sar.c : 61 ] COEX_MWS_OTHER: [SAR] sar_enable=0x%x, num_limit_rows=0x%x commit_limits=0x%x 
787,IIIII,[ wlan_coex_sar.c : 67 ] WLAN_MODULE_COEX: [SAR] band_id=0x%x, chain_id=0x%x, mod_id=0x%x, limit_value=0x%x validity_bitmap=0x%x 
786,IIi,[ wlan_coex_sar.c : 75 ] COEX_MWS_OTHER: [SAR] WMI callback - error in parsing cmd(0x%x) buffer(0x%x) len(%d) 
785,i,[ wlan_coex_sar.c : 325 ] COEX_GENERIC_ERROR: [TAS] Receive CMD: WMI_TAS_POWER_HISTORY_CMDI, subtype:%d 
784,,[ wlan_coex_sar.c : 336 ] COEX_GENERIC_ERROR: [TAS] Receive CMD: WMI_TAS_POWER_HISTORY_CMDI, subtype not support 
783,i,[ wlan_coex_sar.c : 292 ] COEX_GENERIC_ERROR: [TAS] save power history evt->sub_type[%d] and send WMI_TAS_POWER_HISTORY_EVENTID 
782,,[ wlan_coex_sar.c : 307 ] COEX_GENERIC_ERROR: [TAS] restore power history fail 
793,II,[ wlan_coex_cts2s.c : 247 ] WLAN_COEX_CTS2S_TIMEOUT: Now : %u, WbPrepare: %u 
792,I,[ wlan_coex_cts2s.c : 346 ] COEX_GENERIC_ERROR: COEX_ERROR_UNKNOWN_NULLPTR Status(%u) 
794,iIIII,[ wlan_mlme_utils.c : 1337 ] OCV validation failed status = %d freq = %x channel_width = %x bw_offset = %x seg1 = %x 
813,,[ wlan_11k_offload.c : 207 ] 11K_OFFLOAD_neighbor_report_response num_candidates 0 
812,i,[ wlan_11k_offload.c : 214 ] 11K_offload_ACT_FRAME_HDR error_code=%d 
811,i,[ wlan_11k_offload.c : 82 ] BUILD_11K_CHANMAP freq=%d 
810,,[ wlan_11k_offload.c : 597 ] 11K_offload_COMP_CONFIG 
809,ii,[ wlan_11k_offload.c : 407 ] 11K_offload_IS_CHANMAP_AVAIL: radio_measurement_enabled: %d neighbor_report_offloaded %d 
808,i,[ wlan_11k_offload.c : 414 ] 11K_offload_IS_CHANMAP_AVAIL: num_candidates %d 
807,ii,[ wlan_11k_offload.c : 57 ] NEIGHBOR_REPORT_REQ_COMPLETION Status: %d, Dialog Token: %d 
806,i,[ wlan_11k_offload.c : 649 ] wlan_11k_offload_per_notify_handler region: %d 
805,i,[ wlan_11k_offload.c : 235 ] 11K_offload_SEND_NEIGHBOR_REP_REQ radio_measurement_enabled: %d 
804,ii,[ wlan_11k_offload.c : 244 ] 11K_offload_SEND_NEIGHBOR_REP_REQ current_capping %d auth=%d 
803,,[ wlan_11k_offload.c : 463 ] 11K_offload_SETUP_RSSI_THRESHOLDS threshold not set 
802,ii,[ wlan_11k_offload.c : 482 ] 11K_offload_SETUP_RSSI_THRESHOLDS low_rssi_threshold:%d high_rssi_threshold:%d 
801,i,[ wlan_11k_offload.c : 498 ] 11K_offload_SWBMISS_EVT_HDLR evt_type:%d 
800,,[ wlan_11k_offload.c : 574 ] 11K_offload_de_config 
799,ii,[ wlan_11k_offload.c : 673 ] 11K_offload_VDEV_PARAM_CONFIG vdev_id:%d %d 
798,iiiiii,[ wlan_11k_offload.c : 712 ] 11K_offload_VDEV_PARAM_CONFIG bmiss_count_trigger: %d low_rssi_offset: %d neighbor_report_req_cap: %d neighbor_rep_cache_timeout: %d per_threshold_offset: %d time_offset: %d 
797,i,[ wlan_11k_offload.c : 740 ] 11K_INVOKE_NEIGHBOR_REP_REQ ssid_len %d  
796,,[ wlan_11k_offload.c : 346 ] 11k_offload: Current AP is in LRA list 
795,i,[ wlan_11k_offload.c : 363 ] 11K_offload_RSSI_EVT_HDLR: Threshold met evt_type %d 
845,,[ wlan_pmf_offload.c : 1184 ] 11w PMF: PN Replay attack detected 
844,i,[ wlan_pmf_offload.c : 52 ] mmie drop count:%d 
843,,[ wlan_pmf_offload.c : 261 ] 11W PMF: Beacon add MMIE No pmf_info or PMF is disabled 
842,i,[ wlan_pmf_offload.c : 287 ] 11W PMF: Beacon add MMIE can not handle frame size: %d 
841,i,[ wlan_pmf_offload.c : 268 ] 11W PMF: Beacon add MMIE No BIGTK installed key length: %d 
840,iiii,[ wlan_pmf_offload.c : 1064 ] 11w PMF KEY ID MISMATCH MMIE is_bcn = %d key_id = %d, bigtk_key_id = %d igtk_key_id = %d 
839,i,[ wlan_pmf_offload.c : 176 ] 11W PMF : Beacon protection already enabled on vdev %d 
838,i,[ wlan_pmf_offload.c : 748 ] 11w PMF: can not handle frame size: %d 
837,,[ wlan_pmf_offload.c : 767 ] 11w PMF: IE is not Mgmt MIC IE or Invalid length 
836,,[ wlan_pmf_offload.c : 789 ] 11w PMF: BC/MC/Beacon MGMT IPN check Failed 
835,iI,[ wlan_pmf_offload.c : 799 ] 11w PMF: is_bcn=%d, replay_err_cnt=%x 
834,,[ wlan_pmf_offload.c : 861 ] 11w PMF: BC/MC/Beacon CMAC MGMT frame MMIE MIC check Failed 
833,iI,[ wlan_pmf_offload.c : 871 ] 11w PMF: is_bcn=%d,mic_fail_cnt=%x 
832,,[ wlan_pmf_offload.c : 930 ] 11w PMF: BC/MC/Beacon GMAC MGMT frame MMIE MIC check Failed 
831,iI,[ wlan_pmf_offload.c : 940 ] 11w PMF: is_bcn=%d,mic_fail_cnt=%x 
830,,[ wlan_pmf_offload.c : 987 ] 11W PMF: MMIE valid 
829,,[ wlan_pmf_offload.c : 1261 ] 11W PMF mgmt hdlr pmf not enabled 
828,,[ wlan_pmf_offload.c : 1275 ] 11W PMF mgmt hdlr Beacon Protection not enabled 
827,,[ wlan_pmf_offload.c : 1280 ] 11W PMF mgmt hdlr pmf not enabled 
826,,[ wlan_pmf_offload.c : 1295 ] 11W PMF mgmt hdlr frame not from Associated AP  
825,,[ wlan_pmf_offload.c : 1328 ] 11w PMF BIP check failed  
824,I,[ wlan_pmf_offload.c : 1343 ] 11w PMF decrypt error, rx status 0x%x 
823,,[ wlan_pmf_offload.c : 1424 ] 11w PMF SA query rsp with valid transId rcvd 
822,ii,[ wlan_pmf_offload.c : 590 ] 11W PMF: SA query timeout hdlr vdevId=%d, query_state=%d  
821,ii,[ wlan_pmf_offload.c : 595 ] 11W PMF: SA query timeout hdlr cur retry cnt=%d, max retry cnt=%d  
820,iiii,[ wlan_pmf_offload.c : 1121 ] 11W PMF: Send SA query vdevId=%d, transId=%d query_type=%d tx_status=%d 
819,iii,[ wlan_pmf_offload.c : 200 ] 11W PMF: Update BiGTK vdevId=%d, keyIdx=%d, KeyLen=%d 
818,,[ wlan_pmf_offload.c : 220 ] igtk: Same key reinstalled 
817,iii,[ wlan_pmf_offload.c : 683 ] 11W PMF: Update iGTK vdevId=%d, keyIdx=%d, KeyLen=%d 
816,,[ wlan_pmf_offload.c : 700 ] igtk: Same key reinstalled 
815,iii,[ wlan_pmf_offload.c : 643 ] 11W PMF Offload CMD hdlr: WMI_PMF_OFFLOAD_SET_SA_QUERY_CMDID vdevId=%d, interval=%d, retry_count=%d 
814,,[ wlan_pmf_offload.c : 1503 ] 11w PMF is not enabled 
871,IiI,[ wlan_roam.c : 866 ] ROAM_DISABLE client_id = 0x%x curr_state = %d cur_disable_bitmap = 0x%x 
870,II,[ wlan_roam.c : 845 ] ROAM_ENABLE client_id = 0x%x cur_disable_bitmap = 0x%x 
869,I,[ wlan_roam.c : 883 ] ROAM_ENABLE_DISABLE_ERROR client_id = 0x%x 
868,iiiI,[ wlan_roam.c : 1063 ] ROAM_ENABLE_DISABLE_TRIGGER client_id=%d enable=%d reason=%d disable_trigger_mask=0x%x 
867,I,[ wlan_roam.c : 801 ] ROAM_GET_VDEV_ROAM error code = 0x%x 
866,i,[ wlan_roam.c : 2120 ] wlan_roam_send_capability_info_to_host memory allocation failed, %d 
865,iI,[ wlan_roam.c : 919 ] ROAM_UPDATE_BSSID_EXT_CAP len=%d cap=0x%x 
864,I,[ wlan_roam.c : 948 ] ROAM_UPDATE_RME cap=0x%x 
863,iIi,[ wlan_roam.c : 1619 ] ROAM_WLM_NOTIF_HDLR policy=%d flags=0x%x level=%d 
862,I,[ wlan_roam.c : 1079 ] ROAM_PARAM_SET scan_mode 0x%x 
861,iii,[ wlan_roam.c : 1954 ] VDEV_ROAM_MY_BEACON_PARSED malformed id = %d len=%d remain_len=%d 
860,iiI,[ wlan_roam.c : 2021 ] VDEV_ROAM_MY_BEACON_BAD_IE id=%d,len=%d,status=0x%x 
859,ii,[ wlan_roam.c : 2042 ] VDEV_ROAM_HDL_OWN_BEACON neighbor report not offloaded yet %d %d 
858,ii,[ wlan_roam.c : 538 ] ROAM_SET_CFG_PARAM since roam offload is disabled on vdev=%d param = %d 
857,ii,[ wlan_roam.c : 1688 ] Roam Candidate MIN RSSI: reason = %d min_rssi = %d 
856,iIii,[ wlan_roam.c : 448 ] ROAM_FW_OFFLOAD_ENABLE vdev_id=%d flags=0x%x roam_offld=%d roam_offld_num=%d 
855,IIiiiI,[ wlan_roam.c : 474 ] ROAM_SET_SCAN_MODE curr_scan_mode=%x new_scan_mode=%x running=%d roam_state=%d scan_delay_time=%d msec trigger_reason_bitmask=0x%x 
854,i,[ wlan_roam.c : 1247 ] ROAM_DEV_START_FAIL error_code=%d 
853,IIIII,[ wlan_roam.c : 1273 ] ROAM_CMP_CIPHER: auth_mode=%x, ucipher=%x, gcipher=%x, mgmtcipher=%x pmf=%x 
852,,[ wlan_roam.c : 1291 ] ROAM_CHANMAP_VDEV_START reset chanmap due to different ssid 
851,,[ wlan_roam.c : 1309 ] ROAM_CHANMAP_VDEV_START keep chanmap due to same ssid 
850,iI,[ wlan_roam.c : 1327 ] ROAM_DENSE_START is_dense = %d ap|dense_ssid_len = 0x%x 
849,iI,[ wlan_roam.c : 1251 ] ROAM_DEV_START: vdev_id = %d runnning: 0x%x 
848,iIiIi,[ wlan_roam.c : 1265 ] ROAM_CHANMAP_CMP_SSID: vdev_id = %d, prev AP 1st_4B=%lu len=%d, new AP 1st_4B=%lu, len=%d 
847,ii,[ wlan_roam.c : 1374 ] ROAM_DEV_STOP vdev_id=%d running=%d 
846,Iiiiii,[ wlan_roam.c : 575 ] ROAM_TRIGGER_CONFIG_PARAM Reason_ID|enable|scan_mode|reason_code = %x score_delta = %d cnd_min_rssi = %d trigger_rssi = %d cnd_min_rssi_5g = %d cnd_min_rssi_6g = %d 
876,,[ wlan_roam_bg_scan.c : 154 ] ROAM_BETTER_AP_EVENT 
875,ii,[ wlan_roam_bg_scan.c : 219 ] ROAM_SCAN_EXTSCAN_CHECK cur_rssi = %d good_rssi_threshold = %d 
874,,[ wlan_roam_bg_scan.c : 252 ] ROAM_BETTER_AP_EVENT 
873,ii,[ wlan_roam_bg_scan.c : 36 ] ROAM_BG_RSSI data_rssi = %d dBm inactivity_ts = %d 
872,iiII,[ wlan_roam_bg_scan.c : 70 ] ROAM_BG_SCAN_CONFIG bad_rssi_thresh_2g = %d bad_rssi_thresh_5g = %d client_bitmap = 0x%x flags=0x%x 
893,iiiii,[ wlan_roam_candidate.c : 1007 ] ROAM_CANDIDATE_RSSI_ADJUST rssi = %d dBm boost_threshold = %d dBm boost_factor = %d penalty_threshold = %d dBm penalty_factor = %d 
892,iiii,[ wlan_roam_candidate.c : 951 ] ROAM_BETTER_CANDIDATE_FOUND valid_cnd = %d is_beacon = %d candidate_rssi_last = %d dBm curr_rssi_avg = %d dBm 
891,,[ wlan_roam_candidate.c : 1202 ] ROAM_ELIGIBLE: Ignore Score 
890,ii,[ wlan_roam_candidate.c : 1402 ] ROAM_5G_SELF_RSSI_ADJUST rssi = %d dBm adjust_self = %d 
889,iIIIiiIi,[ wlan_roam_candidate.c : 902 ] ROAM_BCN_PRB_CHECK vdev_id=%d bssid = %08x%04x primary ch freq = 0x%x rssi = %d dBm is_roamable = %d seq = 0x%04x roamable_ec=%d 
888,iIIIiiIi,[ wlan_roam_candidate.c : 914 ] ROAM_BCN_PRB_CHECK vdev_id=%d bssid = %08x%04x primary ch freq = 0x%x rssi = %d dBm is_roamable = %d seq = 0x%04x roamable_ec=%d 
887,IIIIiiII,[ wlan_roam_candidate.c : 570 ] ROAM_RSN rsn_mcastmgmtcipherset=0x%x profile->rsn_mcastmgmtcipherset=0x%x mfp_match(8-15)|mfp_enable(0-7)=0x%08x self_mfp_cap(24-31)|self_mfp_req(16-23)|mfp_cab_ap(8-15)|mfp_req_ap(0-7)=0x%08x mfp_match=%d is_sae_h2e_ap=%d prof_authmode=0x%08x authmode=0x%08x 
886,iiIIIiI,[ wlan_roam_candidate.c : 611 ] ROAM_RSN_MISMATCH status=%d rsn&wpa=%d ucipher=0x%08x mcipher=0x%08x mfp_enable(bit2)/ap_cap(bit1)/ap_req(bit0)=%x adaptive_11r=%d sae_h2e_only(bit1)/ap_cap(bit0)=0x%x 
885,iIIii,[ wlan_roam_candidate.c : 156 ] ROAM_RSSI_REJECTED_AP_ALLOW_UPDATE new_list = %d, bssid %08x%04x exp_delay = %d msec, exp_rssi = %ddBm 
884,i,[ wlan_roam_candidate.c : 205 ] valid_entries=%d 
883,i,[ wlan_roam_candidate.c : 339 ] ROAM_CHANMAP_UPDATE_OWE chan_freq=%d 
882,iIIIIIIIii,[ wlan_roam_candidate.c : 1545 ] ROAM_CONFIG_AP_PROFILE ssid_len = %d short_ssid=0x%x rssi_margin|bg_rssi_margin = 0x%08x dBm rsn_authmode = 0x%x rsn_mipher = 0x%x rsn_ucipher = 0x%x rsn_grp_mgmt_cipher = 0x%x flags = 0x%x abs_threh = %d bg_rssi_margin = %d 
881,iiiii,[ wlan_roam_candidate.c : 1580 ] boost_algo = %d boost_threshold = %d dBm boost_factor = %d max_boost = %d, param1 = %d 
880,iiiii,[ wlan_roam_candidate.c : 1588 ] penal_algo = %d penal_threshold = %d dBm penal_factor = %d max_penal = %d, param2 = %d 
879,iIIi,[ wlan_roam_candidate.c : 1672 ] ROAM_PREFERRED_BSSID id = %d bssid = %08x%04x factor = %d 
878,IIiiii,[ wlan_roam_candidate.c : 1508 ] ROAM_CONFIG_ROAM_FILTER flag = 0x%x op_bitmap = 0x%x num_whitelist = %d num_blacklist = %d num_preferred_bssid = %d rssi_rejected_ap = %d 
877,iiIII,[ wlan_roam_candidate.c : 1630 ] ROAM_WHITELIST SSID[%d] ssid_len = %d, ssid[0-3][4-7][8-11] = 0x%08x %08x %08x 
923,iii,[ wlan_roam_scan.c : 725 ] ROAM_CHANMAP_UPDATE_HINT id=%d chan_freq=%d fast_passive_prefer=%d 
922,iiii,[ wlan_roam_scan.c : 738 ] ROAM_CHANMAP_UPDATE_HINT id=%d chan_freq=%d whitessid=%d fast_passive_prefer=%d 
921,ii,[ wlan_roam_scan.c : 751 ] ROAM_CHANMAP_UPDATE id=%d chan_freq=%d 
920,iIiii,[ wlan_roam_scan.c : 243 ] ROAM_FINAL_BMISS_SCAN deauth=%d scan_policy=0x%x,skip_dfs=%d,active_dwell=%d burst_dur=%d 
919,i,[ wlan_roam_scan.c : 467 ] use_11k_chan_map %d 
918,iiiiii,[ wlan_roam_scan.c : 610 ] ROAM_SCAN_REQUESTED id=%d send_beacon_to_host = %d scan_type(FULL 0/CHANLIST 1/CHANMAP 2/FORCED 3/5G_ONLY 4) = %d roam_scan_state (IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d final_scan = %d num_chan = %d 
917,,[ wlan_roam_scan.c : 341 ] ROAM_SCAN_6G fault 
916,iI,[ wlan_roam_scan.c : 365 ] ROAM_SCAN_6G add ssid hint at freq = %d short_ssid = 0x%x 
915,ii,[ wlan_roam_scan.c : 381 ] ROAM_SCAN_6G add ssid hint at freq=%d white_ssid_idx=%d 
914,ii,[ wlan_roam_scan.c : 188 ] ROAM_HO_FILTER_DISALLOW: before cnt=%d, after cnt=%d 
913,iiIii,[ wlan_roam_scan.c : 83 ] ROAM_SCAN_REJECTED_CHECK scan_mode %d trigger_reason %d disabled_trigger_mask 0x%x scan_status %d key_offld_to_host %d 
912,iiiiI,[ wlan_roam_scan.c : 134 ] ROAM_SCAN_REJECTED diff %d (last %d cur %d) < %d trigger_bitmap = 0x%x 
911,iI,[ wlan_roam_scan.c : 690 ] ROAM_CHANMAP[%d] 0x%x 
910,iI,[ wlan_roam_scan.c : 692 ] ROAM_CHANMAP[%d] 0x%x 
909,iI,[ wlan_roam_scan.c : 696 ] ROAM_CHANMAP[%d] 0x%x 
908,,[ wlan_roam_scan.c : 1843 ] ROAM_SCAN_NO_AP 
907,iIiiii,[ wlan_roam_scan.c : 1852 ] ROAM_SCAN_COMPLETE id=%d candidate_found = 0x%x roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d final_scan = %d send_bcn_to_host = %d wlm_mode = %d 
906,iIII,[ wlan_roam_scan.c : 1858 ] ROAM_SCAN_COMPLETE_1  reason(SUCC 0/CANCEL 1/PREEMPTED 2/TIMEOUT 3/INTERNAL FAIL 4) = %d evt_scan_id = 0x%x sta_kickout|invoke_roaming = 0x%x trigger_reason = 0x%x 
905,ii,[ wlan_roam_scan.c : 1952 ] ROAM_SUPRESS_FINAL_SCAN roamable_ap_cnt=%d curr_low=%d dBm 
904,iIIiiiii,[ wlan_roam_scan.c : 2495 ] ROAM_SCAN_STARTED id=%d evt_type 0x%x scan_id = 0x%x roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d is_lazy = %d is_bg_roam = %d cur_rssi = %d dBm bad_rssi_thres = %d dBm 
903,IIIi,[ wlan_roam_scan.c : 2530 ] ROAM_SCAN_CANCELLED  scan_id = 0x%x type = 0x%x reason = 0x%x sta_kickout = %d 
902,i,[ wlan_roam_scan.c : 1607 ] ROAM_NOT_ELIGIBLE_AP ec=%d 
901,,[ wlan_roam_scan.c : 2385 ] ROAM_SCAN_FAIL 
900,i,[ wlan_roam_scan.c : 2242 ] ROAM_CHANMAP_UPDATE_FROM_CHNL_LIST chan_num=%d 
899,iiii,[ wlan_roam_scan.c : 2250 ] ROAM_SET_CHAN_LIST type=%d num_chans=%d chan0_freq=%d chan1_freq=%d 
898,iiiiii,[ wlan_roam_scan.c : 2178 ] ROAM_SCAN_PARAMS dtime_act:%d dtime_pass:%d burst_dur:%d min_rest:%d max_rest:%d repeat_prob:%d 
897,iiiIiI,[ wlan_roam_scan.c : 2188 ] ROAM_SCAN_PARAMS idle_time:%d max_scan_time:%d probe_delay:%d scan_ctrl_flags:0x%x n_probes:%d scan_ctrl_flags_ext:0x%x 
896,ii,[ wlan_roam_scan.c : 2201 ] ROAM_SCAN_PARAMS dtime_act_6g = %d dtime_pass_6g = %d 
895,ii,[ wlan_roam_scan.c : 2263 ] ROAM_SCAN_TIMER_STOP  id = %d (periodic 1/hirssi 2/first bmiss 3/rssi_config 4/per rest 5/final bmiss 6/bss load 7) interval = %d(msec) 
894,ii,[ wlan_roam_scan.c : 2271 ] ROAM_SCAN_TIMER_START  id = %d (periodic 1/hirssi 2/first bmiss 3/rssi_config 4/per rest 5/final bmiss 6/bss load 7) interval = %d(msec) 
933,,[ wlan_roam_trace.c : 968 ] ROAM BUFFER START: 
932,,[ wlan_roam_trace.c : 981 ] ROAM BUFFER END 
931,IIIIIIII,[ wlan_roam_trace.c : 973 ] %x %x %x %x %x %x %x %x 
930,I,[ wlan_roam_trace.c : 978 ] %x 
929,i,[ wlan_roam_trace.c : 1149 ] Roam handoff start: PAGE_FAULT_COUNTER: %d
 
928,i,[ wlan_roam_trace.c : 1153 ] Roam handoff complete: PAGE_FAULT_COUNTER: %d
 
927,ii,[ wlan_roam_trace.c : 1171 ] ROAM_HO_KPI_START PF = %d time = %d 
926,iiii,[ wlan_roam_trace.c : 1185 ] ROAM_HO_KPI_STOP PF = %d [delta: %d] time = %d [delta: %d] 
925,i,[ wlan_roam_trace.c : 1133 ] roam etm log is enable: %d
 
924,i,[ wlan_roam_trace.c : 886 ] ROAM_FAIL_REASON = %d 
976,iiiii,[ wlan_roam_wmi.c : 361 ] ROAM_EVENT_TO_HOST reason=%d, notif=%d, notif_params=%d, ret=%d ev_size=%d 
975,,[ wlan_roam_wmi.c : 1450 ] wlan_roam_get_scan_channel_list_event: Cannot send event as chan listtype is not set 
974,ii,[ wlan_roam_wmi.c : 1504 ] wlan_roam_get_scan_channel_list_event : max event size exceeded %d,max_limit %d 
973,i,[ wlan_roam_wmi.c : 1510 ] wlan_roam_get_scan_channel_list_event : memory allocation failed %d 
972,i,[ wlan_roam_wmi.c : 629 ] VDEV is NULL, invalid vdev_id: %d 
971,ii,[ wlan_roam_wmi.c : 638 ] ROAMING in use=%d, is_buffer_consumed=%d 
970,i,[ wlan_roam_wmi.c : 662 ] ROAM_STATS_EVENT SIZE %d 
969,,[ wlan_roam_wmi.c : 668 ] ROAM_STATS_EVENT_BUFFER_ALLOCATION_FAILED 
968,,[ wlan_roam_wmi.c : 831 ] EVENT not sent as VDEV_ROAM is NULL 
967,,[ wlan_roam_wmi.c : 411 ] Missing lca_disallow_params 
966,iiiI,[ wlan_roam_wmi.c : 415 ] lca_disallow_params disallow_duration = %d rssi_channel_penalization = %d num_disallowed_aps = %d disallow_lca_enable_source_bitmap = %x 
965,i,[ wlan_roam_wmi.c : 846 ] ROAM_WMI_LOG_STAT freq = %d 
964,ii,[ wlan_roam_wmi.c : 867 ] ROAM_WMI_LOG_STAT start_idx=%d count=%d 
963,ii,[ wlan_roam_wmi.c : 885 ] ROAM_WMI_LOG_STAT RSSI: roam_rssi_threshold = %d next_rssi_threshold = %d 
962,ii,[ wlan_roam_wmi.c : 889 ] ROAM_WMI_LOG_STAT CU: rssi = %d cu = %d 
961,iiii,[ wlan_roam_wmi.c : 895 ] ROAM_WMI_LOG_STAT BTM: mode = %d pref_cand_count = %d DI = %d VI = %d 
960,iiiiiiii,[ wlan_roam_wmi.c : 906 ] ROAM_WMI_LOG_STAT WTC_BTM: vsie_trigger_reason=%d sub_code=%d wtc_mode=%d wtc_scan_mode=%d, wtc_rssi_th=%d, wtc_candi_rssi_th=%d, wtc_candi_rssi_th_5g=%d, wtc_candi_rssi_th_6g=%d 
959,ii,[ wlan_roam_wmi.c : 910 ] ROAM_WMI_LOG_STAT DEAUTH: type = %d reason = %d 
958,ii,[ wlan_roam_wmi.c : 916 ] ROAM_WMI_LOG_STAT roam_scan_type = %d num_chan = %d 
957,,[ wlan_roam_wmi.c : 922 ] ROAM_WMI_LOG_STAT Connected AP details 
956,iiiiIi,[ wlan_roam_wmi.c : 878 ] ROAM_WMI_LOG_STAT idx=%d Trigger_ID = %d Trigger_sub_ID = %d client_id = %d ts = %ld host_ref_ts = %d 
955,IIIIII,[ wlan_roam_wmi.c : 926 ] ROAM_WMI_LOG_STAT BSS BSSID = %x %x %x %x %x %x 
954,iii,[ wlan_roam_wmi.c : 928 ] ROAM_WMI_LOG_STAT BSS ts= %d channel = %d cnd_type = %d 
953,iiiiii,[ wlan_roam_wmi.c : 930 ] ROAM_WMI_LOG_STAT BSS rssi= %d rssi_score = %d cu = %d cu_score = %d total_score = %d ETP = %d 
952,i,[ wlan_roam_wmi.c : 932 ] ROAM_WMI_LOG_STAT roam APs count = %d 
951,IIIIII,[ wlan_roam_wmi.c : 937 ] ROAM_WMI_LOG_STAT CND BSSID = %x %x %x %x %x %x 
950,iii,[ wlan_roam_wmi.c : 939 ] ROAM_WMI_LOG_STAT CND ts= %d channel = %d cnd_type = %d 
949,i,[ wlan_roam_wmi.c : 944 ] ROAM_WMI_LOG_STAT CND rssi= %d 
948,iii,[ wlan_roam_wmi.c : 950 ] ROAM_WMI_LOG_STAT BSS roam result: ts = %d status = %d fail_reason = %d 
947,iiii,[ wlan_roam_wmi.c : 957 ] ROAM_WMI_LOG_STAT NR type = %d NRR TS = %d NRS TS = %d channel_count = %d 
946,,[ wlan_roam_wmi.c : 960 ] ROAM_WMI_LOG_STAT NR Channels 
945,ii,[ wlan_roam_wmi.c : 880 ] ROAM_WMI_LOG_STAT trigger_value = %d rssi = %d  
944,iiiiii,[ wlan_roam_wmi.c : 974 ] ROAM_WMI_LOG_STAT FRAME INFO TS = %d SC = %d type = %d sub_type = %d req_resp = %d, seq = %d 
943,iiii,[ wlan_roam_wmi.c : 978 ] ROAM_WMI_LOG_STAT rssi_th=%d, cu_th=%d, full_scan_count=%d, timer_canceled=%d  
942,iiiIIIIII,[ wlan_roam_wmi.c : 983 ] ROAM_WMI_LOG_STAT btm_status=%d, vsie_reason=%d, sendtimestamp=%d, target_bssid=%x %x %x %x %x %x  
941,,[ wlan_roam_wmi.c : 1413 ] ROAM_WMI_LOG_STAT Not sending as host is in Sleep 
940,,[ wlan_roam_wmi.c : 1025 ] ROAM_WMI_LOG_STAT Not sending as host is in Sleep 
939,I,[ wlan_roam_wmi.c : 1030 ] ROAM_WMI_LOG_STAT Not sending event vdev_roam=%x 
938,i,[ wlan_roam_wmi.c : 1046 ] ROAM_WMI_LOG_STAT is_buffer_consumed=%d 
937,I,[ wlan_roam_wmi.c : 1055 ] ROAM_WMI_LOG_STAT Not sending event as stat_in_progress for idx = %x 
936,ii,[ wlan_roam_wmi.c : 1122 ] ROAM_WMI_LOG_STAT Not sending event as event size[%d] exceeds max_buffer length[%d] 
935,,[ wlan_roam_wmi.c : 1131 ] ROAM_WMI_LOG_STAT ROAM_STATS_EVENT_BUFFER_ALLOCATION_FAILED 
934,iiiiiIi,[ wlan_roam_wmi.c : 1387 ] ROAM_WMI_LOG_STAT Event sent length =%d, ev_len =%d total=%d sent=%d current_start_idx=%d, pending_idx=%x start_idx=%d 
980,iiii,[ wlan_roam_bmiss.c : 71 ] ROAM_BMISS_EVT_RECV evt=%d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d curr_rssi_avg = %d dBm bcn_rssi_last = %d dBm 
979,Iii,[ wlan_roam_bmiss.c : 122 ] ROAM_FINAL_BMISS_RECVD bmiss_final_scan = 0x%x is_qnull_fbmiss = %d, final_bmiss_recvd = %d 
978,iii,[ wlan_roam_bmiss.c : 182 ] ROAM_BMISS_EVT_RECV evt=%d roam_offld=disable curr_rssi_avg = %d dBm bcn_rssi_last = %d dBm 
977,i,[ wlan_roam_bmiss.c : 30 ] ROAM_SCAN_TIMER_EXPIRE id = 3 (periodic 1/hirssi 2/first bmiss 3/rssi_config 4/per rest 5/final bmiss 6/bss_load 7) roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d 
986,iiii,[ wlan_roam_high_dense.c : 187 ] ROAM_DENSE_ADJUST_THRESH is_dense = %d old_low_thresh = %d dBm, new_low_thresh = %d dBm, new_hi_thres = %d 
985,iii,[ wlan_roam_high_dense.c : 221 ] ROAM_DENSE_CLIENT_SCAN_START roamable_ap_cnt = %d requestor = %d is_ol_reg = %d 
984,iiiiiii,[ wlan_roam_high_dense.c : 234 ] ROAM_DENSE_CLIENT_SCAN_COMPLETED requestor = %d num_ch = %d roamable_ap_cnt = %d min_dense_ap = %d cur_is_dense = %d cur_rssi_thresh = %d dBm cur_rssi_avg = %d dBm 
983,I,[ wlan_roam_high_dense.c : 77 ] ROAM_TRAFFIC_EVENT_RECV_INFO vdev_id|req_id|thresh_status = 0x%x 
982,iiiiI,[ wlan_roam_high_dense.c : 91 ] ROAM_TRAFFIC_EVENT_RECV_INFO recv_rx_thrghput = %d bytes/sec, recv_tx_thrghput = %d bytes/secreq_rx_thrghput = %d bytes/sec req_tx_thrghput = %d bytes/sec last_traffic_thres_breach|dense_scan_skipped|scan_status = 0x%x 
981,iiiii,[ wlan_roam_high_dense.c : 34 ] ROAM_DENSE_CONFIG rssi_thres_offset = %d traffic_thres = %d dense_min_aps = %d initial_dense_status = %d, fw_dense_status = %d 
991,i,[ wlan_roam_invoke.c : 103 ] ROAM_INVOKE_PARAM_CHAN channel = %d 
990,II,[ wlan_roam_invoke.c : 121 ] ROAM_INVOKE_BSSID BSSID = 0x%08x%04x 
989,IiiiiiiI,[ wlan_roam_invoke.c : 57 ] ROAM_INVOKE_PARAM_CHECK_ERR error_num=0x%x invoke_roam_scan_mode = %d ap_sel_mode = %d roam_delay = %d num_chan = %d num_bssid = %d num_buf = %d p_cmd->flags=0x%x 
988,II,[ wlan_roam_invoke.c : 31 ] ROAM_INVOKE_STATE_CHECK_ERR error_num=0x%x scan_mode = 0x%x 
987,iiiII,[ wlan_roam_invoke.c : 263 ] ROAM_INVOKE_START_SUCCESS id=%d roam_scan_type = %d num_buf = %d flags=0x%x report_failure|is_allow_home_bssid|burst_scan=0x%x 
1029,iiiiiii,[ wlan_roam_per.c : 1230 ] ROAM_PER_CLIENT REQ_INFO vdev_id = %d, req_id = %d, rx_slots = %d, tx_slots = %d, rx_percentage = %d, tx_percentage = %d, total_req = %d 
1028,I,[ wlan_roam_per.c : 1233 ] ROAM_PER_CLIENT REG_ERROR = %u  
1027,iii,[ wlan_roam_per.c : 1266 ] ROAM_PER_CLIENT UNREG_SUCCESS vdev_id = %d req_id = %d num_req = %d 
1026,iiiiiii,[ wlan_roam_per.c : 689 ] ROAM_PER_MON_CALC type = %d(1:rx, 2:tx), tpkt = %d, lowpkt = %d recv_pkt = %d, recv_lopkt = %d, slot_num = %d, pcnt = %d 
1025,iiIIII,[ wlan_roam_per.c : 1135 ] ROAM_PER_CLIENT NOTIFY_CHECK evt = %d, evt_allow = %d tx/rx_slots = 0x%x tx/rx_pcnt = 0x%x curr_tx/rx_slots = 0x%x per_tx/rx_pcnt = 0x%x  
1024,ii,[ wlan_roam_per.c : 178 ] PER_MON_INIT_FAILED status = %d type = %d 
1023,iIIII,[ wlan_roam_per.c : 261 ] ROAM_PER_MON_INIT type = %d, ofdm_low|high = 0x%x 0x%x, cck_low|high = 0x%x 0x%x 
1022,Ii,[ wlan_roam_per.c : 582 ] ROAM_PER_MON_UPDATE ignore vdev_roam=0x%x or evt=%d 
1021,iii,[ wlan_roam_per.c : 589 ] ROAM_PER_EVT_ACTION evt = %d region_tx|rx  %d %d 
1020,,[ wlan_roam_per.c : 639 ] ROAM_PER_FAILED_EVENT 
1019,Iiiiiiii,[ wlan_roam_per.c : 330 ] ROAM_PKT_FILT_MCS type_slot = %06d max_nss_bw = %d max_mcs_index = %d max_pkt = %d hi_per_mcs = %d allow = %d low_per_pkt = %d tot_per_pkt = %d 
1018,Iiiiii,[ wlan_roam_per.c : 362 ] ROAM_PKT_FILT_OFDM type_slot = %06d max_index = %d max_pkt = %d allow = %d lpkt = %d tot_per_pkt = %d 
1017,Iiiiiii,[ wlan_roam_per.c : 397 ] ROAM_PKT_FILT_CCK type_slot = %06d max_index = %d max_pkt = %d allow = %d hirate_pkt = %d lpkt = %d tot_per_pkt = %d 
1016,,[ wlan_roam_per.c : 427 ] ROAM_PER_EVNT_DLVR_FAILED vdev_roam NULL 
1015,iiiIiii,[ wlan_roam_per.c : 439 ] ROAM_PER_EVNT_DLVR_FAILED vdev_id = %d, mac = %d, op = %d, vdev_flag = 0x%x, enable = %d, state = %d, type = %d 
1014,iiii,[ wlan_roam_per.c : 446 ] ROAM_PER_EVNT_DLVR state = %d(0:none, 1:init, 2:active, 3:suspend), type = %d(1:rx, 2:tx, 3:both) time_|last_run = %dmsec, mon_start = %dmsec 
1013,i,[ wlan_roam_per.c : 1093 ] ROAM_PER_INIT_SUCCESS vdev_id %d 
1012,Ii,[ wlan_roam_per.c : 532 ] ROAM_PER_MON_UPDATE vdev_roam=0x%x or mon_type=%d 
1011,iiiIIiii,[ wlan_roam_per.c : 544 ] ROAM_PER_MON_UPDATE suspend = %d, state = %d, type = %d, rx|tx_bitmap = 0x%x, 0x%x tmr = %d rx|tx_region = %d %d 
1010,i,[ wlan_roam_per.c : 732 ] PER_MON_FAILED status = %d 
1009,,[ wlan_roam_per.c : 740 ] PER_MON_FAILED peer NULL 
1008,iiiiiii,[ wlan_roam_per.c : 410 ] ROAM_PER_MON_RESET reason = %d, type = %d(1:rx, 2:tx) pcnt = %d slot = %d tpkt = %d lo_pkt = %d missed_slot = %d 
1007,ii,[ wlan_roam_per.c : 50 ] ROAM_PER_PDEV_UNREG_FAILED status = %d, vdev_id = %d 
1006,i,[ wlan_roam_per.c : 50 ] ROAM_PER_PDEV_WOW_UNREG_FAILED vdev_id = %d 
1005,ii,[ wlan_roam_per.c : 971 ] ROAM_PER_PDEV_REG_FAILED status = %d vdev_id = %d 
1004,i,[ wlan_roam_per.c : 971 ] ROAM_PER_PDEV_WOW_REG_FAILED vdev_id = %d 
1003,ii,[ wlan_roam_per.c : 992 ] ROAM_PER_PDEV_UNREG_FAILED status = %d, vdev_id = %d 
1002,i,[ wlan_roam_per.c : 992 ] ROAM_PER_PDEV_WOW_UNREG_FAILED vdev_id = %d 
1001,ii,[ wlan_roam_per.c : 999 ] ROAM_PER_PDEV_REG_FAILED status = %d vdev_id = %d 
1000,i,[ wlan_roam_per.c : 999 ] ROAM_PER_PDEV_WOW_REG_FAILED vdev_id = %d 
999,III,[ wlan_roam_per.c : 911 ] ROAM_PER_WAL_PDEV_HDR ignore wal_pdev=0x%x event_arg=0x%x event=0x%x 
998,I,[ wlan_roam_per.c : 829 ] ROAM_PER_PARAM_TLV NULL cmd = 0x%x 
997,i,[ wlan_roam_per.c : 838 ] ROAM_PER_CONFIG_INVALID vdev_id = %d 
996,iIIIIiiI,[ wlan_roam_per.c : 852 ] ROAM_PER_CONFIG vdev_id = %d enable = 0x%x hirate_thres = 0x%x, lowrate_thresh = 0x%x, pcnt = 0x%x, rest_time = %d running  = %d per_mon_time = 0x%x 
995,iiiiiiiii,[ wlan_roam_per.c : 886 ] ROAM_PER_CONFIG_2 TX|hirate = %d lowrate = %d pcnt = %d, slot_size = %d RX|hirate = %d lowrate = %d pcnt = %d slot_size = %d, min_rssi = %d 
994,ii,[ wlan_roam_per.c : 897 ] ROAM_PER_PDEV_REG_FAILED status = %d vdev_id = %d 
993,i,[ wlan_roam_per.c : 897 ] ROAM_PER_PDEV_WOW_REG_FAILED vdev_id = %d 
992,iiiiii,[ wlan_roam_per.c : 809 ] ROAM_PER_REST_TMR_EXP id = %d intval = %d(msec) roam_ctrl.running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d scan_status = %d, curr_rssi = %d dBm 
1056,iiiiii,[ wlan_roam_rssi.c : 1532 ] wlan_roam_full_scan_upon_roam_fail_fn id = %d interval = %d(msec) full_roaming_scan = %d trigger_reason = %d initial_conn = %d full_count = %d 
1055,iii,[ wlan_roam_rssi.c : 1615 ] ROAM_SCAN_TIMER_EXPIRE id = %d interval = %d(msec) roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d 
1054,ii,[ wlan_roam_rssi.c : 325 ] ROAM_CONFIG_RSSI_THRESH_CONFIG rssi_threshold1 = %d dBm rssi_threshold2 = %d dBm 
1053,iI,[ wlan_roam_rssi.c : 330 ] ROAM_CONFIG_BG_RSSI_THRESH bad_rssi_thresh = %d dBm flags = 0x%x 
1052,iiiii,[ wlan_roam_rssi.c : 881 ] ROAM_SCAN_HIRSSI_CHECK curr_high_rssi_thresh = %d dBm hirssi_threshold = %d dBm hirssiscan_upperbound = %d dBm curr_hiscan_count = %d, hirssiscan_maxcount = %d 
1051,iiiIIiii,[ wlan_roam_rssi.c : 938 ] ROAM_RSSI_ROAM_STATE roam_rssi_hdlr_v2 = %d tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d curr_low = %d dBm, curr_high = %d dBm 
1050,iiIII,[ wlan_roam_rssi.c : 990 ] ROAM_RSSI_GOOD bcn_rssi_avg = %d dBm bcn_rssi_last = %d dBm roam_scan_mode(PERIODIC 1/RSSI_CHANGE 2/BOTH 3/HO 4) = 0x%x prev_state = 0x%x tmr_running(bit1)/final_scan(bit0) = 0x%02x 
1049,ii,[ wlan_roam_rssi.c : 1066 ] ROAM_LOW_RSSI_INTERRUPT data_rssi = %d dBm inactivity_ts = %d 
1048,iiii,[ wlan_roam_rssi.c : 1103 ] ROAM_LOW_RSSI_INTERRUPT  bcn_rssi_avg = %d dBm bcn_rssi_last = %d dBm hi_thresh = %d dBm lo_thresh = %d dBm 
1047,iiIIiii,[ wlan_roam_rssi.c : 1124 ] ROAM_RSSI_ACTIVE_ROAM  tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d initial_conn = %d rssi_hdlr_v2 = %d 
1046,iiIIi,[ wlan_roam_rssi.c : 1144 ] ROAM_RSSI_ACTIVE_SCAN  tmr_running = %d roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d start_scan = 0x%x prev_state = 0x%x final_scan = %d  
1045,iiiii,[ wlan_roam_rssi.c : 463 ] ROAM_UPDATED_THRESH hirssi_thresh = %d dBm, rssi_thresh1 = %d dBm, curr_rssi = %d dBm, low_rssi_thresh = %d dBm, high_rssi_thresh = %d dBm 
1044,iiii,[ wlan_roam_rssi.c : 487 ] ROAM_SCAN_TIMER_EXPIRE id = %d interval = %d(msec) roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d scan_status = %d 
1043,I,[ wlan_roam_rssi.c : 178 ] ROAM_RSSI_RUNTIME_CFG swbmiss_evt_filter=%x vdev_roam_cfg->swbmiss_evt_filter 
1042,iii,[ wlan_roam_rssi.c : 94 ] ROAM_CONFIG_RSSI_THRESH roam_scan_rssi_thresh = %d dBm roam_rssi_thresh_diff = %d dBm rssi_thresh_offset_5g = %d 
1041,iiii,[ wlan_roam_rssi.c : 117 ] ROAM_CONFIG_RSSI_THRESH rssi_threshold1 = %d dBm rssi_threshold2 = %d dBm rssi_threshold2_2g = %d dBm rssi_threshold2_5g = %d dBm 
1040,iiiii,[ wlan_roam_rssi.c : 153 ] ROAM_SCAN_HIRSSI_THRESHOLD hirssi_scan_delta = %d hirssi_scan_max_count = %d hirssi_upper_bound = %d dBm hirssi_threshold = %d dBm ref_rssi = %d dBm 
1039,,[ wlan_roam_rssi.c : 104 ] ROAM_CONFIG_RSSI_INVALID_THRESH_OFFSET use default value=0 
1038,iiiiii,[ wlan_roam_rssi.c : 211 ] roam_scan_period = %d roam_scan_age = %d roam_ctrl.running = %d inactivity_time_period = %d, roam_inactive_count = %d, roam_scan_period_after_inactivity = %d 
1037,iiiiiii,[ wlan_roam_rssi.c : 1308 ] ROAM_SCAN_TIMER_EXPIRE id = %d source = %d interval = %d(msec) roam_scan_state(IDLE 0/ACTIVE_ROAM 2) = %d curr_rssi = %d dBm full_roaming_scan = %d roam_scan_period_after_inactivity=%d  
1036,i,[ wlan_roam_rssi.c : 1320 ] ROAM_SCAN_PERIODIC_INACTIVE_TIMER stop curr_load_pcnt = %d 
1035,iiii,[ wlan_roam_rssi.c : 1379 ] ROAM_SCAN_TIMER_EXPIRE id = %d tx_stats=%d, rx_stats=%d inactive_duration_count=%d 
1034,iiiiiii,[ wlan_roam_rssi.c : 1217 ] ROAM_SCAN_TIMER_EXPIRE id = %d source = %d interval = %d(msec) roam_scan_state(IDLE 0/ACTIVE_SCAN 1/ACTIVE_ROAM 2) = %d curr_low=%d dBm curr_high=%d dBm curr_rssi=-%d dBm 
1033,i,[ wlan_roam_rssi.c : 1231 ] ROAM_SCAN_PERIODIC_TIMER stop curr_load_pcnt = %d 
1032,ii,[ wlan_roam_rssi.c : 41 ] ROAM_CONFIG_RSSI_CHANGE  change_val = %d rssi_threshold1 = %d -> cap it to rssi_threshold1 
1031,iii,[ wlan_roam_rssi.c : 57 ] ROAM_CONFIG_RSSI_CHANGE  change_val = %d dBm bcn_rssi_weight = %d hi_rssi_timer_interval = %d msec 
1030,Iii,[ wlan_roam_rssi.c : 25 ] ROAM_CONFIG_DATA_RSSI flags=0x%x thres=%d rx_inactivity_ms=%d 
1062,i,[ wlan_roam_bss_load.c : 470 ] wlan_oem_send_event_for_cu_data: memory allocation failed, %d 
1061,IIII,[ wlan_roam_bss_load.c : 284 ] WLAN_ROAM_BSS_LOAD self_channel_utilization tx_ticks_diff=%u rx_ticks_diff=%u beacon_timestamp_diff=%u(msec) self_cu=%u 
1060,IIIIIiii,[ wlan_roam_bss_load.c : 380 ] WLAN_ROAM_BSS_LOAD qbss_cu=%u bss_load_avg=%u self_load_avg=%u load_pcnt=%u timer_running=%x (0:None, 1:BSS_LOAD, 2:PERIODIC) current_rssi=%d flow_started=%d scan_running=%d 
1059,iiiiii,[ wlan_roam_bss_load.c : 75 ] WLAN_ROAM_BSS_LOAD_MONITOR_ENABLE bss_avg_alpha = %d self_avg_alpha = %d monitor_threshold_pcnt = %d timer_value = %d(msec) rssi_2g_threshold = %d rssi_5g_threshold = %d 
1058,iii,[ wlan_roam_bss_load.c : 239 ] ROAM_SCAN_TIMER_EXPIRE id = %d interval=%d(msec) monitoring_running = %d 
1057,iiiii,[ wlan_roam_bss_load.c : 206 ] WLAN_ROAM_BSS_LOAD curr_bss_average=%d, curr_self_average=%d load_pcnt=%d monitor_thres=%d current_rssi=%d 
1069,i,[ wlan_roam_idle.c : 160 ] ROAM_IDLE: Check timer expiry: idle_check_count=%d 
1068,iiiiiii,[ wlan_roam_idle.c : 367 ] ROAM_IDLE: Params: vdev_id=%d enable=%d band=%d rssi_delta=%d, min_rssi=%d time=%d packet_count=%d 
1067,,[ wlan_roam_idle.c : 67 ] ROAM_IDLE: Monitor Start 
1066,i,[ wlan_roam_idle.c : 49 ] ROAM_IDLE: Monitor Reset=%d 
1065,ii,[ wlan_roam_idle.c : 225 ] ROAM_IDLE: vdev_id=%d monitor_start=%d 
1064,iii,[ wlan_roam_idle.c : 125 ] ROAM_IDLE: Inactivity check: TX = %d RX = %d Count = %d 
1063,iii,[ wlan_roam_idle.c : 98 ] ROAM_IDLE: current_rssi = %d best_rssi = %d least_rssi = %d 
1070,iiiiii,[ wlan_roam_sta_kickout.c : 108 ] ROAM_STA_KICKOUT_RECV in_use = %d, running = %d, scan_status = %d, roaming = %d, cur_rssi = %d dBm send_to_host = %d 
1071,,[ wlan_roam_pmk_timeout.c : 36 ] PMK Expire timeout 
1075,iII,[ wlan_dsm_filter.c : 213 ] DSM_LIST_UPDATE bssid_type = %d bssid removed is %08x%04x 
1074,iIIiiiii,[ wlan_dsm_filter.c : 104 ] i | bssid_type = %d, bssid_disallow_ap = %08x%04x retry_delay = %d msec, rssi = %d dbm source|reason = %d original_timestamp = %d original_timeout = %d 
1073,iIIiiiii,[ wlan_dsm_filter.c : 196 ] FW added:  i | bssid_type = %d, bssid_disallow_ap = %08x%04x retry_delay = %d msec, rssi = %d dbm source|reason = %d original_timestamp = %d original_timeout = %d 
1072,iIIii,[ wlan_dsm_filter.c : 346 ] AP Blacklisted: bssid_type = %d, bssid %08x%04x exp_delay = %d msec, exp_rssi = %ddBm 
1080,I,[ wlan_framegen.c : 2183 ] WLAN_FRMGEN_GET_ACTION_SMPS incorrect sm_power_control:0x%x 
1079,iIiIiIiI,[ wlan_framegen.c : 1861 ] WLAN_FRMGEN_GET_ACTION_TM lci_ie_len:%d lci_ie:0x%x civ_ie_len:%d civ_ie:0x%x ftm_ie_len:%d ftm_ie:0x%x vendor_ie_len:%d vendor_ie:0x%x 
1078,iIiIiIiI,[ wlan_framegen.c : 1688 ] WLAN_FRMGEN_GET_ACTION_TMR lci_ie_len:%d lci_ie:0x%x civ_ie_len:%d civ_ie:0x%x ftm_ie_len:%d ftm_ie:0x%x vendor_ie_len:%d vendor_ie:0x%x 
1077,iIi,[ wlan_framegen.c : 5906 ] frmgen_get_default_ie vdev_id=%d fc_type=0x%x length=%d 
1076,III,[ wlan_framegen.c : 263 ] WLAN_FRMGEN_GET_NULLFUNC_WITH_HTCTRL FAIL! peer:0x%x addr1:0x%x addr3:0x%x 
1112,ii,[ wlan_frameparse.c : 5214 ] FRAME_PARSER frm_len=%d fils_d_size=%d 
1111,iii,[ wlan_frameparse.c : 588 ] FRMPARSE_WARN ie->ie_len %d (exp %d) remaining_len %d. ignore this IE 
1110,iii,[ wlan_frameparse.c : 1395 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE rate_index %d (> %d)-> trimmed to %d 
1109,I,[ wlan_frameparse.c : 1406 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE skipped unknown rate 0x%x 
1108,,[ wlan_frameparse.c : 1413 ] MLME_FRMPARSE_WARN_EXT_SUPP_RATE no known rate value 
1107,ii,[ wlan_frameparse.c : 4560 ] BTM_OFLD_PARSE_BTM_REQ_GET_PREFERENCE Sub IE ID = %d, Length = %d 
1106,II,[ wlan_frameparse.c : 631 ] he_ppe_threshold ppet: 0x%x, ie_len:0x%x 
1105,ii,[ wlan_frameparse.c : 4812 ] FRM_PARSE_IE_ITERATOR ERROR remaining_length(%d) < ie_hdr_size(%d) 
1104,ii,[ wlan_frameparse.c : 4819 ] FRM_PARSE_IE_ITERATOR ERROR remaining_length(%d) < ie_len(%d) 
1103,ii,[ wlan_frameparse.c : 4900 ] 11K_offload_PARSE_NEIGH_REP_RSP_ERROR remaining_length(%d) < fixed_length(%d) 
1102,ii,[ wlan_frameparse.c : 4908 ] 11K_offload_PARSE_NEIGH_REP_RSP_ERROR remaining_length(%d) < ie_hdr_len(%d) 
1101,ii,[ wlan_frameparse.c : 4923 ] 11K_offload_PARSE_NEIGH_REP_RSP_ERROR remaining_length(%d) < ie_len(%d) 
1100,ii,[ wlan_frameparse.c : 4936 ] 11K_offload_PARSE_NEIGH_REP_RSP_ERROR Unknown IE found. ID = %d, Len = %d 
1099,i,[ wlan_frameparse.c : 4946 ] 11K_OFFLOAD_neighbor_report_response num_candidates %d 
1098,iii,[ wlan_frameparse.c : 5022 ] FRMPARSE_WARN ie->ie_len %d (exp %d) remaining_len %d. ignore this IE 
1097,I,[ wlan_frameparse.c : 1347 ] MLME_FRMPARSE_WARN_SUPP_RATE skipped unknown rate 0x%x 
1096,,[ wlan_frameparse.c : 1356 ] MLME_FRMPARSE_WARN_SUPP_RATE no known rate value 
1095,i,[ wlan_frameparse.c : 4477 ] MLME_FRMPARSE_VENDOR_VHT unknown type %d 
1094,ii,[ wlan_frameparse.c : 4494 ] MLME_FRMPARSE_WARN_VENDOR_VHT remaining_len %d (exp %d) ignore this IE 
1093,I,[ wlan_frameparse.c : 4507 ] MLME_FRMPARSE_WARN_VENDOR_VHT ERROR vht_caps. status %x
 
1092,I,[ wlan_frameparse.c : 4521 ] MLME_FRMPARSE_WARN_VENDOR_VHT ERROR vht_oper. status %x
 
1091,iIII,[ wlan_frameparse.c : 1811 ] MLME_FRMPARSE_WPA_RSN_CIPHER index %d unknown vendor oui 0x%08x 0x%08x 0x%08x 
1090,I,[ wlan_frameparse.c : 1838 ] MLME_FRMPARSE_WPA_RSN_CIPHER_ERR can't use_group for suite type 0x%x 
1089,iIi,[ wlan_frameparse.c : 1854 ] MLME_FRMPARSE_WPA_RSN_CIPHER index %d unknown suite type 0x%08x cipher_suite_type = %d 
1088,ii,[ wlan_frameparse.c : 1912 ] MLME_FRMPARSE_ERROR_WPA_RSN version (%d) is not 1. remaining ie_len %d 
1087,i,[ wlan_frameparse.c : 1922 ] MLME_FRMPARSE_WARN_WPA_RSN incomplete group cipher suite. remaining_len = %d (< 4) 
1086,,[ wlan_frameparse.c : 1990 ] MLME_FRMPARSE_WARN_WPA_RSN rsn_caps.pre_auth set in WPA. 
1085,iIII,[ wlan_frameparse.c : 1726 ] MLME_FRMPARSE_WPA_RSN_AKM index %d unknown vendor oui 0x%08x 0x%08x 0x%08x 
1084,iI,[ wlan_frameparse.c : 1772 ] MLME_FRMPARSE_WPA_RSN_AKM index %d unknown suite type 0x%08x
 
1083,iiIII,[ wlan_frameparse.c : 1778 ] MLME_FRMPARSE_WPA_RSN_AKM akm_suite_count %d is_rsn %d proto 0x%08x key_mgmt 0x%08x ie_status 0x%x 
1082,i,[ wlan_frameparse.c : 1099 ] MLME_PHYMODE invaild center freq0 phymode=%d 
1081,i,[ wlan_frameparse.c : 1200 ] MLME_PHYMODE invaild center freq0 phymode=%d 
1131,iii,[ wlan_key_mgmt.c : 40 ] KEYMGMT_ADD_PEER_ENTRY  key_ciper:%d key_len:%d is_mcast:%d 
1130,iIi,[ wlan_key_mgmt.c : 77 ] KEYMGMT_ADD_KEY_ENTRY_REINSTALLATION ERROR id=%d flags=0x%x len=%d 
1129,i,[ wlan_key_mgmt.c : 104 ] KEYMGMT_ADD_PEER_ENTRY WEP ERROR key_len:%d 
1128,i,[ wlan_key_mgmt.c : 120 ] KEYMGMT_ADD_PEER_ENTRY AES CCM ERROR key_len:%d  
1127,i,[ wlan_key_mgmt.c : 137 ] KEYMGMT_ADD_PEER_ENTRY AES GCM ERROR key_len:%d  
1126,i,[ wlan_key_mgmt.c : 172 ] KEYMGMT_ADD_PEER_ENTRY ERROR key_ciper:%d 
1125,iii,[ wlan_key_mgmt.c : 195 ] wal_peer_set_key type=%d, keyid=%d,pairwise=%d failed 
 
1124,i,[ wlan_key_mgmt.c : 43 ] KEYMGMT_ADD_PEER_ENTRY open key_ciper:%d 
1123,,[ wlan_key_mgmt.c : 57 ] KEYMGMT_ADD_PEER_ENTRY ERROR! wal_peer is NULL 
1122,i,[ wlan_key_mgmt.c : 412 ] KEYMGMT_CLR_KEY_ENTRY id=%d 
1121,i,[ wlan_key_mgmt.c : 429 ] KEYMGMT_CLR_KEY_ENTRY id=%d 
1120,,[ wlan_key_mgmt.c : 244 ] KEYMGMT_ADD_GROUP_KEY ERROR! wal_peer is NULL 
1119,i,[ wlan_key_mgmt.c : 270 ] KEYMGMT_ADD_GROUP_KEY WEP ERROR key_len:%d 
1118,i,[ wlan_key_mgmt.c : 323 ] KEYMGMT_ADD_GROUP_KEY ERROR key_ciper:%d 
1117,iII,[ wlan_key_mgmt.c : 523 ] KEYMGMT_RESET_KEY id=%d peer_addr=%08x%04x 
1116,iiIi,[ wlan_key_mgmt.c : 363 ] KEYMGMT_ADD_KEY_ENTRY id=%d key_idx=%d flags=0x%x len=%d 
1115,iIi,[ wlan_key_mgmt.c : 378 ] KEYMGMT_ADD_KEY_ENTRY_EXISTING key_idx=%d flags=0x%x len=%d 
1114,ii,[ wlan_key_mgmt.c : 390 ] KEYMGMT_ADD_KEY_ENTRY_NO_MEM id=%d key_idx=%d 
1113,iiIiII,[ wlan_key_mgmt.c : 475 ] KEYMGMT_INSTALL_KEY_ENTRY id=%d idx=%d key_flags_bitmap=0x%x len=%d peer_addr=0x04%x08%x 
1138,II,[ wlan_beacon.c : 648 ] tsf_beacon: 0x%08x%08x 
1137,Iiii,[ wlan_beacon.c : 2714 ] wlan_beacon_lio_update_li_on_resume: flags=0x%x, moddtim=%d, dyndtim=%d, maxli=%d,  
1136,Iiiiii,[ wlan_beacon.c : 2608 ] wlan_beacon_lio_update_li_on_suspend: flags=0x%x, moddtim=%d, dyndtim=%d, maxli=%d forced_dtim_cnt = %d , bss->ni_dtimperiod = %d  
1135,i,[ wlan_beacon.c : 2643 ] Forced dtim LI > 15 (%d) 
1134,iii,[ wlan_beacon.c : 2695 ] wlan_beacon_lio_update_li_on_suspend: params are wrong , moddtim = %d, dyndtim = %d, max_li = %d 
1133,iI,[ wlan_beacon.c : 2759 ] wlan_beacon_lio_wow_notif_handler: wow_notify=%d, suspend_flags=0x%x 
1132,iii,[ wlan_beacon.c : 2362 ] BEACON_RESYNC_ARBITER_RESOLVE: vdev_id=%d, is_vdev_holding=%d, SLIST_EMPTY(hold_list)=%d 
1154,iI,[ wlan_mbssid.c : 660 ] MBSS: NONTRAN_BSSID_CAP IE length: %d, NontxBssidCap: 0x%x 
1153,iI,[ wlan_mbssid.c : 665 ] MBSS: SSID IE length:%d ssid:%s 
1152,iIIIIIIii,[ wlan_mbssid.c : 681 ] MBSS: Couldn't find (mbssid_ind %d) %x:%x:%x:%x:%x:%x, DP: %d, DC:%d 
1151,iiii,[ wlan_mbssid.c : 690 ] MBSS: UPDATE: mbssid_idx:%d, period:%d, *dtim_cnt:%d, vdev_dtim_intval:%d 
1150,iiiiii,[ wlan_mbssid.c : 699 ] MBSS: SET: mbssid_idx: %d, dtimperiod:%d, frm_dtimcnt:%d, vdev_dtim_cnt %d, recvd_dtim:%d, settingdtm:%d 
1149,i,[ wlan_mbssid.c : 717 ] MBSS: Unhandled wlan_mbss_index_update_type: %d 
1148,ii,[ wlan_mbssid.c : 724 ] MBSS: ELEMENT ID: %d, IE length: %d 
1147,ii,[ wlan_mbssid.c : 535 ] WLAN_MBSSID_GET_MAX_INDICATOR mismatch cur = %d previous = %d 
1146,ii,[ wlan_mbssid.c : 540 ] WLAN_MBSSID_GET_MAX_INDICATOR Big max_bssid_ind = %d (max = %d) 
1145,iiIIIIII,[ wlan_mbssid.c : 599 ] MBSSID_GET_NONTRANS_BSSID profile_id = %d bssid_index = %d mac addr = %02x:%02x:%02x:%02x:%02x:%02x 
1144,ii,[ wlan_mbssid.c : 438 ] MBSSID_GET_NONTRANS_BSSID_PROF_NUM profile_num = %d max_mbssid_indicator = %d 
1143,ii,[ wlan_mbssid.c : 829 ] WLAN_MBSSID_GET_MAX_INDICATOR mismatch cur = %d previous = %d 
1142,ii,[ wlan_mbssid.c : 834 ] WLAN_MBSSID_GET_MAX_INDICATOR Big max_bssid_ind = %d (max = %d) 
1141,ii,[ wlan_mbssid.c : 302 ] MBSSID_IS_BSSID_MATCHED fail, len:%d err_code:%d (5:invalid_idx, 6:invalid_prof_id) 
1140,,[ wlan_mbssid.c : 327 ] MBSSID_IS_SSID_MATCHED legacy case 
1139,ii,[ wlan_mbssid.c : 361 ] MBSSID_IS_SSID_MATCHED profile_id = %d ssid_len = %d 
1157,ii,[ wlan_phyerr_internal.c : 121 ] phyerr event err: buf_len:%d>%d 
1156,,[ wlan_phyerr_internal.c : 207 ] phyerr event: alloc event failure 
1155,iiiii,[ wlan_phyerr_internal.c : 222 ] phyerr event, lo:%d, now_mac:%d, now_os:%d, phy0:%d, phy1:%d 
1166,i,[ wlan_dfs_phyerr_offload.c : 385 ] PHYERR offload enable pdev_id=%d 
1165,i,[ wlan_dfs_phyerr_offload.c : 427 ] PHYERR offload disable pdev_id=%d 
1164,,[ wlan_dfs_phyerr_offload.c : 258 ] PHYERR offload cac check not DFS chan 
1163,ii,[ wlan_dfs_phyerr_offload.c : 263 ] PHYERR offload not enabled, mac_id=%d vdev_id=%d 
1162,i,[ wlan_dfs_phyerr_offload.c : 95 ] PHYERR offload cac timeout vdevId=%d 
1161,ii,[ wlan_dfs_phyerr_offload.c : 238 ] PHYERR offload mac_id=%d enabled=%d 
1160,,[ wlan_dfs_phyerr_offload.c : 580 ]  register - WMI_SERVICE_DFS_PHYERR_OFFLOAD  
1159,i,[ wlan_dfs_phyerr_offload.c : 347 ] PHYERR offload send radar detection evt WMI pdevId=%d 
1158,iiii,[ wlan_dfs_phyerr_offload.c : 349 ] PHYERR offload det mode=%d, chan_freq=%d det_id=%d seg_id=%d 
1176,II,[ wlan_txbf.c : 1468 ] TXBFEE_DBGID_HOST_CONFIG_CMDID  ID=0x%x Value=0x%x 
1175,IIIIi,[ wlan_txbf.c : 1207 ] TXBF: SUBFee=0x%x MUBFee=0x%x SUBFer=0x%x MUBFer=0x%x chan->phy_mode=%d 
1174,,[ wlan_txbf.c : 1223 ]  VDEV Registration Failed 
1173,iI,[ wlan_txbf.c : 1362 ] TXBFEE_DBGID_BRPOLL_RECEIVED vdev_id = %d fbSegBmap=0x%x 
1172,,[ wlan_txbf.c : 1384 ] Non-directed GID frame
 
1171,iII,[ wlan_txbf.c : 1436 ] TXBFEE_DBGID_GID_RECEIVED vdev_id = %d gid=0x%x userpos=0x%x 
1170,i,[ wlan_txbf.c : 1427 ] Gid=%d
 
1169,iiIi,[ wlan_txbf.c : 1341 ]  TXBFEE_DBGID_NDPA_RECEIVED vdev_id=%d vht_he=%d staInfo=0x%x token_num=%d 
1168,IIII,[ wlan_txbf.c : 681 ] wlan_vdev_txbf_rogue_ndpa_ap_check flags = 0x%x, OUI = %x : %x : %x 
1167,ii,[ wlan_txbf.c : 1039 ] wmi_send_uploadh_event: buf_len:%d>%d 
1177,I,[ wlan_txbf_unit_test.c : 78 ] WLAN_TXBF_CONFIG param = 0x%x 
1179,II,[ unit_test.c : 417 ] UNIT_TEST_GEN  0x%x 0x%x 
1178,,[ unit_test.c : 180 ] DTF Disabled 
1205,iI,[ wlan_regdb_offload.c : 116 ] REGDB set current country command pdev_id=%d cc=%x 
1204,iiI,[ wlan_regdb_offload.c : 175 ] REGDB set init country command pdev_id=%d, cc_type=%d, cc_value=%x 
1203,,[ wlan_regdb_offload.c : 252 ]  register - WMI_SERVICE_REGULATORY_DB  
1202,i,[ wlan_regdb_offload.c : 577 ] REGDB EXT send reg rules failed - status=%d 
1201,i,[ wlan_regdb_offload.c : 510 ] REGDB send reg rules failed - status=%d 
1200,iii,[ wlan_regdb_offload.c : 516 ] REGDB rdCtl: %d %d %d 
1199,II,[ wlan_regdb_offload.c : 523 ] REGDB send default reg rules for alpha2: %c %c 
1198,iiiiii,[ wlan_regdb_offload.c : 525 ] REGDB send def reg rules phy_id=%d status_code=%d, ctry_id=%d dom_code=%d, num_2g_rules=%d, num_5g_rules=%d 
1197,IIiiii,[ wlan_regdb_offload.c : 528 ] REGDB dfs_reg=%x, phybitmap=%x minbw2g=%d maxbw2g=%d minbw5g=%d maxbw5g=%d 
1196,,[ wlan_regdb_offload.c : 408 ] REGDB EXT fail - invalid country code input 
1195,,[ wlan_regdb_offload.c : 412 ] REGDB EXT fail - invalid get type 
1194,II,[ wlan_regdb_offload.c : 438 ] REGDB send reg rules for alpha2: %c %c 
1193,iiiI,[ wlan_regdb_offload.c : 294 ] REGDB send reg rules for mac_id=%d get_type=%d cc_type=%d cc_value=%x 
1192,i,[ wlan_regdb_offload.c : 363 ] REGDB send reg rules failed - status=%d 
1191,II,[ wlan_regdb_offload.c : 367 ] REGDB send reg rules for alpha2: %c %c 
1190,,[ wlan_regdb_offload.c : 309 ] REGDB fail - invalid country code input 
1189,,[ wlan_regdb_offload.c : 313 ] REGDB fail - invalid get type 
1188,i,[ wlan_regdb_offload.c : 748 ] RegDB EXT Rules Assert - %d
 
1187,,[ wlan_regdb_offload.c : 757 ] RegDB EXT wmi buf alloc fail 
1186,i,[ wlan_regdb_offload.c : 849 ] RegDB - VLP Prioritization Frequency %d
 
1185,,[ wlan_regdb_offload.c : 851 ] RegDB - Sent WMI_REG_CHAN_LIST_CC_EXT_EVENT
 
1184,II,[ wlan_regdb_offload.c : 620 ] REGDB read reg rules alpha2 %c %c 
1183,iiii,[ wlan_regdb_offload.c : 631 ] REGDB max_rules=%d 2g_rules=%d 5g_rules=%d, evt_len=%d 
1182,,[ wlan_regdb_offload.c : 634 ] REGDB wmi buf alloc fail 
1181,,[ wlan_regdb_offload.c : 705 ] REGDB send WMI_REG_CHAN_LIST_CC_EVENTID 
1180,iiI,[ wlan_regdb_offload.c : 70 ] REGDB test command num_args=%d testId=%d value1=%x 
1224,,[ wlan_11d_scan_offload.c : 699 ] 11d scan start scan not allowed, non-sta is up 
1223,,[ wlan_11d_scan_offload.c : 400 ] 11d: invalid country code. ignore 
1222,,[ wlan_11d_scan_offload.c : 420 ] 11d: too much ap11d. ignore 
1221,,[ wlan_11d_scan_offload.c : 443 ] 11d: too much cc. ignore 
1220,iiII,[ wlan_11d_scan_offload.c : 331 ] 11d: bcn max_votes=%d idx=%d, cc=%c %c 
1219,,[ wlan_11d_scan_offload.c : 369 ] 11d: wake evt not set, ignore scan 
1218,iiii,[ wlan_11d_scan_offload.c : 335 ] 11d: US_bcn=%d, cc_cnt=%d, fcc=%d, aps11d_cnt=%d 
1217,IIII,[ wlan_11d_scan_offload.c : 361 ] 11d: new cc code = %c %c cur cc code = %c %c 
1216,,[ wlan_11d_scan_offload.c : 490 ] 11d: No CTRY IE  
1215,,[ wlan_11d_scan_offload.c : 494 ] 11d: Length shorter than expected ieee80211_country_ie. 
1214,i,[ wlan_11d_scan_offload.c : 114 ] 11d: send new cc evt_id=%d 
1213,i,[ wlan_11d_scan_offload.c : 577 ] 11d: SCAN_START_COMMAND_FAILED, %d 
1212,i,[ wlan_11d_scan_offload.c : 606 ] 11d: STOP_COMMAND_FAILED, %d 
1211,ii,[ wlan_11d_scan_offload.c : 32 ] 11d: test command num_args=%d testId=%d 
1210,ii,[ wlan_11d_scan_offload.c : 135 ] 11d: scan evt_handler notif->type = %d,vdev->id=%d 
1209,i,[ wlan_11d_scan_offload.c : 187 ] 11d: SCAN_SCH_START_ALLOC_FAIL, %d 
1208,i,[ wlan_11d_scan_offload.c : 631 ] 11d: No such VDEV is created, vdev_id=%d 
1207,ii,[ wlan_11d_scan_offload.c : 637 ] 11d: scan_vdev_start_handler vdev id=%d, period=%d 
1206,i,[ wlan_11d_scan_offload.c : 665 ] 11d: scan_vdev_stop_handler, vdev_id=%d 
1233,IIII,[ wlan_nan.c : 133 ] %s: cmd=%u, buffer=%p, length=%u 
1232,,[ wlan_nan.c : 137 ] NAN_WmiCmdHdlr: NULL command buffer
 
1231,,[ wlan_nan.c : 209 ] Unknown NAN command 
1230,,[ wlan_nan.c : 224 ] NAN_WmiEvtComplete:Null Ptr error 
1229,IIii,[ wlan_nan.c : 231 ] NAN_WmiEvtComplete:wmi_buffer pointers sent:0x%X received:0x%Xwmi_event_buf[%d].wmi_buf_assigned %d 
1228,i,[ wlan_nan.c : 250 ] NAN_WmiEvtComplete:Pending_WMI_buffer_freed and WMI_buffer rellocated :%d 
1227,,[ wlan_nan.c : 449 ] wmi_packet_prepared to be sent 
1226,,[ wlan_nan.c : 728 ] NAN_set_chan_list_hdlr: Read config error 
1225,i,[ wlan_nan.c : 1217 ] wlan_nan_register_event_notify:Invalid call back function module_id=%d 
1235,,[ wlan_nan_attr.c : 84 ] NANATTR_Init: pNan is Null returning A_EFAULT 
1234,,[ wlan_nan_attr.c : 1732 ] NANATTR : INVALID SERVICE NAME 
1236,i,[ wlan_nan_beacon_ie.c : 381 ] NAN Service ID Attr has bad length %d 
1239,IIiIIII,[ wlan_nan_beacon_rx.c : 320 ] NAN-BEACON_RX: from %04x%08x RSSI %d  valid %u  cluster 0x%04x  BI %u  statusFlags 0x%08x 
1238,i,[ wlan_nan_beacon_rx.c : 345 ] Subscribe SID Attr: contains %d IDs 
1237,IIIIIIIII,[ wlan_nan_beacon_rx.c : 446 ] NAN-SYNC_BEACON_DW_STATS: total rx %u  c1=(%u/%u/%u  %u) c2=(%u/%u/%u  %u) 
1240,,[ wlan_nan_beacon_tx.c : 311 ] NAN: Beacon Tx is already in progress. Skipping new request to send 
1256,,[ wlan_nan_bloom_filter.c : 210 ] Invalid bloom filter pointer
 
1255,,[ wlan_nan_bloom_filter.c : 232 ] Invalid data pointer
 
1254,II,[ wlan_nan_bloom_filter.c : 240 ] Invalid data len (%u vs %u)
 
1253,,[ wlan_nan_bloom_filter.c : 246 ] Invalid counter pointer
 
1252,II,[ wlan_nan_bloom_filter.c : 255 ] Invalid counter len (%u vs %u)
 
1251,II,[ wlan_nan_bloom_filter.c : 263 ] Invalid counterStart (%u), max %u
 
1250,II,[ wlan_nan_bloom_filter.c : 218 ] Invalid numElements (%u) or bitsPerElement (%u)
 
1249,II,[ wlan_nan_bloom_filter.c : 226 ] Invalid index (%u), must be less than %u
 
1248,,[ wlan_nan_bloom_filter.c : 292 ] Invalid bloom filter pointer
 
1247,II,[ wlan_nan_bloom_filter.c : 300 ] Invalid bloom filter numElements (%u) or bitsPerElement (%u)
 
1246,II,[ wlan_nan_bloom_filter.c : 308 ] Invalid bloom filter index (%u), must be less than %u
 
1245,,[ wlan_nan_bloom_filter.c : 314 ] Invalid bloom filter data pointer
 
1244,II,[ wlan_nan_bloom_filter.c : 324 ] Invalid bloom filter data len (%u vs %u)
 
1243,,[ wlan_nan_bloom_filter.c : 330 ] Invalid bloom filter counter pointer
 
1242,II,[ wlan_nan_bloom_filter.c : 339 ] Invalid bloom filter counter len (%u vs %u)
 
1241,II,[ wlan_nan_bloom_filter.c : 347 ] Invalid bloom filter counterStart (%u), max %u
 
1262,i,[ wlan_nan_cluster_sm.c : 976 ] ClusterSM: state=%d attempting to post event=WLAN_NAN_CLUSTER_EVENT_NONE 
1261,i,[ wlan_nan_cluster_sm.c : 1196 ] WLANNAN_ClusterSm_Merge: state is %d, ignoring request! 
1260,ii,[ wlan_nan_cluster_sm.c : 154 ] ClusterSM: Timer already set. Event: current=%d new=%d 
1259,,[ wlan_nan_cluster_sm.c : 609 ] ClusterSM: join timeout 
1258,,[ wlan_nan_cluster_sm.c : 891 ] ClusterSM: merge timeout 
1257,II,[ wlan_nan_cluster_sm.c : 1269 ] WLANNAN_ClusterSM_WOWSuspendResume: diff=0x%x 0x%x 
1298,,[ wlan_nan_ctrl.c : 4044 ] wlan_nan_mac: wakeup for nan_disable 
1297,,[ wlan_nan_ctrl.c : 4078 ] NAN-DISABLE 
1296,iiiii,[ wlan_nan_ctrl.c : 2812 ] Config tx_rx_chains:%d dw_early_termination_flag:%d disc_mac_rand_interval:%d disc_bcn_int:%d ranging_enable:%d 
1295,I,[ wlan_nan_ctrl.c : 3025 ] NANCTRL_ConfigurationReqHdlr: Invalid nanDbInterval %u setting to default
 
1294,,[ wlan_nan_ctrl.c : 5240 ] EnableReqHdlr: Failed to Enable MAC 
1293,,[ wlan_nan_ctrl.c : 5247 ] EnableReqHdlr:NAN Basic mode started  
1292,i,[ wlan_nan_ctrl.c : 183 ] NAN-ENABLE status=%d (0:success else failure)  
1291,,[ wlan_nan_ctrl.c : 185 ] nan_ctrl_enable: NAN_ENABLE sleep 
1290,,[ wlan_nan_ctrl.c : 3298 ] NANCTRL_EnableReqHdlr : NAN vdev not created 
1289,I,[ wlan_nan_ctrl.c : 3771 ] NANCTRL_EnableReqHdlr: Invalid nanDbInterval %u setting to default
 
1288,,[ wlan_nan_ctrl.c : 3827 ] Enable 5G Bcn 
1287,,[ wlan_nan_ctrl.c : 3831 ] Enable 5G Sdf  
1286,iiiii,[ wlan_nan_ctrl.c : 3845 ] NANCTRL_EnableReqHdlr: Config tx_rx_chains:%d dw_early_termination_flag:%d disc_mac_rand_interval:%d disc_bcn_int:%d ranging_enable:%d 
1285,i,[ wlan_nan_ctrl.c : 3859 ] postpone NAN-ENABLE, cur_hw_mode = %d 
1284,i,[ wlan_nan_ctrl.c : 269 ] NANCTRL_NANDisable cmd_requestor: %d 
1283,ii,[ wlan_nan_ctrl.c : 221 ] NANCTRL_NAN_Enable_timeout: do postponed nan enable, hw_mode=%d, enable_pending = %d 
1282,IIII,[ wlan_nan_ctrl.c : 1300 ] NaN is not allowed, p2p, TDLS or STA + STA on(0x%x, 0x%x, 0x%x, 0x%x) 
1281,,[ wlan_nan_ctrl.c : 1313 ] NaN is not allowed, SAP is present 
1280,,[ wlan_nan_ctrl.c : 257 ] NANCTRL_ResmgrEvtHdlr: start timer for postponed nan enable 
1279,,[ wlan_nan_ctrl.c : 853 ] WMI_EVENT_BUFFER not available for NAN 
1278,i,[ wlan_nan_ctrl.c : 693 ] Disabled :%d event 
1277,,[ wlan_nan_ctrl.c : 619 ] NANCTRL_SendFollowupInd 
1276,,[ wlan_nan_ctrl.c : 528 ] WMI_EVENT_BUFFER not available for NAN 
1275,,[ wlan_nan_ctrl.c : 4302 ] NANCTRL_StatsReqHdlr: Received 
1274,,[ wlan_nan_ctrl.c : 4356 ] NANCTRL_StatsReqHdlr: Received Timing Sync Req 
1273,II,[ wlan_nan_ctrl.c : 4875 ] Invalid testmode command length %u, should be greater than %u
 
1272,i,[ wlan_nan_ctrl.c : 4880 ] NEW WFA NAN TCP: Received Testmode command:%d 
1271,i,[ wlan_nan_ctrl.c : 5185 ] Testmode command received device mode:%d 
1270,i,[ wlan_nan_ctrl.c : 5190 ] Unknown Testmode command received:%d 
1269,i,[ wlan_nan_ctrl.c : 2024 ] nan_config: Discovery beacon interval length error tlv.length: %d 
1268,Ii,[ wlan_nan_ctrl.c : 2084 ] Discovery_Ind %x %d
 
1267,,[ wlan_nan_ctrl.c : 2133 ] NAN Enable/Config: DW_EARLY_TERMINATION_LENGTH ERROR 
1266,,[ wlan_nan_ctrl.c : 2140 ] NAN Enable/Config: NAN_TX_RX_CHAINS_TLV_LENGTH_ERROR 
1265,i,[ wlan_nan_ctrl.c : 1496 ] NANCTRL_TransmitFollowupReqHdlr trId - %d 
1264,i,[ wlan_nan_ctrl.c : 1900 ] NANCTRL_TransmitFollowupReqHdlr trId : %d 
1263,i,[ wlan_nan_ctrl.c : 204 ] NANCTRL_UpdateScanPolicy: NAN disableAsyncScanFlag %d 
1337,i,[ wlan_nan_de_if.c : 649 ] wlan_nan_de_if_tx_completion_bcn: completion status: %d 
1336,,[ wlan_nan_de_if.c : 708 ] nan_sched: Disc beacon completion sleep 
1335,,[ wlan_nan_de_if.c : 662 ] Error processing Tx completion for Beacon 
1334,III,[ wlan_nan_de_if.c : 846 ] Ignoring processing Tx completion for SDF/NMF nan_ctxt:%x nan_ctxt->vdevp:%x abf:%x 
1333,,[ wlan_nan_de_if.c : 860 ] Error processing Tx completion for SDF 
1332,,[ wlan_nan_de_if.c : 867 ] nan_de_if: wlan_nan_de_if_tx_completion_sdf awake 
1331,iiIi,[ wlan_nan_de_if.c : 896 ] NAN-TX_COMPLETE - frame_type:%d DWCM_RETRY:%d status:%u followup_queued:%d 
1330,,[ wlan_nan_de_if.c : 904 ] nan_de_if: wlan_nan_de_if_tx_completion_sdf sleep 
1329,iiII,[ wlan_nan_de_if.c : 917 ] NAN-TX_COMPLETE - frame_type:%d DWCM_RETRY:%d status:%u abf->flag=0x%x 
1328,,[ wlan_nan_de_if.c : 931 ] nan_de_if: wlan_nan_de_if_tx_completion_sdf sleep 
1327,,[ wlan_nan_de_if.c : 951 ] nan_de_if: wlan_nan_de_if_tx_completion_sdf sleep 
1326,i,[ wlan_nan_de_if.c : 964 ] NAN-TX_COMPLETE frame_type:%d 
1325,,[ wlan_nan_de_if.c : 966 ] NAN-TX_COMPLETE - power state awake setting back-off-params 
1324,,[ wlan_nan_de_if.c : 995 ] nan_de_if: wlan_nan_de_if_tx_completion_sdf sleep 
1323,,[ wlan_nan_de_if.c : 1649 ] nan_ctrl_pm_arb_req: NULL pointer ctxt or NULL pointer Vdev 
1322,i,[ wlan_nan_de_if.c : 1657 ] nan_ctrl_pm_arb_req: sleep not allowed! freq:%d 
1321,,[ wlan_nan_de_if.c : 1888 ] nan_ctrl_pm_arb_req: NULL pointer ctxt or NULL pointer vdev 
1320,iii,[ wlan_nan_de_if.c : 1907 ] nan_ctrl_pm_arb_req: mac_id=%d awake_status %d is_cluster_joining_merging: %d 
1319,ii,[ wlan_nan_de_if.c : 733 ] wlan_nan_de_if_FollowupInd transactionId : %d Status : %d 
1318,I,[ wlan_nan_de_if.c : 1331 ] wlan_nan_de_if_bcn_send frame_hdr is NULL or len %x 
1317,ii,[ wlan_nan_de_if.c : 1385 ] NAN_DE_IF: BCN local send failed tx_status:%d queueing_in_progress:%d 
1316,,[ wlan_nan_de_if.c : 189 ] nan_de_if_delete: Sleep 2g 
1315,,[ wlan_nan_de_if.c : 193 ] nan_de_if_delete: Sleep 5g 
1314,ii,[ wlan_nan_de_if.c : 758 ] Followup_tx_complete retry_count : count:%d completion_status : %d  
1313,,[ wlan_nan_de_if.c : 1031 ] wlan_nan_de_if_sdf_send repeative call in same context, return 
1312,i,[ wlan_nan_de_if.c : 1042 ] wlan_nan_de_if_sdf_send SDF/NMF-%d Queued 
1311,iiIiIi,[ wlan_nan_de_if.c : 1114 ] wlan_nan_de_if_sdf_send frame_type=%d seq_num=%d abf->flag=0x%x in_dw_only:%d in_dw:0x%x mac_id:%d 
1310,ii,[ wlan_nan_de_if.c : 1148 ] NAN_DBGID_DWCM Trsp timer = %d %d 
1309,,[ wlan_nan_de_if.c : 1158 ] Too close to DW hence skipping attempt to send SDF01 
1308,i,[ wlan_nan_de_if.c : 1173 ] NAN_DBGID_DWCM dw time left = %d 
1307,i,[ wlan_nan_de_if.c : 1187 ] NAN_DE_IF: Too close to DW on retry hence skipping attempt to send SDF %d 
1306,,[ wlan_nan_de_if.c : 1192 ] NAN_DBGID_DWCM dw unknown 
1305,,[ wlan_nan_de_if.c : 1200 ] wlan_nan_de_if_sdf_send: Skipping frame transmission as outside dw 
1304,i,[ wlan_nan_de_if.c : 1205 ] NAN_DE_IF: Sending frame outside DW; filer time = %d 
1303,I,[ wlan_nan_de_if.c : 1209 ] NAN_DE_IF: Can't send frame outside dw/faw state (0x%x) 
1302,ii,[ wlan_nan_de_if.c : 1283 ] NAN_DE_IF: local send failed tx_status:%d queueing_in_progress:%d 
1301,,[ wlan_nan_de_if.c : 589 ] Tx completion received with NULL abf frame 
1300,ii,[ wlan_nan_de_if.c : 623 ] Tx completion received with %d  and not %d 
1299,ii,[ wlan_nan_de_if.c : 334 ] Setting CRITICAL priority %d, Setting Dtim Period %d 
1339,IIIII,[ wlan_nan_log.c : 51 ] NAN -> API_MSG_HEADER: msgId %u  msgVersion %u  msgLen %u  handle %u  transId %u 
1338,IIIII,[ wlan_nan_log.c : 67 ] NAN ->     MSG_DATA: %02X %02X %02X %02X %02X 
1366,ii,[ wlan_nan_mac.c : 1452 ] Config Changed: nss %d -> %d 
1365,II,[ wlan_nan_mac.c : 1501 ] Config Changed: discMacaddrRandInterval %u -> %u 
1364,ii,[ wlan_nan_mac.c : 1465 ] Config Changed: committed dw 5g %d -> %d 
1363,ii,[ wlan_nan_mac.c : 1480 ] Config Changed: committed dw 2g %d -> %d 
1362,,[ wlan_nan_mac.c : 2154 ] NAN_FOLLOWUP : Frame allocation failed 
1361,ii,[ wlan_nan_mac.c : 5180 ] NANMAC_ConfigCommittedDW %d:%d 
1360,I,[ wlan_nan_mac.c : 1630 ] discMacRandomTimeout = %u 
1359,iii,[ wlan_nan_mac.c : 1735 ] NANMAC_GetScanInterval default_interval:%d Chosen_interval:%d inWowSuspend:%d 
1358,i,[ wlan_nan_mac.c : 3909 ] PrepareForDw : Free dwTxSdfBuf Len:%d 
1357,IIII,[ wlan_nan_mac.c : 4349 ] NAN DW_STOP tsf_lower: 0x%x tsf_upper: 0x%x tsf2_sanity_lower: 0x%x tsf2_sanity_upper: 0x%x  
1356,,[ wlan_nan_mac.c : 4369 ] NAN <==================================] DW_STOP 
1355,IIII,[ wlan_nan_mac.c : 4235 ] NAN DW_START tsf_lower: 0x%x tsf_upper: 0x%x tsf2_sanity_lower: 0x%x tsf2_sanity_upper: 0x%x  
1354,I,[ wlan_nan_mac.c : 4249 ] NAN [==================================> DW_START (pri=%u) 
1353,II,[ wlan_nan_mac.c : 4263 ] DWStart TxOp %x %x 
1352,iII,[ wlan_nan_mac.c : 3329 ] NAN_MAC: SDF Invalid frame framelen = %d attrId = 0x%x attrlen = 0x%x 
1351,iII,[ wlan_nan_mac.c : 3336 ] NAN_MAC: SDF framelen = %d attrId = 0x%x attrlen = 0x%x 
1350,I,[ wlan_nan_mac.c : 3351 ] NAN_MAC: SDF invalid SD attribute attr_len = 0x%x 
1349,ii,[ wlan_nan_mac.c : 2893 ] NANMAC_SdfTxComplete : Building Followup Frame followupBuilt:%d Len:%d 
1348,ii,[ wlan_nan_mac.c : 5109 ] Forced#1: committed dw 2g %d -> %d 
1347,ii,[ wlan_nan_mac.c : 5134 ] NANMAC_Set5gCommittedDW: Existing Config dw 5g %d  new %d 
1346,II,[ wlan_nan_mac.c : 4923 ] NANMAC ClusterId changed: 0x%04x -> 0x%04x
 
1345,II,[ wlan_nan_mac.c : 5632 ] role 0x%x, debuggingflags 0x%x 
1344,,[ wlan_nan_mac.c : 2758 ] NANMAC_TransmitDwFollowupFrame : FollowupBuf NULL 
1343,i,[ wlan_nan_mac.c : 2778 ] NANMAC_TransmitDwFollowupFrame : DW FollowupFrame queued for transmit status %d 
1342,i,[ wlan_nan_mac.c : 2748 ] TransmitDwServiceDiscoveryFrame : status %d 
1341,iii,[ wlan_nan_mac.c : 4079 ] NAN_MAC: Current TW params: twSize=%d n=%d twIndex=%d
 
1340,i,[ wlan_nan_mac.c : 753 ] NANMAC_WowNotifHandler: wow_notify=%d 
1382,,[ wlan_nan_publish.c : 219 ] NANPUB_Init: pNan is Null returning A_EFAULT 
1381,,[ wlan_nan_publish.c : 2045 ] Function name NANPUB_PrepareForNextDw 
1380,II,[ wlan_nan_publish.c : 2057 ] NAN-PUBSUB_PREPARED: handle %u  flags 0x%X 
1379,IIII,[ wlan_nan_publish.c : 1870 ] NAN-SUBSCRIBE_MATCH_LOG: handle %u  match handle %u  match timestamp %u  timestamp %u 
1378,IIIIIIIII,[ wlan_nan_publish.c : 1976 ] NAN-PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04X  macAddr %02X:%02X:%02X:%02X:%02X:%02X inId/reqId %x0x 
1377,i,[ wlan_nan_publish.c : 1757 ] NAN-PUB : isServiceUpdateId : %d 
1376,IIIIIIIII,[ wlan_nan_publish.c : 1780 ] NAN-PUBSUB_MATCHED: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X inID/reqId 0x%x svcCtrl/len 0x%x 
1375,I,[ wlan_nan_publish.c : 1456 ] NAN-PUBSUB_REMOVE_DEFERRED: handle %u 
1374,I,[ wlan_nan_publish.c : 1461 ] NAN-PUBSUB_REMOVE_PENDING: handle %u 
1373,I,[ wlan_nan_publish.c : 1466 ] NAN-PUBSUB_REMOVED: handle %u 
1372,i,[ wlan_nan_publish.c : 578 ] NANPUB - txType = %d 
1371,I,[ wlan_nan_publish.c : 1071 ] No space available for publish %u
 
1370,III,[ wlan_nan_publish.c : 1316 ] NAN-PUBSUB_PROCESSED: handle %u  status %u  value %u 
1369,I,[ wlan_nan_publish.c : 1081 ] Invalid publish handle %u
 
1368,I,[ wlan_nan_publish.c : 1095 ] NAN-PUBSUB_UPDATED: handle %u 
1367,,[ wlan_nan_publish.c : 1529 ] WMI_EVENT_BUFFER not available for NAN 
1386,III,[ wlan_nan_rx.c : 372 ] MyBcn dropping %0x %0x %0x 
1385,,[ wlan_nan_rx.c : 221 ] INVALID SDF: ieee80211_frame not found 
1384,,[ wlan_nan_rx.c : 243 ] INVALID SDF: ieee80211_action_nan not found 
1383,ii,[ wlan_nan_rx.c : 298 ] _wlan_nan_if_internal_rx_sdf_handler drop this frame seq_no:%d retry_bit:%d 
1422,ii,[ wlan_nan_sched.c : 3431 ] NANCHANSCHED_GetBandCenterFreq invalid center freq given primary freq:%d phymode:%d 
1421,iiiI,[ wlan_nan_sched.c : 2042 ] NAN-CHREQ status %d freq %d type %d tsfLo 0x%08x 
1420,ii,[ wlan_nan_sched.c : 2754 ] NANSCHED_ConfigureFaw: Failed to startSlot:%d numSlots:%d 
1419,IIIII,[ wlan_nan_sched.c : 3372 ] NAN_SCHED: NAN_DBGID_TSF_DUMP#1 curr_tsf_upper 0x%X, curr_tsf_lower 0x%X, nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X ULW distance to the next DW 0x%x 
1418,IIii,[ wlan_nan_sched.c : 3382 ] $$$ NAN_SCHED: NAN_DBGID_TSF_DUMP#4 nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X DwInterval:%d 2GCommittedDW:%d 
1417,i,[ wlan_nan_sched.c : 1769 ] NAN_DBGID_BEACON_TX_SEND DB Bcn Tbd= %d 
1416,ii,[ wlan_nan_sched.c : 2219 ] nan_sched: no time for one more DB diff:%d interval:%d 
1415,iii,[ wlan_nan_sched.c : 2224 ] nan_sched: offset %d pSync->nextDwTsf %d curr_tsf %d  
1414,IIIIIIi,[ wlan_nan_sched.c : 1374 ] NAN_DBGID_TSF_DUMP: curr_tsf_upper 0x%X, curr_tsf_lower 0x%X, nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X diff 0x%x, skip_dw 0x%x, late_in_dw = %d  
1413,i,[ wlan_nan_sched.c : 1875 ] nansched: faw_awake freq=%d 
1412,,[ wlan_nan_sched.c : 1833 ] nan_faw_channel_grant: Wake 
1411,,[ wlan_nan_sched.c : 1863 ] nan_sched: dw_sleep after faw_channel_grant 
1410,IIiiii,[ wlan_nan_sched.c : 698 ] NANSCHED_CurrSlot: Tsf:0x%x(U) 0x%x(L) dwOffset:%d dw0SlotNum:%d slotNum:%d slotOffset:%d 
1409,,[ wlan_nan_sched.c : 3325 ] NANSCHED_GetNANDwEnd_Tsf() pSync NULL !!! 
1408,IIII,[ wlan_nan_sched.c : 3339 ] NAN-Dw End Tsf: offset %x start_time %x currSlot %x slotOffset %x 
1407,i,[ wlan_nan_sched.c : 759 ] NANSCHED_GetSlotTimer_Dur: Skipping conditional FA idx:%d 
1406,iiii,[ wlan_nan_sched.c : 777 ] NANSCHED_GetSlotTimer_Dur: FA[%d] currdw0:%d tempslotdw0:%d num_slots:%d 
1405,IIII,[ wlan_nan_sched.c : 637 ] NAN_DBGID_TSF_DUMP: #2 curr_tsf_upper 0x%X, curr_tsf_lower 0x%X,nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X 
1404,iiii,[ wlan_nan_sched.c : 1057 ] NANSCHED_NanTimeoutSlotStart: currSlotDw0:%d currSlot:%d slotOffset:%d timerDur:%d 
1403,IIII,[ wlan_nan_sched.c : 1080 ] NAN_DBGID_TSF_DUMP: #3 curr_tsf_upper 0x%X, curr_tsf_lower 0x%X, nextDwTsf_upper 0x%X, nextDwTsf_lower 0x%X 
1402,ii,[ wlan_nan_sched.c : 125 ] NAN_PRINT_DBG_STATS: FAType:%d chan:%d 
1401,IIiiIIII,[ wlan_nan_sched.c : 136 ] NAN_PRINT_DBG_STATS: faTotalTime:%u faActiveTime:%u(Percentage:%d) faSkippedCount:%dfaInLateTime:%u faOutInBetweenTime:%u faOutEarlyTime:%u faUlwTime:%u 
1400,III,[ wlan_nan_sched.c : 180 ] NAN-RX: 0xBCF rssi %u freq %u seq %u 
1399,III,[ wlan_nan_sched.c : 225 ] NAN-RX: 0xDEF rssi %u freq %u seq %u 
1398,iIii,[ wlan_nan_sched.c : 2458 ] nan_sched: StartDw_5g() status: %d fa_entry: %p dw_sec_started: %d nanSecFreq: %d 
1397,iI,[ wlan_nan_sched.c : 2616 ] nan_sched: Stop Db req freq:%d status:%s 
1396,iIii,[ wlan_nan_sched.c : 2527 ] nan_sched: StopDw_5g() status: %d fa_entry: %p dw_sec_started: %d dw_sec_active: %d 
1395,iiIIi,[ wlan_nan_sched.c : 3018 ] NANSCHED_FaSched: FA index:%d FA type:%d tsf_lower: 0x%x tsf_upper: 0x%x Active:%d  
1394,,[ wlan_nan_sched.c : 1151 ] nan_sched:wal_tsf_dw_timer: 2g wake 
1393,,[ wlan_nan_sched.c : 1157 ] nan_sched:wal_tsf_dw_timer: 5g wake 
1392,II,[ wlan_nan_sched.c : 1184 ] NAN-TSF_TIMEOUT: currTsf 0x%08x  usecs %u 
1391,,[ wlan_nan_sched.c : 1199 ] nan_sched:wal_tsf_dw_timer: 2g wake 
1390,,[ wlan_nan_sched.c : 1205 ] nan_sched:wal_tsf_dw_timer: 5g wake 
1389,IIIII,[ wlan_nan_sched.c : 311 ] NAN-TX_COMP: type 0x%X  handle %p  buf %p  status %u  currTsf 0x%08x 
1388,,[ wlan_nan_sched.c : 3241 ] nan_sched_resmgr_link: NAN Ctxt NULL 
1387,,[ wlan_nan_sched.c : 3253 ] nan_sched_resmgr_link: Channel->mhz zero or channel is NULL or vdev is NULL 
1440,,[ wlan_nan_subscribe.c : 337 ] NANSUB_Deinit: pNan is Null returning A_EFAULT 
1439,I,[ wlan_nan_subscribe.c : 440 ] NAN-PUBSUB_REMOVED: handle %u 
1438,,[ wlan_nan_subscribe.c : 285 ] NANSUB_Init: pNan is Null returning A_EFAULT 
1437,IIII,[ wlan_nan_subscribe.c : 2208 ] NAN-SUBSCRIBE_MATCH_LOG: handle %u  match handle %u  match timestamp %u  timestamp %u 
1436,IIIIIIIII,[ wlan_nan_subscribe.c : 2321 ] NAN-PUBSUB_FOLLOWUP_RECEIVED: handle %u  matchHandle 0x%04XmacAddr %02X:%02X:%02X:%02X:%02X:%02X inId(16-31)/reqId(0-15) 0x%08x 
1435,,[ wlan_nan_subscribe.c : 1800 ] Updating Match Info Failed#3
 
1434,,[ wlan_nan_subscribe.c : 1838 ] Updating Match Info Failed#1
 
1433,III,[ wlan_nan_subscribe.c : 1900 ] NAN-SUBSCRIBE_MATCH_NEW: handle %u  match handle %u	timestamp %u 
1432,III,[ wlan_nan_subscribe.c : 2018 ] NAN-SUBSCRIBE_MATCH_REPEAT: handle %u  match handle %u  timestamp %u 
1431,iii,[ wlan_nan_subscribe.c : 2092 ] NAN-SUBSCRIBE ServiceIdMatch = %d, MatchRangeFilter = %d,inRange = %d 
1430,IIIIIIIII,[ wlan_nan_subscribe.c : 2113 ] NAN-PUBSUB_MATCHED_SKIPPED_SSI: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X inId|reqId 0x%x svcCtrl|len 0x%x 
1429,IIIIIIIII,[ wlan_nan_subscribe.c : 2144 ] NAN-PUBSUB_MATCHED: handle %u  svcId %02X:%02X:%02X:%02X:%02X:%02X inId|reqId 0x%x svcCtrl|len 0x%x 
1428,I,[ wlan_nan_subscribe.c : 1553 ] NAN-PUBSUB_REMOVE_DEFERRED: handle %u 
1427,I,[ wlan_nan_subscribe.c : 1563 ] NAN-PUBSUB_REMOVED: handle %u 
1426,I,[ wlan_nan_subscribe.c : 1558 ] NAN-PUBSUB_REMOVE_PENDING: handle %u 
1425,I,[ wlan_nan_subscribe.c : 1107 ] NAN-PUBSUB_UPDATED: handle %u 
1424,IIIi,[ wlan_nan_subscribe.c : 1403 ] NAN-PUBSUB_PROCESSED: handle %u  status %u  value %u SDEA updated_INDI %d 
1423,i,[ wlan_nan_subscribe.c : 1652 ] NANSUB_SubscribeUpdateLocalMatchFilter : %d 
1451,ii,[ wlan_nan_sync.c : 1677 ] NANSYNC_EnableDisableDiscMacRandomization(): %d RandomTimeout: %d 
1450,IIIIIII,[ wlan_nan_sync.c : 1126 ] NAN-BEACON_RX_DBG2: BcnTsf 0x%x 0x%x CurrTsf 0x%x 0x%x RxBcnHwTsf 0x%x, nowHwTsf 0x%x HwTsf2 0x%x 
1449,Ii,[ wlan_nan_sync.c : 1129 ] NAN TSF Update: diff %c%d 
1448,III,[ wlan_nan_sync.c : 913 ] NAN-BEACON_TX (prepare): buf %p  len %u  rval %u 
1447,I,[ wlan_nan_sync.c : 1543 ] NANSYNC_SetClusterId: %x 
1446,IIII,[ wlan_nan_sync.c : 66 ] NANSYNC_SetTsf: newTsf 0x%x 0x%x, currTsf 0x%x 0x%x 
1445,iii,[ wlan_nan_sync.c : 492 ] NAN-ROLE_CHANGE: %d -> %d (isFORCED=%d) 
1444,IIii,[ wlan_nan_sync.c : 143 ] NAN-NEW_ANCHORMASTER: rank=0x%08x_%08x (mp=%d  rf=%d) 
1443,III,[ wlan_nan_sync.c : 180 ] NAN-ANCHORMASTER_RECORD_UPDATE_LAST:  rank=0x%08x_%08x BTT=0x%08x 
1442,IIiI,[ wlan_nan_sync.c : 223 ] NAN-ANCHORMASTER_RECORD_UPDATE: rank=0x%08x_%08x HC=%d BTT=0x%08x 
1441,IIii,[ wlan_nan_sync.c : 251 ] NAN-NEW_MASTERRANK: rank=0x%08x_%08x (mp=%d  rf=%d) 
1459,II,[ wlan_nan_match.c : 309 ] NAN-REQUESTOR_ID: code 0x%X  requestorId 0x%X 
1458,II,[ wlan_nan_match.c : 351 ] NAN-REQUESTOR_ID: code 0x%X  requestorId 0x%X 
1457,I,[ wlan_nan_match.c : 357 ] NAN_SD_ATTR_INSTANCE_ID_DONT_CARE: code 0x%04x 
1456,,[ wlan_nan_match.c : 68 ] NANMATCH_Init: pNan is Null returning A_EFAULT 
1455,Iiiiii,[ wlan_nan_match.c : 867 ] NAN : SUBSCRIBE_MATCH_EXPIRED serviceHandle:0x%x handle:%d timestamp1:%d timestamp2:%d delta:%d unmatchTimeout:%d 
1454,iiii,[ wlan_nan_match.c : 560 ] NANMATCH_RepeatMatchCheck: matchFilterMatch:%d serviceInfoMatch:%d service_update_indicator:%d service_update_indicator:%d 
1453,,[ wlan_nan_match.c : 1265 ] WMI_EVENT_BUFFER not available for NAN 
1452,Ii,[ wlan_nan_match.c : 1494 ] NAN : SUBSCRIBE_MATCH_EXPIRED serviceHandle:0x%x handle:%d 
1474,II,[ wlan_nan_fa_pool.c : 416 ] NAN_FACombineTimeBitMap: ERR Incorrect input params inChanSchedSlotMap1:0x%x inChanSchedSlotMap2:0x%x  
1473,iiiiiiiii,[ wlan_nan_fa_pool.c : 429 ] NAN_FACombineTimeBitMap: Operation:%d inFaTimebitmap1 BD:%d Period:%d StartOffset:%d TMBLen:%d inFaTimebitmap2 BD:%d Period:%d StartOffset:%d TMBLen:%d  
1472,iI,[ wlan_nan_fa_pool.c : 432 ] NAN_FACombineTimeBitMap: TMB1[%d]:0x%x 
1471,iI,[ wlan_nan_fa_pool.c : 436 ] NAN_FACombineTimeBitMap: TMB2[%d]:0x%x 
1470,iiii,[ wlan_nan_fa_pool.c : 585 ] NAN_FACombineTimeBitMap: outFaTimebitmap BD:%d Period:%d StartOffset:%d TMBLen:%d  
1469,iI,[ wlan_nan_fa_pool.c : 588 ] NAN_FACombineTimeBitMap: OutTMB[%d]:0x%x 
1468,Ii,[ wlan_nan_fa_pool.c : 292 ] NAN_FAFindContiguousScheduleSlots: ERR fa_timebitmap:0x%x curr_slot_dw0:%d  
1467,iii,[ wlan_nan_fa_pool.c : 402 ] NAN_FAFindContiguousScheduleSlots: currSlotDw0:%d startSlotdw0:%d numSlots:%d 
1466,IiI,[ wlan_nan_fa_pool.c : 196 ] NAN_FAGenerate8SecondSlotMap: ERR Incorrect input params fa_timebitmap:0x%x fa_tmb_len:%d outChanSchedSlotMap:0x%x  
1465,i,[ wlan_nan_fa_pool.c : 203 ] NAN_FAGenerate8SecondSlotMap: ERR Incorrect FA BitDuration:%d  
1464,iiii,[ wlan_nan_fa_pool.c : 260 ] NAN_FAGenerate8SecondSlotMap: Input BitDuration:%d Period:%d StartOffset:%d TimeBitmapLen:%d 
1463,i,[ wlan_nan_fa_pool.c : 173 ] NAN_FAIsSlotSet ERR: BitDuration(%d) Conversion failed 
1462,i,[ wlan_nan_fa_pool.c : 667 ] NANCHANSCHED_FindMaximumContiguousSlotMap: bitmap_len:%d 
1461,,[ wlan_nan_fa_pool.c : 65 ] NAN_IsFaActiveOnSameMac: INVALID MAC!!! 
1460,,[ wlan_nan_fa_pool.c : 43 ] NAN_IsFaChanActiveOnSameMac: INVALID MAC!!! 
1492,iiiiii,[ wlan_nan_chan_sched.c : 544 ] NANCHANSCHED_ChanHdlr: Chan:%d status:%d currSlotDw0:%d, currSlot:%d slotOffset:%d currTime:%d 
1491,i,[ wlan_nan_chan_sched.c : 628 ] NANCHANSCHED_ChanSched: Channel Scheduler is blocked count = %d 
1490,iiIiii,[ wlan_nan_chan_sched.c : 824 ] NANCHANSCHED_ChanSched: schedIdx:%d, chanHndlrType:%d chanHndlrTypeMask:%x start_time:%d duration:%d end_time:%d 
1489,,[ wlan_nan_chan_sched.c : 941 ] NANCHANSCHED_ChanSched ERR: Channel scheduling failed 
1488,iI,[ wlan_nan_chan_sched.c : 948 ] NANCHANSCHED_ChanSched ERR: Invalid schedIdx:%d and/or chanHndlr:0x%x 
1487,iiiii,[ wlan_nan_chan_sched.c : 649 ] NANCHANSCHED_ChanSched: slot_dw0:%d slot:%d currslotdw0:%d currslot:%d offset:%d 
1486,iiIiii,[ wlan_nan_chan_sched.c : 739 ] NANCHANSCHED_ChanSched: Entry[%d] chan_mhz:%d start_time:0x%x duration:%d start_slot:%d num_slots:%d 
1485,iii,[ wlan_nan_chan_sched.c : 360 ] NAN_CHAN_SCHED RemoveChanReq hdlr_type=%d, active=%d num_slots=%d 
1484,ii,[ wlan_nan_chan_sched.c : 1410 ] NANCHANSCHED_UpdateChanSched: Invalid FA_index %d or FA_valid:%d 
1483,III,[ wlan_nan_chan_sched.c : 1524 ] NANCHANSCHED_UpdateChanSched: link_update(8)|m_fa_idx(8)|m_ch_idx(8)|f_ch_idx(8):0x%x fa_idx(8)|phy_mode(8)|ch_freq(16):0x%x schedule(8)|selected_phymode(8)|resmgr_link_present(16):0x%x 
1482,,[ wlan_nan_chan_sched.c : 1560 ] NANCHANSCHED_UpdateChanSched: Can't generate channel schedule map #1 
1481,,[ wlan_nan_chan_sched.c : 1614 ] NANCHANSCHED_UpdateChanSched: Can't generate channel schedule map #2 
1480,,[ wlan_nan_chan_sched.c : 1646 ] NANCHANSCHED_UpdateChanSched: Can't generate channel schedule map #3 
1479,,[ wlan_nan_chan_sched.c : 1663 ] NANCHANSCHED_UpdateChanSched: Can't get pmac for the channel 
1478,iIIii,[ wlan_nan_chan_sched.c : 1693 ] NANCHANSCHED_UpdateChanSched: freq:%d fa_mask:0x%x chan_mask:0x%x schedule_updated:%d link_update:%d 
1477,i,[ wlan_nan_chan_sched.c : 1337 ] NANCHANSCHED_UpdateResMgrLinkInfo: create new link channel failed for idx %d 
1476,iiiii,[ wlan_nan_chan_sched.c : 1347 ] NANCHANSCHED_UpdateResMgrLinkInfo: Link created/updated for chan_mhz %d nss %d phy_mode %d home_chan %d slot_cnt %d 
1475,i,[ wlan_nan_chan_sched.c : 1810 ] NANCHANSCHED_update_chan_link_param NSS %d 
1493,ii,[ wlan_nan_init.c : 475 ] NAN_ENABLE_DBG_STATS: enabled:%d period:%d 
1514,,[ wlan_anqp_offload.c : 1412 ] the cur match is sending to host, drop this frame 
1513,II,[ wlan_anqp_offload.c : 1513 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 
1512,III,[ wlan_anqp_offload.c : 1849 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1511,III,[ wlan_anqp_offload.c : 1598 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1510,III,[ wlan_anqp_offload.c : 1195 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1509,III,[ wlan_anqp_offload.c : 2256 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1508,III,[ wlan_anqp_offload.c : 2112 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1507,III,[ wlan_anqp_offload.c : 2118 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1506,III,[ wlan_anqp_offload.c : 2124 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1505,III,[ wlan_anqp_offload.c : 2134 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1504,III,[ wlan_anqp_offload.c : 2205 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1503,III,[ wlan_anqp_offload.c : 2212 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1502,II,[ wlan_anqp_offload.c : 489 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 
1501,III,[ wlan_anqp_offload.c : 1897 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1500,IIII,[ wlan_anqp_offload.c : 722 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
1499,IIII,[ wlan_anqp_offload.c : 1063 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
1498,III,[ wlan_anqp_offload.c : 1071 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x  
1497,III,[ wlan_anqp_offload.c : 764 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1496,IIII,[ wlan_anqp_offload.c : 534 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
1495,IIII,[ wlan_anqp_offload.c : 551 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 0x%x 
1494,III,[ wlan_anqp_offload.c : 288 ] VDEV_MGR_VDEV_UP  vdev_id/use_cnt = 0x%x 0x%x 0x%x 
1534,iiIII,[ wlan_beacon_tx_offload.c : 1279 ] WOW_BEACON_OFFLOAD_TX  pdev_id = %d vdev_id = %d completion_status = 0x%x bcn_pending_count = 0x%x bcn_buf_initialized = 0x%x 
1533,i,[ wlan_beacon_tx_offload.c : 2452 ] WOW_PROBE_RESP_TX: tx done cb, compl status=%d 
1532,ii,[ wlan_beacon_tx_offload.c : 918 ] tmplt_idx %d >= profile_period %d 
1531,IIIII,[ wlan_beacon_tx_offload.c : 1030 ] QUIET IE AP: vdev_id= %x period = %x duration = %x off = %x flag = %x 
1530,iI,[ wlan_beacon_tx_offload.c : 1084 ] WOW_PROBE_RESP_TX: PRB TMPL CMDID, probe_resp_len=%d flags=%x 
1529,IIIIiiI,[ wlan_beacon_tx_offload.c : 1496 ] BEACON TX ignored, vdev id:%x, mac_id:%x, bcn_tx_paused:%x, pdev_id:%x, swba_delay:%d consec_beacon_skip:%d, on_chan = %x 
1528,I,[ wlan_beacon_tx_offload.c : 1619 ] WOW_RECV_MGMT frame_type = 0x%x 
1527,ii,[ wlan_beacon_tx_offload.c : 2094 ] MU_EDCA_DEBUG: id: %d, update_cnt: %d 
1526,iiiii,[ wlan_beacon_tx_offload.c : 2099 ] MU_EDCA_DEBUG: id: %d, BK: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
1525,iiiii,[ wlan_beacon_tx_offload.c : 2104 ] MU_EDCA_DEBUG: id: %d, BE: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
1524,iiiii,[ wlan_beacon_tx_offload.c : 2109 ] MU_EDCA_DEBUG: id: %d, VI: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
1523,iiiii,[ wlan_beacon_tx_offload.c : 2114 ] MU_EDCA_DEBUG: id: %d, VO: cwmin: %d, cwmax: %d, aifsn: %d, edca_timer: %d 
1522,I,[ wlan_beacon_tx_offload.c : 3026 ] QUIET IE AP: num_args= %x failed 
1521,IIIII,[ wlan_beacon_tx_offload.c : 3038 ] QUIET IE AP: vdev_id= %x period = %x duration = %x off = %x flag = %x 
1520,iiiiii,[ wlan_beacon_tx_offload.c : 370 ] OPTDBG: vdevid:%d,  vdev chan_idx:%d, vdev opclass:%d, regdomain:%d, rnr opclass: %d, rnr_chidx:%d 
1519,,[ wlan_beacon_tx_offload.c : 3120 ] 11w Bcn prot test : CSA IE not added by host 
1518,,[ wlan_beacon_tx_offload.c : 2890 ] WOW_PROBE_RESP_TX: wps ie recv, wakeup host 
1517,Ii,[ wlan_beacon_tx_offload.c : 2910 ] WOW_PROBE_RESP_TX offload flags = 0x%x enabled = %d 
1516,ii,[ wlan_beacon_tx_offload.c : 2519 ] WOW_PROBE_RESP_TX: Err sending probe response not on home channel vdev home channel = %d, mac cahnnel = %d 
1515,,[ wlan_beacon_tx_offload.c : 2657 ] WOW_PROBE_RESP_TX: send probe resp 
1541,iii,[ wlan_nth_beacon_offload.c : 59 ] wlan_nth_bcn_ctx_deint nth_value = %d, timer_status = %d, is_nth_beacon_enable = %d 
1540,iii,[ wlan_nth_beacon_offload.c : 120 ] wlan_nth_bcn_ofld_run_timer error can't start timer nvalue = %d, ifup = %d, active = %d 
1539,iiiiiIII,[ wlan_nth_beacon_offload.c : 173 ] wlan_nth_bcn_ofld_run_timer timeout_val_ms = %d, nvalue = %d, status = %d, is_nth_beacon_enable = %d, drift_ms = %d, next_tbtt = 0x%x, cur_tsf =0x%x bi_us = 0x%x  
1538,iiiii,[ wlan_nth_beacon_offload.c : 339 ] wlan_nth_beacon_ofld_handler bcn received n_value = %d, nth_ctx->tmr_status = %d, is_nth_beacon_enable = %d, WOW_STATE = %d , host_wake_alwd = %d  
1537,,[ wlan_nth_beacon_offload.c : 211 ] nth beacon vdev notification registration failed 
1536,iii,[ wlan_nth_beacon_offload.c : 222 ] wlan_nth_beacon_to_host_ofld_init nth_value = %d, timer_status = %d, is_ofld_active = %d 
1535,iii,[ wlan_nth_beacon_offload.c : 260 ] wlan_update_value_nth_bcn_ofld nth_value = %d, timer_ststus = %d, is_ofld_active = %d  
1542,iiiii,[ wlan_nth_beacon_offload_unit_test.c : 26 ] wlan_nth_bcn_offload_unit_test num_args = %d, args[0] = %d, args[1] = %d, vdev_id = %d, ifUp = %d 
1555,Ii,[ csa_offload_main.c : 545 ] _csa_action_frame_handler: wbw_ie 0x%x len: %d 
1554,II,[ csa_offload_main.c : 56 ] CSA_OFFLOAD_WMI_CHANSWITCH_RECV  cur_ch_freq=0x%x new_ch_freq=0x%x 
1553,II,[ csa_offload_main.c : 136 ] CSA_OFFLOAD_CSA_TIMER_ERROR  vdev_id=0x%x state=0x%x 
1552,iII,[ csa_offload_main.c : 148 ] CSA_OFFLOAD_CSA_TIMER_ERROR vdev_id = %d csa_proc/bcn_tsf=0x%x curr_tsf=0x%x 
1551,iIIiII,[ csa_offload_main.c : 322 ] CSA_OFFLOAD_BEACON_CSA_RECV, XCSA_IE  vdev_id = %d tbtt_cnt=0x%x, curr_chan_freq :0x%x, csa_chan %d csa_freq:0x%x, prev csa ch freq:0x%x 
1550,iI,[ csa_offload_main.c : 347 ] CSA_OFFLOAD_CSA_RECV_ERROR_IE vdev_id = %d tbtt_cnt=0x%x 
1549,iIi,[ csa_offload_main.c : 400 ] CSA_OFFLOAD_CSA_RECV_ERROR_IE  vdev_id = %d tbtt_cnt=0x%x csa_ies_valid = %d 
1548,i,[ csa_offload_main.c : 431 ] CSA_OFFLOAD_CSA_RECV_ERROR_IE: CSWRAP IE len: %d 
1547,I,[ csa_offload_main.c : 453 ] pause vdev, csa:%x 
1546,iIIiII,[ csa_offload_main.c : 338 ] CSA_OFFLOAD_BEACON_CSA_RECV, CSA_IE  vdev_id = %d tbtt_cnt=0x%x, curr_chan_freq :0x%x, csa_chan %d csa_freq:0x%x, prev csa ch freq:0x%x 
1545,iii,[ csa_offload_main.c : 267 ] csa_check_ies_valid chan_valid = %d, tbtt_valid = %d pcl = %d 
1544,iI,[ csa_offload_main.c : 118 ] CSA_OFFLOAD_WMI_EVENT_ERROR  vdev_id = %d csa_proc=0x%x 
1543,ii,[ csa_offload_main.c : 667 ] SSID MATCH fail len:%d err_code:%d 
1556,i,[ obss_offload_api.c : 104 ] bss color: SCAN_SCH_START_ALLOC_FAIL, %d 
1574,i,[ bss_color_offload_int.c : 684 ] bss color offload: not support: vdev id:%d 
1573,ii,[ bss_color_offload_int.c : 692 ] bss color offload: vdev id:%d, enable=%d 
1572,iii,[ bss_color_offload_int.c : 86 ] bss color chg ie: new_bss_color=%d countdown=%d remain_time_us=%d 
1571,ii,[ bss_color_offload_int.c : 119 ] bss color he op ie: new_rts_thres=%d curr_rts_thres=%d 
1570,i,[ bss_color_offload_int.c : 638 ] bss color: bss clr chg timeout hdlr vdev_id=%d 
1569,,[ bss_color_offload_int.c : 545 ] BSS COLOR: SCAN_START_COMMAND_FAILED, vdev bss NULL 
1568,i,[ bss_color_offload_int.c : 592 ] BSS COLOR: SCAN_START_COMMAND_FAILED, %d 
1567,i,[ bss_color_offload_int.c : 613 ] 11d: STOP_COMMAND_FAILED, %d 
1566,iii,[ bss_color_offload_int.c : 442 ] bss color: check color collision detection vdev_id=%d vdev_mode=%d col_detect=%d 
1565,i,[ bss_color_offload_int.c : 710 ] bss color offload: not support: vdev id:%d 
1564,ii,[ bss_color_offload_int.c : 730 ] bss color offload: collision det cmd: vdev id:%d, evt_type=%d 
1563,iii,[ bss_color_offload_int.c : 736 ] bss color vdev cfg: det_per=%d scan_per=%d expiry_per=%d 
1562,i,[ bss_color_offload_int.c : 657 ] bss color: obss clr colli det timeout hdlr vdev_id=%d 
1561,ii,[ bss_color_offload_int.c : 344 ] bss color: Send evt report vdevId=%d, tx_status=%d 
1560,ii,[ bss_color_offload_int.c : 365 ] bss color: event report fails in wow, vdev id:%d, evt_type:%d  
1559,iiII,[ bss_color_offload_int.c : 390 ] bss color: event report,vdev id:%d, evt_type:%d, color bitmap:32to63 0x%x 0to31 0x%x 
1558,i,[ bss_color_offload_int.c : 423 ] bss color: restart color collision detection vdev_id=%d 
1557,i,[ bss_color_offload_int.c : 401 ] bss color: stop color collision detection vdev_id=%d 
1576,i,[ bss_color_offload_unit_test.c : 94 ] bss_color ofld unit test fails: bss_color vdev not exist id:%d 
1575,iiii,[ bss_color_offload_unit_test.c : 105 ] bss color ofld unit test: args %d %d %d %d 
1579,i,[ obss_offload_priv.c : 64 ] bss color: len wrong:%d 
1578,ii,[ obss_offload_priv.c : 73 ] bss color: wrong type:%d, sub:%d 
1577,I,[ obss_offload_priv.c : 106 ] obss rx, myfrm/dfs=0x%x 
1582,i,[ obss_ru26_offload_priv.c : 112 ] obss ru26 det timeout hdlr vdev_id=%d 
1581,i,[ obss_ru26_offload_priv.c : 36 ] obss ru26 hdlr, sta_ulmu_enable_status=%d 
1580,ii,[ obss_ru26_offload_priv.c : 71 ] obss ru26 ru_tolerent_ap_det=%d ru_disabled=%d 
1588,i,[ obss_spatial_reuse_api.c : 60 ] spatial reuse: len wrong:%d 
1587,,[ obss_spatial_reuse_api.c : 106 ] spatial reuse: peer != HE  
1586,,[ obss_spatial_reuse_api.c : 65 ] spatial reuse: vdev > 1 
1585,ii,[ obss_spatial_reuse_api.c : 74 ] spatial reuse : wrong type:%d, sub:%d 
1584,ii,[ obss_spatial_reuse_api.c : 179 ] obss spatial reuse: vdev_id = %d, enable=%d 
1583,,[ obss_spatial_reuse_api.c : 290 ] obss spatial reuse: pdev init num_vdev: 
1599,Iiii,[ wlan_p2p_listen_offload.c : 509 ] _wlan_p2p_lo_frames_handler, subtype:%x, length:%d,vdevid:%d, state:%d 
1598,,[ wlan_p2p_listen_offload.c : 528 ] _wlan_p2p_lo_frames_handler,drop2 
1597,i,[ wlan_p2p_listen_offload.c : 559 ] _wlan_p2p_lo_frames_handler receive p2p action frame,wow_enable=%d 
1596,,[ wlan_p2p_listen_offload.c : 523 ] _wlan_p2p_lo_frames_handler,drop 1 
1595,iii,[ wlan_p2p_listen_offload.c : 444 ] _wlan_p2p_lo_listen_interval_timeout p2p_lo_cfg_cnt = %d, p2p_lo_cur_cnt=%d,wow_enable=%d 
1594,i,[ wlan_p2p_listen_offload.c : 407 ] _wlan_p2p_lo_scan_evt_handler evt->type = %d 
1593,iii,[ wlan_p2p_listen_offload.c : 170 ] _wlan_p2p_lo_vdev_evt_handler notif->type = %d,vdev->id=%d,vdev->ic_opmode=%d 
1592,i,[ wlan_p2p_listen_offload.c : 339 ] _wlan_p2p_lo_vdev_init SCAN_SCH_START_ALLOC_FAIL, %d 
1591,ii,[ wlan_p2p_listen_offload.c : 210 ] _wlan_p2p_lo_vdev_start_handler lo_pdev->p2p_lo_vdev->vdev_id = %d, vdev id=%d 
1590,iiiiiii,[ wlan_p2p_listen_offload.c : 226 ] _wlan_p2p_lo_vdev_start_handler vdev id=%d,channel=%d,period=%d,interval=%d,count=%d,device_types_len=%d,prob_resp_len=%d 
1589,i,[ wlan_p2p_listen_offload.c : 266 ] _wlan_p2p_lo_vdev_stop_handler, vdev_id=%d 
1610,iIi,[ wlan_p2p_listen_offload_int.c : 842 ] wlan_p2p_lo_parse_subelement ERROR.attr_type=%d,data=0x%x,attr_len=%d 
1609,Ii,[ wlan_p2p_listen_offload_int.c : 860 ] wlan_p2p_lo_wps_parse_msg ERROR,ie_buf=0x%x,ie_len=%d 
1608,Ii,[ wlan_p2p_listen_offload_int.c : 641 ] wlan_p2p_lo_vendor_ie_parse ERROR pos=0x%x, pos[1] =%d 
1607,iIi,[ wlan_p2p_listen_offload_int.c : 967 ] wlan_p2p_lo_wps_set_attr ERROR,type=%d,pos=0x%x, len=%d 
1606,I,[ wlan_p2p_listen_offload_int.c : 1277 ] WPS: Invalid Requested Device Type length %u 
1605,I,[ wlan_p2p_listen_offload_int.c : 1283 ] WPS: Skipped Requested Device Type attribute (max %u types) 
1604,i,[ wlan_p2p_listen_offload_int.c : 559 ] _wlan_p2p_lo_scan_start P2P LO SCAN_START_COMMAND_FAILED, %d 
1603,ii,[ wlan_p2p_listen_offload_int.c : 564 ] _wlan_p2p_lo_scan_start p2p_lo_cfg_interval = %d,p2p_lo_state=%d 
1602,i,[ wlan_p2p_listen_offload_int.c : 595 ] _wlan_p2p_lo_scan_stop P2P LO SCAN_STOP_COMMAND_FAILED, %d 
1601,,[ wlan_p2p_listen_offload_int.c : 62 ] allocate mgmt failure 
1600,i,[ wlan_p2p_listen_offload_int.c : 119 ] mgmt send failure:%d 
1624,iii,[ wlan_quiet_ie_ap.c : 107 ] QUIET IE AP: timer cb-next evt:%d, cac:%d, paused:%d 
1623,I,[ wlan_quiet_ie_ap.c : 131 ] QUIET IE AP: quiet duration time-usec:0x%x 
1622,i,[ wlan_quiet_ie_ap.c : 59 ] QUIET IE AP: vdev init vdevId=%d 
1621,II,[ wlan_quiet_ie_ap.c : 232 ] QUIET IE AP: not appending quiet IE. time_to_quite_period_start = 0x%x, time_to_bcn_tx = 0x%x 
1620,iiI,[ wlan_quiet_ie_ap.c : 188 ] QUIET IE AP: bi_us=%d diff=%d curr_wal_time=0x%x 
1619,iiii,[ wlan_quiet_ie_ap.c : 313 ] QUIET IE AP: start quiet IE: module id=%d, vdev id=%d, dur=%d, beaconing_cnt=%d 
1618,,[ wlan_quiet_ie_ap.c : 335 ] QUIET IE AP: cancel current quiet IE config 
1617,III,[ wlan_quiet_ie_ap.c : 380 ] QUIET IE AP: quiet IE Start time=0x%x Curr_time=0x%x timeout=0x%x 
1616,i,[ wlan_quiet_ie_ap.c : 324 ] QUIET IE AP: start quiet IE: input duration out of range, duration_us = %d 
1615,iiii,[ wlan_quiet_ie_ap.c : 454 ] QUIET IE AP: test input num_args=%d vdevId=%d dur=%d cnt=%d 
1614,,[ wlan_quiet_ie_ap.c : 463 ] QUIET IE AP: test cfg fail 
1613,I,[ wlan_quiet_ie_ap.c : 466 ] QUIET IE AP: test cfg success start_time=0x%x 
1612,i,[ wlan_quiet_ie_ap.c : 444 ] QUIET IE AP: test cb status=%d 
1611,iii,[ wlan_quiet_ie_ap.c : 423 ] QUIET IE AP: post migration,vdevId:%d, cac:%d, vdevPaused:%d 
1636,IiiiiI,[ wlan_quiet_ie_sta.c : 141 ] QUIET IE STA, time-usec:0x%x, vdevId=%d, evt:%d, all_tids_tx_blocked:%d, supend_alwd:%d, period:0x%x 
1635,iiiii,[ wlan_quiet_ie_sta.c : 232 ] QUIET IE STA: vdevId=%d, next_start=%d, period=%d, duration=%d, quiet_enabled=%d 
1634,Ii,[ wlan_quiet_ie_sta.c : 273 ] QUIET IE STA: Quiet period starts in=0x%x, vdevId=%d 
1633,iiii,[ wlan_quiet_ie_sta.c : 327 ] QUIET IE STA: test input num_args=%d vdevId=%d dur=%d per=%d 
1632,,[ wlan_quiet_ie_sta.c : 337 ] QUIET IE STA: test cfg, vdev not up or incorrect mode 
1631,,[ wlan_quiet_ie_sta.c : 354 ] QUIET IE STA: test cfg fail 
1630,,[ wlan_quiet_ie_sta.c : 357 ] QUIET IE STA: test cfg success 
1629,,[ wlan_quiet_ie_sta.c : 332 ] QUIET IE STA: test cfg, vdev is NULL 
1628,IiiiiIi,[ wlan_quiet_ie_sta.c : 396 ] QUIET IE STA: PS SM callback , time-usec:0x%x, vdevId=%d, next_evt:%d, all_tids_tx_blocked:%d, supend_alwd:%d, period:0x%x, sleep = %d 
1627,IIIII,[ wlan_quiet_ie_sta.c : 437 ] QUIET IE STA: time_diff_us = 0x%x , current_quite_ie = 0x%x, sum =0x%x, ref_time = 0x%x, curr_ts=0x%x 
1626,Ii,[ wlan_quiet_ie_sta.c : 460 ] QUIET IE STA: wake recved in ON period timer:0x%x, nxt_evnt:%d 
1625,Ii,[ wlan_quiet_ie_sta.c : 474 ] QUIET IE STA: wake recved in OFF period timer:0x%x, nxt_evnt:%d 
1641,I,[ wlan_wow_mgmt.c : 58 ] WOW_RECV_MGMT  frame_type = 0x%x 
1640,iii,[ wlan_wow_mgmt.c : 228 ] WOW action frame received wh->i_fc[0] = %d, action_category = %d, action_sub_category_bitmap = %d 
1639,i,[ wlan_wow_mgmt.c : 259 ] Dropping action frame with action_sub_category_bitmap = %d greater than max supported value 
1638,I,[ wlan_wow_mgmt.c : 135 ] WOW_RECV_MGMT  frame_type = 0x%x 
1637,,[ wlan_wow_mgmt.c : 216 ] Length less than frame_length + action_category + sub_category_bitmap. 
1670,,[ wlan_arp_ns_offload.c : 841 ] Resetting ARP frame in air parm 
1669,,[ wlan_arp_ns_offload.c : 844 ] Resetting NS frame in air parm 
1668,I,[ wlan_arp_ns_offload.c : 1634 ] WOW ARP OFLD CCE add flt tgt ip = 0x%x  
1667,,[ wlan_arp_ns_offload.c : 1641 ] WOW ARP OFLD CCE del flt 
1666,iI,[ wlan_arp_ns_offload.c : 928 ] OFLD ARP RECEIVED vdevId=%d srcIp=0x%x 
1665,,[ wlan_arp_ns_offload.c : 951 ] ARP req frame dropped ,arp reply frame allready in air 
1664,iI,[ wlan_arp_ns_offload.c : 1038 ] OFLD ARP REPLIED vdev_id = %d ip_addr = 0x%x 
1663,I,[ wlan_arp_ns_offload.c : 107 ] WOW_RECV_DATA_PKT  ARPPKT_REQUEST received :0x%x 
1662,III,[ wlan_arp_ns_offload.c : 230 ] WOW_RECV_DATA_PKT  tgt_ip = 0x%x src_ip = 0x%x ops = 0x%x 
1661,iIIII,[ wlan_arp_ns_offload.c : 1863 ] WOW_NS_OFLD_ENABLE_0 vdev_id = %d ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
1660,iIIII,[ wlan_arp_ns_offload.c : 1909 ] WOW_NS_OFLD_ENABLE_1 vdev_id = %d ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
1659,iI,[ wlan_arp_ns_offload.c : 1945 ] WOW_ARP_OFLD_ENABLE vdev_id =%d  ip_addr = 0x%x 
1658,iii,[ wlan_arp_ns_offload.c : 1956 ] WOW enable cmd vdevId=%d ARP %d NS %d 
1657,II,[ wlan_arp_ns_offload.c : 2003 ] HW CCE ns offload disabled, vdev id:%x, ns_cnt:%x 
1656,i,[ wlan_arp_ns_offload.c : 2018 ] WOW_NS_ARP_OFLD_DISABLE vdev_id = %d 
1655,iI,[ wlan_arp_ns_offload.c : 1727 ] WOW_NS_OFLD add flt CCE j=%d TGT IPv6 last 4 bytes ipv6_addr_127_96 = 0x%x 
1654,,[ wlan_arp_ns_offload.c : 1737 ] WOW NS OFLD CCE del flt 
1653,iIIII,[ wlan_arp_ns_offload.c : 1149 ] OFLD NS RECEIVED vdev_id = %d TGT IP ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
1652,,[ wlan_arp_ns_offload.c : 1209 ] NS req frame dropped , NS reply frame allready in air 
1651,iIIII,[ wlan_arp_ns_offload.c : 1290 ] OFLD NS REPLIED vdev_id = %d ipv6_addr_31_0 = 0x%x ipv6_addr_63_32 = 0x%x ipv6_addr_95_64 = 0x%x ipv6_addr_127_96 = 0x%x 
1650,,[ wlan_arp_ns_offload.c : 1300 ] warning:ns invalid,drop 
1649,ii,[ wlan_arp_ns_offload.c : 600 ] ns_validate: buffer length-%d, should be greater than payload of the ip_header-%d 
1648,,[ wlan_arp_ns_offload.c : 671 ] ns_validate: OFLD NS error, option_hdr->TotalLength greater than option_length 
1647,III,[ wlan_arp_ns_offload.c : 621 ] OFLD NS validate checksum fail, expect checksum:%x checksum in frame:%x payload_len:%x
 
1646,,[ wlan_arp_ns_offload.c : 664 ] OFLD NS error,invalid option 
1645,iii,[ wlan_arp_ns_offload.c : 2097 ] OFLD send periodic ptrn vdev_id=%d ptrnId=%d ptrnLen=%d 
1644,i,[ wlan_arp_ns_offload.c : 2217 ] Invalid pattern id %d 
1643,i,[ wlan_arp_ns_offload.c : 2231 ] Pattern id %d is not configured 
1642,i,[ wlan_arp_ns_offload.c : 2294 ] set proc pattern err, unsupported len:%d 
1677,I,[ bpf_offload.c : 302 ] bpf pdev is not initialized: %x
 
1676,I,[ bpf_offload.c : 312 ] WMI_BPF_GET_VDEV_STATS_CMDID not supported from APF V3 %x
 
1675,I,[ bpf_offload.c : 343 ] bpf pdev is not initialized: %x
 
1674,ii,[ bpf_offload.c : 94 ] unicast recv count = %d, unicast allow count = %d 
1673,IIIII,[ bpf_offload.c : 265 ] bpf filter can not run: vdev:%x, program:%x, memory:%x, read:%x, set:%x 
1672,III,[ bpf_offload.c : 287 ] dropped:v:%x c:%x d:%x
 
1671,I,[ bpf_offload.c : 202 ] No memory for vdev v:%x 
1704,II,[ bpf_offload_int.c : 716 ] WMI_BPF_SET_VDEV_ENABLE_CMDID vdev_id = %x, enable = %x 
1703,I,[ bpf_offload_int.c : 735 ] WMI_BPF_SET_VDEV_ENABLE_CMDID: APF state unchanged %x 
1702,i,[ bpf_offload_int.c : 639 ] Adaptive BPF: (curr_time - bpf_last_sleep_timestamp) = %d 
1701,i,[ bpf_offload_int.c : 664 ] Adaptive BPF next_timeout = %d 
1700,i,[ bpf_offload_int.c : 577 ] BPF PS SLEEP curr_time = %d 
1699,i,[ bpf_offload_int.c : 593 ] BPF PS AWAKE curr_time = %d 
1698,III,[ bpf_offload_int.c : 907 ] WMI_BPF_GET_VDEV_WORK_MEMORY_CMDID vdev_id %x addr_offset %x length %x 
1697,ii,[ bpf_offload_int.c : 416 ] evaluate next state curr_time = %d, uc_bitmap = %d 
1696,,[ bpf_offload_int.c : 421 ] Next state is non APF 
1695,,[ bpf_offload_int.c : 434 ] Next state is APF 
1694,I,[ bpf_offload_int.c : 384 ] wlan_bpf_notify_handler: Notification type %x not handled 
1693,I,[ bpf_offload_int.c : 33 ] _wlan_bpf_offload_cmd_handle_get_cap: no buf %x
 
1692,II,[ bpf_offload_int.c : 309 ] Active APF command mcbc_mode = %x, uc_mode = %x 
1691,I,[ bpf_offload_int.c : 328 ] Active APF for unicast mode = %x is not supported 
1690,I,[ bpf_offload_int.c : 318 ] Active APF for MCBC mode = %x is not supported 
1689,III,[ bpf_offload_int.c : 72 ] invalid, t:%x, c:%x, l:%x
 
1688,I,[ bpf_offload_int.c : 85 ] no memory for instruction:%x
 
1687,I,[ bpf_offload_int.c : 169 ] vdev not created:%x
 
1686,,[ bpf_offload_int.c : 872 ] APF: No memory for event 
1685,IIII,[ bpf_offload_int.c : 751 ] WMI_BPF_SET_VDEV_WORK_MEMORY_CMDID vdev_id = %x, addr_offset = %x, length = %x, program_len = %x 
1684,III,[ bpf_offload_int.c : 773 ] invalid memory access offset %x, length %x, bpf_memory_len %x 
1683,,[ bpf_offload_int.c : 778 ] Buf is null 
1682,i,[ bpf_offload_int.c : 550 ] Disable Adaptive APF curr_time = %d 
1681,i,[ bpf_offload_int.c : 504 ] Enable Adaptive APF curr_time = %d 
1680,III,[ bpf_offload_int.c : 230 ] WOW notify for active APF: uc mode = %x, mcbc mode = %x, data path config = %x 
1679,II,[ bpf_offload_int.c : 256 ] Active APF conf for MCBC: MCBC APF mode = %x, data path conf = %x 
1678,II,[ bpf_offload_int.c : 289 ] Active APF conf for unicast: uc APF mode = %x, data path conf = %x 
1711,ii,[ bpf_offload_unit_test.c : 655 ] bpf dump vdev:%d, total_len:%d
 
1710,IIII,[ bpf_offload_unit_test.c : 661 ] hex:%02x%02x%02x%02x 
1709,ii,[ bpf_offload_unit_test.c : 173 ] OFLD BPF unit test cmd: Route UC active vdevId=%d, enable=%d 
1708,,[ bpf_offload_unit_test.c : 209 ] OFLD BPF unit test disable UC route in active mode 
1707,,[ bpf_offload_unit_test.c : 180 ] OFLD BPF unit test enable UC route in active mode 
1706,,[ bpf_offload_unit_test.c : 205 ] OFLD BPF unit test enable UC route in active mode fails as bpf not enabled 
1705,iii,[ bpf_offload_unit_test.c : 698 ] Adaptive APF params: Allow percentage = %d, Min monitored packet = %d, Traffic threshold = %d
 
1731,,[ wlan_gtk_offload.c : 1135 ] WOW gtk_offload_process_rekey:Already sending
 
1730,,[ wlan_gtk_offload.c : 1141 ] gtk offload drop the frame. 
1729,,[ wlan_gtk_offload.c : 1163 ] WOW gtk_offload_can_deliver_rxdata_tohost: not eapol_key. 
 
1728,,[ wlan_gtk_offload.c : 1176 ] WOW gtk_offload_can_deliver_rxdata_tohost: gtk_error. 
 
1727,ii,[ wlan_gtk_offload.c : 1007 ] FILS_DEBUG gtk_offload_check_rekey: Buffer is not enough to contain keyData length %d keydata_length %d 
1726,II,[ wlan_gtk_offload.c : 343 ] gtk_offload_compute_mic: ver = 0x%x, auth_mode = 0x%x 
1725,,[ wlan_gtk_offload.c : 378 ] gtk_offload_compute_mic: WPA: EAPOL-Key MIC using AES-CMAC (AKM-defined - SAE) 
1724,I,[ wlan_gtk_offload.c : 373 ] gtk_offload_compute_mic: WPA: EAPOL-Key MIC using HMAC-SHA%u (AKM-defined - OWE) 
1723,iiiIi,[ wlan_gtk_offload.c : 566 ] _gtk_offload_decrypt_key: keydatalen = %d, descType = %d, key_desc_type = %d, keyinfo = %x, kek_len = %d 
1722,,[ wlan_gtk_offload.c : 206 ] _gtk_offload_deferred_m2_callback, allocate buffer failure 
1721,I,[ wlan_gtk_offload.c : 236 ] _gtk_offload_deferred_m2_callback, txrx status:%x 
1720,iii,[ wlan_gtk_offload.c : 1393 ] FILS_DEBUG GTK OFFLOAD command recvd vdev id %d flags %d kek_len %d 
1719,iiiiiiii,[ wlan_gtk_offload.c : 1403 ] FILS_DEBUG GTK OFFLOAD repay_counter %d %d %d %d %d %d %d %d 
1718,i,[ wlan_gtk_offload.c : 1444 ] WOW gtk_offload_dispatch_wmi_cmd: wrong kek_len = %d 
1717,II,[ wlan_gtk_offload.c : 833 ] _gtk_offload_process_rekey, replay:%x, cur:%x 
1716,i,[ wlan_gtk_offload.c : 854 ] gtk_offload_process_rekey: neither MIC or encrKeyData is present %d 
1715,,[ wlan_gtk_offload.c : 870 ] gtk_offload_process_rekey:decrypt_key fail 
1714,,[ wlan_gtk_offload.c : 890 ] gtk_offload_process_rekey:mic fail 
1713,,[ wlan_gtk_offload.c : 900 ] gtk_offload_process_rekey:type is not AES/TKIP 
1712,,[ wlan_gtk_offload.c : 1052 ] _gtk_offload_send_rekey_failure_event: no evt 
1736,,[ wlan_hw_data_filtering.c : 264 ] Add NON ARP BC CCE filter 
1735,,[ wlan_hw_data_filtering.c : 268 ] Delete NON ARP BC CCE filter 
1734,,[ wlan_hw_data_filtering.c : 320 ] Add NON ICMPv6 MC CCE filter 
1733,,[ wlan_hw_data_filtering.c : 324 ] Delete NON ICMPv6 MC CCE filter 
1732,iiiiii,[ wlan_hw_data_filtering.c : 65 ] OFFLOAD HDLR CCE UNIT TEST CMD: num_args=%d vdevId=%d args =%d %d %d %d  
1749,iii,[ wlan_mcast_filter_offload.c : 76 ] Not for enhanced mcast %d %d %d 
1748,iI,[ wlan_mcast_filter_offload.c : 204 ] wlan_mcast_handler mcbc_ret = %d vdev_id = 0x%x 
1747,i,[ wlan_mcast_filter_offload.c : 210 ] wlan_mcast_handler bpf_enable_status = %d 
1746,ii,[ wlan_mcast_filter_offload.c : 241 ] WOW MC addr matched vdevId=%d reason=%d 
1745,iii,[ wlan_mcast_filter_offload.c : 207 ] wlan_mcast_handler pktflt_enabled:%d MC:%d UC:%d 
1744,IIIII,[ wlan_mcast_filter_offload.c : 291 ] WLAN_CHATTER_MC_FILTER_ADD_EX  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x status = 0x%x, index:%x 
1743,i,[ wlan_mcast_filter_offload.c : 351 ] OFLD MC_FILTER_ADD_EX hash flt idx=%d 
1742,IIII,[ wlan_mcast_filter_offload.c : 375 ] WLAN_CHATTER_MC_FILTER_ADD_EX	vdev_id = 0x%x mac_addr31to0 = 0x%x num_flt|mac_addr47to32 = 0x%x, index:%x 
1741,III,[ wlan_mcast_filter_offload.c : 413 ] WLAN_CHATTER_MC_FILTER_DEL_EX  vdev_id = 0x%x mac_addr31to0 = 0x%x num_flt|mac_addr47to32 = 0x%x 
1740,IIII,[ wlan_mcast_filter_offload.c : 467 ] WLAN_CHATTER_MC_FILTER_DEL_EX  vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x status = 0x%x 
1739,,[ wlan_mcast_filter_offload.c : 130 ] L2 not valid 
1738,iIII,[ wlan_mcast_filter_offload.c : 162 ] WLAN_MC_FILTER mcbc_status = %d vdev_id = 0x%x mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x 
1737,i,[ wlan_mcast_filter_offload.c : 635 ] Enhanced mcast enable %d 
1750,iiiiii,[ wlan_mcast_filter_offload_unit_test.c : 205 ] MCAST FILT unit test input: type=%d, args[1]=%d,args[2]=%d,args[3]=%d,args[4]=%d,args[5]=%d 
1760,,[ wlan_pktFilter_offload.c : 169 ] pkt fltr data handler: vdev is NULL  
1759,,[ wlan_pktFilter_offload.c : 176 ] vdev pktFltrInfo is NULL  
1758,,[ wlan_pktFilter_offload.c : 436 ] pkt filter registering  
1757,i,[ wlan_pktFilter_offload.c : 784 ] pkt filter command =%d  
1756,,[ wlan_pktFilter_offload.c : 787 ] pkt filter is not enabled by host 
1755,i,[ wlan_pktFilter_offload.c : 528 ] num of sub-filters exceeds allowed =%d  
1754,i,[ wlan_pktFilter_offload.c : 570 ] data length out of bounds =%d  
1753,,[ wlan_pktFilter_offload.c : 667 ] pkt filter error: No filters set 
1752,ii,[ wlan_pktFilter_offload.c : 733 ] pkt filter vdevPtr count =%d filter id = %d 
1751,i,[ wlan_pktFilter_offload.c : 533 ] All pkt fltrs used =%d  
1770,,[ wlan_wow_data.c : 200 ] _wlan_natkeepalive_handler  OFFLOAD_STATUS_DROP 
1769,i,[ wlan_wow_data.c : 220 ] dispatch_ipsec_natkeepalive_filter_cmd: action = %d 
1768,iiii,[ wlan_wow_data.c : 731 ] WOW add ptrn vdev id=%d idx=%d ptrn id=%d ptrn len=%d 
1767,iii,[ wlan_wow_data.c : 1324 ] WOW add timer ptrn vdev_id=%d, ptrn_id=%d, timeout_ms=%d 
1766,II,[ wlan_wow_data.c : 588 ] WOW_RECV_BITMAP_PATTERN  vdev_id = 0x%x, pattern_id = 0x%x 
1765,ii,[ wlan_wow_data.c : 788 ] WOW del ptrn vdev id=%d ptrn id=%d 
1764,ii,[ wlan_wow_data.c : 535 ] WOW Eapol check match vdevId=%d reason=%d 
1763,ii,[ wlan_wow_data.c : 503 ] WOW Magic pkt rcvd vdevId=%d reason=%d 
1762,i,[ wlan_wow_data.c : 452 ] WOW NA drop unsolicity na, vdev:%d 
1761,ii,[ wlan_wow_data.c : 459 ] WOW RA filter match vdevId=%d reason=%d 
1784,i,[ wlan_igmp_offload.c : 722 ] igmp_offload_proc_frame igmp_status=%d 
1783,iiIiI,[ wlan_igmp_offload.c : 999 ] IGMP_UNIT_TEST vdev_id = %d, test_case = %d, vdev = 0x%x, is_free = %d igmp = 0x%x 
1782,iIIIIIi,[ wlan_igmp_offload.c : 34 ] IGMP_INFO : err_status = %d, vdev_id|num_mc_addr_cnt = 0x%x, max_resp_time|num_grp = 0x%x, last_query_time = 0x%x, spec_grp = 0x%x flags = 0x%x data = %d 
1781,iIIIiii,[ wlan_igmp_offload.c : 60 ] IGMP_SANITY_FAILED err_status = %d, vdev_|id|up|bss = 0x%x 0x%x 0x%x, igmp_|enable|vdev_id|num_ipv4_mc = %d %d %d 
1780,iIiIIIII,[ wlan_igmp_offload.c : 70 ] IGMP_OFFLD_QUERY_FAILED err_status = %d, vdev_id|l3_valid|is_mcast|mcbc_ret = 0x%x, proto = %d, offset|length = 0x%x ipv4_|dest|src = 0x%x 0x%x igmp_|type|resp_time|csum|grp_addr = 0x%x 0x%x 
1779,iIIIIIII,[ wlan_igmp_offload.c : 79 ] IGMP_OFFLD_QUERY err_status = %d, ver_bitmask|version = 0x%x grp_addr = 0x%x csum =(0x%x 0x%x) curr|last_query|resp|_time = 0x%x 0x%x 0x%x 
1778,iiIIIi,[ wlan_igmp_offload.c : 88 ] IGMP_FRAME_REPLY : err_status = %d, vdev_id = %d, num_report_req|num_ipv4_list = 0x%x, ipv4_|src|dest 0x%x 0x%x, ret = %d 
1777,IIIIIIII,[ wlan_igmp_offload.c : 96 ] IGMP data parse %x %x %x %x %x %x %x %x 
1776,IIIIIIII,[ wlan_igmp_offload.c : 99 ] IGMP data parse %x %x %x %x %x %x %x %x 
1775,IIIIIIII,[ wlan_igmp_offload.c : 102 ] IGMP data parse %x %x %x %x %x %x %x %x 
1774,iiIiiiI,[ wlan_igmp_offload.c : 43 ] IGMP_WMI_FIXED_PARAM vdev_id = %d enable = %d ver_bitmask = 0x%x num_ipv4_list = %d %d, is_offld_reg = %d vdev_flags = 0x%x 
1773,IIIIIIII,[ wlan_igmp_offload.c : 105 ] IGMP data parse %x %x %x %x %x %x %x %x 
1772,IIIIIIII,[ wlan_igmp_offload.c : 108 ] IGMP data parse %x %x %x %x %x %x %x %x 
1771,IIIIIII,[ wlan_igmp_offload.c : 52 ] IGMP_WMI_IPV4_ADDR_LIST : 0x%x, 0x%x, 0x%x, 0x%x, 0x%x, 0x%x, 0x%x 
1786,i,[ offload_unit_test.c : 135 ] OFFLOAD HDLR UNIT TEST: status = %d 
1785,iii,[ offload_unit_test.c : 180 ] Offload unit test input: vdevid:%d, group=%d, type=%d 
1804,II,[ p2p_go_ps.c : 1455 ] P2P_SCHEDULE_TIMEOUT  0x%x 0x%x 
1803,II,[ p2p_go_ps.c : 1476 ] Current Priority=0x%x  Next Priority=0x%x 
1802,III,[ p2p_go_ps.c : 1559 ] P2P_SCHEDULE_TIMEOUT  0x%x 0x%x 0x%x 
1801,IIII,[ p2p_go_ps.c : 127 ] P2P_GO_BCN_TX_COMP: bcn_tx_status = 0x%x chan_mhz = 0x%x cur_wal_time = 0x%x cur_vdev_tsf = 0x%x 
1800,,[ p2p_go_ps.c : 67 ] p2p_notify_sta_sleep: vdev is NULL 
1799,i,[ p2p_go_ps.c : 74 ] p2p_notify_sta_sleep: %d 
1798,i,[ p2p_go_ps.c : 423 ] p2p_ps_set_noa: vdev_id = %d, Host NOA Disabled 
1797,I,[ p2p_go_ps.c : 448 ] p2p_ps_set_noa: Host Periodic NOA Configuration FAILED, FW_Periodic_NOA_Map=0x%x 
1796,IIII,[ p2p_go_ps.c : 490 ] p2p_ps_set_noa: start_time=0x%x, duration=%u, interval=%u, type_count=%u 
1795,IIii,[ p2p_go_ps.c : 369 ] p2p_ps_set_oppps: Host OPPPS enable FAILED, FW_Periodic_NOA_Map=0x%x, Host_Periodic_NOA_Map = 0x%x, ctwin = %d, bcn_intval = %d 
1794,iii,[ p2p_go_ps.c : 380 ] p2p_ps_set_oppps: vdev_id = %d, oppps_enable = %d, ctwindow = %d 
1793,II,[ p2p_go_ps.c : 569 ] P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
1792,II,[ p2p_go_ps.c : 918 ] P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
1791,II,[ p2p_go_ps.c : 689 ] P2P_NOA_GO_ABSENT  0x%x 0x%x 
1790,II,[ p2p_go_ps.c : 732 ] P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
1789,II,[ p2p_go_ps.c : 712 ] P2P_NOA_GO_PRESENT  0x%x 0x%x 
1788,II,[ p2p_go_ps.c : 1007 ] P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
1787,II,[ p2p_go_ps.c : 824 ] P2P_UPDATE_SCHEDULE_OPPS  0x%x 0x%x 
1818,i,[ p2p_main.c : 1323 ] p2p_client_recal_noa: vdev_id = %d  
1817,III,[ p2p_main.c : 1203 ] P2P_CALC_SCHEDULES_CALL_ALL_NEXT_EVENT_FROM_WHILE_LOOP  0x%x 0x%x 0x%x 
1816,IIIIIII,[ p2p_main.c : 233 ] P2P_GO_GET_NOA_INFO  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
1815,III,[ p2p_main.c : 349 ] P2P_GO_ADD_ONE_SHOT_NOA  0x%x 0x%x 0x%x 
1814,IIIII,[ p2p_main.c : 395 ] P2P_GO_ADD_ONE_SHOT_NOA  0x%x 0x%x 0x%x 0x%x 0x%x 
1813,IIIII,[ p2p_main.c : 642 ] p2p_go_notify_periodic_noa: noa_idx=%u, start_time=0x%x, duration=%u, interval=%u, type_count=%u 
1812,i,[ p2p_main.c : 159 ] P2P_HANDLE_NOA: NoaPresent = %d 
1811,i,[ p2p_main.c : 182 ] P2P_HANDLE_NOA: NoaPresent = %d 
1810,I,[ p2p_main.c : 1258 ] P2P_GO_GET_NOA_INFO  0x%x 
1809,ii,[ p2p_main.c : 747 ] p2p_vdev_evt_handler  vdev_id = %d, evt = %d 
1808,I,[ p2p_main.c : 509 ] P2P_GO_TBTT_OFFSET  0x%x 
1807,IIIII,[ p2p_main.c : 986 ] wlan_p2p_add_noa: boa_idx=%u, start_time=0x%x, duration=%u, interval=%utype_count=%u 
1806,I,[ p2p_main.c : 1308 ] P2P_GO_GET_NOA_INFO  0x%x 
1805,IIIIII,[ p2p_main.c : 1075 ] P2P_GO_GET_NOA_IE  0x%x 0x%x 0x%x 0x%x 0x%x 0x%x 
1819,iiIi,[ p2p_parse.c : 37 ] p2p_is_valid_noa_desc: Ignore invalid NOA descriptor, duration=%d,interval=%d start_time=0x%x type_count=%d 
1830,IIII,[ p2p_schedules.c : 627 ] P2P_CALC_SCHEDULES_FIRST_VALUE  0x%x 0x%x 0x%x 0x%x 
1829,IIIII,[ p2p_schedules.c : 658 ] P2P_CALC_SCHEDULES_CALL_ALL_NEXT_EVENT_FROM_WHILE_LOOP  0x%x 0x%x 0x%x 0x%x 0x%x 
1828,IIIII,[ p2p_schedules.c : 519 ] P2P_FIND_ALL_NEXT_EVENTS_INDIVIDUAL_REQ_AFTER_CHANGE  0x%x 0x%x 0x%x 0x%x 0x%x 
1827,II,[ p2p_schedules.c : 264 ] P2P_NOA_GO_PRESENT  0x%x 0x%x 
1826,II,[ p2p_schedules.c : 92 ] P2P_NOA_EXPIRY_DELTA: curr_time = 0x%x pkt_exp_time = 0x%x 
1825,IIIi,[ p2p_schedules.c : 130 ] P2P_NOA_GO_STATE %x 0x%x 0x%x %d 
1824,IIIII,[ p2p_schedules.c : 742 ] P2P_PROCESS_SCHEDULE_AFTER_CALC  0x%x 0x%x 0x%x 0x%x 0x%x 
1823,IIIiI,[ p2p_schedules.c : 793 ] P2P_PROCESS_SCHEDULE_STARTED_TIMER  0x%x 0x%x 0x%x, Go_Awake=%d, next_timeout=0x%x 
1822,IIIII,[ p2p_schedules.c : 1011 ] P2P_UPDATE_SCHEDULE_OPPS: duration = %u go_sched_type = %u interval = %u start_time = 0x%x type_count = %u 
1821,IIII,[ p2p_schedules.c : 1041 ]  P2P_UPDATE_SCHEDULE: duration = %u interval = %u start_time = 0x%x type_count = %u 
1820,IIII,[ p2p_schedules.c : 934 ] P2P_UPDATE_START_TIME: curr_go_tsf = 0x%x, noa_start_time_go_tsf = 0x%x, curr_wal_time = 0x%x, noa_start_wal_time = 0x%x 
1832,I,[ wlan_pps.c : 266 ] set ebt resync timeout to %u msec
 
1831,II,[ wlan_pps.c : 124 ] PPS wmi_set_vdev_pkt_pwr_save: old:0x%x, new:0x%x 
1836,,[ wlan_pps_priv.c : 665 ] pps arbiter ebt: quit ie detected 
1835,,[ wlan_pps_priv.c : 672 ] pps arbiter ebt: dfs channel detected 
1834,IIiii,[ wlan_pps_priv.c : 705 ] pps arbiter ebt result: features:0x%x, ebt sub:0x%x, macid:%d, old:%d, new:%d 
1833,i,[ wlan_pps_priv.c : 769 ] pps ebt cac timeout result:%d 
1975,,[ wlan_rtt.c : 11133 ] wlan_internal_disable_responder 
1974,,[ wlan_rtt.c : 683 ] Event buffer allocation for cancel measurement response failed 
1973,iii,[ wlan_rtt.c : 4628 ] wlan_oem_rtt_measreq_hdl: client %d running. cannot new req from client: %d. So Dropping req_id: %d 
1972,i,[ wlan_rtt.c : 4651 ] wlan_oem_rtt_measreq_hdl: Request with id %d won't be served because of an error 
1971,i,[ wlan_rtt.c : 4683 ] wlan_oem_rtt_measreq_hdl: asm_req  status %d would be served from call back due to NACK 
1970,ii,[ wlan_rtt.c : 1125 ] wlan_rtt_band_change_req: rtt_2g: %d result: %d 
1969,iIi,[ wlan_rtt.c : 1038 ] wlan_rtt_band_change_req_init_cb: event: %d init_ctxt: %p rtt_2g: %d 
1968,,[ wlan_rtt.c : 3235 ] RTT_CALL_FLOW: WLAN_RTT_BEACON_RX 
1967,iiiiiiii,[ wlan_rtt.c : 4905 ] wlan_rtt_burst_instance_done: num_burst_done:%d total_bursts:%d curr_state:%d burst_duration:%d, index:%d ftm1_done:%d num_meas:%d ftm_per_burst:%d 
1966,,[ wlan_rtt.c : 5012 ] Wait for NAN module to finish sending NAN ranging termination frame 
1965,iI,[ wlan_rtt.c : 11252 ] wlan_rtt_cancel_all_rtt_operation attached to vdev_id: %d p_pdev_rtt_ctxt: %p 
1964,iiiiii,[ wlan_rtt.c : 3825 ] wlan_rtt_cap_msg_req_hdl: client_id: %d Req:%d Reqid:%d Major:%d Minor:%d Revision:%d 
1963,,[ wlan_rtt.c : 3840 ] Event buffer allocation for wlan_rtt_cap_msg_req response failed 
1962,iiiI,[ wlan_rtt.c : 940 ] wlan_rtt_chainmask_change_req() chm_req.t2_req.req_id: %d num_selfgen_chains: %d rtt_chm_state: %d ret: 0x%x 
1961,iii,[ wlan_rtt.c : 976 ] wlan_rtt_chainmask_notif_handler(): ev type: %d rtt_chm_state: %d resp_id: %d 
1960,,[ wlan_rtt.c : 1006 ] RTT CHAIN MASK GRANTED 
1959,iIII,[ wlan_rtt.c : 7462 ] RTT_CHANNEL_SWITCH_GRANT  ev_id = %d p_chnl_switch_ctxt = 0x%x p_owner = 0x%x p_rtt_ctxt = 0x%x 
1958,,[ wlan_rtt.c : 3187 ] RTT_CALL_FLOW: WLAN_RTT_DFS_EXIT 
1957,iII,[ wlan_rtt.c : 3380 ] RTT_CHANNEL_DFS_SWITCH_HDL  ev = %d sw_ctxt->arg = %p sw_ctxt->cb_fn %p 
1956,,[ wlan_rtt.c : 3169 ] RTT_CALL_FLOW: WLAN_RTT_DFS_TIMEOUT_HANDLER 
1955,iiii,[ wlan_rtt.c : 7686 ] RTT_CHANNEL_SWITCH_REQ  module_id %d duration = %d channel = %d priority = %d 
1954,i,[ wlan_rtt.c : 2990 ] wlan_rtt_exit_clean() rtt_chm_state: %d is not expected 
1953,I,[ wlan_rtt.c : 1923 ] wlan_rtt_free_init_ctxt() usage flags = 0x%x 
1952,II,[ wlan_rtt.c : 1960 ] Unregistered wlan_rtt_vdev_notify_handler() for init context vdev = %p status = 0x%x 
1951,I,[ wlan_rtt.c : 6595 ] wlan_rtt_ftm_delta_timeout() Ignore ctxt freed %p 
1950,IIiiiii,[ wlan_rtt.c : 6447 ] wlan_rtt_ftm_init_burst_periodic_timeout: dest_mac:%x%x is_multiburst(%d) is_repetitive_ss(%d) current_burst:%d total_bursts:%d curr_state: %d 
1949,iII,[ wlan_rtt.c : 6503 ] wlan_rtt_ftm_init_burst_periodic_timeout: ERR: Some other request is in progress; skip current burst %d for dest_mac:%x%x 
1948,II,[ wlan_rtt.c : 6535 ] Init PTSF fired resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
1947,iii,[ wlan_rtt.c : 6419 ] wlan_rtt_ftm_resp_burst_timeout: ftm_state: %d num_burst_exp: %d no_burst_count: %d 
1946,II,[ wlan_rtt.c : 11215 ] wlan_rtt_get_clear_stats ranging_dur: %x resp_dur: %x  
1945,iii,[ wlan_rtt.c : 5259 ]  wlan_rtt_get_ftm_chnl_code bw:%d preamble:%d phy_mode:%d 
1944,II,[ wlan_rtt.c : 5205 ] wlan_rtt_get_ie: received invalid frame, ie_len=%u, len=%u 
1943,iiiII,[ wlan_rtt.c : 883 ] wlan_rtt_get_nss_tx_chain_mask_config: mac_id: %d band: %d BW: %d nss1_tx_chm: 0x%x selfgen: 0x%x 
1942,,[ wlan_rtt.c : 5712 ] RTT_ERROR_REPORT :RTT_RESP_CTXT_EXIST 
1941,,[ wlan_rtt.c : 5743 ] RTT_ERROR_REPORT :RTT_RESP_REQ_ACCEPT 
1940,,[ wlan_rtt.c : 5753 ] RTT_ERROR_REPORT :RTT_RESP_BUSY 
1939,iiiIii,[ wlan_rtt.c : 2449 ] wlan_rtt_init_update_channel mhz=%d bw=%d preamble=%d rate_info=0x%x chnl_format=%d error_code=%d 
1938,IIiIIiII,[ wlan_rtt.c : 3638 ] wlan_rtt_init_handler: Starting initiator with mac_addr = %08x%02x  init_idx = %d init_ctxt_usage_flags = 0x%x pmac: %p mac_id: %d vdev: %p rate_info: 0x%x 
1937,,[ wlan_rtt.c : 3643 ] RTT request on a different vdev than the one set during channel change 
1936,IiI,[ wlan_rtt.c : 3665 ] Registered wlan_rtt_vdev_notify_handler() for init context : vdev = %p vdevid = %d status = 0x%x 
1935,iii,[ wlan_rtt.c : 7365 ] vdev mac id(%d) not same as pmac mac id(%d): change PM lock & set mac address: %d 
1934,iiiiI,[ wlan_rtt.c : 7386 ] Channel Granted(Initiator): RTT requested freq: %d phymode: %d Grant came on freq: %d phymode: %d chan_flags: 0x%04x 
1933,iII,[ wlan_rtt.c : 7419 ] Downgraded the BW: New bw: %d chnl_format: %u rate_info: %u 
1932,II,[ wlan_rtt.c : 2062 ] wlan_rtt_init_scheduler => curr_init:0x%x init_ctxt_usage_flags:0x%x 
1931,ii,[ wlan_rtt.c : 2097 ] wlan_rtt_init_scheduler => diff1:%d diff2:%d 
1930,i,[ wlan_rtt.c : 2127 ] wlan_rtt_init_scheduler => next_mb_slot_index:%d  
1929,i,[ wlan_rtt.c : 2172 ] wlan_rtt_init_scheduler: Skipping initiator with index %d as it may creep into next multiburst start time 
1928,iiii,[ wlan_rtt.c : 2189 ] wlan_rtt_init_scheduler => index:%d curr_index:%d schedule_timeout:%d next_mb_slot_index: %d 
1927,iiiiiiiI,[ wlan_rtt.c : 2771 ] RTT_MEAS_REQ_HEAD ch_mhz = %d, center_freq1 = %d ch_mode = %d sta_num:%d, max_reg_power: %d antenna_max: %d, max_tx_power: %d, ch_flags: 0x%04x 
1926,IIIII,[ wlan_rtt.c : 10279 ] Received FTMR resp_tsf_h = 0x%x resp_tsf_l = 0x%x curslot_slot_idx: 0x%x cur_diff: 0x%x resp_ref_tsf: 0x%x 
1925,III,[ wlan_rtt.c : 10296 ] wlan_rtt_is_burst_in_slot: diff_tesf: %u next_burst_tsf: %u cur_tsf: %u 
1924,i,[ wlan_rtt.c : 731 ] wlan_rtt_is_wmi_event_to_send: invalid client_id (%d) 
1923,iiiIIii,[ wlan_rtt.c : 7801 ] wlan_rtt_local_send()status: %d pmac_mac_id: %d vdev_mac_id: %d selfgen_chm: 0x%x abf: %p peer_type: %d vdev_id: %d 
1922,IIIII,[ wlan_rtt.c : 5235 ] RTT_FTM_PARAM_INFO  arg1 = 0x%x arg2 = 0x%x arg3 = 0x%x arg4 = 0x%x arg5 = 0x%x 
1921,iiii,[ wlan_rtt.c : 2916 ] RTT_MEAS_REQ_HEAD  req_id = %d num_chan = %d sps = %d client: %d 
1920,iIii,[ wlan_rtt.c : 7109 ] wlan_rtt_measurement_report: client_id: %d curr_init_ctxt:%p size: %d freq: %d 
1919,iII,[ wlan_rtt.c : 10443 ] nan_ranging_terminate_completion_handler: req_id: %d init_ctxt: %p wait_status: %x 
1918,i,[ wlan_rtt.c : 10466 ] nan_ranging_terminate_completion_handler for req_id: %d is not processed !!! 
1917,iiii,[ wlan_rtt.c : 8862 ] RTT Null frame Tx status: %d tx_fail_count: %d num_meas: %d terminate: %d 
1916,I,[ wlan_rtt.c : 8606 ] RTT add_random_mac_addr failed. status: 0x%x 
1915,i,[ wlan_rtt.c : 4115 ] _wlan_wmi_oem_req: Non TLV format msg received; tlv_head: %d 
1914,iii,[ wlan_rtt.c : 4132 ] wlan_wmi_oem_req: INFO: OEM Req received with sub_type:%d, req_id:%d client: %d 
1913,IIIII,[ wlan_rtt.c : 362 ] wlan_rtt_page_log: %c caller %p stop_count %5u fault_counter %10d fault_delta %10d 
1912,IIII,[ wlan_rtt.c : 372 ] wlan_rtt_page_log_reentrancy: %c%c caller %p entry_count %4d 
1911,ii,[ wlan_rtt.c : 3128 ] wlan_rtt_pm_arb_req(): mac_id: %d state: %d  
1910,IIIIII,[ wlan_rtt.c : 5606 ] wlan_rtt_populate_resp_ftm_param: next_sched_tsf: %u resp_ref_tsf: %u partial_tsf: %u diff_tsf: %u current_resp_tsf64: 0x%08x%08x 
1909,IIIIII,[ wlan_rtt.c : 5635 ] wlan_rtt_populate_resp_ftm_param: next_sched_tsf: %u diff_tsf: %u nearest_tsf: %u resp_partial_tsf: %u next_burst_tsf: 0x%08x%08x 
1908,II,[ wlan_rtt.c : 5690 ] wlan_rtt_populate_resp_ftm_param: ftm_param.burst_period: %u resp_param_info.burst_period: %u 
1907,Ii,[ wlan_rtt.c : 518 ] wlan_rtt_proceed: init_ctxt: %p wait_status: %d 
1906,iIIIIIIII,[ wlan_rtt.c : 2717 ] RTT_MEAS_REQ_BODY idx = %d dest_mac_0to31 = 0x%x dest_mac_32to47 = 0x%x sppof_bssid_0to31 = 0x%x spoof_bssid_32to47 = 0x%x control_inf = 0x%x meas_inf = 0x%x meas_params1 = 0x%x meas_params2 = 0x%x 
1905,IIIII,[ wlan_rtt.c : 10547 ] wlan_rtt_ranging_negotiation_status_notif_handler: timeout_us:%u burst_start_time_h:%u burst_start_time_l:%u StartTsf:%u curr_time%u 
1904,iIi,[ wlan_rtt.c : 10574 ] wlan_rtt_ranging_negotiation_status_notif_handler: ranging_ind_data->RangingParams.ReqId %d init_ctxt %p event_handled %d 
1903,iii,[ wlan_rtt.c : 7286 ] wlan_rtt_resp_chan_switch_hdl()  ev_id = %d ftm_state:%d is_ftmr_pending:%d 
1902,II,[ wlan_rtt.c : 3094 ] Unregistered wlan_rtt_vdev_notify_handler() for resp context vdev = %p status = 0x%x 
1901,IIIII,[ wlan_rtt.c : 10236 ] wlan_rtt_resp_free_existing_slot 0x%x 0x%x 0x%x dest_mac:%08x%02x 
1900,iiI,[ wlan_rtt.c : 6346 ] wlan_rtt_resp_ftm1_timeout: ftm_state: %d asap: %d resp_ctxt: %p 
1899,IIIIIIII,[ wlan_rtt.c : 10222 ] wlan_rtt_resp_get_free_slot 0x%x 0x%x 0x%x 0x%x 0x%x 0x%x dest_mac:%08x%02x 
1898,ii,[ wlan_rtt.c : 6192 ] wlan_rtt_resp_init:current session is active: session_index: %d slot: %d 
1897,ii,[ wlan_rtt.c : 6203 ] wlan_rtt_resp_init: Received a frame which we are not in slot send FTM stop frame. session_index: %d slot: %d 
1896,iii,[ wlan_rtt.c : 6074 ] wlan_rtt_resp_init_body: session_active: %d init_new_session: %d ftm_state: %d 
1895,iii,[ wlan_rtt.c : 6078 ] wlan_rtt_resp_init_body: asap: %d ftm_state: %d session_active: %d 
1894,iiI,[ wlan_rtt.c : 6112 ] wlan_rtt_resp_init_body:ftm_state: %d asap: %d resp_ctxt: %p 
1893,III,[ wlan_rtt.c : 6132 ] wlan_rtt_resp_init_body: ftm_state: %u asap: %u resp_ctxt: %p 
1892,IiII,[ wlan_rtt.c : 5883 ] Registered wlan_rtt_vdev_notify_handler() for resp context vdev: %p vdev_type: %d pmac: %p status: 0x%x 
1891,ii,[ wlan_rtt.c : 6024 ] wlan_rtt_resp_init_new_session: slot: %d param_info.status: %d 
1890,iiI,[ wlan_rtt.c : 6033 ] END_FTM_INVALID_REQUEST: ftm_state: %d asap: %d resp_ctxt: %p 
1889,iiiiiiii,[ wlan_rtt.c : 5494 ] wlan_rtt_resp_init_rate: vdev_id: %d phy_mode: %d mhz: %d ftm_chnl_format: %d param_ie_valid: %d tx_bw: %d tx_preamble: %d mcs: %d 
1888,IIIi,[ wlan_rtt.c : 7269 ] Channel Granted(Responder): Responder operating freq = 0x%x pmac = %p Granted on freq: 0x%x phymode: %d 
1887,ii,[ wlan_rtt.c : 10382 ] wlan_rtt_resp_house_keeping: channel_mhz: %d nearest_sched_resp_tsf_ctxt_index: %d 
1886,,[ wlan_rtt.c : 2272 ] All requests done nothing to schedule 
1885,iiiI,[ wlan_rtt.c : 6958 ] RTT_ERROR_WMI_EVENT: ERROR: client_id: %d req_id:%d reason:%d init_ctxt: %p 
1884,,[ wlan_rtt.c : 7002 ] Event buffer allocation for send_rtt_error_report failed 
1883,iIiiiIi,[ wlan_rtt.c : 7159 ] wlan_rtt_send_measurement_report_hdl: client_id: %d curr_init_ctxt: %p token_id:%d frag_idx:%d more_frag: %d buf:%p buf_len:%d 
1882,IIIi,[ wlan_rtt.c : 7866 ] wlan_rtt_send_null_frame: abf: %p channel: %x pmac = %p spoofed_seqno = %d 
1881,Ii,[ wlan_rtt.c : 7884 ] RTT NULL frame Tx failed: abf: %p ret: %d 
1880,,[ wlan_rtt.c : 8389 ] wlan_rtt_send_tm_frame: vdev is seen as NULL in resp_ctxt 
1879,,[ wlan_rtt.c : 8543 ] RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
1878,IiIIiiiiI,[ wlan_rtt.c : 8552 ] wlan_rtt_send_tm_frame: abf: %p freq: %d pmac = %p resp_ctxt: %p tkn = %d follow_tkn = %d tx_bw = %d resp_ctxt ftm state = %d chan_flags = 0x%04x 
1877,,[ wlan_rtt.c : 8121 ] Selfgen chainmask granted is zero. return error 
1876,II,[ wlan_rtt.c : 8227 ] Sending RTT Trigger frame resp_tsf_h = 0x%x resp_tsf_l = 0x%x 
1875,,[ wlan_rtt.c : 8258 ] RTT_ERROR_REPORT :ALLOCATE_FRAME_BUFFER_ERROR 
1874,IIi,[ wlan_rtt.c : 8282 ] wlan_rtt_send_tmr_frame: channel: %x pmac = %p spoofed_seqno = %d 
1873,,[ wlan_rtt.c : 8323 ] RTT_TIMER_STOP 
1872,I,[ wlan_rtt.c : 8072 ] RTT_CALL_FLOW: WLAN_RTT_SET_VENDOR_IE_HT_VHT_ACK ts = %u 
1871,iii,[ wlan_rtt.c : 11095 ] wlan_rtt_sta_resp_chan_switch: channel.mhz: %d band_center_freq1: %d phy_mode: %d 
1870,i,[ wlan_rtt.c : 1508 ] wlan_rtt_start_burst_periodic_timer: timeout_ms:%dms 
1869,iIIi,[ wlan_rtt.c : 1263 ] wlan_rtt_terminate_all_ftm_resp_context() idx: %d resp_ctxt = %p vdev = %p ftm_state = %d 
1868,iiii,[ wlan_rtt.c : 1341 ] cancel_measurement_req: vdev_type: %d, req_id: %d, free_curr_init: %d, is_cancelled: %d 
1867,iIII,[ wlan_rtt.c : 2030 ] wlan_rtt_terminate_repetitive_ss_request: red_id:%d init_ctxt_usage_flags:0x%x dest_mac :%x %x 
1866,iii,[ wlan_rtt.c : 1215 ] wlan_rtt_terminate_resp_context() state: %d busrt_exp: %d burst_count: %d 
1865,iii,[ wlan_rtt.c : 9176 ] wlan_rtt_tm_ack_handle_completion: ftm_state: %d num_burst_exp: %d no_burst_count: %d 
1864,IiIII,[ wlan_rtt.c : 9208 ] wlan_rtt_tm_ack_handle_completion: init_ftmr_rx_ts: %10u completion_status: %d ftm_tx_ts: %10u init_ftmr_offset: %6u delta_ftm_act: %6u 
1863,i,[ wlan_rtt.c : 9290 ] RTT TM frame Tx status: %d 
1862,i,[ wlan_rtt.c : 9237 ] RTT_TWOSIDED_RESP_CNT  number = %d 
1861,iii,[ wlan_rtt.c : 9257 ] wlan_rtt_tm_ack_success: ftm_state: %d num_burst_exp: %d no_burst_count: %d 
1860,iii,[ wlan_rtt.c : 9262 ] wlan_rtt_tm_ack_success:Don't continue burst: ftm_state: %d num_burst_exp: %d no_burst_count: %d  
1859,iIIiIII,[ wlan_rtt.c : 9638 ] state = %d tsf_sync_info = 0x%x resp_tsf = 0x%x Diff: %d ftm_req_start_time = 0x%x ftm_req_complete_time = 0x%x current_tsf = 0x%x 
1858,II,[ wlan_rtt.c : 9649 ] RTT TM FTM curr_tsf_delta = 0x%x new_tsf_delta = 0x%x 
1857,,[ wlan_rtt.c : 9825 ] RTT_ERROR_REPORT :TM_TOKEN_MISMATCH 
1856,,[ wlan_rtt.c : 9828 ] RTT_ERROR_REPORT :TM_CFR_CAPTURE_ERROR 
1855,,[ wlan_rtt.c : 9830 ] RTT_ERROR_REPORT :TM_SEQUENCE_RESTART 
1854,,[ wlan_rtt.c : 9884 ] RTT_ERROR_REPORT :RTT_GET_TM_NOTWAIT_TM 
1853,,[ wlan_rtt.c : 9902 ] RTT_ERROR_REPORT :RTT_GET_TM_NOTWAIT_TM 
1852,IIiIIII,[ wlan_rtt.c : 9985 ] wlan_rtt_tm_rx_hdl: status: 0x%x RTT_TWOSIDED_RESP_CNT  number = %2d recv_state: %d init_ftmr_tx_ts: %10u ftm_rx_ts: %10u init_ftmr_offset: %6u delta_ftm_act: %6u 
1851,I,[ wlan_rtt.c : 8704 ] RTT add_random_mac_addr failed. status: 0x%x 
1850,,[ wlan_rtt.c : 9516 ] rtt_tmr_rx_hdl() vdev not found 
1849,,[ wlan_rtt.c : 9522 ] rtt_tmr_rx_hdl() wal_vdev not found 
1848,II,[ wlan_rtt.c : 9557 ] rtt_tmr_rx_hdl() ftmr_rx_ts: %10u begin_tsf_sap_resp: %10u 
1847,,[ wlan_rtt.c : 9576 ] RTT_ERROR_REPORT :RTT_GET_INVALID_TMR_STOP 
1846,,[ wlan_rtt.c : 9596 ] RTT_ERROR_REPORT :RTT_GET_INVALID_TMR_STOP 
1845,iiI,[ wlan_rtt.c : 8923 ] RTT TMR frame Tx status: %d curr_state: %d ftmr_tx_ts: %u 
1844,iiii,[ wlan_rtt.c : 4281 ] RTT_UNIT_TEST_CMD 1  num_args = %d arg0 = %d vdev_id = %d mac_id = %d 
1843,,[ wlan_rtt.c : 4332 ] Channel not configured 
1842,iiiiii,[ wlan_rtt.c : 4344 ] RTT_UNIT_TEST_CMD numFrms= %d ChnlFrmt= %d frmType= %d reportType= %d burstDr= %d asap_mode= %d 
1841,i,[ wlan_rtt.c : 4573 ] RTT_UNIT_TEST_CMD 2  status = %d 
1840,,[ wlan_rtt.c : 4321 ] MAC address not configured 
1839,Iii,[ wlan_rtt.c : 1435 ] wlan_rtt_vdev_notify_handler() vdev = %p vdev_id = %d notification type = %d 
1838,,[ wlan_rtt.c : 10779 ] Event buffer allocation for send_responder_cfg_info response failed 
1837,iiIii,[ wlan_rtt.c : 7063 ] wmi_send_rtt_error_report_event: req_id: %d reason: %d init_ctxt: %p vdev_type: %d nan_req_active: %d 
1993,i,[ wlan_rtt_tlv_helper.c : 194 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Couldn't get expected number of TLVs for sub_type=%d
 
1992,ii,[ wlan_rtt_tlv_helper.c : 223 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: No TLV attributes found for sub_type=%d Tag_order=%d
 
1991,iii,[ wlan_rtt_tlv_helper.c : 247 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Can't get  the first TLV Tag ID (tlv_index:%d) for last entered loop start (cnt=%d) for sub_type=%d
 
1990,iiii,[ wlan_rtt_tlv_helper.c : 255 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: First TLV Tag ID (%d) for last entered loop start (index=%d) doesn't match; skipping this tlv with tag:%d for sub_type=%d 
1989,iii,[ wlan_rtt_tlv_helper.c : 278 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: TLV has wrong tag in order for sub_type=%d. Given=%d, Expected=%d.
 
1988,iii,[ wlan_rtt_tlv_helper.c : 284 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: TLV has wrong tag in order for sub_type=%d. Given=%d, Expected=%d.
 
1987,ii,[ wlan_rtt_tlv_helper.c : 292 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Wrong TLV length %d for loop end for sub_type:%d 
1986,i,[ wlan_rtt_tlv_helper.c : 297 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Loop start and End mismatch for sub_type:%d 
1985,iii,[ wlan_rtt_tlv_helper.c : 320 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Exceeded given max loop count %d, for sub_type:%d tlv_index:%d 
1984,ii,[ wlan_rtt_tlv_helper.c : 329 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Wrong TLV length %d for loop start for sub_type:%d 
1983,i,[ wlan_rtt_tlv_helper.c : 334 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Maximum inner loops reached for sub_type:%d 
1982,i,[ wlan_rtt_tlv_helper.c : 367 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: ERROR Need to handle this tag ID %d for variable length
 
1981,ii,[ wlan_rtt_tlv_helper.c : 378 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: TLV truncated. tlv_size_diff=%d, curr_tlv_len=%d
 
1980,i,[ wlan_rtt_tlv_helper.c : 393 ] RTTTLV_CHECK_AND_PAD_TLVS: WARN: TLV needs padding. tlv_size_diff=-%d
 
1979,ii,[ wlan_rtt_tlv_helper.c : 458 ] RTTTLV_CHECK_AND_PAD_TLVS: Some loop(cnt = %d) didn't ended properly for sub_type:%d 
1978,iiiiii,[ wlan_rtt_tlv_helper.c : 214 ] RTTTLV_CHECK_AND_PAD_TLVS: ERROR: Invalid TLV length for sub_type=%d Tag_order=%d buf_idx=%d Tag:%d Len:%d TotalLen:%d
 
1977,iiii,[ wlan_rtt_tlv_helper.c : 99 ] ERROR: TLV order %d greater than num_of_tlvs:%d for is_req:%d rtt_cmd_event_id: %d 
1976,ii,[ wlan_rtt_tlv_helper.c : 119 ] ERROR: Didn't found WMI TLV attribute definitions for is_req:%d rtt_cmd_event_id: %d 
1999,,[ wlan_obss_scan_offload.c : 433 ] obss scan TE-A rec null 
1998,i,[ wlan_obss_scan_offload.c : 705 ] obss scan stop, refer cnt:%d, status 
1997,I,[ wlan_obss_scan_offload.c : 184 ] obss coex action frame buf null, vdev id:%x 
1996,i,[ wlan_obss_scan_offload.c : 581 ] obss scan vdev pool alloc failed=%d 
1995,,[ wlan_obss_scan_offload.c : 628 ] Channel not in 2.4 GHz sent 
1994,,[ wlan_obss_scan_offload.c : 640 ] Channel not in 2.4 GHz sent 
2009,i,[ wlan_network_list_offload.c : 285 ] nlo_ssid_match: ssid_len=%d exceeds MAX_SSID_LEN 
2008,iiiI,[ wlan_network_list_offload.c : 1429 ] NLO_CONFIG_1 vdev_id %d no_of_ssids %d num_of_channels %d flags 0x%x 
2007,iiii,[ wlan_network_list_offload.c : 1692 ] NLO ADD SSID bcast_nw_type.valid:%d bcast_nw_type.type:%d num_ssid:%d ssid_len:%d 
2006,i,[ wlan_network_list_offload.c : 1697 ] NLO ADD BCAST PROBE ssid_len:%d 
2005,iiiii,[ wlan_network_list_offload.c : 1437 ] NLO_CONFIG_2 fast_scan_period %d slow_scan_period %d delay_start_time %d probe_bundle_size %d backoff_multiplier %d 
2004,iiiii,[ wlan_network_list_offload.c : 1444 ] NLO_CONFIG_3 active_dwell %d passive_dwell %d fast_max_cycle %d  rest_time %d max_rest %d 
2003,,[ wlan_network_list_offload.c : 269 ] Sacn cycle failed 
 
2002,,[ wlan_network_list_offload.c : 1200 ] Sacn cycle failed 
 
2001,iiiiii,[ wlan_network_list_offload.c : 2017 ] NLO_START_UNIT_TEST max_cycles = %d fast_period = %d slow_period = %d backoff_multiplier = %d delay_start_time = %d num_args = %d 
2000,i,[ wlan_network_list_offload.c : 2063 ] NLO_STOP_UNIT_TEST vdev_id %d 
2022,IIII,[ wlan_latency_manager.c : 640 ] WLM could not populate WMI config: isUp:%x, conc:%x, wow:%x, wlm_vdev:%x 
2021,iiI,[ wlan_latency_manager.c : 538 ] WLM deliver notif: new lvl:%d, last lvl:%d, flags:0x%x
 
2020,I,[ wlan_latency_manager.c : 175 ] WLM deregistered by module: %x
 
2019,ii,[ wlan_latency_manager.c : 480 ] ll_vdev_num:%d set ll_flag:%d 
2018,I,[ wlan_latency_manager.c : 120 ] WLM registered by module: %x
 
2017,I,[ wlan_latency_manager.c : 156 ] WLM registered after WMI config: %x
 
2016,II,[ wlan_latency_manager.c : 665 ] wlm_vdev=%x is NULL or WLM already in default settings:%x 
2015,I,[ wlan_latency_manager.c : 669 ] WLM request for default config:%x 
2014,II,[ wlan_latency_manager.c : 695 ] wlm_vdev=%x is NULL or WLM already in latest settings:%x 
2013,I,[ wlan_latency_manager.c : 703 ] WLM notify by %x module of WMI config 
2012,I,[ wlan_latency_manager.c : 364 ] WLM vdev evt handler: %x
 
2011,I,[ wlan_latency_manager.c : 59 ] WLM vdev had been initialized: %x
 
2010,iiiiII,[ wlan_latency_manager.c : 597 ] WLM config, vdev_id:%d, ifUp:%d, cur lvl:%d, wmi lvl:%d (0:Normal, 1:Mod, 2:Low, 3:Ultra low), cur_flags:0x%x, wmi_flags:0x%x 
2025,i,[ wlan_latency_manager_unit_test.c : 32 ] wlan_vdev_latency_config_wmi_test entry:%d
 
2024,iIii,[ wlan_latency_manager_unit_test.c : 101 ] wlan_wlm_get_cur_config: latency_level:%d, flags:%x, ul_latency(ms):%d, dl_latency(ms):%d 
2023,i,[ wlan_latency_manager_unit_test.c : 111 ] wlan_wlm_set_wow_state entry:%d
 
2031,IIi,[ umac_wmi_events.c : 576 ] WMI_CHAN_INFO_EVENT_ALLOC_FAILURE  EventId = 0x%x chan_freq = 0x%x PendingEvents = %d 
2030,iII,[ umac_wmi_events.c : 624 ] WMI_EVENT_ALLOC_FAILURE vdev_id = %d EventId = 0x%x AssocId/VdevMap = 0x%x 
2029,iII,[ umac_wmi_events.c : 725 ] WMI_EVENT_ALLOC_FAILURE vdev_id = %d EventId = 0x%x AssocId/VdevMap = 0x%x 
2028,ii,[ umac_wmi_events.c : 99 ] drop mgmt as size:%d,limit:%d 
2027,,[ umac_wmi_events.c : 256 ] BEACON_EVENT_SWBA_SEND_FAILED 
2026,I,[ umac_wmi_events.c : 700 ] TX_PAUSE EventId = 0x%x 
2045,,[ wlan_wmi.c : 340 ] WMI_OEM_DATA_CMD_SET_BURST_DURATION: read TLV failed 
2044,ii,[ wlan_wmi.c : 358 ] wlan_oem_vdev_set_burst_duration configuration ac=%d, duration=%d 
2043,,[ wlan_wmi.c : 361 ] wlan_oem_vdev_set_burst_duration warning: wrong TLV type 
2042,ii,[ wlan_wmi.c : 492 ] WMI_OEM_DATA_CMDID: vdev_id=%d pdev_id:%d 
2041,,[ wlan_wmi.c : 509 ] wlan_wmi_oem_data_cmd: read header TLV failed
 
2040,ii,[ wlan_wmi.c : 520 ] wlan_wmi_oem_data_cmd: Header TLV=%d, length=%d 
2039,i,[ wlan_wmi.c : 596 ] wlan_wmi_oem_data_cmd: cmd=%d doesn't support 
2038,,[ wlan_wmi.c : 610 ] wlan_wmi_oem_dispatch_cmds 
2037,,[ wlan_wmi.c : 287 ] wlan_wmi_read_tlv: p_in_tlv is NULL 
2036,,[ wlan_wmi.c : 293 ] wlan_wmi_read_tlv: p_out_tlv is NULL 
2035,III,[ wlan_wmi.c : 316 ] wlan_wmi_read_tlv: type=%u, length=%u, read_len=%u 
2034,,[ wlan_wmi.c : 247 ] wlan_wmi_write_tlv: p_in_tlv is NULL 
2033,,[ wlan_wmi.c : 253 ] wlan_wmi_write_tlv: p_out_tlv is NULL 
2032,III,[ wlan_wmi.c : 273 ] wlan_wmi_write_tlv: type=%u, length=%u, write_len=%u 
2067,iiii,[ wlan_wmi_events.c : 577 ] wlan_debug_mesg_flush_compete stall_type:%d vdev_bmap:%d reason_code1:%d reason_code2:%d 
2066,II,[ wlan_wmi_events.c : 685 ] WMI handle send WMI evt msg fail, evt_id:0x%x, evt_len:0x%x
 
2065,II,[ wlan_wmi_events.c : 689 ] WMI handle send WMI evt msg, evt_id:0x%x, evt_len:0x%x
 
2064,IIIII,[ wlan_wmi_events.c : 263 ] bdf_version = %x ref_design_id=%x, customer_id=%x, project_id=%x, board_data_rev=%x 
2063,IIIIIIII,[ wlan_wmi_events.c : 1611 ] WMI Service Ready Ext: wmi_svc_bitmap(ext) = 0x%08x %08x %08x %08x (%08x %08x %08x %08x) 
2062,III,[ wlan_wmi_events.c : 734 ] DISPLAY_TPC_STATS: 1st event tpcEvSize is %lu wal_pdev_get_reg_array_len is %lu reg_mask is %u 
2061,,[ wlan_wmi_events.c : 738 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
2060,,[ wlan_wmi_events.c : 746 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
2059,I,[ wlan_wmi_events.c : 973 ] DISPLAY_TPC_STATS: 4th event tpcEvSize is %lu 
2058,I,[ wlan_wmi_events.c : 975 ] DISPLAY_TPC_STATS: wal_pdev_get_ctl_array_len is %lu 
2057,,[ wlan_wmi_events.c : 982 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
2056,,[ wlan_wmi_events.c : 989 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
2055,I,[ wlan_wmi_events.c : 995 ] DISPLAY_TPC_STATS: event starting ptr is %lu 
2054,,[ wlan_wmi_events.c : 710 ] DISPLAY_TPC_STATS: wmi_tpc_stats_event_complete 
2053,II,[ wlan_wmi_events.c : 809 ] DISPLAY_TPC_STATS: 2nd event tpcEvSize is %lu wal_pdev_get_rates_array_len is %lu 
2052,,[ wlan_wmi_events.c : 813 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
2051,,[ wlan_wmi_events.c : 820 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
2050,I,[ wlan_wmi_events.c : 826 ] DISPLAY_TPC_STATS: event starting ptr is %lu 
2049,I,[ wlan_wmi_events.c : 885 ] DISPLAY_TPC_STATS: 3rd event tpcEvSize is %lu 
2048,,[ wlan_wmi_events.c : 892 ] DISPLAY_TPC_STATS: Event size exceeds WMI_SVC_MSG_SIZE!! 
2047,,[ wlan_wmi_events.c : 899 ] DISPLAY_TPC_STATS: WMI tpc stats evt, allocation failed! 
2046,,[ wlan_wmi_events.c : 654 ] WOW send initial wakeup wmi cmd 
2105,i,[ wlan_wow_enhance.c : 1189 ]  Auto detect: Failure handling - Sending Event to Host - reason id %d 
2104,i,[ wlan_wow_enhance.c : 2907 ] wow_assert_tmr start  %d 
2103,,[ wlan_wow_enhance.c : 2913 ] Excessive time bw consecutive NACKs 
2102,iii,[ wlan_wow_enhance.c : 2928 ] wow_assert_tmr wow_asserted @ %d, wow_continus_nack_period %d first_wow_nack_time %d 
2101,i,[ wlan_wow_enhance.c : 2076 ] WOW data msg hdlr msgId %d 
2100,i,[ wlan_wow_enhance.c : 1985 ] WOW host intf handle msg_status=%d 
2099,i,[ wlan_wow_enhance.c : 2150 ] WOW event comp handle  msg_status=%d 
2098,I,[ wlan_wow_enhance.c : 2192 ] WOW Error, page prefetch failure count is %x 
2097,i,[ wlan_wow_enhance.c : 2267 ] WOW enter failure, wow state:%d 
2096,i,[ wlan_wow_enhance.c : 2293 ] WOW awake complete,  page_fault no=%d 
2095,ii,[ wlan_wow_enhance.c : 493 ] HTT msg saved failure:%d, type %d 
2094,i,[ wlan_wow_enhance.c : 506 ] HTT msg type %d 
2093,ii,[ wlan_wow_enhance.c : 1017 ] Not in wow entered state wow state=%d wake reason=%d 
2092,,[ wlan_wow_enhance.c : 945 ] WOW handle wakeup host msg in RT 
2091,iii,[ wlan_wow_enhance.c : 906 ] WOW wakeup host wake reason=%d, packet_len:%d, len:%d 
2090,,[ wlan_wow_enhance.c : 966 ] WOW data wakeup host msg to RT 
2089,i,[ wlan_wow_enhance.c : 2359 ] is_wow_close_to_tbtt: time_to_next_wakeup %d: 
2088,,[ wlan_wow_enhance.c : 1108 ] Wow error mac operation fail 
2087,i,[ wlan_wow_enhance.c : 1128 ] Wow enable full d2log capture %d 
2086,,[ wlan_wow_enhance.c : 1118 ] Wow error mac operation fail 
2085,iiII,[ wlan_wow_enhance.c : 2434 ] WOW CMD hdlr: pause=%d, mod_dtim_ini=%d, suspend_flags=0x%x is_system_suspend=0x%x 
2084,,[ wlan_wow_enhance.c : 2449 ] WOW CMD hdlr: WOW Command deferred due to TWT 
2083,iI,[ wlan_wow_enhance.c : 2484 ] WOW event flag: idx=%d evt %x
 
2082,,[ wlan_wow_enhance.c : 2489 ] WOW error in WFA mode 
2081,I,[ wlan_wow_enhance.c : 2495 ] WOW error mgmt tx pending %x 
2080,,[ wlan_wow_enhance.c : 2501 ] WOW error RTT active 
2079,,[ wlan_wow_enhance.c : 2517 ] WOW error Fatal Event Log Flush in progress 
2078,,[ wlan_wow_enhance.c : 2543 ] Wow error : wow entry close to TBTT 
2077,,[ wlan_wow_enhance.c : 2550 ] Wow error : TWT Pause not successful 
2076,,[ wlan_wow_enhance.c : 2557 ] Wow error : WOW Deferred timeout 
2075,,[ wlan_wow_enhance.c : 2570 ] Wow error mac operation fail 
2074,i,[ wlan_wow_enhance.c : 2606 ] wow_acked @ %d 
2073,ii,[ wlan_wow_enhance.c : 2889 ] WOW enable wake event vdevId=%d isAdd=%d 
2072,III,[ wlan_wow_enhance.c : 2892 ] WOW wake event bitmap input:%x pdev:%x vdev:%x 
2071,I,[ wlan_wow_enhance.c : 2814 ] WOW host awake ind wake reason %x 
2070,I,[ wlan_wow_enhance.c : 1634 ] WOW_STA_VDEV_DISALLOW  0x%x 
2069,I,[ wlan_wow_enhance.c : 1644 ] WOW_P2PGO_VDEV_DISALLOW  0x%x 
2068,III,[ wlan_wow_enhance.c : 1661 ] WOW_AP_VDEV_DISALLOW  allow_status = 0x%x, is_all_sleep:%x, is_twt:%x 
2132,III,[ cmdLp.c : 328 ] lowpowerHandler: lowPowerMode:0x%x, lowPowerFeatureMask:0x%x, phyIdMask:0x%x, 
 
2131,,[ cmdLp.c : 428 ] lowpowerHandler: lowPowerMode:done 
2130,i,[ cmdLp.c : 255 ] lowpowerHandler_btclock: BT CLOCK enable=0x%d 
2129,i,[ cmdLp.c : 122 ] lowpowerHandler_ddssdisable: g_ddss_disable_all=%d
 
2128,i,[ cmdLp.c : 108 ] lowpowerHandler_dss: g_synth_control_ftm[0]=%d
 
2127,I,[ cmdLp.c : 297 ] lowpowerHandler_hdl_psMask: phyId:0x%x, No effect as phy is inactive! 
 
2126,I,[ cmdLp.c : 302 ] lowpowerHandler_hdl_psMask: phyId:0x%x, No effect as phy is in sleep! 
 
2125,II,[ cmdLp.c : 314 ] lowpowerHandler_hdl_psMask: phyId:0x%x, hdlpsMask=0x%x 
 
2124,II,[ cmdLp.c : 75 ] lowpowerHandler_imps_bmps: phyId:0x%x, g_ftm_lowPowerMode_imps_bmps:0x%x 
 
2123,,[ cmdLp.c : 84 ] lowpowerHandler_imps_bmps: issue wal_pm_ftm_set_power_state sleep 
 
2122,,[ cmdLp.c : 91 ] lowpowerHandler_imps_bmps: issue wal_pm_ftm_set_power_state wakeup 
 
2121,i,[ cmdLp.c : 247 ] lowpowerHandler_lpSynthForLegacyRx: g_ftm_lpSynthForLegacyRx_enable=0x%d 
 
2120,i,[ cmdLp.c : 240 ] lowpowerHandler_lpSynthForLegacyTx: g_ftm_lpSynthForLegacyTx_enable=0x%d 
 
2119,II,[ cmdLp.c : 219 ] lowpowerHandler_ocl: phyId:0x%x, ocl_enable=0x%x, No effect as phy is inactive! 
 
2118,II,[ cmdLp.c : 232 ] lowpowerHandler_ocl: phyId:0x%x, ocl_enable=0x%x 
 
2117,I,[ cmdLp.c : 269 ] lowpowerHandler_pbs: phyId:0x%x, No effect as phy is inactive! 
2116,I,[ cmdLp.c : 274 ] lowpowerHandler_pbs: phyId:0x%x, No effect as phy is in sleep! 
2115,iii,[ cmdLp.c : 283 ] lowpowerHandler_pbs: phyId:%d, pbs_enable=%d, pbs_flag=%d 
2114,I,[ cmdLp.c : 161 ] lowpowerHandler_phydbgEnable: phyId:0x%x, No effect as phy is inactive! 
 
2113,I,[ cmdLp.c : 166 ] lowpowerHandler_phydbgEnable: phyId:0x%x, No effect as phy is in sleep! 
 
2112,i,[ cmdLp.c : 176 ] lowpowerHandler_phydbgEnable: g_phydbg_disable=%d
 
2111,I,[ cmdLp.c : 135 ] lowpowerHandler_phydbgdisable: phyId:0x%x, No effect as phy is inactive! 
 
2110,I,[ cmdLp.c : 140 ] lowpowerHandler_phydbgdisable: phyId:0x%x, No effect as phy is in sleep! 
 
2109,i,[ cmdLp.c : 149 ] lowpowerHandler_phydbgdisable: g_phydbg_disable=%d
 
2108,II,[ cmdLp.c : 189 ] lowpowerHandler_xlnabypass: phyId:0x%x, xlna_bypass=0x%x, No effect as phy is inactive! 
 
2107,II,[ cmdLp.c : 194 ] lowpowerHandler_xlnabypass: phyId:0x%x, xlna_bypass=0x%x, No effect as phy is in sleep! 
 
2106,II,[ cmdLp.c : 201 ] lowpowerHandler_xlnabypass: phyId:0x%x, xlna_bypass=0x%x 
 
2189,i,[ cmdProcessTlv2.c : 517 ] FTM Tx ChainMask %d overwrite to 0x2 due to BT2ed Harmonic! 
2188,Ii,[ cmdProcessTlv2.c : 4871 ] %s: #### Getting cal version:bdfvertype: %d  !
 
2187,ii,[ cmdProcessTlv2.c : 2032 ] PHYDBGdump2Handler(Phy:%d, Option:%d)
 
2186,IiI,[ cmdProcessTlv2.c : 2040 ] ### data_ptr %p size %d status 0x%x
 
2185,Ii,[ cmdProcessTlv2.c : 2049 ] ### data_ptr %p stream_cnt %d
 
2184,,[ cmdProcessTlv2.c : 2052 ] ### Data buffer stream ended
 
2183,ii,[ cmdProcessTlv2.c : 2444 ] PHYDBGdumpHandler(Phy:%d, Option:%d)
 
2182,IiI,[ cmdProcessTlv2.c : 2452 ] ### data_ptr %p size %d status 0x%x
 
2181,Ii,[ cmdProcessTlv2.c : 2461 ] ### data_ptr %p stream_cnt %d
 
2180,,[ cmdProcessTlv2.c : 2464 ] ### Data buffer stream ended
 
2179,Ii,[ cmdProcessTlv2.c : 4848 ] %s :set cal version , bdfvertype: %d !
 
2178,i,[ cmdProcessTlv2.c : 4108 ] Channel index out of bounds %d 
2177,i,[ cmdProcessTlv2.c : 4116 ] Power offset Index out of bounds %d 
2176,ii,[ cmdProcessTlv2.c : 4124 ] 2G index %d flag %d 
2175,ii,[ cmdProcessTlv2.c : 4137 ] values written 2G %d 5G %d 
2174,i,[ cmdProcessTlv2.c : 4198 ] Channel index out of bounds %d 
2173,i,[ cmdProcessTlv2.c : 4279 ] Channel index out of bounds %d 
2172,i,[ cmdProcessTlv2.c : 4309 ] Gain index out of bounds %d 
2171,i,[ cmdProcessTlv2.c : 4294 ] Target Power index out of bounds %d 
2170,,[ cmdProcessTlv2.c : 4625 ] OPC_OTP_WRITE:Ready to send response!
 
2169,I,[ cmdProcessTlv2.c : 4626 ] OTP Write status, 0x%x 
2168,,[ cmdProcessTlv2.c : 4638 ] OPC_OTP_WRITE:send response done!
 
2167,,[ cmdProcessTlv2.c : 3064 ] bdGetSizeHandler
 
2166,iIii,[ cmdProcessTlv2.c : 3091 ] bdReadHandler: bdSize %d, offset 0x%x, size %d, source %d
 
2165,i,[ cmdProcessTlv2.c : 3132 ] error in bdReadHandler: status %d
 
2164,Ii,[ cmdProcessTlv2.c : 4525 ] bdWriteHandler: offset 0x%x, size %d
 
2163,IIIII,[ cmdProcessTlv2.c : 3838 ] COEX Req Handler(wght0= 0x%x,wght1= 0x%x,wght2= 0x%x,wght3= 0x%x,wght4= 0x%x)
 
2162,IIIIII,[ cmdProcessTlv2.c : 3847 ] COEX Req Handler(wght5= 0x%x,wght6= 0x%x,wght7= 0x%x,wght8= 0x%x,wght9= 0x%x,wght10= 0x%x)
 
2161,iIi,[ cmdProcessTlv2.c : 3853 ] COEX Req Handler(enableDynamicAggr= %d,shareChainMask= 0x%x,enableConcurrentTxChain0= %d)
 
2160,iIii,[ cmdProcessTlv2.c : 3860 ] COEX Req Handler(btRxAllowWlanTxUnshared= %d,btTxAllowWlanTxShared= 0x%x,wlanTxAllowBtRxShared= %d,wlanRxAllowBtTxShared= %d)
 
2159,iIi,[ cmdProcessTlv2.c : 3866 ] COEX Req Handler(concurrentTxEnable= %d,btRxAllowWlanUnsharedTx= 0x%x,wlan1sTxBtTx= %d)
 
2158,ii,[ cmdProcessTlv2.c : 2336 ] combCalGroupHandler(): phyId = %d; cmdid = %d 
2157,IIII,[ cmdProcessTlv2.c : 4750 ] %s: offset %ld, size %ld, totalsize %ld 
2156,III,[ cmdProcessTlv2.c : 4819 ] %s: offset %ld, size %ld 
2155,,[ cmdProcessTlv2.c : 187 ] ftm_termperature_timer_handler::MAC sleeping 
2154,,[ cmdProcessTlv2.c : 1772 ] Failed Rx Stop 
2153,,[ cmdProcessTlv2.c : 1783 ] ### genericUtfCmdHandler: InValid CmdID#### 
2152,i,[ cmdProcessTlv2.c : 482 ]  FATAL ERROR!! Trying to access phy %d which is not present 
2151,i,[ cmdProcessTlv2.c : 493 ]  FATAL ERROR!! Trying to access phy %d which is inactive 
2150,I,[ cmdProcessTlv2.c : 4379 ] modifyBDFOTPFlagsHandler: modifyBdfOtpFlags 0x%x 
2149,,[ cmdProcessTlv2.c : 4397 ] modifyBDFOTPFlagsHandler: pCmdStream is NULL 
2148,,[ cmdProcessTlv2.c : 3757 ] OFDMA TonePlan
 
2147,ii,[ cmdProcessTlv2.c : 896 ] A: pktgen_complete_timer_handler: Pktgen Tx STOP completion callback failure for phyId %d g_pktgen_done_assert_count %d 
2146,iiiiiii,[ cmdProcessTlv2.c : 1149 ] rxHandler: phyId %d rxMode %d wlanMode %d freq %d freq2 %d chainMask %d wifiStandard %d 
2145,ii,[ cmdProcessTlv2.c : 1155 ] rxHandler: issue ftm_imps_wakeup: phyId=%d, rxMode=%d
 
2144,i,[ cmdProcessTlv2.c : 1163 ] RX operation not allowed on phyID %d one operation ongoing 
2143,,[ cmdProcessTlv2.c : 4416 ] #### per chain forced pwr TLV called!
 
2142,iI,[ cmdProcessTlv2.c : 2755 ] setPhyRfModeHandler: DBS/SBS is not supported, phyRfMode %d status 0x%x  
2141,I,[ cmdProcessTlv2.c : 1307 ] pdev %u 
2140,iiiiiII,[ cmdProcessTlv2.c : 1322 ] curChan->band_center_freq1 %d, curChan->band_center_freq2 %d, PHYRF_BW_IDX(curChan) %d curChan->phy_mode %d num_20_bw %d rx_CM %x, tx_CM %x 
2139,ii,[ cmdProcessTlv2.c : 1390 ] pilot_evm pilot_evm_dB_mean[%d] = %d 
2138,iiii,[ cmdProcessTlv2.c : 3532 ] Tx Gain Control:Chain %d, Gain %d, dacGain %d, forceCal %d 
 
2137,iiiiiii,[ cmdProcessTlv2.c : 614 ] txHandler: phyId %d txMode %d freq %d freq2 %d wlanMode %d chainMask %d wifiStandard %d 
2136,i,[ cmdProcessTlv2.c : 665 ] TX operation not allowed on phyID %d one operation ongoing 
2135,ii,[ cmdProcessTlv2.c : 638 ] txHandler: issue ftm_imps_wakeup: phyId=%d, txMode=%d 
 
2134,iI,[ cmdProcessTlv2.c : 943 ] A: INSIDE txStatusHandler phyId [%d] | Time : %u 
2133,IIII,[ cmdProcessTlv2.c : 990 ] txStatusHandler ret:0x%x, ret1:0x%x, ret2:0x%x, ret3:0x%x 
2190,i,[ getTgtPwr.c : 311 ] OFDMA_ru_size: %d invalid 
2219,I,[ tcmd.c : 5029 ] Invalid pdev %lu 
2218,ii,[ tcmd.c : 4274 ] ftm_txoff_dur_calc: txtime = %d->%d 
2217,,[ tcmd.c : 1228 ] A: NEW COMMAND ISSUED 
2216,iiiiI,[ tcmd.c : 2386 ] [UL-OFDMA]ruIdx=%d, dataRate=%d, NSS=%d, pktSz=%d, miscFlags=0x%x 
2215,iiiii,[ tcmd.c : 2408 ] [UL-OFDMA] ru_start_pos=%d, ru_end_pos=%d, ru_size=%d, max_length=%d, pkt_len=%d 
2214,,[ tcmd.c : 4373 ] Could not find valid ruIdx in tone plan 
2213,i,[ tcmd.c : 3567 ] tcmd_cont_rx_begin: phyId=%d, chain mask 0
 
2212,i,[ tcmd.c : 3606 ] tcmd_cont_rx_begin: phyId=%d, tcmd_setup_channel failure
 
2211,Ii,[ tcmd.c : 3163 ] tcmd_cont_rx_cmd - flags 0x%x; act %d 
2210,ii,[ tcmd.c : 3171 ] aId[%d] = %d 
2209,,[ tcmd.c : 3177 ] Could not find valid aID in tone plan 
2208,ii,[ tcmd.c : 3433 ] pilot_evm g_ftmrxstats[phyId].pilotEvmDbMean[%d] = %d 
2207,iii,[ tcmd.c : 2650 ] TPC force glutindex: chain%d: gainindex%d: dacgain=%d
 
2206,iii,[ tcmd.c : 2677 ] PAPRD TCMD: Chain %d Glut Idx %d Gain Idx %d
 
2205,iiii,[ tcmd.c : 2791 ] Setup chan failed: freq %d, freq2 %d, wlanMd %d, bw %d
 
2204,i,[ tcmd.c : 4135 ] Enabled SIFS bursting for Tx99 (dpd_tx_counter=%d) 
2203,i,[ tcmd.c : 1802 ] Invalid frequency %d.
 
2202,,[ tcmd.c : 1940 ] 11AC VHT20 
 
2201,i,[ tcmd.c : 2182 ] 165 MHz frequency %d 
2200,i,[ tcmd.c : 2186 ] Invalid frequency %d 
2199,i,[ tcmd.c : 2022 ] pktType Invalid %d
 
2198,Iiiii,[ tcmd.c : 2135 ] get_ch wlanMode: %lu ch: %d freq1 %d freq2 %d, fcMode %d
 
2197,iiII,[ tcmd.c : 3843 ] tcmd_setup_channel_real: phyId=%d,Failure: chan.phy_mode=%d, rx_tcmdParms.u.para.pktType=0x%x, rx_tcmdParms.miscFlags=0x%x
 
2196,II,[ tcmd.c : 3953 ] tcmd() Before GI 0x%x LTF 0x%x 
2195,II,[ tcmd.c : 3988 ] tcmd() After GI 0x%x LTF 0x%x 
2194,iI,[ tcmd.c : 1504 ] A: TCMD TX COMP CB - MADE STOP TX = 2 phyId [%d] | Time : %u 
2193,I,[ tcmd.c : 4527 ] tcmd() Before RC flag 0x%x 
2192,Iii,[ tcmd.c : 4552 ] tcmd() After RC flag 0x%x GI %d LTF %d 
2191,ii,[ tcmd.c : 4719 ] [UL-OFDMA]gi=%d, ltf=%d 
2226,,[ tcmd_rx.c : 335 ] A: RETURN if((g_ftm_frame_enacap_config[phyId].da_addr == NULL) || (g_ftm_frame_enacap_config[phyId].bss_addr == NULL)) 
2225,,[ tcmd_rx.c : 364 ] RX WAL PEER A_PANIC 
2224,ii,[ tcmd_rx.c : 383 ] A: wal_vdev_attach vdevId[%d]=%d 
2223,,[ tcmd_rx.c : 389 ] A: wal_peer_alloc rx peer 1 
2222,,[ tcmd_rx.c : 399 ] A: wal_peer_alloc rx peer 2 
2221,,[ tcmd_rx.c : 352 ] A: page fault condition, all vdev is null 
2220,,[ tcmd_rx.c : 361 ] A: Inside if(g_tcmd_wal_rx_ctxt[phyId].vdev == NULL) 
2243,ii,[ tcmd_tx.c : 1406 ] [MU] sched_algo_mu_tx_peer_assoc() peer[%d] AID %d 
2242,,[ tcmd_tx.c : 1522 ] A: INSIDE tcmd_wal_peer_free 
2241,ii,[ tcmd_tx.c : 413 ] ftm_tid_create_handler: phyId %d, tid %d 
2240,,[ tcmd_tx.c : 1547 ] A: RETURN if((g_ftm_frame_enacap_config[phyId].bss_addr == NULL) || (g_ftm_frame_enacap_config[phyId].da_addr == NULL))  
2239,,[ tcmd_tx.c : 1553 ] A: if((g_tcmd_wal_config[phyId].vdev) == NULL)  
2238,,[ tcmd_tx.c : 1556 ] A: if(((g_bss_peer[phyId]) == NULL) || (g_ftm_ctxt[phyId].peer == NULL))  
2237,,[ tcmd_tx.c : 1561 ] A: RETURN if((g_bss_track_peer != NULL) || (g_ctxt_track_peer != NULL)) 
2236,,[ tcmd_tx.c : 1166 ] A: peer_use_4cal 
2235,iiI,[ tcmd_tx.c : 1186 ] A: g_bss_peer[%d]=%d g_ftm_bss_peer[phyId]= %08x 
2234,I,[ tcmd_tx.c : 1187 ] cwc wal_peer_alloc for bss_peer %08x <= 
2233,I,[ tcmd_tx.c : 1190 ] A: ctxt->peer=0x%x 
2232,iI,[ tcmd_tx.c : 1191 ] A: g_ftm_frame_enacap_config[%d].da_addr=0x%x 
2231,iI,[ tcmd_tx.c : 1192 ] A: g_ftm_frame_enacap_config[%d].bss_addr=0x%x 
2230,Ii,[ tcmd_tx.c : 1202 ] A: wal_peer_alloc ctxt->peer[%08x] %d times  
2229,,[ tcmd_tx.c : 1205 ] A: wal_peer_alloc peer_use_4cal ctxt->peer  
2228,iiI,[ tcmd_tx.c : 1169 ] A: g_bss_peer[%d]=%d g_ftm_bss_peer[phyId]= %08x 
2227,,[ tcmd_tx.c : 1176 ] A: peer_use_4cal wal_peer_alloc bss_peer 
2251,ii,[ ftm_lowpower.c : 125 ] ftm_bmps_timer_handler: phyId=%d, isTx=%d, BMPS sleep timeout and wakeup
 
2250,i,[ ftm_lowpower.c : 133 ] ftm_bmps_timer_handler: phyId=%d, BMPS wakeup done
 
2249,i,[ ftm_lowpower.c : 115 ] ftm_imps_sleep: phyId:%d, issue wal_pm_ftm_set_power_state sleep 
 
2248,i,[ ftm_lowpower.c : 99 ] ftm_imps_wakeup: phyId=%d, wakeup from IMPS 
 
2247,i,[ ftm_lowpower.c : 102 ] ftm_imps_wakeup: phyId=%d, wakeup from IMPS, done 
 
2246,II,[ ftm_lowpower.c : 238 ] ftm_ocl_tx_done: phyId:0x%x, ocl_flag=0x%x 
2245,II,[ ftm_lowpower.c : 220 ] ftm_ocl_tx_start: phyId:0x%x, ocl_enable=0x%x 
2244,ii,[ ftm_lowpower.c : 152 ] ftm_tx_rx_trigger_bmps: phyId=%d, isTx=%d, BMPS sleep as g_ftm_lowPowerMode is 1
 
2268,Iiii,[ tpcOnepointCal.c : 296 ] tpcOnepointCal::Starting Tx for phy %u, freq %d, chainMask %d, txPwr_db2 %d 
2267,Iiii,[ tpcOnepointCal.c : 299 ] tpcOnepointCal::Stopping Tx for phy %u, freq %d, chainMask %d, txPwr_db2 %d 
2266,iii,[ tpcOnepointCal.c : 529 ] tpcOnepointCal::Failure at BandIdx:%d chanIdx:%d chainIdx:%d 
2265,,[ tpcOnepointCal.c : 539 ] tpcOnepointCal:: end loop 1 
2264,,[ tpcOnepointCal.c : 549 ] tpcOnepointCal:: break 
2263,,[ tpcOnepointCal.c : 595 ] tpcOnepointCal:: end loop 
2262,i,[ tpcOnepointCal.c : 136 ] tpccal chan::2g %d 
2261,i,[ tpcOnepointCal.c : 142 ] tpccal chan::5g %d 
2260,ii,[ tpcOnepointCal.c : 170 ] tpcOnepointCal::TPC_DBG 5G numChain %d 2G numChain %d 
2259,ii,[ tpcOnepointCal.c : 613 ] tpcOnepointCal::TPC_DBG band %d idxChan %d 
2258,IIII,[ tpcOnepointCal.c : 431 ] tpcOnepointCal::Requesting pwr measurement for phy %u, freq %u, chainMask %u,tgtPwr_db8 %u 
2257,IIII,[ tpcOnepointCal.c : 445 ] tpcOnepointCal::Requesting pwr measurement for phy %u, freq %u, chainMask %u,tgtPwr_db8 %u 
2256,,[ tpcOnepointCal.c : 668 ] tpcOnepointcal::Completed 
2255,,[ tpcOnepointCal.c : 322 ] tpcOnepointCAL::Starting... 
2254,,[ tpcOnepointCal.c : 709 ] tpcOnepointcal::Failure, -999 power detected 
2253,IIIiiI,[ tpcOnepointCal.c : 731 ] tpcOnepointCal::Pwr measurement for phy %u, freq %u, chainMask %u, glutOffset %d, thermOffset %d, measPwr_db8 is %u 
2252,,[ tpcOnepointCal.c : 102 ] tpcOnepointCal::tpcPowerMeasurementDelayTimeout 
2270,ii,[ xtalCal.c : 256 ] [TLV2_CTRL_W_OTP]capIn=%d, capOut=%d 
2269,ii,[ xtalCal.c : 260 ] [ERROR][TLV2_CTRL_W_OTP]OTP has data %d, %d 
2366,iii,[ tpcCal.c : 606 ] chk1 Max_TX_CAL_Gain_ID_5G:%d Max_TX_CAL_Gain_ID_2G %d Max_TX_CAL_Gain_ID_6G %d 
2365,Ii,[ tpcCal.c : 780 ] greenTxGainIndGrpFlag2G:%x, greenTxGainIndGrpFlag5G:%d 
 
2364,iiii,[ tpcCal.c : 865 ]  5G IdxGainEndGrp1:%d IdxGainEndGrp2:%d IdxGainEndGrp3:%d IdxGainEndGrp4:%d
 
2363,IIII,[ tpcCal.c : 680 ] tpccal::2G opcChan[%u] %u, tpcChan[%u] %u 
2362,IIII,[ tpcCal.c : 700 ] tpccal::5G opcChan[%u] %u, tpcChan[%u] %u 
2361,iiiii,[ tpcCal.c : 1230 ] freq %d gIdx %d dacGain %d paCfg %d chMask %d
 
2360,III,[ tpcCal.c : 1268 ] tpccal::Stopping tx before starting for Chan %u, Chain %u, Gain %u 
2359,,[ tpcCal.c : 2402 ] tpccal::Generating Caldata 
2358,ii,[ tpcCal.c : 2446 ] tpcCal::Generating Caldata for Channel %d dacGainforCal %d 
2357,i,[ tpcCal.c : 2450 ] tpcCal::Generating Caldata for Chain %d 
2356,iii,[ tpcCal.c : 2456 ] tpcCal::Generating Caldata for GLUT Gain Idx %d txgainIdx %d meas_pwr %d 
2355,iii,[ tpcCal.c : 2466 ] tpcCal::Generating Caldata for GLUT EXT Gain Idx %d txgainIdx %d meas_pwr %d 
2354,iii,[ tpcCal.c : 2476 ] tpcCal::Generating Caldata for PLUT Gain Idx %d pdadc_read %d meas_pwr %d 
2353,iii,[ tpcCal.c : 2505 ] tpcCal::Generating Caldata for Chain %d sbsOffset %d NUM_CAL_GAINS_SELECTED_4_GLUT:%d 
2352,iii,[ tpcCal.c : 2512 ] tpcCal::Generating Caldata for GLUT Gain Idx %d txgainIdx %d meas_pwr %d 
2351,iiii,[ tpcCal.c : 2522 ] tpcCal::Generating Caldata for GLUT EXT Gain Idx %d txgainIdx %d meas_pwr %d numGlutEntries_5G:%d 
2350,iii,[ tpcCal.c : 2532 ] tpcCal::Generating Caldata for PLUT Gain Idx %d pdadc_read %d meas_pwr %d 
2349,iii,[ tpcCal.c : 2548 ] phyId:%d cmask:%d pwrAtPdadc:%d 
2348,I,[ tpcCal.c : 2631 ] TPC2G: &scanCalPierData2G = 0x%x 
2347,I,[ tpcCal.c : 2632 ] TPC5G: &scanCalPierData5G = 0x%x 
2346,ii,[ tpcCal.c : 2640 ] TPC: chain = %d, iChanIdx = %d 
2345,iii,[ tpcCal.c : 2645 ] TPC2G: scanMeasPwr2G[%d][%d] = %d 
2344,iii,[ tpcCal.c : 2649 ] TPC5G: scanMeasPwr5G[%d][%d] = %d 
2343,III,[ tpcCal.c : 1690 ] getNextLoop fail curLoop->idxCalPt %u, Chain %u, Gain %u 
2342,iiiii,[ tpcCal.c : 1717 ] bef, band %d ch %d numCh %d chain %d gain %d
 
2341,,[ tpcCal.c : 1722 ] end loop0
 
2340,iiii,[ tpcCal.c : 1735 ] inc calPt %d ch %d chn %d, numGain %d
 
2339,ii,[ tpcCal.c : 1743 ] inc chain AI %d %d
 
2338,ii,[ tpcCal.c : 1751 ] inc ch AI %d %d
 
2337,ii,[ tpcCal.c : 1759 ] inc band AI %d %d
 
2336,,[ tpcCal.c : 1763 ] end loop
 
2335,iiii,[ tpcCal.c : 1824 ] pwr est %d band %d numEst %d, idx %d 
2334,iiiii,[ tpcCal.c : 1828 ] sG %d %d %d %d %d  
2333,i,[ tpcCal.c : 1829 ] %d
 
2332,i,[ tpcCal.c : 3171 ] available_gainIdxs:%d 
2331,iiii,[ tpcCal.c : 3177 ] Iteration m:%d glutsfilled[%d]:%d Max_Glut_Map[band][grpId]:%d 
2330,i,[ tpcCal.c : 3178 ] tpcCalResult[band][chan].measPwr[chain][m]:%d 
2329,,[ tpcCal.c : 3181 ] ERR: BAD CAL TARGETs CONFIGURED for:  
2328,i,[ tpcCal.c : 3188 ] Picked limiting gainidx:%d 
2327,i,[ tpcCal.c : 3202 ] Picked gainidx:%d  
2326,,[ tpcCal.c : 3206 ] Moving up gainidxs to guarantee GLUT count! 
2325,ii,[ tpcCal.c : 3209 ] currIndx:%d Updated endPwrIdxGrp:%d 
2324,,[ tpcCal.c : 3214 ] BAD CAL TARGETs CONFIGURED for 
2323,ii,[ tpcCal.c : 3219 ] Picked max gainidx:%d from group :%d  
2322,,[ tpcCal.c : 3222 ] Invalid pick_glut_entry condition! 
2321,,[ tpcCal.c : 1905 ] populateScanArray 
2320,ii,[ tpcCal.c : 1948 ] populateScanArray 2G: ScanGainIdx = %d, measPwr = %d 
2319,iiii,[ tpcCal.c : 1951 ] populateScanArray 5G: iBand = %d, scanMeasPwr5G[%d][%d] = %d 
2318,iiiii,[ tpcCal.c : 1952 ] populateScanArray 5G: tpcCalResult[%d][%d].measPwr[%d][%d] = %d 
2317,,[ tpcCal.c : 2071 ] tpccal::Post processing CLPC Caldata 
2316,ii,[ tpcCal.c : 2117 ] tpccal::skip gainIdx %d (< thresh %d) 
2315,,[ tpcCal.c : 2178 ] tpccal::Post processing CLPC Caldata 
2314,ii,[ tpcCal.c : 2237 ] tpccal::skip gainIdx %d (< thresh %d) 
2313,,[ tpcCal.c : 1966 ] tpccal::Post processing OLPC Caldata 
2312,,[ tpcCal.c : 1974 ] pp OLPC
 
2311,iiiii,[ tpcCal.c : 1997 ] meaPwr %d tgtPwr %d, bn %d ch %d chn %d, 
 
2310,i,[ tpcCal.c : 1998 ] numValidMeas = %d
 
2309,iiii,[ tpcCal.c : 2005 ] bkof %d bn %d ch %d chn %d
 
2308,iiii,[ tpcCal.c : 2016 ] stPwrIdx %d bn %d ch %d chn %d
 
2307,iiiiiiii,[ tpcCal.c : 2041 ] iMeas %d iGainIdx %d tgt %d ch %d chn %d sel pwr %d gIdx %d dac %d
 
2306,,[ tpcCal.c : 3241 ] postProcessingOLPCCALData_gtx 
2305,iiii,[ tpcCal.c : 3272 ] BegiN: Band:%d chan:%d startPwrIdxGrp:%d  endPwrIdxGrp:%d  
2304,ii,[ tpcCal.c : 3273 ] gtx tgtpwridx:%d , GlutPwrMapGrpNum:%d  
2303,iii,[ tpcCal.c : 3280 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d modifiedTarget:%d 
2302,i,[ tpcCal.c : 3282 ] endPwrIdxGrp:%d 
2301,iii,[ tpcCal.c : 3288 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d modifiedTarget:%d 
2300,i,[ tpcCal.c : 3290 ] endPwrIdxGrp:%d 
2299,iiii,[ tpcCal.c : 3297 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d tpcCfg[band].IdxGainEndGrp3:%d modifiedTarget:%d 
2298,i,[ tpcCal.c : 3299 ] endPwrIdxGrp:%d 
2297,iiii,[ tpcCal.c : 3305 ] gtx startPwrIdxGrp:%d , endPwrIdxGrp:%d tpcCfg[band].IdxGainEndGrp4:%d modifiedTarget:%d 
2296,i,[ tpcCal.c : 3307 ] endPwrIdxGrp:%d 
2295,iii,[ tpcCal.c : 3311 ] gtx Invalid TPC_GLUT_PWR_MAP_GRP Id ! from Band:%d Chain:%d tgtpwridx:%d 
2294,ii,[ tpcCal.c : 1052 ] Sending to host freq2G %d, freq5G %d
 
2293,iii,[ tpcCal.c : 1593 ] Sending to host freq2G %d, freq5G %d, chain %d 
2292,iiii,[ tpcCal.c : 1594 ] gain %d pwr %d numChain %d numCalpt %d
 
2291,IIII,[ tpcCal.c : 1598 ] tpccal::Sending to host to look for measurements inChan2G %u, Chan5G %u, ChainMask(User) %u, Gain %u 
2290,iii,[ tpcCal.c : 1600 ] Sending to host freq2G %d, freq5G %d, chain %d
 
2289,iiii,[ tpcCal.c : 1601 ] gain %d pwr %d numChain %d numCalpt %d
 
2288,,[ tpcCal.c : 2353 ] tpccal::Sending Caldata to host 
2287,,[ tpcCal.c : 1337 ] tpccal::Starting ... 
2286,,[ tpcCal.c : 1434 ] TPC Cal message check 
 
2285,ii,[ tpcCal.c : 1476 ] tpcCALScheme: %d, phyID %d
 
2284,,[ tpcCal.c : 1870 ] tpccal::Completed 
2283,,[ tpcCal.c : 1884 ] tpcCalCompleteCallback() 
2282,iIIII,[ tpcCal.c : 2834 ] tpccal::Got measurement %d from host for Chan %u Chain %u Chain(user) %u Gain %u 
2281,iIIIII,[ tpcCal.c : 2854 ] tpccal::Thermoffset %d for Band %u tpcChan %u opcChan[%u] %u  Chain %u 
2280,iiii,[ tpcCal.c : 2870 ] Got Power from host Chan %d ,  GainIdx %d , MeasPwr  %d , Read pdadc %d  
2279,ii,[ tpcCal.c : 2923 ] Received identical power meas:%d prevMeas:%d .Failing calloop 
2278,iii,[ tpcCal.c : 2952 ] Get 10Log(pdadc) prev:%d curr:%d slope:%d 
2277,ii,[ tpcCal.c : 2955 ] Get Power meas:%d prevMeas:%d 
2276,iiii,[ tpcCal.c : 2956 ]  calFail:%d, gainIdx:%d, idxCalPt:%d skipSlope_gtx_bndry:%d 
2275,i,[ tpcCal.c : 2960 ] skipping slope for gainIdx = %d 
2274,III,[ tpcCal.c : 1855 ] tpccal::Starting tx for Chan %u, Chain %u, Gain %u 
2273,iiiii,[ tpcCal.c : 3138 ] Write to tpcCalPostProcResult[%d][%d].olpc.measPwrExt[%d][%d]:%d 
2272,iiiii,[ tpcCal.c : 3145 ] Write to tpcCalPostProcResult[%d][%d].olpc.measPwr[%d][%d]:%d 
2271,ii,[ tpcCal.c : 3155 ] glutsfilled[%d]:%d 
2375,iiiiii,[ rxGainCal.c : 130 ] rxGainCal:: Starting Rx on phyId %d, is2Ghz %d, Chain %d Chan %d, rxMode %d refISS Level %d 
2374,i,[ rxGainCal.c : 205 ] rxGainCal:: Error on chainIdx %d
 
2373,i,[ rxGainCal.c : 215 ] rxGainCal:: Error on chainIdx %d
 
2372,i,[ rxGainCal.c : 228 ] rxGainCal:: Error on chainIdx status %d
 
2371,ii,[ rxGainCal.c : 271 ] rxGainCal:: Host error: phyId %d,  veryFirstRxGainCal %d 
2370,iiiiii,[ rxGainCal.c : 284 ] rxGainCal:: Host error: phyId %d, chainIdx %d, ChanIdx %d, Expected Pkt Cnt %d, Actual Pkt Cnt %d,  rxGainCalState.status %d 
2369,iiiiiii,[ rxGainCal.c : 318 ] rxGainCal:: Saving Results for phyId %d, chainIdx %d, ChanIdx %d, PNFdBr %d, PNFdBm %d, Expected Pkt Cnt %d, Actual Pkt Cnt %d 
2368,iiiiii,[ rxGainCal.c : 324 ] rxGainCal:: Saving Results for phyId %d, chainIdx %d, ChanIdx %d, Expected Pkt Cnt %d, Actual Pkt Cnt %d totalPkt=%d 
2367,,[ rxGainCal.c : 333 ] nextLoopRxCal is NULL 
2376,ii,[ wmi_ftm_attach.c : 224 ] ERROR: ftm_parse_unifiedcmd: dataLen %d is LESS than sizeof(segHdrInfo) %d 
2377,iIIII,[ data_rx.c : 662 ] DATA_TXRX_DBGID_DUP_CHECK vdev_id = %d tcp_info=0x%x SN=0x%x last_pn_valid=0x%x offset_winsize=0x%x 
2379,III,[ data_rx_pn.c : 151 ] DATA_TXRX_DBGID_REPLAY_CHECK_WAR KeyId=0x%x oldPN=0x%llx newPN=0x%llx 
2378,IIII,[ data_rx_pn.c : 194 ] DATA_TXRX_DBGID_REPLAY_CHECK 0x%x KeyId=0x%x oldPN=0x%x newPN=0x%x 
2387,IIIIII,[ blockack.c : 1020 ] peer:%x, %x, op:%x, caller:%x %x %x 
2386,ii,[ blockack.c : 412 ] ADDBA Req dropped WEP:%d MFP_SUPPORT:%d 
2385,ii,[ blockack.c : 204 ] wal_ba_event_peer_rx: amsdusupported=%d, buffersize=%d 
2384,ii,[ blockack.c : 1680 ] wal_ba_rx_sm: their_buf_size:%d, our_buf_size:%d 
2383,ii,[ blockack.c : 2065 ] wal_ba_send_addba_rsp: amsdusupported=%d, buffersize=%d 
2382,,[ blockack.c : 2539 ] BA-Link-Monitor implementation Start 
2381,i,[ blockack.c : 1137 ] Error: ba_handle is NULL for wal_peer_id = %d 
2380,iI,[ blockack.c : 1196 ] TX_BA_LOG: ADDBA request pending in frameQ: tid=%d bmap=0x%x 
2395,iiii,[ htt_tgt_rx.c : 225 ] htt_fisa_config:[%d] [%d] [%d]  RT: [%d]
 
2394,iiiIIi,[ htt_tgt_rx.c : 333 ] htt_tgt_fse_setup:[%d] [%d] [%d] [0x%lx] [0x%lx] RT: [%d]
 
2393,iiiii,[ htt_tgt_rx.c : 396 ] htt_tgt_fse_operation pdev,ipsec,src/dest ports,proto:[%d][%d] [%d][%d] [%d]
 
2392,IIIIIIII,[ htt_tgt_rx.c : 406 ] IP src [%x][%x][%x][%x] dest [%x][%x][%x][%x]
 
2391,II,[ htt_tgt_rx.c : 483 ] 3-tuple Configuration value rcvd : 
 flow_id_toeplitz_enable : [%x]
 toeplitz_2_or_4_field_enable : [%x]
 
2390,IIIIIII,[ htt_tgt_rx.c : 751 ] ring_selection_cfg [%x] [%x] [%x] [%x] [%x] [%x] [%x]
 
2389,iiiiii,[ htt_tgt_rx.c : 60 ] htt_tgt_sring_setup [%d] [%d] [%d] [%d] [%d] [%d]
 
2388,i,[ htt_tgt_rx.c : 640 ] htt_tgt_sring_setup_done -[%d]
 
2396,III,[ htt_tgt_rx_event.c : 332 ] RX event msg buf_len type[%x] peer_id [%x] vdev_id [%x]
 
2404,III,[ offloadif_data_hdlr.c : 297 ] buffer_addr_39_32 %x, buffer_addr_31_0 %x, sw_buffer_cookie %x 
2403,iiiI,[ offloadif_data_hdlr.c : 582 ] OFLDIF local data hdlr vdev_id=%d, peer_id=%d, tid=%d, flags=%x 
2402,iii,[ offloadif_data_hdlr.c : 635 ] OFLDIF local data hdlr len=%d, status=%d pad_size=%d 
2401,ii,[ offloadif_data_hdlr.c : 602 ] OFLDIF local data hdlr local_data_flags=%d, status=%d 
2400,ii,[ offloadif_data_hdlr.c : 381 ] OFLD data flush pdev id=%d cnt=%d 
2399,ii,[ offloadif_data_hdlr.c : 188 ] OFLD data store pdev id=%d cnt=%d 
2398,,[ offloadif_data_hdlr.c : 194 ] OFLD data store err- No memory 
2397,iii,[ offloadif_data_hdlr.c : 883 ] OFLDIF remote data hdlr vdev_id=%d, len=%d, status=%d 
2408,I,[ offloadif_wow_hdlr.c : 77 ] WOW error tx pending %x 
2407,,[ offloadif_wow_hdlr.c : 262 ] WOW error RXDMA2REO not empty 
2406,,[ offloadif_wow_hdlr.c : 89 ] WOW error DPD calibration is going on 
2405,,[ offloadif_wow_hdlr.c : 100 ] WOW error tx REO not idle 
2416,i,[ offloadif_cce.c : 89 ] CCE datapath routing: non STA mode not allowed,  mode=%d 
 
2415,i,[ offloadif_cce.c : 126 ] CCE datapath routing: invalid route_type=%d 
 
2414,i,[ offloadif_cce.c : 144 ] CCE datapath routing: default UC rules not allowed filter id=%d 
 
2413,i,[ offloadif_cce.c : 249 ] CCE datapath routing: invalid proto_type=%d 
 
2412,,[ offloadif_cce.c : 98 ] CCE datapath routing: Proto_type_all not supported for pdev rule 
 
2411,i,[ offloadif_cce.c : 110 ] CCE datapath routing: invalid addr_type=%d 
 
2410,I,[ offloadif_cce.c : 314 ] %s: invalid addr_type 
 
2409,,[ offloadif_cce.c : 339 ] CCE route cfg msg in RT 
2418,III,[ mac_core_main.c : 225 ] assert:r0=0x%x, r1=0x%x, line:0x%x
 
2417,I,[ mac_core_main.c : 147 ] mac_core_work_loop_init: invalid wlan_driver_mode 0x%x 
2430,iii,[ pktgen.c : 197 ] pktgen_calc_aggr_size: adjust pkt len: orig=%d adjust=%d mpdu=%d 
2429,iii,[ pktgen.c : 1676 ] pktgen_tx_msg_handler msg hdlr: pkt len = %d pdev_id = %d mode = %d
 
2428,I,[ pktgen.c : 1636 ] pktgen_data_tx_start_msg_send  dev->running=0x%x 
2427,,[ pktgen.c : 1859 ] pktgen_data_tx_stop_msg_send
 
2426,I,[ pktgen.c : 876 ] %s: Unable to get tcl entry 
 
2425,I,[ pktgen.c : 1179 ] 0x%X  
2424,I,[ pktgen.c : 894 ] %s: Unable to get tcl entry 
 
2423,II,[ pktgen.c : 1170 ] %s: we're dead - %u is in use now
Bitmap  
2422,I,[ pktgen.c : 769 ] Tx done MAC id %lu
 
2421,II,[ pktgen.c : 1312 ] %s: we're dead - try to free cookie %lu notused
Bitmap: 
2420,I,[ pktgen.c : 1321 ] 0x%x  
2419,,[ pktgen.c : 1324 ] 
 
2434,IiIIII,[ wal_channel_change_hw.c : 430 ] WAL_DBGID_CHANNEL_CHANGE_FORCE_RESET: mhz = %04d mac_id = %d phy_mode = %02d flags = 0x%04x rx_stop|tx_stop = 0x%x pf_cnt = %02d 
2433,IiIII,[ wal_channel_change_hw.c : 439 ] WAL_DBGID_CHANNEL_CHANGE: mhz = %04d mac_id = %d phy_mode = %02d flags = 0x%04x pf_cnt = %02d 
2432,iiii,[ wal_channel_change_hw.c : 622 ] wal_channel_change: DPD_AbortSpectral = %d AbortTxRx = %d WhalChanSwitch_TxRxResume = %d DPD_ResumeSpectral = %d 
2431,iiii,[ wal_channel_change_hw.c : 656 ] GreenAP wal_set_greenap_channel error tx/rx chainmask: %d/%d, phy_mode: %d, flag: %d 
2451,ii,[ ar_wal_tx_de.c : 2813 ] security: sw_peer_id=%d WAL_DBGID_TX_EAPOL_PKT type=%d 
2450,iiiiI,[ ar_wal_tx_de.c : 2910 ] security: sw_peer_id=%d WAL_DBGID_TX_EAPOL_PKT M%d or G%d key_type:%d key_val:0x%02x 
2449,,[ ar_wal_tx_de.c : 1832 ] DE classify: invalid bcast mcast 
2448,ii,[ ar_wal_tx_de.c : 2001 ] DE enq: DHCP|actual_tid_num = %d %d 
2447,i,[ ar_wal_tx_de.c : 2454 ] Drop frame: qos_to_nonqos_switch in progress, peer_id:%d 
2446,iiii,[ ar_wal_tx_de.c : 2488 ] tx_de classify: drop due to qos tid req in non_qos state, tid %d qpeer %d peer %d counter %d 
2445,,[ ar_wal_tx_de.c : 2533 ] WAL_DBGID_TX_EAPOL_PKT peer is disassoced 
2444,,[ ar_wal_tx_de.c : 2545 ] WAL_DBGID_TX_EAPOL_PKT qpeer is not valid 
2443,ii,[ ar_wal_tx_de.c : 1965 ] DE enq: ARP req|actual_tid_num = %d %d 
2442,iiIiIiI,[ ar_wal_tx_de.c : 1664 ] DE enq: sw_peer_id=%d tid=%d fc=0x%x type=%d msdu_flags=0x%x len=%d id=0x%x 
2441,iii,[ ar_wal_tx_de.c : 495 ] qos_to_nonqos_switch: Received tcl dummy frame compl peer_id:%d status:%d buffer_id:%d 
2440,,[ ar_wal_tx_de.c : 509 ] qos_to_nonqos_switch: Received tqm dummy frame compl in wbm2fw release ring 
2439,iii,[ ar_wal_tx_de.c : 122 ] tx_de: ipa stats offset %d line %d total:%d 
2438,IiIiii,[ ar_wal_tx_de.c : 3049 ] DE wbm2fw: cookie=0x%x sw_peer_id=%d flags=0x%x msdu_len=%d rel_md=%d,rel_reason=%d 
2437,,[ ar_wal_tx_de.c : 3171 ] invalid_msdu - about to free to FW 
2436,,[ ar_wal_tx_de.c : 3176 ] invalid_msdu - about to free to host 
2435,IIII,[ ar_wal_tx_de.c : 3687 ] restore SN: tid=%x, mpdu_last_seq_num=%X, frameq=%p %x 
2492,IIIIIIII,[ wal_phy_dev_hw.c : 8655 ] dynamic_cca_algo: pdev_id=%u, tx= %u, my_rx=%u, rx=%u, pre_rx=%u, cycle_cnt=%u,cca_busy=%u, rx_frame_det_accuracy=%u 
2491,IIIiIii,[ wal_phy_dev_hw.c : 8659 ] dynamic_cca_algo: num_gi_corr_toggle=%u, num_pre_rx_toggle=%u, a_ms=%u, durxrssi=%d, dur=%u, rssi=%d, ed_cca_thr_p20=%d 
2490,iii,[ wal_phy_dev_hw.c : 8766 ] Force RTS:vdev %d channel_util %d cca_busy %d 
2489,iII,[ wal_phy_dev_hw.c : 6832 ] RXPCU WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2488,iII,[ wal_phy_dev_hw.c : 6884 ] TXDMA WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2487,iII,[ wal_phy_dev_hw.c : 6942 ] RXOLE WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2486,iII,[ wal_phy_dev_hw.c : 6959 ] TXOLE WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2485,iII,[ wal_phy_dev_hw.c : 6972 ] CRYPTO WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2484,iII,[ wal_phy_dev_hw.c : 6991 ] RXDMA WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2483,iII,[ wal_phy_dev_hw.c : 7008 ] PDG WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2482,iII,[ wal_phy_dev_hw.c : 7030 ] HWSCH WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2481,iII,[ wal_phy_dev_hw.c : 7110 ] MXI WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2480,iII,[ wal_phy_dev_hw.c : 7120 ] AMPI WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2479,iIII,[ wal_phy_dev_hw.c : 6859 ] TXPCU WDOG error interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x, PhyErr 0x%x 
2478,iII,[ wal_phy_dev_hw.c : 7217 ] CRYPTO panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2477,iII,[ wal_phy_dev_hw.c : 7815 ] SFM panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2476,iII,[ wal_phy_dev_hw.c : 7859 ] RXDMA_SRC_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2475,iII,[ wal_phy_dev_hw.c : 7870 ] RXDMA_DST_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2474,iII,[ wal_phy_dev_hw.c : 7894 ] RXDMA1_DST_RNG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2473,iII,[ wal_phy_dev_hw.c : 7905 ] MCMN panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2472,iII,[ wal_phy_dev_hw.c : 7268 ] TXPCU0 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2471,iII,[ wal_phy_dev_hw.c : 7407 ] TXDMA panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2470,iII,[ wal_phy_dev_hw.c : 7506 ] RXDMA panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2469,iII,[ wal_phy_dev_hw.c : 7516 ] RXPCU0 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2468,iII,[ wal_phy_dev_hw.c : 7526 ] RXPCU1 panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2467,iII,[ wal_phy_dev_hw.c : 7536 ] PDG panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2466,i,[ wal_phy_dev_hw.c : 7573 ] PDG WDOG due to flush %d 
2465,i,[ wal_phy_dev_hw.c : 7579 ] PDG WDOG due to flush while receiving ofdma_trigger_details %d 
2464,iII,[ wal_phy_dev_hw.c : 7651 ] HWSCH panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2463,iII,[ wal_phy_dev_hw.c : 7666 ] MXI panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2462,iII,[ wal_phy_dev_hw.c : 7721 ] AMPI panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2461,iII,[ wal_phy_dev_hw.c : 7732 ] TXOLE panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2460,iII,[ wal_phy_dev_hw.c : 7804 ] RXOLE panic interrupt on PDEV ID-%d, mask 0x%x, total count 0x%x
 
2459,iIIIIII,[ wal_phy_dev_hw.c : 8523 ] ucode_stats(%d):rx 11a=%08X,11b=%08X,11n=%08X,11ac=%08X,11ax=%08X,gf=%08X 
2458,iIIIIII,[ wal_phy_dev_hw.c : 8532 ] ucode_stats(%d):tx 11a=%08X,11b=%08X,11n=%08X,11ac=%08X,11ax=%08X,gf=%08X 
2457,,[ wal_phy_dev_hw.c : 2041 ] Don't reset as CHIP IS IN POWER DOWN STATE 
2456,II,[ wal_phy_dev_hw.c : 2530 ] ctrl_path_stats_dbg: mac_addr31to0 = 0x%x mac_addr47to32 = 0x%x
 
2455,I,[ wal_phy_dev_hw.c : 6688 ] PHY M3 requested WARM reset for PHY: %x 
 
2454,I,[ wal_phy_dev_hw.c : 6706 ] PHY M3 Assert for PHY: %x 
 
2453,iii,[ wal_phy_dev_hw.c : 1912 ] WAL_PDEV_RESUME_REQ req = %d, is_pdev_pause = %d pdev_state = %d  
2452,iiiiii,[ wal_phy_dev_hw.c : 1824 ] WAL_PDEV_SUSPEND_REQ req = %d, reason %d, is_pdev_pause = %d, force_sync = %d, resume_inline = %d pdev_state = %d  
2514,II,[ wal_soc_dev_hw.c : 527 ] TCL0 panic interrupt mask : 0x%x, total count 0x%x
 
2513,II,[ wal_soc_dev_hw.c : 538 ] TCL1 panic interrupt mask : 0x%x, total count 0x%x
 
2512,II,[ wal_soc_dev_hw.c : 648 ] TQM0 panic interrupt mask : 0x%x, total count 0x%x
 
2511,II,[ wal_soc_dev_hw.c : 745 ] TQM2 panic interrupt mask : 0x%x, total count 0x%x
 
2510,II,[ wal_soc_dev_hw.c : 681 ] TQM1 panic interrupt mask : 0x%x, total count 0x%x
 
2509,II,[ wal_soc_dev_hw.c : 869 ] APB panic interrupt mask : 0x%x, total count 0x%x
 
2508,II,[ wal_soc_dev_hw.c : 878 ] MEM panic interrupt mask : 0x%x, total count 0x%x
 
2507,II,[ wal_soc_dev_hw.c : 887 ] WBM0 panic interrupt mask : 0x%x, total count 0x%x
 
2506,i,[ wal_soc_dev_hw.c : 927 ] WBM0 WDOG crash ignored %d 
2505,II,[ wal_soc_dev_hw.c : 947 ] WBM1 panic interrupt mask : 0x%x, total count 0x%x
 
2504,II,[ wal_soc_dev_hw.c : 963 ] WBM2 panic interrupt mask : 0x%x, total count 0x%x
 
2503,II,[ wal_soc_dev_hw.c : 976 ] RE0 panic interrupt mask : 0x%x, total count 0x%x
 
2502,II,[ wal_soc_dev_hw.c : 985 ] REO1 panic interrupt mask : 0x%x, total count 0x%x
 
2501,II,[ wal_soc_dev_hw.c : 994 ] REO2 panic interrupt mask : 0x%x, total count 0x%x
 
2500,II,[ wal_soc_dev_hw.c : 1003 ] REO3 panic interrupt mask : 0x%x, total count 0x%x
 
2499,I,[ wal_soc_dev_hw.c : 1010 ] SM_IX_2 value:%x 
2498,II,[ wal_soc_dev_hw.c : 1035 ] REO4 panic interrupt mask : 0x%x, total count 0x%x
 
2497,II,[ wal_soc_dev_hw.c : 1044 ] GXI panic interrupt mask : 0x%x, total count 0x%x
 
2496,iII,[ wal_soc_dev_hw.c : 1369 ] Enter/Exit  WoW mode :%d,timestamp:%x, reo2sw1:0x%x 
2495,,[ wal_soc_dev_hw.c : 1415 ] Entering into WoW mode is done 
2494,,[ wal_soc_dev_hw.c : 1440 ] Exiting from WoW mode is done 
2493,I,[ wal_soc_dev_hw.c : 1571 ] in wow mode skip evt_id 0x%x 
2515,iIiiii,[ ar_wal_vdev_hw.c : 414 ] VDEV migration sync: ba_migrate, thread_id=%d, peer=%p, vdev_id=%d, vdev_type=%d, pdev_id=%d:%d 
2528,,[ wal_soc_debug.c : 1537 ] TXRX events in WoW --------------- 
2527,IIIIIIII,[ wal_soc_debug.c : 1558 ] %u,ts:%x,TX,cmd_res:%x,seq:%x,peer:%x,tid:%x,hwqid:%x,fc:%x 
2526,IIII,[ wal_soc_debug.c : 1565 ] %u,ts:%x,RXBCN,seq:%x,num_bcn_rcv:%x 
2525,IIIII,[ wal_soc_debug.c : 1573 ] %u,ts:%x,RX,fc:%x,seq:%x,num_mpdu:%x 
2524,IIIII,[ wal_soc_debug.c : 1581 ] %u,ts:%x,OFLD,eth:%x,proto:%x,addr:%x 
2523,IIIII,[ wal_soc_debug.c : 1589 ] %u,ts:%x,HTT,hw_flags:%x,flags:%x,status:%x 
2522,iiii,[ wal_soc_debug.c : 490 ] wal_unit_test: num_args = %d test_cmd = %d arg[1] = %d arg[2] = %d  
2521,,[ wal_soc_debug.c : 968 ] Recorded page fault count reset to 0 
2520,i,[ wal_soc_debug.c : 970 ] Total page fault count: %d 
2519,i,[ wal_soc_debug.c : 974 ] Recorded page fault count: %d 
2518,i,[ wal_soc_debug.c : 976 ] Total page fault count: %d 
2517,I,[ wal_soc_debug.c : 837 ] page fault in wow: 0x%x 
2516,i,[ wal_soc_debug.c : 967 ] Recorded page fault count: %d 
2529,Ii,[ direct_dma_config.c : 212 ] dma_prepare %p status %d 
2535,IIIIIIII,[ host_ring_reader.c : 348 ] host ring reader %p has base address 0x%08x%08x, %u elements, tail address 0x%08x%08x, head address 0x%08x%08x 
2534,IIIIII,[ host_ring_reader.c : 162 ] host_ring_reader_read_elems: reader %p head_idx %u tail_idx %u shadow_tail_idx %u num_avail %u num_free %u 
2533,III,[ host_ring_reader.c : 183 ] tail dirty host ring reader %p head index is %u, shadow tail index is %u 
2532,II,[ host_ring_reader.c : 81 ] host_ring_reader_read_elems_compl: host ring reader %p read %u elements 
2531,I,[ host_ring_reader.c : 298 ] host ring reader %p stop request 
2530,IIIi,[ host_ring_reader.c : 39 ] host ring reader %p failed to copy from address 0x%08x%08x with status %d 
2540,iiI,[ pcss_ring_feeder.c : 241 ] PHY %d ring %d has %u elements remaining 
2539,III,[ pcss_ring_feeder.c : 267 ] pcss_ring_feeder_handle_ipc : head = %u shadow_head = %u and num_elems = %u for out_ring 
2538,I,[ pcss_ring_feeder.c : 278 ] pcss_ring_feeder_handle_ipc : num elems_dmaed = %u for out_ring 
2537,iiII,[ pcss_ring_feeder.c : 382 ] PHY %d ring %d needs %u elements; have %u 
2536,iiIIIIII,[ pcss_ring_feeder.c : 499 ] pcss_ring_status_print: PHY %d ring %d event %c%u head_idx %u tail_idx %u num_avail %u num_free %u 
2568,IIiIi,[ ar_wal_local_frames.c : 2398 ] LOCAL abf completion internal,peer=%x,abf=%x,flags=%d,abf_thread=%x,cur_thread=%d 
2567,IIiIi,[ ar_wal_local_frames.c : 2405 ] LOCAL abf completion internal,peer=%x,abf=%x,flags=%d,abf_thread=%x,cur_thread=%d 
2566,IIiIiI,[ ar_wal_local_frames.c : 2296 ] LOCAL abf completion msg:peer_id=%x,abf=%x,flag=%d,abf_thread=%x,cur_thread=%d,target_thread=%x 
2565,IIIiII,[ ar_wal_local_frames.c : 2253 ] Deliver LOCAL buffer sending msg failure: tid=%x,peer=%x,abf=%x,flag=%d,target_thread=%x, is_data:%x 
2564,ii,[ ar_wal_local_frames.c : 1245 ] Local data send: use default tid, requested TID:%d, tid_alloc_status=%d 
2563,II,[ ar_wal_local_frames.c : 1447 ] Local EAPOL M4 duplicated, peer:%x, qpeer-flag=%x 
2562,iiI,[ ar_wal_local_frames.c : 1502 ] Local data send: use tqm-tid %d, num:%d, flags:0x%x 
2561,iiIII,[ ar_wal_local_frames.c : 1558 ] local_data_frame_send  vdev_id=%d mac_id=%d seq_num=0x%x type=0x%x status =0x%x 
2560,I,[ ar_wal_local_frames.c : 180 ] MGMT_TX_WMI_FROM_HOST TX COMP: flags = 0x%x 
2559,iI,[ ar_wal_local_frames.c : 337 ] WAL_DBGID_TX_MGMT_COMP_DESCID_STATUS vdev_id=%d  tx_status=0x%x 
2558,IIIiii,[ ar_wal_local_frames.c : 389 ] local_frame_handle_completion: SN=%u/%u, type=0x%x, thread=%d/%d, status=%d 
2557,iii,[ ar_wal_local_frames.c : 393 ] local_frame_handle_completion: thread=%d/%d, status=%d 
2556,III,[ ar_wal_local_frames.c : 215 ] Long lifetime expiry,FC=%x,dur=%x,count=%x 
2555,iiIIIIi,[ ar_wal_local_frames.c : 333 ] WAL_DBGID_TX_MGMT_COMP_DESCID_STATUS vdev_id=%d mac_id=%d dec_id=0x%x tx_status=0x%x tid=0x%x buffer_id=0x%x reset_cnt=%d 
2554,IIIIiiIiI,[ ar_wal_local_frames.c : 482 ] local_frame_handle_completion_tqm, DA:%X-%X,type=0x%X,DATA:0x%X,thread=%d/%d,cookie=%X,status=%d,flags=0x%x 
2553,ii,[ ar_wal_local_frames.c : 917 ] WAL_DBGID_TX_MGMT_ENQUEUE_FAILED vdev_id = %d tid:%d 
2552,II,[ ar_wal_local_frames.c : 945 ] tid=%x isnt pre-allocated, qpeer_flags=%x 
2551,iiIIIII,[ ar_wal_local_frames.c : 1119 ] DBG WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d cookie=0x%x seq_num=0x%x type=0x%x len=0x%x tid_flg=0x%x 
2550,IIi,[ ar_wal_local_frames.c : 1136 ] ctrl_path_stats_dbg: mac_address equal mac_0 = 0x%x mac_2 =0x%x subtype = %d
 
2549,iII,[ ar_wal_local_frames.c : 2181 ] send local buffer fail: sw_peer_id=%d migration in progress mac_addr_31_0=%x mac_addr_47_32=%x 
2548,II,[ ar_wal_local_frames.c : 2211 ] send local buffer fail: status=%x, flags=%x 
2547,IIII,[ ar_wal_local_frames.c : 2145 ] local_data, peer(%p, sw_peer_id:%x) pdev mismatch(%p:%p) 
2546,IIII,[ ar_wal_local_frames.c : 2090 ] local_mgmt, peer(%p, sw_peer_id:%x) pdev mismatch(%p:%p) 
2545,ii,[ ar_wal_local_frames.c : 1718 ] WAL_DBGID_TX_MGMT_ENQUEUE_FAILED vdev_id = %d tid:%d 
2544,IIII,[ ar_wal_local_frames.c : 1766 ] host_mgmt, peer(%p, sw_peer_id:%x) pdev mismatch(%p:%p) 
2543,iiIIII,[ ar_wal_local_frames.c : 1910 ] DBG WAL_DBGID_TX_MGMT_DESCID_SEQ_TYPE_LEN vdev_id=%d mac_id=%d cookie=0x%x seq_num=0x%x type=0x%x len=0x%x 
2542,IIi,[ ar_wal_local_frames.c : 1926 ] ctrl_path_stats_dbg: mac_address equal mac_0 = 0x%x mac_2 =0x%x subtype = %d
 
2541,iIiiI,[ ar_wal_local_frames.c : 1949 ] WAL_DBGID_MGMT_TX_FAIL vdev_id=%d, err_code=%x, cookie=%d, status=%d, fc[0]=%x 
2582,iiiii,[ ar_wal_monitor.c : 1914 ] wal_monitor, wbm2sw2 monitor: pdev %d: timestamp(ms)=%d ring hp=%d tp=%d free_buf_cnt=%d 
2581,i,[ ar_wal_monitor.c : 1925 ] dev-%d:POLICY_ENFORCE_STATE --> MONITOR_TIMER_RUNNING_STATE 
2580,i,[ ar_wal_monitor.c : 357 ] dev-%d:TIMER_RUNNING_STATE  --> MONITOR_STATS_COLLECTION_STATE 
2579,i,[ ar_wal_monitor.c : 384 ] dev-%d:WAIT_POLICY_ENFORCE_STATE -->                 MONITOR_POLICY_ENFORCE_STATE 
2578,i,[ ar_wal_monitor.c : 1430 ] dev-%d:STATS_COLLECTION_STATE -->                 MONITOR_WAIT_POLICY_ENFORCE_STATE 
2577,ii,[ ar_wal_monitor.c : 1442 ] dev-%d:STATS_COLLECTION_STATE -->                 MONITOR_STATS_COLLECTION_STATE last_peer_idx:%d 
2576,i,[ ar_wal_monitor.c : 332 ] dev-%d:INIT_STATE  --> MONITOR_TIMER_RUNNING_STATE 
2575,IIiI,[ ar_wal_monitor.c : 336 ] %s %s send signal=%d to thread=%s to start timer 
 
2574,IIiI,[ ar_wal_monitor.c : 105 ] %s %s send signal=%d to thread=%s to yield 
 
2573,iiii,[ ar_wal_monitor.c : 1639 ] CONGCTRL HOST_CONTROL UPDATE peer_id:%d tid_num:%d threshold_1:%d threshold_2:%d
 
2572,iii,[ ar_wal_monitor.c : 1665 ] CONGCTRL HOST_CONTROL UPDATE peer_id:%d tid_num:%d new drop_threshold:%d  
2571,iii,[ ar_wal_monitor.c : 1706 ] CONGCTRL FW_CONTROL UPDATE peer_id:%d tid_num:%d new drop_threshold:%d  
2570,iiI,[ ar_wal_monitor.c : 1767 ] CONGCTRL peer_id:%d tid_num:%d msduq_mask:0x%08x 
2569,iiiiiii,[ ar_wal_monitor.c : 1559 ] CONGCTRL HOST_CONTROL peer_id:%d tid_num:%d traffic_enq:%d drop:%d deq:%d old_threshold:%d new_threshold:%d 
2597,,[ ar_wal_ast.c : 419 ] WAL_DBGID_AST_ENTRY_FULL WAL_ENOSPC 
2596,,[ ar_wal_ast.c : 1517 ] WAL_DBGID_AST_ENTRY_EXIST WAL_EEXIST 
2595,IIII,[ ar_wal_ast.c : 1526 ] WAL_AST_ALLOC_PEER peer_mac:0x%x ast_index:0x%x sw_peer_id:0x%x ast_flags:0x%x 
2594,i,[ ar_wal_ast.c : 1476 ] ar_wal_ast_dummy_alloc_peer ast_index = %d 
2593,III,[ ar_wal_ast.c : 491 ] WAL_DBGID_AST_DEL_WDS_ENTRY  0x%x 0x%x 0x%x 
2592,IIIII,[ ar_wal_ast.c : 1118 ] WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
2591,IIIII,[ ar_wal_ast.c : 1152 ] WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x 
2590,IIIIIi,[ ar_wal_ast.c : 1161 ] WAL_DBGID_AST_ADD_WDS_ENTRY  0x%x 0x%x 0x%x 0x%x 0x%x pdev_id:%d 
2589,II,[ ar_wal_ast.c : 1295 ] WAL_DBGID_AST_FREE_WDS_ENTRY des_mac is not next_hop or monitor direct 0x%x 0x%x 
2588,I,[ ar_wal_ast.c : 2196 ] SW peer key not found, peer_mac-0x%x 
2587,IiIIIII,[ ar_wal_ast.c : 2209 ] Update reorder queue peer_mac-0x%x, sw_peer_id-%d, queue_addr-0x%x:0x%x, queue-%x, ba_win-0x%x:0x%x 
2586,IIi,[ ar_wal_ast.c : 1210 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY FAILED due to peer mac search failed 0x%x 0x%x pdev_id:%d 
2585,IIi,[ ar_wal_ast.c : 1218 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY FAILED due to dest mac search failed 0x%x 0x%x pdev_id:%d 
2584,IIII,[ ar_wal_ast.c : 1239 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY 0x%x 0x%x 0x%x 0x%x 
2583,IIII,[ ar_wal_ast.c : 1246 ] WAL_DBGID_AST_UPDATE_WDS_ENTRY des_mac is not next_hop 0x%x 0x%x 0x%x 0x%x 
2688,ii,[ ar_wal_peer.c : 10449 ] _wal_peer_alloc_tid: got tid flush handle for tidno %d sw_peer_id:%d
 
2687,i,[ ar_wal_peer.c : 10581 ] _wal_peer_alloc_tid: adding tid %d to temp tid list
 
2686,iIIIII,[ ar_wal_peer.c : 947 ] pdev_id: %d ar_wal_peer_clean_up_flow:%x,%x,%x,%x,%x, 
2685,III,[ ar_wal_peer.c : 960 ] ar_wal_peer_clean_up_flow:%x,%x,%x 
2684,IIIII,[ ar_wal_peer.c : 3351 ] FREE_AST_ENTRY: peer=%p mac_addr=0x%x %x ast_index=0x%x valid_bmap[ast_index]=0x%x 
2683,IIIII,[ ar_wal_peer.c : 3095 ] FREE_AST_ENTRY: peer=%p mac_addr=0x%x %x  ast_index=0x%x valid_bmap[ast_index]=0x%x 
2682,ii,[ ar_wal_peer.c : 10685 ] _ar_wal_peer_free_tid:                sw_peer_id=%d, tidno=%d 
2681,ii,[ ar_wal_peer.c : 10699 ] _ar_wal_peer_free_tid: sending tid flush cmd to tac thread_id=%d, tidno=%d
 
2680,iiIiII,[ ar_wal_peer.c : 14035 ] mpdu_reconstruct_block_cb:pdev(%d)peer %d,flags=0x%x,del=%d,block=0x%x,recon=0x%x 
2679,IIIIII,[ ar_wal_peer.c : 4784 ] pdev(%x)peer %x blocked for tidLen update,refcnt=%x,htc=%x,remap=%x,security=%x 
2678,iIiI,[ ar_wal_peer.c : 4955 ] security: ar_wal_peer_set_key_block_cb: peer_id:%d  peer_flags:%02x authrized:%d qpeer_flags:%x 
2677,iIi,[ ar_wal_peer.c : 4998 ] security: ar_wal_peer_set_mcast_key_block_cb: peer_id:%d  peer_flags:%02x authrized:%d 
2676,,[ ar_wal_peer.c : 9699 ] qdepth_thresh_update_cmd_handler:                     Invalid sw_peer_key 
2675,,[ ar_wal_peer.c : 9706 ] qdepth_thresh_update_cmd_handler:                     Invalid peer 
2674,,[ ar_wal_peer.c : 9716 ] qdepth_thresh_update_cmd_handler:                    is_self_peer or bss_peer 
2673,,[ ar_wal_peer.c : 9727 ] qdepth_thresh_update_cmd_handler:                    peer delete in progress 
2672,i,[ ar_wal_peer.c : 9748 ] qdepth_thresh_update_cmd_handler:                    not valid TID give tidno:%d 
2671,i,[ ar_wal_peer.c : 9760 ] qdepth_thresh_update_cmd_handler:                   not valid tqm tid tidno:%d 
2670,ii,[ ar_wal_peer.c : 9777 ] qdepth_thresh_update_cmd_handler:                        qtype:%d host_drop_th:%d  
2669,ii,[ ar_wal_peer.c : 10728 ] _ar_wal_peer_tidq_empty: thread_id =%d,tidq->tid_num=%d
 
2668,IIIIIII,[ ar_wal_peer.c : 4694 ] update MPDUq hdrlen, peer=%x,tid_num=%x,tid_flg=%x %x,orig=%x,new=%x,wow=%x 
2667,,[ ar_wal_peer.c : 12604 ] wal_htt_peer_stats_reset: Peer pointer is NULL  
2666,IIi,[ ar_wal_peer.c : 2281 ] WAL_ALLOC_PEER_AST_FAIL peer_addr 0x04%x08%x type %d  
2665,II,[ ar_wal_peer.c : 2796 ] ADDR_TYPE_A: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
2664,II,[ ar_wal_peer.c : 2799 ] ADDR_TYPE_B peer: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
2663,II,[ ar_wal_peer.c : 2802 ] ADDR_TYPE_C self: mac_adr_31_0=0x%x, mac_addr_32_47=0x%x 
2662,i,[ ar_wal_peer.c : 2581 ] PEER_ALLOC: peer_id=%d: Fail to allocate wmm_param 
2661,III,[ ar_wal_peer.c : 13019 ] OMI: Change a_ctrl from 0x%lx to 0x%lx, ULMU Disable is 0x%lx
 
2660,ii,[ ar_wal_peer.c : 3651 ] wal_peer_delete_conf_msg_hdlr: peer=%d,num_del_in_pro=%d 
2659,ii,[ ar_wal_peer.c : 3677 ] wal_peer_delete_conf_msg_hdlr: peer = %d, pdev_peer_deletes_in_progress = %d
 
2658,iiI,[ ar_wal_peer.c : 3563 ] _wal_peer_del_msg_hdlr:  thread_id =%d, sw_peer_id=%d, peer->peer_flgs=0x%x
 
2657,iii,[ ar_wal_peer.c : 3872 ] wal_peer_delete_resume: peer = %d, delete_in_progress %d pdev_peer_deletes_in_progress = %d
 
2656,iII,[ ar_wal_peer.c : 13879 ] security: WAL_DBGID_SECURITY_PM4_SENT peer_id:%d, peer_flag:0x%x, qpeer_flag:0x%x 
2655,i,[ ar_wal_peer.c : 11421 ] wal_peer_mcast_cfg AST entry not found for key_id:%d 
2654,Iii,[ ar_wal_peer.c : 11425 ] wal_peer_fill_mcast_key_info: peer :%0x key_id:%d key_id_type:%d 
2653,ii,[ ar_wal_peer.c : 3792 ] _wal_peer_free: peer = %d delete_in_progress %d 
2652,iii,[ ar_wal_peer.c : 11500 ] wal_pm_mcast_cfg: enable :%d encr_en:%d decap_type:%d 
2651,Ii,[ ar_wal_peer.c : 11386 ] _wal_peer_mcast_key_id_update: peer :%0x key_id:%d 
2650,IIII,[ ar_wal_peer.c : 13624 ] peer_migrate failed: rx:%x, tx:%x MAC:%x, reset_cause %x 
2649,iiIiI,[ ar_wal_peer.c : 14077 ] mpdu_reconstruct:pdev(%d)peer %d,flags=0x%x,del=%d,recon=0x%x 
2648,,[ ar_wal_peer.c : 14121 ] reconstruct_tqm_mpdus: no TIDs to block 
2647,iIII,[ ar_wal_peer.c : 13958 ] Index= %d,  time_stamp_32_61 = 0x%x, time_stamp_0_31= 0x%x, flags = 0x%x  
2646,II,[ ar_wal_peer.c : 13963 ] A_TIMER_CURRENT_TIME_IN_TICKS time_stamp_32_61 = 0x%x time_stamp_0_31 = 0x%x  
2645,iIiiiI,[ ar_wal_peer.c : 4036 ] security: wal_peer_set_key: peer:%d, key_info:%p, key_id:%d is_mcast:%d key_type:%d key_flags:%02x  
2644,i,[ ar_wal_peer.c : 4059 ] _wal_peer_set_key: key_id:%d ignored, PMF 
2643,i,[ ar_wal_peer.c : 4259 ] _wal_peer_set_key: is_already_set_key_pending:%d 
2642,II,[ ar_wal_peer.c : 4374 ] WAL_DBGID_SECURITY_UCAST_KEY_SET  0x%x MAC:%x 
2641,I,[ ar_wal_peer.c : 4383 ] WAL_DBGID_SECURITY_MCAST_KEY_SET  0x%x 
2640,iI,[ ar_wal_peer.c : 4550 ] security: postponing set key for peer_id:%d peer_flags:%02x 
2639,iI,[ ar_wal_peer.c : 4580 ] security: wal_peer_set_key: peer:%d  peer_flags:%02x 
2638,i,[ ar_wal_peer.c : 6313 ] WAL_DBGID_SECURITY_SAFE_MODE on: %d  
2637,Ii,[ ar_wal_peer.c : 6400 ] nonqos to qos switch received during peer assoc for peer = %p, peer->qos_enabled = %d 
2636,iI,[ ar_wal_peer.c : 6460 ] security: set_param_authorized: peer:%d  peer_flags:%02x 
2635,Iii,[ ar_wal_peer.c : 6574 ] security: WAL_PEER_PARAM_TX_KEYID peer_key:%p and peer:%d val:%d 
 
2634,iIIII,[ ar_wal_peer.c : 6706 ] security: WAL_DBGID_SECURITY_ENCR_EN, peer %d, refcnt=%x,htc=%x,remap=%x,security=%x 
2633,I,[ ar_wal_peer.c : 7077 ] OMI: Set new nss = 0x%lx
 
2632,I,[ ar_wal_peer.c : 7084 ] OMI: Set new bw = 0x%lx
 
2631,I,[ ar_wal_peer.c : 7090 ] OMI: Set new a_ctrl = 0x%lx
 
2630,I,[ ar_wal_peer.c : 7102 ] HTC-block tids, peer:%x 
2629,I,[ ar_wal_peer.c : 7268 ] WAL_PEER_PARAM_FW_CONGESTION_DISABLE:%x 
2628,iii,[ ar_wal_peer.c : 6369 ] qos: flag: %d and peer_id is %d and qos_flag_rcvd:%d 
2627,,[ ar_wal_peer.c : 6393 ] qos_to_nonqos_switch: Sent dummy frame request to TX_DE 
2626,Iii,[ ar_wal_peer.c : 5540 ] security: WAL_PEER_PARAM_TX_KEYID peer_key:%p and peer:%d val:%d 
 
2625,iI,[ ar_wal_peer.c : 5665 ] security: set_param_authorized: peer:%d  peer_flags:%02x 
2624,i,[ ar_wal_peer.c : 5733 ] WAL_DBGID_SECURITY_SAFE_MODE on: %d  
2623,iii,[ ar_wal_peer.c : 5789 ] qos: flag: %d and peer_id is %d and qos_flag_rcvd:%d 
2622,,[ ar_wal_peer.c : 5813 ] qos_to_nonqos_switch: Sent dummy frame request to TX_DE 
2621,Ii,[ ar_wal_peer.c : 5820 ] nonqos to qos switch received during peer assoc for peer = %p, peer->qos_enabled = %d 
2620,iIIII,[ ar_wal_peer.c : 5876 ] security: WAL_DBGID_SECURITY_ENCR_EN, peer %d, refcnt=%x,htc=%x,remap=%x,security=%x 
2619,I,[ ar_wal_peer.c : 6076 ] OMI: Set new nss = 0x%lx
 
2618,I,[ ar_wal_peer.c : 6083 ] OMI: Set new bw = 0x%lx
 
2617,I,[ ar_wal_peer.c : 6089 ] OMI: Set new a_ctrl = 0x%lx
 
2616,I,[ ar_wal_peer.c : 6101 ] HTC-block tids, peer:%x 
2615,iiIii,[ ar_wal_peer.c : 13745 ] PDEV:%d, peer id=%d, QCU:%x/%d, ena=%d 
2614,,[ ar_wal_peer.c : 12050 ] _wal_peer_state_publish: Entry  
2613,ii,[ ar_wal_peer.c : 12055 ] _wal_peer_state_publish: bytes is %d, less than output size = %d  
2612,iiii,[ ar_wal_peer.c : 12084 ] _wal_peer_state_publish: peer_keyid0_ast_index is %d, vdev_id = %d, qos_enabled = %d, ba_tx_state_bmap = %d 
2611,iiiiii,[ ar_wal_peer.c : 12093 ] _wal_peer_state_publish: mac_address is %d:%d:%d:%d:%d:%d  
2610,,[ ar_wal_peer.c : 12099 ] _wal_peer_state_publish: Exit  
2609,iIi,[ ar_wal_peer.c : 5017 ] security: wal_peer_tid_flush_handler: peer_id:%d  peer_flags:%02x authrized:%d 
2608,ii,[ ar_wal_peer.c : 10178 ] wal_peer_tid_free_mem: sw_peer_id=%d, tidno = %d 
2607,i,[ ar_wal_peer.c : 10212 ] qos_to_nonqos_switch: it is last data TID got deleted peer_id:%d 
2606,II,[ ar_wal_peer.c : 13505 ] TRIGGER PDEV MISMATCH, thread:%x, tid:%x 
2605,i,[ ar_wal_peer.c : 3466 ] qos_to_nonqos_switch: wal_qos_to_nonqos_conf_msg_hdlr switching is done peer_id:%d 
2604,ii,[ ar_wal_peer.c : 3424 ] qos_to_nonqos_switch: wal_qos_to_nonqos_switch_msg_hdlr peer_id:%d thread_id:%d 
2603,IIIIIII,[ ar_wal_peer.c : 4646 ] security:pdev(%x)peer %x,flag %x, unblocked for tidLen update,refcnt=%x,htc=%x,remap=%x,security=%x 
2602,iII,[ ar_wal_peer.c : 5120 ] security: wal_tqm_setkey_update_sync_cb_func: sw_peer_id:%d peer_flags:0x%x, qpeer_flags=0x%x 
2601,II,[ ar_wal_peer.c : 5146 ] security: wal_tqm_setkey_update_unblock_cb_func: peer:%p  peer_flags:%02x 
2600,ii,[ ar_wal_peer.c : 537 ] HW overwritten tx_flow_number:%d and corressponding sw_peer_id:%d 
2599,iii,[ ar_wal_peer.c : 11857 ] wal_vdev_delete_all_peer_queue_dummy_frame_into_tcl: vdev = %d, sw_cookie = %d, buffer_id = %d 
 
2598,iii,[ ar_wal_peer.c : 11748 ] wal_vdev_delete_all_peer_queue_dummy_frame_into_tqm: vdev = %d, sw_cookie = %d, buffer_id = %d 
 
2695,I,[ wal_rc.c : 247 ] Phy rate=0, rix=%x 
2694,ii,[ wal_rc.c : 394 ] CHAINMASk_DBG  orig_cm=%d pdev_cm=%d 
2693,Iiii,[ wal_rc.c : 401 ] CHAINMASk_DBG overwrite tx chainmask, peer%p, sw_peer_id:%d  rate_Sched_chainmask %d tx_mask %d 
2692,i,[ wal_rc.c : 1352 ] [HT Sig]MCS value is not correct (%d) 
2691,i,[ wal_rc.c : 1563 ] [he_sig_b2_ofdma]MCS value is not correct (%d) 
2690,i,[ wal_rc.c : 1688 ] [he_sig_a]MCS value is not correct (%d) 
2689,i,[ wal_rc.c : 1433 ] MCS value is not correct (%d) 
2711,IiI,[ ar_wal_rtt.c : 1001 ] Deliver RX Ind msg:%p s_thr:%d to RT at ticks:0x%x 
2710,iiIIII,[ ar_wal_rtt.c : 829 ] DEBUG-TKNS: %d,%d,%lu,%lu,%lu,%lu 
2709,II,[ ar_wal_rtt.c : 847 ] DEBUG-PERF: %lu,%lu 
2708,IIIIIIIIi,[ ar_wal_rtt.c : 841 ] DEBUG-PERF: %lu,%lu,%lu,%lu,%lu,%lu,%lu,%lu,%d 
2707,iiIIIIII,[ ar_wal_rtt.c : 798 ] DEBUG-PERF: %d,%d,%lu,%lu,%lu,%lu,%lu,%lu 
2706,II,[ ar_wal_rtt.c : 804 ] DEBUG-PERF: %lu,%lu 
2705,IIIIIIIII,[ ar_wal_rtt.c : 223 ] RXLocInf1 0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x,0x%08x 
2704,I,[ ar_wal_rtt.c : 224 ] RXLocInf2 %u 
2703,I,[ ar_wal_rtt.c : 343 ] ar_wal_get_rssi_chain: invalid rssi_info for %p 
2702,IiIiii,[ ar_wal_rtt.c : 777 ] rtt_get_toda: txrx_msg_buf=%p toda_type=%d toda_phy_clk=%u ppdu_id=%d txrx_delay=%d status=%d 
2701,Ii,[ ar_wal_rtt.c : 632 ] recv sta rssi 0x%08x chain:%d 
2700,ii,[ ar_wal_rtt.c : 892 ] rtt_recv_sta_get_rxbw: rx_bw=%d rx_preamble=%d 
2699,Ii,[ ar_wal_rtt.c : 659 ] send sta rssi 0x%08x chain:%d 
2698,I,[ ar_wal_rtt.c : 934 ] rtt_send_sta_get_rxbw: rtt_pkt_bw=0x%x 
2697,I,[ ar_wal_rtt.c : 914 ] rtt_send_sta_get_txbw: packet_bw=0x%x 
2696,,[ ar_wal_rtt.c : 1120 ] ar_wal_rtt_tx_ppdu_completion_handler: excess zero values in receive_rssi_info 
2735,IIIIiiI,[ ar_wal_rx.c : 2387 ] rx frame wh:0x%p, type|subtype|seq: 0x%x, i_addr1:%x, i_addr2:%x, len:%d, gid:%d, mask:0x%lx 
2734,IIIIII,[ ar_wal_rx.c : 2433 ] rxdma_error_code: %x, sw_peer_id =%x ,sw group_id %x, %x,%x, ts= %u 
2733,IIi,[ ar_wal_rx.c : 2689 ] ctrl_path_stats_dbg rx: mac_address equal mac_0 = 0x%x mac_2 =0x%x subtype = %d
 
2732,IIIIIIII,[ ar_wal_rx.c : 1878 ] peer_rx_data_event: sw_peer_id__ast_idx=0x%x, FC=%x, SN/QOS=%x, msdu_len_route_arp=0x%x, mpdu_ok/f=0x%x, mcs_nss_msdu_cnt=0x%x, mpdu_bytes_count = 0x%x, bw_gi_pream_ppdu_dur=0x%x 
2731,iiIIIii,[ ar_wal_rx.c : 1779 ] peer_rx_event: sw_peer_id=%d,ast_idx=%d,FC=%x,mpdu_SN=%x,ok/fail=%X,mpdu_len=%d,buf0_len=%d 
2730,,[ ar_wal_rx.c : 3187 ] rx_lp_pcie_cancel_timer: timer cancelled! 
2729,ii,[ ar_wal_rx.c : 3212 ] rx pdev_id:%d pcie lp state changed to active mode counter part state:%d 
2728,ii,[ ar_wal_rx.c : 3231 ] rx pdev_id:%d pcie lp state changed to sleep mode counter part state:%d 
2727,ii,[ ar_wal_rx.c : 6998 ] tx pdev_id:%d pcie lp state appled to HW:%d 
2726,iII,[ ar_wal_rx.c : 3932 ] RX PhyErr:dev=%d,err=%x,rx_err_cnt=%x 
2725,iiII,[ ar_wal_rx.c : 7040 ] rx resume on pdev :%d, module:%d, flag:%x, caller:0x%x 
2724,IiI,[ ar_wal_rx.c : 673 ] pdev %x, rx reap error sq %d, buffer 0x%x 
2723,Ii,[ ar_wal_rx.c : 917 ] pdev %x, rx drop bcast amsdu[%d] frame 
2722,I,[ ar_wal_rx.c : 927 ] pdev %x, rx drop mcbc WDS (4 address) frame 
2721,IIIIIII,[ ar_wal_rx.c : 3353 ] AVGCFO Print: delta_time %x, cur_cfo %x, avg_alphya %x, old_cfo %x, new_cfo %x, %x, program to phy %x 
2720,iiiII,[ ar_wal_rx.c : 6916 ] rx_suspend on pdev:%d, module:%d, status:%d, flags %x, caller: %x 
2719,IIIIIII,[ ar_wal_rx.c : 7266 ] wal_rx_restore_ring_from_offload: [%x] [%x] [%x] [%x] [%x] [%x] [%x]
 
2718,II,[ ar_wal_rx.c : 7285 ] wal_rx_setup_ring_for_offload: [%x] [%x]
 
2717,III,[ ar_wal_rx.c : 1524 ] rx local notify: 0x%p, flags: 0x%x, ts: %u 
2716,IIII,[ ar_wal_rx.c : 1600 ] %s: empty len: 0x%x, addr:0x%x:0x%x 
2715,IIII,[ ar_wal_rx.c : 1637 ] %s: offload len: 0x%x, addr:0x%x:0x%x 
2714,III,[ ar_wal_rx.c : 7899 ] %s: filter0 (0x%x) filter1 (0x%x)
 
2713,IIIIII,[ ar_wal_rx.c : 7177 ] WAL_DBGID_RX_BA_SETUP  0x%x 0x%x 0x%x 0x%x 0x%x MAC:%x 
2712,iiIIII,[ ar_wal_rx.c : 6374 ] rx_suspend_resume_msg on pdev:%d, data_value:%d, status ring flag %x, head %x, tail %x, ms:%x 
2753,IiI,[ ar_wal_rx_recovery.c : 287 ] pdev %x, rx empty recovery sq %d, buffer[%x] 
2752,IiI,[ ar_wal_rx_recovery.c : 317 ] pdev %x, rx reap recovery sq %d, buffer[%x] 
2751,iI,[ ar_wal_rx_recovery.c : 441 ] rx reap recovery sq %d, buffer[%x] 
2750,iII,[ ar_wal_rx_recovery.c : 997 ] UL OFDMA usr index: %d, HE Control value: 0x%x, HE Control count: 0x%x
 
2749,iII,[ ar_wal_rx_recovery.c : 1024 ] UL OFDMA usr index: %d, Qos Control value: 0x%x, Qos Control count: 0x%x
 
2748,ii,[ ar_wal_rx_recovery.c : 1229 ] pkt_route: %d type_bmap: %d 
2747,iIIII,[ ar_wal_rx_recovery.c : 1305 ] RX ppdu sfm no resource drop count is valid? %d :%x,%x mpdu drop count:%x,%x 
2746,IIi,[ ar_wal_rx_recovery.c : 1404 ] SFM_PENDING_RXPCU DETECTION_TYPE: 0x%x RECOVERY_TYPE = 0x%x NUM_RESETS : %d 
2745,I,[ ar_wal_rx_recovery.c : 1473 ] RX set crash mask 0x%x 
2744,,[ ar_wal_rx_recovery.c : 1477 ] clear crash mask 
2743,I,[ ar_wal_rx_recovery.c : 1489 ] g_dbg_local_buf_debug_enable %x 
2742,IIIIIIIII,[ ar_wal_rx_recovery.c : 144 ] rx dma pdev/hung 0x%x, last_group_id: 0x%x/0x%x, err:0x%x, pop:0x%x, free:0x%x, forward:0x%x, requeue:0x%x, notify:0x%x 
2741,IIIIIIIII,[ ar_wal_rx_recovery.c : 54 ] rx ole pdev/hung 0x%x, last_group_id: 0x%x/0x%x, err:0x%x, pop:0x%x, free:0x%x, forward:0x%x, requeue:0x%x, notify:0x%x 
2740,IIIIIIIII,[ ar_wal_rx_recovery.c : 100 ] rx pcu pdev/hung 0x%x, last_group_id: 0x%x/0x%x, err:0x%x, pop:0x%x, free:0x%x, forward:0x%x, requeue:0x%x, notify:0x%x 
2739,IIII,[ ar_wal_rx_recovery.c : 551 ] SFM_PENDING_RXPCU (SFM_REG) detected dev_id:0x%x,rxpcu_sfm_num_dwords=0x%x,MCMN_R0_MCMN_MAC_IDLE=0x%x,detection_type= 0x%x 
2738,i,[ ar_wal_rx_recovery.c : 502 ] restart remote timers for pdev:%d 
2737,ii,[ ar_wal_rx_recovery.c : 472 ] wal_rx_rings_reset pdev:%d, cnt:%d 
2736,,[ ar_wal_rx_recovery.c : 531 ] SFM_PENDING_RXPCU ignored.. 
2768,iiiiiii,[ ar_wal_rx_refill.c : 1290 ] error_frame from module %d, rxdma_push_reason %d, rxdma err:%d cnt %d reo_push_reason %d, reo err:%d cnt %d 
2767,IIIIIIII,[ ar_wal_rx_refill.c : 1301 ] error buffer %x, %x, rbm %x, cookie %x, wbm2sw1[0x%x:0x%x], wbm2sw3[0x%x:0x%x] 
2766,i,[ ar_wal_rx_refill.c : 106 ] Skip host ring TP updating for inactive pdev %d 
2765,i,[ ar_wal_rx_refill.c : 193 ] Skip monitor ring HP updating for inactive pdev %d 
2764,i,[ ar_wal_rx_refill.c : 290 ] Skip refill ring HP updating on pdev %d 
2763,ii,[ ar_wal_rx_refill.c : 2091 ] pdev %d CE pending in refill ring %d  
2762,ii,[ ar_wal_rx_refill.c : 2100 ] pdev %d CE pending in dest ring %d  
2761,ii,[ ar_wal_rx_refill.c : 2108 ] pdev %d CE pending in dest ring %d  
2760,ii,[ ar_wal_rx_refill.c : 2117 ] pdev %d CE pending in src ring %d  
2759,IiiI,[ ar_wal_rx_refill.c : 1663 ] ipa switch (HI) to REO2SW1-last=0x%x,counters=%d.%d,tp_stall_state=0x%x 
2758,IiiI,[ ar_wal_rx_refill.c : 1765 ] ipa switch (MED) continue on REO2SW1-last=0x%x,counters=%d.%d,tp_stall_state=0x%x 
2757,IiiI,[ ar_wal_rx_refill.c : 1684 ] ipa switch continue (HI) on REO2SW1-last=0x%x,counters=%d.%d,tp_stall_state=0x%x 
2756,IiiI,[ ar_wal_rx_refill.c : 1740 ] ipa switch (LO) traffic to REO2SW4-last=0x%x,counters=%d.%d,tp_stall_state=0x%x 
2755,IIIIiiI,[ ar_wal_rx_refill.c : 64 ] ipa switch-curr=0x%x, last=0x%x, ena_hi_lo_pndg=0x%08x hp_tp=0x%08x, counters=%d.%d, tp_stall_state=0x%x 
2754,iiii,[ ar_wal_rx_refill.c : 573 ] ipa_drop setup high_th %d low_th %d refill_ring_sz %d wbm2ipa_release_ring_sz %d 
2783,,[ wal_htt_ppdu_stats.c : 512 ] Dropped ppdu stats due to ring full 
2782,,[ wal_htt_ppdu_stats.c : 1048 ] Dropped ppdu stats due to full QHEAP 
2781,,[ wal_htt_ppdu_stats.c : 1675 ] Dropped ppdu stats due to full QHEAP 
2780,,[ wal_htt_ppdu_stats.c : 1731 ] Dropped ppdu stats due to full QHEAP 
2779,,[ wal_htt_ppdu_stats.c : 619 ] Dropped ppdu stats due to full QHEAP 
2778,,[ wal_htt_ppdu_stats.c : 1206 ] Dropped ppdu stats due to full QHEAP 
2777,,[ wal_htt_ppdu_stats.c : 766 ] Dropped ppdu stats due to full QHEAP 
2776,,[ wal_htt_ppdu_stats.c : 986 ] Dropped ppdu stats due to full QHEAP 
2775,,[ wal_htt_ppdu_stats.c : 927 ] Dropped ppdu stats due to full QHEAP 
2774,,[ wal_htt_ppdu_stats.c : 1408 ] Dropped ppdu stats due to full QHEAP 
2773,,[ wal_htt_ppdu_stats.c : 1309 ] Dropped tqm ppdu stats due to ring full 
2772,,[ wal_htt_ppdu_stats.c : 1323 ] Dropped tqm ppdu stats due to full QHEAP 
2771,,[ wal_htt_ppdu_stats.c : 1511 ] Dropped tac ppdu stats due to full QHEAP 
2770,,[ wal_htt_ppdu_stats.c : 1993 ] Dropped ppdu stats due to full QHEAP 
2769,i,[ wal_htt_ppdu_stats.c : 1895 ] Dropped self gen ppdu tlv due to ring full ring_id:%d 
2791,iii,[ ar_wal_thermal.c : 1046 ] WAL_TT_SCHED_RESUME_HNDLR thrd_id = %d pdev_id = %d time_diff %dusec 
2790,ii,[ ar_wal_thermal.c : 821 ] WAL_TT_SCHED_SUSPEND_DISPATCH thrd_id = %d pdev_id = %d 
2789,ii,[ ar_wal_thermal.c : 863 ] WAL_TT_SCHED_RESUME_DISPATCH thrd_id = %d pdev_id = %d 
2788,ii,[ ar_wal_thermal.c : 993 ] WAL_TT_SCHED_SUSPEND_HNDLR thrd_id = %d pdev_id = %d 
2787,ii,[ ar_wal_thermal.c : 320 ] WAL_TT_TSENS_TEMP pdev_id = %d, temp = %ddegC 
2786,iiiii,[ ar_wal_thermal.c : 162 ] WAL_TT_TSENS_PID_SUSPEND pdev_id = %d curr_temp = %ddegC sensor_id = %d zone = %d tx_off_dc = %d 
2785,iiii,[ ar_wal_thermal.c : 451 ] pdev_id(%d),tx_chainmask(%d), rx_chainmask(%d), num_chains(%d) 
2784,iii,[ ar_wal_thermal.c : 959 ] THERMAL_INST_TEMP_REQ ret = %d pdev_id = %d thrd_id = %d 
2805,IIII,[ ar_wal_tqm.c : 612 ] peer_id=0x%x, _set_flow_to_be_cleanup:%x, tx_flow_number:%x,caller:%x 
2804,ii,[ ar_wal_tqm.c : 739 ] qos:  %d and peer_id is %d tickle tid 
2803,I,[ ar_wal_tqm.c : 777 ] wal_tqm_process_flow_not_empty_status new flow:%x  
2802,ii,[ ar_wal_tqm.c : 7292 ] soft_msduq_delete: Requesting soft msduq delete :%d qtype:%d 
2801,II,[ ar_wal_tqm.c : 352 ] wal_tqm_flow_update_helper not_init, fw_initialized:%x, counter:%x 
2800,,[ ar_wal_tqm.c : 4204 ] TCL rings unpaused 
2799,i,[ ar_wal_tqm.c : 4210 ] Fired timer again             TQM link descriptor counter:%d 
2798,iii,[ ar_wal_tqm.c : 2366 ] qos_to_nonqos_switch: Received tqm add_msdu status peer_id:%d status:%d buffer_id:%d 
2797,iiii,[ ar_wal_tqm.c : 2668 ] Fired timer and paused TCL rings             ring link descriptor counters mac0:%d mac1:%d mac2:%d sum:%d 
2796,IIII,[ ar_wal_tqm.c : 2425 ] peer_id= 0x%x, wal_tqm_process_flush_cache_status:%x,%x,%x 
2795,,[ ar_wal_tqm.c : 1092 ] wal_tqm_process_gen_mpdus_status: Null ptid 
2794,ii,[ ar_wal_tqm.c : 435 ] _wal_tqm_process_update_tx_msdu_flow_status tx_flow_number:%d update_requirements_not_met:%d  
2793,ii,[ ar_wal_tqm.c : 2064 ] soft_msduq_delete: msduq got deleted :%d qtype:%d 
2792,ii,[ ar_wal_tqm.c : 2068 ] soft_msduq_delete: delete req dropped :%d qtype:%d 
2810,IIIIIIII,[ ar_tx_q_enque.c : 687 ] pn_alloc:fc=%x,comp_type=%x,flen=%lx,msdu_flags=%lx,id=%x,buffer_id=%x,enque_id=%x,pending_local=%x 
2809,II,[ ar_tx_q_enque.c : 921 ] WAL_DBGID_TX_DISCARD id: %x, flag:%lx
 
2808,,[ ar_tx_q_enque.c : 734 ] pn_alloc: invalid PN assigned 
2807,IIIIIII,[ ar_tx_q_enque.c : 772 ] pn_alloc_complete:fc=%x,flen=%lx,msdu_flags=%lx,tid_num=%x,enque_id=%x,pn_idx=%x,pn=%llx 
2806,IIIIII,[ ar_tx_q_enque.c : 815 ] pn_alloc failed: id:%x,flags:%x,tid_no:%x,fc:%x,enqeu_id=%x,pending_local=%x 
2882,IIIIIIIIIII,[ ar_wal_tx_dbg.c : 822 ] txbf_su_ppdu_stats (legacy su = %lu)(ol ac su = %lu)(txbf ac su =  %lu)(txbf ac %% = %lu)(ol ax su = %lu)(txbf ax su =  %lu)(txbf ax %% = %lu) 
2881,Ii,[ ar_wal_tx_dbg.c : 3026 ] sifs burst enable: 0x%x, pdev=%d
 
2880,IIIIII,[ ar_wal_tx_dbg.c : 3148 ] flush_38_hist: %02d %02d %02d %02d %02d %02d 
2879,IIIII,[ ar_wal_tx_dbg.c : 3316 ] PHYDBG: g_dbg_phydbg_default_events: 0x%08x, g_dbg_phydbg_pmi_events: 0x%08x, g_dbg_phydbg_mpi_events: 0x%08x, g_dbg_phydbg_rxtd_events: 0x%08x, g_dbg_phydbg_robe_events: 0x%08x 
2878,IIIII,[ ar_wal_tx_dbg.c : 3482 ] twt_dbg_leak_hist_dl: Bins0-4: %u, %u, %u, %u, %u 
2877,IIIII,[ ar_wal_tx_dbg.c : 3487 ] twt_dbg_leak_hist_dl: Bins5-9: %u, %u, %u, %u, %u 
2876,III,[ ar_wal_tx_dbg.c : 871 ] txbf_su_mpdu_stats AX OL(ol ax su tried = %lu)(ol ax su failed = %lu)(ol ax su retried = %lu) 
2875,IIIII,[ ar_wal_tx_dbg.c : 3493 ] twt_dbg_leak_hist_ul: Bins0-4: %u, %u, %u, %u, %u 
2874,IIIII,[ ar_wal_tx_dbg.c : 3499 ] twt_dbg_leak_hist_ul: Bins0-4: %u, %u, %u, %u, %u 
2873,i,[ ar_wal_tx_dbg.c : 3935 ] SelfGenResp: Dev id %d is in power saving state, not able to print. 
2872,ii,[ ar_wal_tx_dbg.c : 3986 ] LOCAL: msduq_pool_ctxt total_alloc_cnt:%d cur_alloc_cnt:%d 
2871,ii,[ ar_wal_tx_dbg.c : 3990 ] REMOTE: msduq_pool_ctxt total_alloc_cnt:%d cur_alloc_cnt:%d 
2870,ii,[ ar_wal_tx_dbg.c : 4003 ] LOCAL: tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2869,ii,[ ar_wal_tx_dbg.c : 4006 ] REMOTE: tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2868,ii,[ ar_wal_tx_dbg.c : 4010 ] LOCAL: ul_tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2867,ii,[ ar_wal_tx_dbg.c : 4013 ] REMOTE: ul_tid_state_pool total_alloc_cnt:%d cur_alloc_cnt:%d 
2866,ii,[ ar_wal_tx_dbg.c : 4219 ]  Profile Enabled : %d   hist_intvl : %d 
2865,IIIIII,[ ar_wal_tx_dbg.c : 888 ] txbf_su_mpdu_stats AX (txbf sifs ax su tried = %lu)(txbf sifs ax su failed = %lu)(txbf sifs ax su retried = %lu)(txbf rbo ax su tried = %lu)(txbf rbo ax su failed = %lu)(txbf rbo ax su retried = %lu) 
2864,iiii,[ ar_wal_tx_dbg.c : 4247 ]  Profile ID : %d  Count: %d  Min : %d  Max : %d  
2863,iiiii,[ ar_wal_tx_dbg.c : 4259 ]  Profile ID : %d  hist_intvl: %d  hist[0] : %d  hist[1] : %d  hist[2] : %d  
2862,,[ ar_wal_tx_dbg.c : 4399 ] ctrl_path_stats_dbg : Disabling peer_dbg logs
 
2861,,[ ar_wal_tx_dbg.c : 4406 ] ctrl_path_stats_dbg : Error seen 
 Usage 
ctrl_path_stats_dbg: To Enable  Stats: wifitool athX setUnitTestCmd 0x48 8 244 1 <mac_addr_0> <mac_addr_1> <mac_addr_2>  <mac_addr_3> <mac_addr_4> <mac_addr_5>
ctrl_path_stats_dbg: To Disable Stats: wifitool athX setUnitTestCmd 0x48 2 244 0
 
2860,II,[ ar_wal_tx_dbg.c : 4432 ] ctrl_path_stats_dbg : mac_addr_31_0 = 0x%x mac_addr_47_32 = 0x%x
 
2859,,[ ar_wal_tx_dbg.c : 4434 ] ctrl_path_stats_dbg: SW Peer ID Check
 
2858,i,[ ar_wal_tx_dbg.c : 4437 ] ctrl_path_stats_dbg: vdev %d 
 
2857,,[ ar_wal_tx_dbg.c : 4445 ] ctrl_path_stats_dbg: bss  
2856,,[ ar_wal_tx_dbg.c : 4447 ] ctrl_path_stats_dbg: self  
2855,iII,[ ar_wal_tx_dbg.c : 4450 ] ctrl_path_stats_dbg: peer %d, mac %x %x
 
2854,II,[ ar_wal_tx_dbg.c : 899 ] txbf_snd_stats(txbf_ac_snd = %lu)(txbf_ax_snd = %lu) 
2853,iII,[ ar_wal_tx_dbg.c : 4452 ] ctrl_path_stats_dbg: sw_peer_id found peer %d, mac %x %x
 
2852,II,[ ar_wal_tx_dbg.c : 4545 ] s_stats: dbg_num_bufs: %u, dbg_num_evt: %u 
 
2851,III,[ ar_wal_tx_dbg.c : 4546 ] s_stats: HOST_ring_HI : %u, TI : %u, S_TI : %u  
2850,IIII,[ ar_wal_tx_dbg.c : 4547 ] s_stats: IN/SHADOW_ring_HI : %u, TI : %u, S_TI : %u, S_HI : %u 
2849,IIII,[ ar_wal_tx_dbg.c : 4548 ] s_stats: OUT_ring_HI : %u TI : %u, S_TI : %u, S_HI : %u 
2848,IIIII,[ ar_wal_tx_dbg.c : 4551 ] s_stats: IPC_ring_%u : HI : %u TI : %u, S_TI : %u, S_HI : %u 
2847,,[ ar_wal_tx_dbg.c : 4553 ] s_stats: VREG_DET0 : 
 
2846,III,[ ar_wal_tx_dbg.c : 4554 ] s_stats: ScanPri : %u, SCount : %u, SPrd : %u 
 
2845,III,[ ar_wal_tx_dbg.c : 4555 ] s_stats: ChnMask : %u, SEna : %u, SUpdtMask : 0x%x 
 
2844,IIII,[ ar_wal_tx_dbg.c : 4556 ] s_stats: SRdyIntrpt : %u, SPfmd : %u, IntrptsSent : %u, Scanpending : %u 

 
2843,iii,[ ar_wal_tx_dbg.c : 911 ] %dms Burst: avg_txop_burst(ms) = %d,txop_on_burst_complete(ms) = %d 
 
2842,,[ ar_wal_tx_dbg.c : 4558 ] s_stats: VREG_DET1: 
 
2841,III,[ ar_wal_tx_dbg.c : 4559 ] s_stats: ScanPri : %u, SCount : %u, SPrd : %u 
 
2840,III,[ ar_wal_tx_dbg.c : 4560 ] s_stats: ChnMask : %u, SEna : %u, SUpdtMask : 0x%x 
 
2839,IIII,[ ar_wal_tx_dbg.c : 4561 ] s_stats: SRdyIntrpt : %u, SPfmd : %u, IntrptsSent : %u , Scanpending : %u 
 
2838,iiii,[ ar_wal_tx_dbg.c : 4947 ] delimiter user track: Number of total MU PPDU %d, MU PPDUs with delimiter users: %d, Percent:%d                    Average MU number of delimiter users %d 
2837,iiiii,[ ar_wal_tx_dbg.c : 5494 ] CONG_CTRL Multicast_DBG buf_id:%d hcm_bin_idx:%d cur:%d, min:%d, max:%d 
2836,i,[ ar_wal_tx_dbg.c : 5532 ] IPA wbm2sw2 ring monitor configure: logging hp/tp in every %d sec 
2835,i,[ ar_wal_tx_dbg.c : 5542 ] IPA TCL exception path logging: %d 
2834,ii,[ ar_wal_tx_dbg.c : 5592 ] 6G FCC: Debug counters TSF - %d, CCA counter - %d 
2833,ii,[ ar_wal_tx_dbg.c : 5600 ] 6G FCC: Resp frame stats Blocked %d times unblocked %d times 
2832,iiiiiiii,[ ar_wal_tx_dbg.c : 1112 ] sched_cmd_result[0] to sched_cmd_result[6] for HWQ id %d = {%d,%d,%d,%d,%d,%d,%d}
 
2831,ii,[ ar_wal_tx_dbg.c : 5632 ] 6G FCC: BW based recipe max_bw_restricted - %d, drop_bw - %d 
2830,iiiiiii,[ ar_wal_tx_dbg.c : 1122 ] sched_cmd_result[7] to sched_cmd_result[12] for HWQ id %d = {%d,%d,%d,%d,%d, %d}
 
2829,i,[ ar_wal_tx_dbg.c : 1170 ] TX_IST_TRIGGER SENT %d
 
2828,IIIIII,[ ar_wal_tx_dbg.c : 843 ] txbf_su_mpdu_stats (legacy su tried = %lu)(legacy su failed = %lu)(legacy su retried = %lu) ------------------------txbf_su_mpdu_stats AC OL(ol ac su tried = %lu)(ol ac su failed = %lu)(ol ac su retried = %lu) 
2827,iiiiiiii,[ ar_wal_tx_dbg.c : 1234 ] WHAL_STATS for pdev id =  %d: last_unpause_ppdu_id = %d hwsch_unpause_wait_tqm_write = %d hwsch_dummy_tlv_skipped = %d hwsch_misaligned_offset_received = %d hwsch_reset_count = %d hwsch_dev_reset_war = %d hwsch_delayed_pause = %d 
2826,iiiiiiii,[ ar_wal_tx_dbg.c : 1254 ] hwsch_long_delayed_pause = %d sch_rx_ppdu_no_response = %d sch_selfgen_response = %d sch_rx_sifs_resp_trigger = %d sch_mpdu_info_bitmap_missed = %d hwsch_qcdd03911334 = %d hwsch_qcdd04031456 = %d hwsch_qcdd03955078 = %d 
2825,iiiiiiii,[ ar_wal_tx_dbg.c : 1274 ] hwsch_backpressure_wdog = %d hwsch_pause_wdog = %d hwsch_fes_start_wdog = %d hwsch_life_time_expiry_valid_fes_offset = %d crypto_wdog_tmout = %d hwsch_fes_end_offset_wraparound = %d pdg_sfm_leak_rst_cnt = %d hwsch_cmd_ring_reset_war_dummy_completions = %d 
2824,iiiiiiii,[ ar_wal_tx_dbg.c : 1294 ] hwsch_flush_not_done = %d flush_tx_not_idle = %d hwsch_wd_unknown_reset = %d hwsch_mtu_wrap_wdog = %d crypto_fatal_unknown = %d txdma_fatal_unknown = %d sfm_fatal_unknown = %d mcmn_fatal_unknown = %d 
2823,iiiiiiii,[ ar_wal_tx_dbg.c : 1314 ] txpcu_wdog_tout = %d txpcu_recd_lt_mpdu = %d txpcu_recd_gt_mpdu= %d pdg_fatal_unknown = %d hwsch_fatal_unknown = %d hwsch_wdog_unknown = %d mxi_fatal_unknown = %d txole_fatal_unknown = %d 
2822,iiiiiii,[ ar_wal_tx_dbg.c : 1362 ] tx_flush_tlv_tag_oor_err = %d tx_flush_tlv_len_oor_err = %d tx_flush_tlv_taglen_mismatch_err = %d tx_flush_unexpected_tlv_end_err = %d tx_steer_frm_cnt = %d txdma_gxi_tmout_count = %d phy_warm_reset = %d 
2821,,[ ar_wal_tx_dbg.c : 1389 ] No ul_resp_vdev assigned !! 
2820,II,[ ar_wal_tx_dbg.c : 1393 ] ac:%x already in MU mode, reset timer to %x 
2819,I,[ ar_wal_tx_dbg.c : 1396 ] ac:%x switch to MU mode 
2818,I,[ ar_wal_tx_dbg.c : 1542 ] flush hwq mask:%x 
2817,IIIIII,[ ar_wal_tx_dbg.c : 860 ] txbf_su_mpdu_stats AC (txbf sifs ac su tried = %lu)(txbf sifs ac su failed = %lu)(txbf sifs ac su retried = %lu)(txbf rbo ac su tried = %lu)(txbf rbo ac su failed = %lu)(txbf rbo ac su retried = %lu) 
2816,I,[ ar_wal_tx_dbg.c : 1547 ] flush hwq mask:%x, ul_resp is not enabled 
2815,IIII,[ ar_wal_tx_dbg.c : 1769 ] TXDEWDOG TCL1:%u full_ignore:%u dummy_queued:%u last_time:%u 
2814,III,[ ar_wal_tx_dbg.c : 1772 ] TXDEWDOG TQM1:%u dummy_queued:%u last_time:%u 
2813,,[ ar_wal_tx_dbg.c : 2069 ] No ul_resp_vdev or BSS-peer assigned !! 
2812,II,[ ar_wal_tx_dbg.c : 2460 ] read addr: 0x%x, value = 0x%x 
2811,III,[ ar_wal_tx_dbg.c : 497 ] data_stall debug support is not allowed as the vdev_type is not            STA pdev_id:8/vdev_id:8 0x%08x vdev:0x%x pdev:0x%x 
2923,I,[ ar_wal_tx_send.c : 11868 ] TX_ABORT FAILED 0x%x 
2922,Ii,[ ar_wal_tx_send.c : 3474 ] tx_send_attach failed 0x%x, line:%d 
2921,iI,[ ar_wal_tx_send.c : 12059 ] tx_hw_stuck(%d): consecutive data lifetime exp=%x 
2920,Iii,[ ar_wal_tx_send.c : 11596 ] SEC_RETRY ptid 0x%x tid_num %d in NON_AGGR Seq, enable tid for sw_retry %d
 
2919,ii,[ ar_wal_tx_send.c : 16258 ] pdev %d, WIFIMISSING_MPDU_INFO_E cnt: %d
 
2918,i,[ ar_wal_tx_send.c : 16344 ] Retried BAR for %d times, clear BAR flag
 
2917,iI,[ ar_wal_tx_send.c : 16357 ] BAR tx failure tid_num: %d, tid_flags:0x%x
 
2916,IiIIi,[ ar_wal_tx_send.c : 16387 ] SET BAR for ptid %p(%d), tid_flags:0x%x due to sch_cmd_result=0x1 ssn__basn=%08x cnt=%d
 
2915,III,[ ar_wal_tx_send.c : 16595 ] seq not cleaned ! queue_id:%x, txq:%p, seq_ctrl:%p
 
2914,ii,[ ar_wal_tx_send.c : 10518 ] Data stall force reset, cal fdmt, rssi %d tx_res %d 
2913,ii,[ ar_wal_tx_send.c : 10521 ] Data stall force reset, rssi %d tx_res %d 
2912,ii,[ ar_wal_tx_send.c : 10593 ] tx_send_dsr_ppdu_done increment peer->ext->consecutive_eap_cnt : %d, sw_peer_id: %d 
2911,ii,[ ar_wal_tx_send.c : 10600 ] tx_send_dsr_ppdu_done clear peer->ext->consecutive_eap_cnt : %d, sw_peer_id: %d 
2910,Iii,[ ar_wal_tx_send.c : 10615 ] tx_send_dsr_proc_ppdu_done consecutive_pm_filter_cnt %0x %d, %d MAC reset counter
 
2909,,[ ar_wal_tx_send.c : 10644 ] detect pdg sfm consecutive leakage, reset 
2908,iiiIIiii,[ ar_wal_tx_send.c : 10699 ] twt_dbg/ul_tcp: dsr_proc_ppdu_done txqid=%d, sched_id=%d, tx_status=%d, peer=%u, ftype=%u, queued=%d, tried=%d, failed=%d 
 
2907,II,[ ar_wal_tx_send.c : 17243 ] Pause UL ring - wal_txq_id:%x,wal_txq_id_sta_ul:%x 
2906,iiiiiIII,[ ar_wal_tx_send.c : 17257 ] TTL tid:%d ppdu:%d %d,cmd:%d txq_id:%d,flg:%x %x,caller:%x 
2905,iiii,[ ar_wal_tx_send.c : 17111 ] MSDUTTL TQM peer_id:%d deq:%d tid_num:%d qtype:%d 
2904,I,[ ar_wal_tx_send.c : 18114 ] Received GTK frame for Qpeer=%p, but PTK not set 
2903,III,[ ar_wal_tx_send.c : 19032 ] pdev:%u, RING(%x) pause finished(%x) 
2902,III,[ ar_wal_tx_send.c : 19102 ] pdev:%u, pause ring(%x:%x) 
2901,Iiiii,[ ar_wal_tx_send.c : 7806 ] allow_n_flags 0x%x sendn_frms_allowed %d sendn_frms_tried %d subfrms_max %d encap_type %d 
2900,iiI,[ ar_wal_tx_send.c : 7915 ] post_user_data: tid_num %d sw_retry_failure %d ppdu_flags_ext2 %x 
2899,II,[ ar_wal_tx_send.c : 17933 ] peer:%p, tid:16/SSN:16 0x%08x 
2898,II,[ ar_wal_tx_send.c : 17939 ] peer:%p, PN=%X 
2897,I,[ ar_wal_tx_send.c : 5925 ] legacy frame with HT-ctrl not allowed if QPEER_ALLOW_DATA, tid=%x 
2896,I,[ ar_wal_tx_send.c : 5928 ] legacy frame with HT-ctrl, tid=%x 
2895,IIIIIIIII,[ ar_wal_tx_send.c : 14384 ] TXPPDU_0 peerid_tidnum_hwq:0x%08x ppdu_id:0x%08x tstamp:0x%08x%08x dur:%5u sw_sched_id__mpdutried__failed:0x%08x mcs_nss_bw_pream:0x%08x seqnum__sifs__sch:0x%08x tries__fes__flush:0x%08x 
2894,IIIII,[ ar_wal_tx_send.c : 14400 ] TXPPDU_1_064 ssn__basn:0x%08x enq_bitmap:%08x_%08x compl_bitmap:%08x_%08x 
2893,IIIIIIIII,[ ar_wal_tx_send.c : 14414 ] TXPPDU_1_256 ssn__basn:0x%08x compl_bitmap:%08x_%08x_%08x_%08x_%08x_%08x_%08x_%08x 
2892,IIIIIIIII,[ ar_wal_tx_send.c : 14462 ] TXPPDU_2 sched_id:%08x sch_flg:%08x swppdu_flg:%08x msdu_mpdu:%08x tpc_lb1_lb0_cmndpwr1_pwr0:%08x cca_cycle:%08x txrx_frm:%08x pwrsurge_timestmp_size1cnt_rssi:%08x pad1_ani_cck_ofdma_leg_ovs_abort_crc:%08x 
2891,III,[ ar_wal_tx_send.c : 18963 ] pdev:%u, RING(%x) pause WAR triggered(%x) 
2890,iiIiiiiII,[ ar_wal_tx_send.c : 14628 ] twt_dbg: update_dl_stats txqid=%d, sched_id=%d, ftype=%u, tx_status=%d, queued=%d, tried=%d, failed=%d,sched_ref_time_start=%u, sched_ref_time_end=%u 
 
2889,IIIII,[ ar_wal_tx_send.c : 14655 ] twt_dbg_leak: update_dl_stats: start_tsTstamp=%u, duration_us=%u, sch_eval_end_ts=%u, twt_sp_end=%u, offset_tsf2=%u 
 
2888,I,[ ar_wal_tx_send.c : 14659 ] twt_dbg_leak: update_dl_stats twt_sp leakage detected by %u us 
2887,iiiIII,[ ar_wal_tx_send.c : 14690 ] twt_dbg_leak_ul: update_ul_stats: txqid=%d, sched_id=%d, tx_sw_status=%d, fes_start=%u, fes_end=%u, fes_duration=%u,  
2886,IIII,[ ar_wal_tx_send.c : 14725 ] twt_dbg_leak_ul: update_ul_stats: sch_eval_start_ts=%u, sch_eval_end_ts=%u, twt_sp_end=%u, offset_tsf2=%u 
 
2885,I,[ ar_wal_tx_send.c : 14729 ] twt_dbg_leak_ul: update_ul_stats twt_sp leakage detected by %u us 
2884,IIIIIIII,[ ar_wal_tx_send.c : 12663 ] update_hw_wmm_params: ac:%x,ul_resp=%x,txqid=%x,cw_min/cw_max:%x,aifs:%x,type=%x,txop_limit=%x %x 
2883,iIi,[ ar_wal_tx_send.c : 2244 ] update pdev(%d) vdev(%p) wmm params, type=%d 
2924,,[ ar_wal_tx_seq.c : 3703 ] CW reset 
2938,ii,[ ar_wal_tx_halphy_send.c : 1042 ] PAPRD: Entering halphy_schedule_mem_dpd_post_processing(); PHY Id %d g_edpd_rt_thread_id %d 
2937,iii,[ ar_wal_tx_halphy_send.c : 1049 ] PAPRD: eDPD thread ID %d BG thread status %d start time %d 
2936,iiii,[ ar_wal_tx_halphy_send.c : 1078 ] PAPRD: halphy_signal_mem_dpd_post_processing_complete: PHY id %d BG thread status %d, thread_id %d rt_thread_id %d 
2935,,[ ar_wal_tx_halphy_send.c : 1080 ] PAPRD: halphy_signal_mem_dpd_post_processing_complete: exit() 
2934,iI,[ ar_wal_tx_halphy_send.c : 1094 ] PAPRD: halphy_start_mem_dpd_post_processing() Entering thread_id %d pHandle 0x%x 
2933,,[ ar_wal_tx_halphy_send.c : 625 ]  HALPHY_TX_TBTT_FLUSH : DPD packet is flushed out  
2932,,[ ar_wal_tx_halphy_send.c : 634 ]  HALPHY_TX_ABORT : DPD packet is  aborted 
2931,,[ ar_wal_tx_halphy_send.c : 728 ]  tx_send_halphy_abort_ppdu : DPD packet is  aborted 
2930,i,[ ar_wal_tx_halphy_send.c : 246 ] PAPRD dpd start tlv event : start evt latency %d 
2929,i,[ ar_wal_tx_halphy_send.c : 1242 ]  wal_check_ppdu_status DPD ppdu is stuck in the hardware queue %d 
2928,i,[ ar_wal_tx_halphy_send.c : 1228 ]  thread id %d 
2927,i,[ ar_wal_tx_halphy_send.c : 1109 ] PAPRD: wal_mem_dpd_rt_exchange received %d  
2926,ii,[ ar_wal_tx_halphy_send.c : 1140 ] PAPRD: wal_mem_dpd_thread_hdlr phyId %d, thread_id %d 
2925,iiiii,[ ar_wal_tx_halphy_send.c : 899 ] PAPRD Total PHY OFF %d Tx suspend fail %d Rx suspend fail %d Tx suspend %d, Tx suspend %d 
2939,iI,[ ar_wal_tx_flush.c : 435 ] _wal_peer_flush_tids: send msg to SCHED_ALGO, thread_id =%d tid_bitmap=0x%x
 
2942,,[ fips_unit_test.c : 115 ] FIPS_UINT_TEST pass 
2941,,[ fips_unit_test.c : 117 ] FIPS_UINT_TEST fail 
2940,IIIIIIII,[ fips_unit_test.c : 131 ] FIPS DATA: %08x%08x%08x%08x%08x%08x%08x%08x 
2945,II,[ ar_wal_tx_send_isr.c : 3130 ] too many page fault: page fault begin count =0x%x, page fault end count =0x%x 
2944,i,[ ar_wal_tx_send_isr.c : 504 ] TX_IST_TRIGGER RECEIVED %d
 
2943,iIII,[ ar_wal_tx_send_isr.c : 2432 ] WAR ring-paused: pdev=%d, sched_id=%x, hp=%x, tp=%x 
2952,iiiiiiiii,[ tx_cong_ctrl.c : 278 ] CONGCTRL FW_CONTROL *OVERRIDE* peer_id:%d tid_num:%d traffic_enq:%d drop:%d deq:%d tot_deq:%d rate_max_allowed:%d old_threshold:%d max_extra:%d 
2951,iiiiiiiii,[ tx_cong_ctrl.c : 291 ] CONGCTRL FW_CONTROL *DISABLED* peer_id:%d tid_num:%d traffic_enq:%d drop:%d deq:%d tot_deq:%d rate_max_allowed:%d old_threshold:%d max_extra:%d 
2950,iIiiiiiii,[ tx_cong_ctrl.c : 307 ] CONGCTRL FW_CONTROL peer_id:%d tid_num__qtype__msduq_masks:0x%08x traffic_enq:%d drop:%d deq:%d tot_deq:%d rate_max_allowed:%d old_threshold:%d max_extra:%d 
2949,iiiiii,[ tx_cong_ctrl.c : 51 ] CONG_CTRL_FD sw_pid:%d tid_num:%d buf_id:%d desc_id:%d bin_idx:%d cur:%d 
2948,iii,[ tx_cong_ctrl.c : 69 ] CONG_CTRL_DiscD sw_pid:%d tid_num:%d buf_id:%d 
2947,iiiiii,[ tx_cong_ctrl.c : 57 ] CONG_CTRL_AD sw_pid:%d tid_num:%d buf_id:%d desc_id:%d bin_idx:%d cur:%d 
2946,iii,[ tx_cong_ctrl.c : 63 ] CONG_CTRL_DropD sw_pid:%d tid_num:%d buf_id:%d 
2965,,[ ar_wal_txbf.c : 1395 ] WAL_POWER_STATE_FULL_SLEEP 
2964,,[ ar_wal_txbf.c : 1422 ] WAL_POWER_STATE_AWAKE 
2963,IIII,[ ar_wal_txbf.c : 1260 ] txbf_peer_setup:Peer_caps VHT:SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2962,IIII,[ ar_wal_txbf.c : 1268 ] txbf_peer_setup:Peer_caps HE :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2961,IIII,[ ar_wal_txbf.c : 1276 ] txbf_peer_setup:Vdev_caps VHT :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2960,IIII,[ ar_wal_txbf.c : 1284 ] txbf_peer_setup:Vdev_caps HE :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2959,II,[ ar_wal_txbf.c : 1303 ] txbf_peer_setup:Txbfer:0x%x and txbfee count:0x%x 
2958,IIII,[ ar_wal_txbf.c : 555 ] txbf_peer_teardown:Peer_caps VHT :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2957,IIII,[ ar_wal_txbf.c : 563 ] txbf_peer_teardown:Peer_caps HE :SU:bfee=%x,bfer=%x MU:Bfee=%x,bfer=%x 
2956,III,[ ar_wal_txbf.c : 578 ] txbf_peer_setup:vdev %x Txbfer:0x%x and txbfee count:0x%x 
2955,iI,[ ar_wal_txbf.c : 1369 ] wal_txbf_update_txbfee_filter:en:%d,txbfee_dis_bitmap:0x%x 
2954,iI,[ ar_wal_txbf.c : 1320 ] wal_txbfee_set_disable_ndpa_for_rogue_ap enable = %d, rfilt = 0x%x 
2953,ii,[ ar_wal_txbf.c : 946 ] PHY set gid:%d, pos:%d 
2966,I,[ whal_coex.c : 423 ] WHAL_COEX_PHY_IDLE: Invalid WLAN id(%u) 
2969,IIIIiIIII,[ whal_mci.c : 1021 ] WAL_COEX_CONT_INFO: INFO|NACK|RST|TX[0x%x]: Prio(%u), LinkId(%u) Ch(%u) Rssi_pwr(%d) btClock|priIdx[0x%x] nack_wght(%u) PT|JO|FRAB|POT[0x%x] po_bm(0x%x)  
2968,ii,[ whal_mci.c : 204 ] BTCOEX_DBG_MCI_2: Coex Band setting. WLAN1(%d),  WLAN2(%d)
 
2967,I,[ whal_mci.c : 490 ] COEX_GENERIC_ERROR: MCIIntfTimeout(%u) 
2971,ii,[ whal_mws_tx_grant.c : 126 ] WHAL_MWS_TX_GRANT:[Get] wlan=%d, result=%d 
2970,iIII,[ whal_mws_tx_grant.c : 104 ] WHAL_MWS_TX_GRANT:WLAN=%d, ctrl_value=0x%x, threshold1=0x%x, threshold2=0x%x 
2978,iiiii,[ whal_mws_utils.c : 128 ] COEX_MWS_OTHER: print_wci2_cnt : Time:%d,T1_Send_Cnt(Curr:%d,Total:%d),T3_Send_CnT(Curr:%d,Total:%d) 
2977,I,[ whal_mws_utils.c : 465 ] WHAL_MWS_MAC:band mac map=0x%x 
2976,I,[ whal_mws_utils.c : 618 ] COEX_MWS_RAT_ID: WLAN_1_RAT_ID=%u  
2975,I,[ whal_mws_utils.c : 620 ] COEX_MWS_RAT_ID: WLAN_2_RAT_ID=%u  
2974,iiiii,[ whal_mws_utils.c : 155 ] COEX_MWS_OTHER: Reg_Restore : event_id:%d, write_ptr:%d Currtime:%d,T1_Send_Cnt(Curr:%d,Total:%d) 
2973,iiI,[ whal_mws_utils.c : 113 ] WHAL_MWS_TPC:[Get]mac_id=%d, tpc=%d, status=0x%x 
2972,iiiI,[ whal_mws_utils.c : 82 ] WHAL_MWS_TPC:[Set]2G tpc=%d, 5G tpc=%d, 6G tpc=%d, status=0x%x 
2989,I,[ whal_mws_wci2.c : 116 ] WHAL_MWS_WCI2_DIRMSG_SEND:data=0x%x 
2988,,[ whal_mws_wci2.c : 121 ] WHAL_MWS_WCI2_DIRMSG_SEND:Trigger bit is not zero 
2987,i,[ whal_mws_wci2.c : 139 ] WHAL_MWS_WCI2_DIRMSG_SEND:out of retry count =%d 
2986,I,[ whal_mws_wci2.c : 627 ] COEX_MWS_ERROR:  [Err] received invalid Uart clock value: %u 
2985,IIII,[ whal_mws_wci2.c : 450 ] WHAL_MWS_INTERRUPT:intr1=0x%x, intr2=0x%x, intr3=0x%x, intr_type7=0x%x 
2984,I,[ whal_mws_wci2.c : 417 ] WHAL_MWS_WCI2_TYPE0:RX raw data=0x%x 
2983,I,[ whal_mws_wci2.c : 401 ] WHAL_MWS_WCI2_TYPE3:RX raw data=0x%x 
2982,I,[ whal_mws_wci2.c : 378 ] WHAL_MWS_WCI2_TYPE4:RX raw data=0x%x 
2981,I,[ whal_mws_wci2.c : 362 ] WHAL_MWS_WCI2_TYPE5:RX raw data=0x%x 
2980,I,[ whal_mws_wci2.c : 346 ] WHAL_MWS_WCI2_TYPE6:RX raw data=0x%x 
2979,I,[ whal_mws_wci2.c : 330 ] WHAL_MWS_WCI2_TYPE7:RX raw data=0x%x 
2999,Iii,[ whal_mws_wci2_tdm.c : 118 ] WHAL_MWS_WCI2_TYPE2:[RX]byte=0x%x, depth=%d, valid=%d 
2998,I,[ whal_mws_wci2_tdm.c : 72 ] WHAL_MWS_WCI2_TYPE2:[Tx]byte=0x%x 
2997,,[ whal_mws_wci2_tdm.c : 78 ] WHAL_MWS_WCI2_TYPE2:[Tx]flush FIFO 
2996,,[ whal_mws_wci2_tdm.c : 83 ] WHAL_MWS_WCI2_TYPE2:[Tx] FIFO over flow 
2995,iIii,[ whal_mws_wci2_tdm.c : 184 ] WHAL_MWS_WCI2_TYPE2:[POR=  0][1]Valid:%d,temp_data:0x%x,(%d),init_depth:%d 
2994,iIiii,[ whal_mws_wci2_tdm.c : 201 ] WHAL_MWS_WCI2_TYPE2:[POR=  1][2]Valid:%d,data:0x%x,(%d),depth:%d,init_depth:%d 
2993,iIiii,[ whal_mws_wci2_tdm.c : 218 ] WHAL_MWS_WCI2_TYPE2:[POR=  0][3]Valid:%d,data:0x%x,(%d),depth:%d,init_depth:%d 
2992,iIiii,[ whal_mws_wci2_tdm.c : 239 ] WHAL_MWS_WCI2_TYPE2:[POR=1-0][4]Valid:%d,data:0x%x,(%d),depth:%d,init_depth:%d 
2991,iIii,[ whal_mws_wci2_tdm.c : 261 ] WHAL_MWS_WCI2_TYPE2:[POR=  0][5]Valid:%d,temp_data:0x%x,(%d),init_depth:%d 
2990,iI,[ whal_mws_wci2_tdm.c : 274 ] WHAL_MWS_WCI2_TYPE2:[Warn] Buffer Underflow :Read after delay: init_depth:%d, Data:0x%x 
3002,i,[ whal_coex_init_ext.c : 256 ] En Soft Abort %d 
3001,IIii,[ whal_coex_init_ext.c : 273 ] Flex Req Param                                                          FlushBmap 0x%x                                                          TidBmap   0x%x                                                          CCATimeout%d                                                          MaxReqLim %d 
3000,iiiii,[ whal_coex_init_ext.c : 410 ] WHAL_MWS_INIT:ratid_enable=%d, lte_rat0=%d, lte_rat1=%d, wlan1_rat=%d, wlan2_rat=%d 
3006,,[ whal_coex_gpm.c : 252 ] ERROR_COEX_MCI_GPM: invalid GPM 
3005,II,[ whal_coex_gpm.c : 261 ] ERROR_COEX_MCI_GPM: Drop GPM, Recovery in progress: SWGpmIndex(%u) NumGPM(%u) 
3004,II,[ whal_coex_gpm.c : 162 ] ERROR_COEX_MCI_GPM: Drop GPM, Recovery in progress: SWGpmIndex(%u) NumGPM(%u) 
3003,I,[ whal_coex_gpm.c : 79 ] ERROR_COEX_MCI_GPM: ERROR - MCI Init is NOT complete ! Dropping GPM - 0x%x 
3009,I,[ whal_coex_smh.c : 69 ] WHAL_COEX_SMH_ISR: Error(0x%x) 
3008,I,[ whal_coex_smh.c : 158 ] WHAL_COEX_SMH_HNDLR: Error(0x%x) 
3007,,[ whal_coex_smh.c : 83 ] NULL: Buffers not allocated 
3014,,[ whal_coex_bmh.c : 108 ] COEX_MCI_ISR_IntRaw: BMH ISR overflow 
3013,IIIIIII,[ whal_coex_bmh.c : 125 ] WHAL_COEX_BMH_ISR: Tx(%u) Rx(%u) BmhIntRaw(0x%x) BmhRxMsgRaw(0x%x) BmhInt1Raw(0x%x) invalid_hdr(%u) cont_info_to(%u) 
3012,I,[ whal_coex_bmh.c : 408 ] WHAL_COEX_BMH_HNDLR: Error(0x%x) 
3011,III,[ whal_coex_bmh.c : 507 ] WAL_COEX_SCHED_INFO: sched_info start 0x%x, stop 0x%x wbts 0x%x 
3010,IIIIiII,[ whal_coex_bmh.c : 517 ] WAL_COEX_SCHED_INFO: i=%u Prio(%u) Tag(%u) tx(%u) Txp(%d) Link(%u) Dur(%u) 
3017,iii,[ whal_coex_lmh.c : 49 ] COEX_LNA_LOCK_INFO: gain_idx = %d, lna_in_use= %d, lna_bt_lock= %d 
3016,,[ whal_coex_lmh.c : 52 ] COEX_MCI_ISR_IntRaw: LMH ISR overflow 
3015,I,[ whal_coex_lmh.c : 92 ] WHAL_COEX_LMH_HNDLR: Error(0x%x) 
3019,I,[ whal_coex_mcim.c : 68 ] COEX_MCIM_ISR: Error(0x%x) 
3018,I,[ whal_coex_mcim.c : 204 ] WHAL_COEX_MCIM_HNDLR: Error(0x%x) 
3022,,[ whal_coex_pmh.c : 80 ] COEX_MCI_ISR_IntRaw: PMH ISR overflow 
3021,I,[ whal_coex_pmh.c : 120 ] WHAL_COEX_PMH_ERR: err(0x%x) 
3020,,[ whal_coex_pmh.c : 541 ] BTCOEX_DBG_MCI_2: Trying to power up. due to POWERUP_FAILURE, return 
 
3025,,[ whal_coex_recipes.c : 46 ] BTCOEX_DBG_MCI_2: Calling cxc power down
 
3024,ii,[ whal_coex_recipes.c : 151 ] BTCOEX_DBG_MCI_2: _whal_mci_powerup Power up wmac%d, and band is %dG
 
3023,ii,[ whal_coex_recipes.c : 172 ] BTCOEX_DBG_MCI_2: _whal_mci_powerup Power up wmac%d, and band is %dG
 
3027,ii,[ whal_debug.c : 5794 ] config_reg_dump: Entries exceeded MAX REG DUMP ENTRY :%d! :%d 
 
3026,I,[ whal_debug.c : 5799 ] config_reg_dump: Invalid register physical address! :0x%x 
 
3034,II,[ whal_hwsch.c : 3728 ] hwsch2_wdog_timeout: reg_wdog=%x, reg_cmd_ring_wdog=%x 
3033,III,[ whal_hwsch.c : 3971 ] val_0=%x, val_1=%x, val_2=%x 
3032,I,[ whal_hwsch.c : 4114 ] WHAL_FATAL_ERR_UNKNOWN:%x 
3031,i,[ whal_hwsch.c : 4128 ] WHAL_FATAL_ERR_UNKNOWN: pdev_id:%d - Ignore, since wdog statuses got cleared 
3030,II,[ whal_hwsch.c : 3920 ] cca_watchdog=%x, reg_axi_err=%x 
3029,II,[ whal_hwsch.c : 3965 ] ul-q(%i), reg:%x 
3028,iiIii,[ whal_hwsch.c : 4736 ] config_txop_sel (pdev=%d,q=%d): reg=0x%x, lifetime_exp=%d, txop_sel=%d 
3042,,[ whal_umac_cmn.c : 1152 ] poll UMCMN_R1_UMAC_IDLE/UMAC_IDLE_GEN_MOD_BUSY timeout
 
3041,,[ whal_umac_cmn.c : 1167 ] poll UMCMN_R1_UMAC_IDLE_GEN_INTF_STATUS/VALUE timeout
 
3040,,[ whal_umac_cmn.c : 1320 ] poll UMCMN_R1_UMAC_IDLE_GEN_INTF_STATUS/VALUE timeout
 
3039,,[ whal_umac_cmn.c : 1332 ] poll UMCMN_R1_UMAC_IDLE_GEN_INTF_STATUS/VALUE timeout
 
3038,I,[ whal_umac_cmn.c : 1340 ] whal_umac_request_individual_module_idle: before CONSUMER reset 0x%x 
3037,I,[ whal_umac_cmn.c : 1345 ] whal_umac_request_individual_module_idle: after CONSUMER reset 0x%x 
3036,I,[ whal_umac_cmn.c : 1367 ] whal_umac_request_individual_module_idle: before CONSUMER set 0x%x 
3035,I,[ whal_umac_cmn.c : 1372 ] whal_umac_request_individual_module_idle: after CONSUMER set 0x%x 
3044,II,[ whal_interrupt.c : 993 ] Clear false RXPCU WDOG, status %x, limit %x 
3043,I,[ whal_interrupt.c : 1709 ] GetPendingInterrupts-whalPending:0x%x 
3045,IIIII,[ whal_umac_recipe.c : 2417 ] REGDBG: 0x%x 0x%x 0x%x 0x%x 0x%x 
3045,IIIII,[ whal_umac_recipe.c : 2417 ] REGDBG: 0x%x 0x%x 0x%x 0x%x 0x%x 
3050,iiIi,[ whal_mac_rri.c : 717 ]  meta:%d tbl:%d address:0x%x dwords:%d 
3049,I,[ whal_mac_rri.c : 753 ] load_rri_tbl msk:0x%x
 
3048,,[ whal_mac_rri.c : 309 ] SFM RRI bank not empty
 
3047,,[ whal_mac_rri.c : 375 ] SFM RRI bank not empty
 
3046,,[ whal_mac_rri.c : 1004 ] RRI trigger Restore error 
 
3115,III,[ whal_wmac_recipes.c : 396 ] PMM_TOP_AON INT EN:0x%x STAT:0x%x RAW_STAT:0x%x 
3114,II,[ whal_wmac_recipes.c : 399 ] PMM_TOP_AON SM_CTL:0x%x SLP_TMR_CTL:0x%x 
3113,IIII,[ whal_wmac_recipes.c : 404 ] PMM_TOP_AON_SLP_TMR_VAL LO:0x%x HI:0x%x G_LO:0x%x G_HI:0x%x 
3112,IIII,[ whal_wmac_recipes.c : 411 ] PMM_TOP_WLAN1_SLP_TMR CTL:0x%x STS:0x%x EXP_LO:0x%x EXP_HI:0x%x 
3111,II,[ whal_wmac_recipes.c : 414 ] WFSS_PMM_WLAN1 H2S:0x%x CFG_REG1:0x%x 
3110,II,[ whal_wmac_recipes.c : 417 ] WFSS_PMM_WLAN1_NEXT_WAKEUP_TIME L:0x%x U:0x%x 
3109,II,[ whal_wmac_recipes.c : 420 ] WFSS_PMM_WLAN1_NEXT_WAKEUP_TIME_TO_AON L:0x%x H:0x%x 
3108,IIII,[ whal_wmac_recipes.c : 428 ] PMM_TOP_WLAN2_SLP_TMR CTL:0x%x STS:0x%x EXP_LO:0x%x EXP_HI:0x%x 
3107,II,[ whal_wmac_recipes.c : 431 ] WFSS_PMM_WLAN2 H2S:0x%x CFG_REG1:0x%x 
3106,II,[ whal_wmac_recipes.c : 434 ] WFSS_PMM_WLAN2_NEXT_WAKEUP_TIME L:0x%x U:0x%x 
3105,II,[ whal_wmac_recipes.c : 437 ] WFSS_PMM_WLAN2 NEXT_WAKEUP_TIME_TO_AON L:0x%x H:0x%x 
3104,IIIIIIII,[ whal_wmac_recipes.c : 497 ] testbus dump: 10: 0x%x, 0x%x, 11: 0x%x 0x%x, 12: 0x%x, 0x%x, 13 0x%x, 0x%x 
3103,IIIIIIII,[ whal_wmac_recipes.c : 511 ] testbus dump: 14: 0x%x, 0x%x, 15: 0x%x 0x%x, 16: 0x%x, 0x%x, 17: 0x%x, 0x%x 
3102,iI,[ whal_wmac_recipes.c : 2674 ] SOC retention setting: enable %d, WLAON_SOC_POWER_CTRL 0x%x 
3101,ii,[ whal_wmac_recipes.c : 1532 ] bcn_cnt:%d, bmiss_cnt:%d 
3100,IIIIIIII,[ whal_wmac_recipes.c : 1539 ] b:0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
3099,ii,[ whal_wmac_recipes.c : 148 ] whal_wmac_clr_rogue_ap_type_by_mask: rogue_ap_bit_mask[%d]: %d 
3098,ii,[ whal_wmac_recipes.c : 1854 ] mac%d: enter DTIM NREM success, timestamp %d 
3097,ii,[ whal_wmac_recipes.c : 1863 ] mac%d: enter IMPS NREM success, timestamp %d 
3096,,[ whal_wmac_recipes.c : 1883 ] fw assisted sleep power config failed
 
3095,,[ whal_wmac_recipes.c : 1889 ] fw assisted sleep rri config failed
 
3094,,[ whal_wmac_recipes.c : 1895 ] fw assisted sleep power sequence failed
 
3093,I,[ whal_wmac_recipes.c : 1765 ] MAC power down failed, stuck in WAKE state due to pending WAKEUP INTR %x
 
3092,ii,[ whal_wmac_recipes.c : 1783 ] mac:%d enter HW-DTIM success, current timestamp %d
 
3091,i,[ whal_wmac_recipes.c : 1789 ] mac:%d enter SW-DTIM success
 
3090,,[ whal_wmac_recipes.c : 1806 ] poll failed, PMM WLAN not in WLAN OFF status
 
3089,i,[ whal_wmac_recipes.c : 1811 ] mac:%d enter IMPS success
 
3088,,[ whal_wmac_recipes.c : 1685 ] MAC_RRI_CONFIGURATION failed
 
3087,,[ whal_wmac_recipes.c : 1693 ] Loading RRI table failed
 
3086,Ii,[ whal_wmac_recipes.c : 1571 ] MCMN_R0_MCMN_MAC_IDLE 0x%x, phyon %d 
3085,ii,[ whal_wmac_recipes.c : 1613 ] mac:%d full wake success, current timestamp %d
 
3084,i,[ whal_wmac_recipes.c : 1133 ] dtim_synth_in_use:%d 
3083,I,[ whal_wmac_recipes.c : 1060 ] dtim_rx_chain_mask 0x%x
 
3082,IIII,[ whal_wmac_recipes.c : 449 ] S5:0x%x S4:0x%x S2:0x%x S6:0x%x 
3081,II,[ whal_wmac_recipes.c : 452 ] tsf:0x%x next_tbtt:0x%x 
3080,II,[ whal_wmac_recipes.c : 455 ] RXPCU EBT_DEBUG:0x%x TBTT_BITMAP0:0x%x 
3079,III,[ whal_wmac_recipes.c : 459 ] RXPCU_R1_PHY_INTF_TLV PHYRX_RSSI_LEGACY_CNT:0x%x PHYRX_PKT_END_CNT:0x%x RCVD:0x%x 
3078,III,[ whal_wmac_recipes.c : 463 ] TXPCU_DEBUG_RX_MESSAGE_COUNT 0:0x%x 1:0x%x 2:0x%x 
3077,IIII,[ whal_wmac_recipes.c : 468 ] MCMN_MAC_IDLE:0x%x, RXPCU_FSM_STATUS 0:0x%x 1:0x%x, 2:0x%x 
3076,iIii,[ whal_wmac_recipes.c : 706 ] H2S_TO mac:%d pmm:0x%x dur:%d slp_itl:%d 
3075,iIii,[ whal_wmac_recipes.c : 847 ] H2S_GNT mac:%d pmm:x%x dur:%d max:%d 
3074,Ii,[ whal_wmac_recipes.c : 366 ] PMM state check state=0x%x poll_cnt=%d 
3073,i,[ whal_wmac_recipes.c : 382 ] PMM state check poll_cnt=%d 
3072,i,[ whal_wmac_recipes.c : 1447 ] mac:%d enter HW-DTIM/IMPS fail
 
3071,iI,[ whal_wmac_recipes.c : 589 ] Polling H2S_GRANT_ISSUED failed. mac:%d DEBUG_RX_MESSAGE_COUNT0 0x%x 
3070,II,[ whal_wmac_recipes.c : 598 ] phy off check: MAC_IDLE 0x%x, RXPCU_SFM_STATUS0 0x%x 
3069,ii,[ whal_wmac_recipes.c : 125 ] whal_wmac_robe_clock_config: whal_bw %d bw %d
 
3068,,[ whal_wmac_recipes.c : 552 ] phy off failed 
3067,iii,[ whal_wmac_recipes.c : 1171 ] mac:%d active_phy_config time %d pf %d 
 
3066,iii,[ whal_wmac_recipes.c : 1208 ] mac:%d dtim_phy_config time %d pf %d
 
3065,ii,[ whal_wmac_recipes.c : 1249 ] mac:%d Number of chains %d 
 
3064,ii,[ whal_wmac_recipes.c : 1254 ] mac:%d RSSI Indication Hi/Lo %d 
 
3063,ii,[ whal_wmac_recipes.c : 168 ] whal_wmac_set_rogue_ap_type: rogue_ap_bit_mask[%d]: %d 
3062,IIII,[ whal_wmac_recipes.c : 637 ] sfm full check: 0x%x, 0x%x, 0x%x, 0x%x 
3061,i,[ whal_wmac_recipes.c : 1474 ] mac:%d immediate grant
 
3060,,[ whal_wmac_recipes.c : 1480 ] MAC RRI restore error
 
3059,ii,[ whal_wmac_recipes.c : 1510 ] mac:%d enter partial awake success, current timestamp %d
 
3058,,[ whal_wmac_recipes.c : 986 ] IMPS Sleep Aborted due to stop wlan_ss fail
 
3057,,[ whal_wmac_recipes.c : 880 ] Sleep Aborted due to close to next TBTT
 
3056,,[ whal_wmac_recipes.c : 907 ] Sleep Aborted due to stop wlan_ss fail
 
3055,iii,[ whal_wmac_recipes.c : 914 ] mac:%d Duration of sleep= %d current timestamp %d
 
3054,,[ whal_wmac_recipes.c : 932 ] Sleep Aborted due to close to next TBTT
 
3053,,[ whal_wmac_recipes.c : 959 ] Sleep Aborted due to stop wlan_ss fail
 
3052,iii,[ whal_wmac_recipes.c : 967 ] mac:%d Duration of sleep= %d current timestamp %d
 
3051,I,[ whal_wmac_recipes.c : 1910 ] MAC:%u WDOG bite error
 
3187,ii,[ whal_power_config_seq.c : 1160 ] mac:%d sleep_time_us:%d
 
3186,,[ whal_power_config_seq.c : 1104 ] poll IDLE timeout
 
3185,I,[ whal_power_config_seq.c : 1364 ] WLAN1_NEXT_WAKEUP_TIME_L:0x%x
 
3184,I,[ whal_power_config_seq.c : 1368 ] PMM_WLAN_BACKOFF_TIME:0x%x
 
3183,I,[ whal_power_config_seq.c : 1458 ] WLAN2_NEXT_WAKEUP_TIME_L:0x%x
 
3182,I,[ whal_power_config_seq.c : 1462 ] PMM_WLAN_BACKOFF_TIME:0x%x
 
3181,I,[ whal_power_config_seq.c : 764 ] WFSS_PMM_R2_WLAN1_STATUS_REG1:0x%x
 
3180,I,[ whal_power_config_seq.c : 767 ] WFSS_PMM_R2_WLAN2_STATUS_REG1:0x%x
 
3179,I,[ whal_power_config_seq.c : 770 ] WCSS_CC_WCSS_WLAN1_GDSCR:0x%x
 
3178,I,[ whal_power_config_seq.c : 773 ] WCSS_CC_WCSS_WLAN2_GDSCR:0x%x
 
3177,I,[ whal_power_config_seq.c : 776 ] WFSS_PMM_R2_WLAN1_POWER_SWITCH_CTL:0x%x
 
3176,I,[ whal_power_config_seq.c : 779 ] WFSS_PMM_R2_WLAN2_POWER_SWITCH_CTL:0x%x
 
3175,I,[ whal_power_config_seq.c : 782 ] WFSS_PMM_R0_PMM_WLAN1_CFG_REG1:0x%x
 
3174,I,[ whal_power_config_seq.c : 785 ] WFSS_PMM_R0_PMM_WLAN2_CFG_REG1:0x%x
 
3173,I,[ whal_power_config_seq.c : 938 ] WFSS_PMM_R2_WLAN1_STATUS_REG1:0x%x
 
3172,I,[ whal_power_config_seq.c : 941 ] WFSS_PMM_R2_WLAN2_STATUS_REG1:0x%x
 
3171,I,[ whal_power_config_seq.c : 944 ] WCSS_CC_WCSS_WLAN1_GDSCR:0x%x
 
3170,I,[ whal_power_config_seq.c : 947 ] WCSS_CC_WCSS_WLAN2_GDSCR:0x%x
 
3169,I,[ whal_power_config_seq.c : 950 ] WFSS_PMM_R2_WLAN1_POWER_SWITCH_CTL:0x%x
 
3168,I,[ whal_power_config_seq.c : 953 ] WFSS_PMM_R2_WLAN2_POWER_SWITCH_CTL:0x%x
 
3167,I,[ whal_power_config_seq.c : 956 ] WFSS_PMM_R0_PMM_WLAN1_CFG_REG1:0x%x
 
3166,I,[ whal_power_config_seq.c : 959 ] WFSS_PMM_R0_PMM_WLAN2_CFG_REG1:0x%x
 
3165,,[ whal_power_config_seq.c : 1014 ] poll RRI_RESTORE timeout
 
3164,,[ whal_power_config_seq.c : 1065 ] poll IDLE timeout
 
3163,II,[ whal_power_config_seq.c : 1249 ] ISR_P:0x%x ISR_S5:0x%x
 
3162,II,[ whal_power_config_seq.c : 1319 ] ISR_P:0x%x ISR_S5:0x%x
 
3161,iI,[ whal_power_config_seq.c : 285 ] mac:%d rx_filter:0x%x
 
3160,III,[ whal_power_config_seq.c : 3381 ] RXPCU_FSM_STATUS 0/1/2: 0x%x, 0x%x, 0x%x 
3159,III,[ whal_power_config_seq.c : 3386 ] MAC_IDLE: 0x%x EBT_DEBUG 0x%x SFM_ERROR_STATUS 0x%x 
3158,iii,[ whal_power_config_seq.c : 147 ] mac:%d ebt_en:%d thres:%d
 
3157,ii,[ whal_power_config_seq.c : 1743 ] DmaLeakDetect mac:%d t:%d
 
3156,ii,[ whal_power_config_seq.c : 1757 ] DmaLeakRecovery mac:%d t:%d
 
3155,iIII,[ whal_power_config_seq.c : 612 ] mac: %d flag: 0x%x next_wakeup: 0x%08x_%08x
 
3154,IIII,[ whal_power_config_seq.c : 616 ] next_tbtt: 0x%08x_%08x curr_tsf: 0x%08x_%08x
 
3153,iII,[ whal_power_config_seq.c : 619 ] sleep_slop: %d beaconPeriod: 0x%08x_%08x
 
3152,Ii,[ whal_power_config_seq.c : 2260 ] get_seq_latency msk:0x%x total:%d
 
3151,iIII,[ whal_power_config_seq.c : 3549 ] MAC:%d PMM_WDOG_CHK EN:0x%x CNT:0x%x EXP_STS:0x%x 
3150,I,[ whal_power_config_seq.c : 3206 ] PMM_AON_INT_STAT: 0x%x 
3149,I,[ whal_power_config_seq.c : 3221 ] WD Bite Slp ticks %x too large 
3148,I,[ whal_power_config_seq.c : 3240 ] WD Bite Slp ticks %x too large 
3147,iI,[ whal_power_config_seq.c : 431 ] mac:%d pmm_wlan state:0x%x
 
3146,iI,[ whal_power_config_seq.c : 444 ] mac:%d pmm_wlan state:0x%x
 
3145,ii,[ whal_power_config_seq.c : 1674 ] pmm_wlan_pwr_seq mac:%d pmm_wlan seq:%d
 
3144,iiI,[ whal_power_config_seq.c : 528 ] mac:%d h2s thres:%d ts:0x%x
 
3143,,[ whal_power_config_seq.c : 3412 ] pmm_wlan_test_bus_dump 
3142,II,[ whal_power_config_seq.c : 3420 ] A sel:0x%x sts:0x%x 
3141,II,[ whal_power_config_seq.c : 3427 ] B sel:0x%x sts:0x%x 
3140,I,[ whal_power_config_seq.c : 2708 ] APPS_AGGRE_INTR_STATUS 0x%x
 
3139,,[ whal_power_config_seq.c : 2728 ] abort LS:PHY idle fail 
3138,I,[ whal_power_config_seq.c : 2741 ] PMM WLAN MAC IDLE 0x%x
 
3137,I,[ whal_power_config_seq.c : 2744 ] MCMN MAC IDLE 0x%x
 
3136,I,[ whal_power_config_seq.c : 2753 ] APPS_AGGRE_INTR_STATUS 0x%x
 
3135,,[ whal_power_config_seq.c : 2773 ] abort LS:PHY idle fail 
3134,I,[ whal_power_config_seq.c : 2786 ] PMM WLAN MAC IDLE 0x%x
 
3133,I,[ whal_power_config_seq.c : 2789 ] MCMN MAC IDLE 0x%x
 
3132,i,[ whal_power_config_seq.c : 2566 ] mac:%d ALL PAID match has been assigned
 
3131,I,[ whal_power_config_seq.c : 3331 ] halt_rx:0x%x
 
3130,I,[ whal_power_config_seq.c : 3311 ] dma_hold:0x%x
 
3129,i,[ whal_power_config_seq.c : 1908 ] stop_wlan_ss_seq mac:%d
 
3128,I,[ whal_power_config_seq.c : 1973 ] ISR_RX_OK 0x%x
 
3127,I,[ whal_power_config_seq.c : 1980 ] ISR_SIFS_RESP 0x%x
 
3126,I,[ whal_power_config_seq.c : 1987 ] ISR_TX_OK 0x%x
 
3125,I,[ whal_power_config_seq.c : 2007 ] QDSP_AGGRE_POWER_INTR_STATUS_SET_0 0x%x
 
3124,I,[ whal_power_config_seq.c : 2014 ] QDSP_AGGRE_POWER_INTR_STATUS_SET_1 0x%x
 
3123,I,[ whal_power_config_seq.c : 2020 ] QDSP_AGGRE_FATAL_ERR_INTR_STATUS 0x%x
 
3122,I,[ whal_power_config_seq.c : 2055 ] ISR_P 0x%x
 
3121,i,[ whal_power_config_seq.c : 2102 ] turn_on_wlan_ss_seq mac:%d
 
3120,iII,[ whal_power_config_seq.c : 358 ] mac:%d int en_msk:0x%x dis_mask:0x%x
 
3119,IIII,[ whal_power_config_seq.c : 386 ] msk ISR_S5:0x%x ISR_S6:0x%x ISR_S2:0x%x ISR_RX_OK:0x%x
 
3118,ii,[ whal_power_config_seq.c : 1861 ] rxdma2reo ring check: empty fail cnt %d, stuck_cnt %d 
3117,ii,[ whal_power_config_seq.c : 1864 ] rxdma2reo ring check: empty fail duration %d, stuck duration %d 
3116,II,[ whal_power_config_seq.c : 1867 ] rxdma2reo ring check: reo2sw1 ring hptp:0x%08x reo2tcl ring hptp:0x%08x 
3189,IIi,[ lputils.c : 459 ] poll reg:0x%x for 0x%x timeout, line:%d 
3188,II,[ lputils.c : 461 ] caller:%s, reg_name:%s 
3193,ii,[ whal_retention.c : 695 ] retention_restore mac:%d cost:%dus
 
3192,ii,[ whal_retention.c : 672 ] whal_retention_save mac:%d cost:%dus
 
3191,iii,[ whal_retention.c : 426 ] whal_retention_table_restore id:%d size:%d cost:%dus
 
3190,iii,[ whal_retention.c : 331 ] whal_retention_table_save id:%d size:%d cost:%dus
 
3198,iii,[ whal_cce.c : 245 ] CCE rule no. exceed maximum: last_0 = %d, last_1 = %d, last = %d
 
3197,,[ whal_cce.c : 599 ] poll MCMN_R0_MCMN_MAC_IDLE/HWIO_MCMN_R0_MCMN_MAC_IDLE_RXOLE_BMSK timeout
 
3196,,[ whal_cce.c : 618 ] poll MCMN_R0_MCMN_ISR_S17/RX_PPDU_END timeout
 
3195,,[ whal_cce.c : 698 ] poll MCMN_R0_MCMN_ISR_S17/RX_PPDU_END timeout
 
3194,,[ whal_cce.c : 713 ] poll MCMN_R0_MCMN_ISR_S17/RX_CCE_SW_REQ timeout
 
3209,II,[ whal_recv.c : 9780 ] rxdma2reo_hp 0x%x rxdma2reo_hp 0x%x 
 
3208,iiI,[ whal_recv.c : 4643 ] whalEnableRSS 0xFA mac=%d en=%d flags=%x 
3207,I,[ whal_recv.c : 4645 ] whalEnableRSS 0xFB RXOLE_R0_CONFIG_REO_DESTINATION=%x 
3206,I,[ whal_recv.c : 4647 ] whalEnableRSS 0xFB RXOLE_R0_LRO=%x 
3205,III,[ whal_recv.c : 6774 ] fse_watchdog %x, sm_state_reg %x, cache_response %x 
3204,III,[ whal_recv.c : 7806 ] whalSetBssColor: parameters bsscolor|en|bss_id = %08x, caller = 0x%x:0x%x 
3203,iIIIIIII,[ whal_recv.c : 1346 ] startPcuReceive on mac:%d, phy on-%x, force_rx_abort-%x, leave_phy_off-%x,Before:TXPCU-COUNT0:0x%x, COUNT1:0x%x, COUNT2:0x%x, RXPCU-TLVBMAP:0x%x 
3202,IIIII,[ whal_recv.c : 1491 ] startPcuReceive result:0x%x, TXPCU-COUNT0:0x%x, COUNT1:0x%x, COUNT2:0x%x, RXPCU-TLVBMAP:0x%x 
3201,I,[ whal_recv.c : 9299 ] TxRx overlap TLV_READY reg_val: 0x%x
 
3200,Ii,[ whal_recv.c : 9133 ] %s: invalid lmac id %d
 
3199,,[ whal_recv.c : 9164 ] Link desc leakage due to SFM issue Jira 1206
 
3230,,[ whal_recv_recovery.c : 79 ] SW2RXDMA_BUF ring empty 
3229,,[ whal_recv_recovery.c : 122 ] FW2RXDMA_BUF ring empty 
3228,,[ whal_recv_recovery.c : 143 ] RX_RING_FW_BUF ring empty caused by RX_RING_WMI_EVT 
3227,,[ whal_recv_recovery.c : 167 ] FW2RXDMA_STATBUF ring empty 
3226,,[ whal_recv_recovery.c : 174 ] FW2RXDMA_STATBUF ring empty 
3225,,[ whal_recv_recovery.c : 199 ] WBM2RXDMA_LINK ring empty 
3224,,[ whal_recv_recovery.c : 206 ] WBM2RXDMA_LINK ring empty 
3223,,[ whal_recv_recovery.c : 231 ] FW2RXDMA_LINK ring empty 
3222,,[ whal_recv_recovery.c : 86 ] SW2RXDMA_BUF ring empty 
3221,,[ whal_recv_recovery.c : 238 ] FW2RXDMA_LINK ring empty 
3220,IIIIII,[ whal_recv_recovery.c : 382 ] ring type [0x%x] empty error ts-0x%x, pre hp:0x%x, ts 0x%x, hp 0x%x, tp 0x%x 
3219,IiI,[ whal_recv_recovery.c : 393 ] ring type [0x%x] wmi pending:%d, empty %x 
3218,,[ whal_recv_recovery.c : 115 ] FW2RXDMA_BUF ring empty 
3217,IIIIIIII,[ whal_recv_recovery.c : 516 ] ring [0x%x] full ts-0x%x, hp 0x%x, tp 0x%x, reo2sw1: 0x%x, reo2sw4:0x%x, reo2tcl:0x%x, rxdma2sw:0x%x 
3216,IiIIII,[ whal_recv_recovery.c : 1767 ] RXDMA hang type [0x%x], cnt %d, error ts-0x%x, rin type: %x, mask 0x%x:0x%x 
3215,IiIII,[ whal_recv_recovery.c : 990 ] RXOLE hang type [0x%x], cnt %d, error ts-0x%x, rin type: %x, mask 0x%x 
3214,iIii,[ whal_recv_recovery.c : 1126 ] RD_UNDERFLOW:%d, FSM_STATUS_2: 0x%x, MAC-%d rst_cnt %d 
3213,IIII,[ whal_recv_recovery.c : 1167 ] RXPCU hang type [0x%x] empty error ts-0x%x, mask 0x%x, 0x%x 
3212,IIII,[ whal_recv_recovery.c : 1893 ] RXCRYPTO hang type [0x%x] empty error ts-0x%x, mask 0x%x, 0x%x 
3211,I,[ whal_recv_recovery.c : 761 ] long_pkt_dur_us: %x 
3210,i,[ whal_recv_recovery.c : 774 ] TXRX OVLAP hit on MAC-%d 
3236,iiiii,[ whal_reset.c : 3483 ] channelSwitch: INI = %d TPC = %d Cal = %d Tot = %d PF = %d 
3235,iiiiiii,[ whal_reset.c : 3522 ] channelSwitch: Homechan = %d ANI = %d Reset_Synth_Spur = %d Cal = %d Mutex_Unlock = %d Tot = %d PF = %d 
3234,iiiiiiii,[ whal_reset.c : 3511 ] channelSwitch: Homechan = %d Mac = %d HALPHY_CLK_RESET= %d INI = %d MAC_MTU = %d TPC = %d HALPHY_SetChan = %d WHAL_XMIT = %d 
3233,ii,[ whal_reset.c : 2704 ] whalEnableDSS enable=%d client=%d 
3232,ii,[ whal_reset.c : 609 ] Retry MXI Idle recipe pending_trans %d mxi_idle %d 
3231,,[ whal_reset.c : 635 ] Retry MXI Idle recipe 
3239,,[ whal_rtt.c : 186 ] whal_rtt_frame_prepare() HW is already prepared for RTT return !!! 
3238,,[ whal_rtt.c : 319 ] whal_rtt_frame_recover() HW was not configured for RTT!!! return 
3237,iiIIiIi,[ whal_rtt.c : 138 ] whal_rtt_recv_sta_txrx_chain_handle_event: mode %d event %d tx_mask 0x%02x rx_mask 0x%02x tx_dirty %d rtt_selfgen_tx_chain_idx %u rtt_rx_chain_idx %d 
3242,iii,[ whal_cfir.c : 269 ] whal_cfir_configure: rtt %d capture_cfr %d capture_cir %d 
3241,iiI,[ whal_cfir.c : 194 ] whal_cfir_enable: enaRttPerBurst %d enaFixedStrChain %d fixedStrChainIdx 0x%02x 
3240,III,[ whal_cfir.c : 200 ] whal_cfir_enable bypass: call0 0x%x call1 0x%x call2 0x%x 
3244,I,[ whal_tqm.c : 402 ] link_Desc_tshd register value:%02x 
3243,I,[ whal_tqm.c : 412 ] link_Desc_tshd register value:%02x 
3245,II,[ whal_wbm.c : 1796 ] WBM_IDLE_BUF_RING hp:%x tp:%x 
3263,i,[ whal_xmit.c : 19981 ] NAN virtual CCA: war_enable=%d 
3262,iii,[ whal_xmit.c : 12374 ] numOfHeLtf=%d, ldpcExtraSymbol=%d, aFactor=%d 
3261,ii,[ whal_xmit.c : 12375 ] peDisambiguity=%d, packetExt=%d 
3260,ii,[ whal_xmit.c : 10794 ] InfoTPC: Max TPC = %d Min TPC = %d
 
3259,II,[ whal_xmit.c : 19729 ] FIPS hp %x tp %x 
3258,I,[ whal_xmit.c : 19747 ] FIPS nxt_p %x 
3257,,[ whal_xmit.c : 19771 ] FIPS hp null 
3256,I,[ whal_xmit.c : 19800 ] FIPS %x 
3255,,[ whal_xmit.c : 19811 ] FIPS nxt_p null 
3254,I,[ whal_xmit.c : 19839 ] FIPS %x 
3253,I,[ whal_xmit.c : 19888 ] FIPS %x 
3252,,[ whal_xmit.c : 20002 ] NAN disable CCA profiling 
3251,II,[ whal_xmit.c : 9733 ] whalSetupCbfRateParams: rate code %x, flags %x 
3250,ii,[ whal_xmit.c : 9770 ] PF4: change to force PERM=%d, rate MCS=%d 
3249,Iiiiii,[ whal_xmit.c : 8478 ] whalXmitReset: tpcchange8_cache8_samehomechan8_HomeChan8 = %x Init_ResetTxQueue = %d home_channel_cal = %d  GenRespChainMask_CCK_OFDM/resp_restore = %d Rtt_ER/misc = %d, Total = %d 
3248,II,[ whal_xmit.c : 15503 ] data-chainmask(6G band && POWER_TYPE_LPI):RC 0x%x rc_flags 0x%x 
3247,II,[ whal_xmit.c : 15912 ] Info: TPC = %u, %u
 
3246,II,[ whal_xmit.c : 14938 ] prot-chainmask(6G band && POWER_TYPE_LPI):RC 0x%x rc_flags 0x%x 
3288,Ii,[ wmi_svc.c : 711 ] WMI_CMD_RX CmdId|pf_cnt=0x%x comp_time=%dus 
3287,IIIIIIII,[ wmi_svc.c : 361 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
3286,III,[ wmi_svc.c : 372 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 
3285,IIII,[ wmi_svc.c : 375 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 
3284,IIIII,[ wmi_svc.c : 378 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
3283,IIIIII,[ wmi_svc.c : 381 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
3282,IIIIIII,[ wmi_svc.c : 384 ] WMI_CMD_PARAMS 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 0x%08x 
3281,Ii,[ wmi_svc.c : 554 ] WMI_CMD_RX CmdId=0x%x Len=%d 
3280,IIII,[ wmi_svc.c : 565 ] WMI Logging stats totl_drps=0x%x resume_cnts|suspend_cnts=0x%x apps_evt_drop=0x%x minmem_buff_drp=0x%x 
3279,I,[ wmi_svc.c : 366 ] WMI_CMD_PARAMS 0x%08x 
3278,I,[ wmi_svc.c : 579 ] WMI_SEND_EVENT_WRONG_TLV CmdId/EventId = 0x%x 
3277,I,[ wmi_svc.c : 607 ] start page log CmdId = 0x%x  
3276,I,[ wmi_svc.c : 614 ] stop page log CmdId = 0x%x  
3275,iiiIi,[ wmi_svc.c : 645 ] WMI_CMD_RX send dispatch msg to threads, cmd=%d length=%d endPt=%d, pHTCbuf=%x msg_size=%d 
3274,II,[ wmi_svc.c : 369 ] WMI_CMD_PARAMS 0x%08x 0x%08x 
3273,Ii,[ wmi_svc.c : 881 ] WMI_EVT cmplt msg RT pEvt|th_id=%p|%d 
3272,I,[ wmi_svc.c : 1860 ] WMI_EVT_SND EvtId=0x%x 
3271,I,[ wmi_svc.c : 1977 ] HIF WMI_EVT EvtId|len=0x%x 
3270,iI,[ wmi_svc.c : 1910 ] RT WMI_EVT msg EvtId==%d len|filterac=0x%x 
3269,I,[ wmi_svc.c : 1928 ]  pending EventId = 0x%x 
3268,II,[ wmi_svc.c : 1940 ] WMI_EVENT_SEND drop EventId = 0x%x, action:0x%x 
3267,iiiI,[ wmi_svc.c : 839 ] WMI_CMD_RX cmd comp. handle in hif --free buf cmd=%d length=%d endPt=%d, pHTCbuf=%x 
3266,iiiI,[ wmi_svc.c : 776 ] WMI_CMD_RX handle in BE cmd=%d length=%d endPt=%d, pHTCbuf=%x 
3265,iiiI,[ wmi_svc.c : 742 ] WMI_CMD_RX handle in data offload cmd=%d length=%d endPt=%d, pHTCbuf=%x 
3264,iiiI,[ wmi_svc.c : 810 ] WMI_CMD_RX handle in RT cmd=%d length=%d endPt=%d, pHTCbuf=%x 
3290,iii,[ evt_tracer.c : 859 ] suspend_en:%d, module %d, evt_trace_in_suspend %d 
3289,i,[ evt_tracer.c : 464 ] evt tracer init eror: send evt info by WMI return %d 
3291,i,[ hw_trc_ctrl.c : 2821 ] QDSS mode REQ ignored, g_qdss_debug_only = %d 
3293,Iii,[ platform_page_log.c : 436 ] PF ADDR:0x%X, THREAD:%d, DSR:%d 
3292,Iii,[ platform_page_log.c : 443 ] PF ADDR:0x%X, THREAD:%d, DSR:%d 
3297,,[ platform_m3.c : 1286 ] m3 elf authentication check fail.
 
3296,,[ platform_m3.c : 1201 ] m3 elf authentication check fail.
 
3295,,[ platform_m3.c : 1512 ] m3 authentication check fail.
 
3294,II,[ platform_m3.c : 1791 ] M3 DDR address = %ull, size = 0x%x 
3298,,[ platform_ce.c : 112 ] platform_ce_send_use_hif: Sending msg to HIF thread to do SYNC CE copy 
3303,,[ platform_gpio.c : 285 ] TLMM unit test: wrong num of args. 
3302,II,[ platform_gpio.c : 308 ] TLMM unit test: Op: Write, Reg: 0x%x, Value: 0x%x. 
3301,,[ platform_gpio.c : 311 ] TLMM unit test: wrong operation: read: 0, write: 1. 
3300,I,[ platform_gpio.c : 290 ] TLMM unit test: reg addr (0x%x) is out of range of TLMM. 
3299,II,[ platform_gpio.c : 300 ] TLMM unit test: Op: Read, Reg: 0x%x, Value: 0x%x. 
3319,I,[ platform_bdf_and_cal.c : 1118 ] Initiating cal download (halphy)...temp_bin = 0x%x 
3318,i,[ platform_bdf_and_cal.c : 1138 ] Cal download complete...cal file size = %d 
3317,Ii,[ platform_bdf_and_cal.c : 1188 ] Initiating cal update (halphy)...temp_bin = 0x%x | file_size = %d 
3316,,[ platform_bdf_and_cal.c : 409 ] bdf type is not elf file.
 
3315,,[ platform_bdf_and_cal.c : 423 ] bdf elf hash element may not exist.
 
3314,,[ platform_bdf_and_cal.c : 445 ] bdf elf authentication check fail.
 
3313,,[ platform_bdf_and_cal.c : 1324 ] QMI Platform: Cold Cal done signal received 
3312,,[ platform_bdf_and_cal.c : 1376 ] QMI Platform: Sending FW READY ind... 
3311,,[ platform_bdf_and_cal.c : 1390 ] QMI Platform: Sending FW READY ind... 
3310,i,[ platform_bdf_and_cal.c : 658 ] platorm_idx__download_req= %d, 
3309,i,[ platform_bdf_and_cal.c : 492 ] platorm_idx= %d, 
3308,i,[ platform_bdf_and_cal.c : 581 ] platform_proc_bdf_download_req: BDF download curr_size = %d, 
3307,i,[ platform_bdf_and_cal.c : 623 ] platform_proc_bdf_download_req: BDF download done, current_size = %d, 
3306,I,[ platform_bdf_and_cal.c : 292 ] QMI Platform: Cal download REQ received, seg_id 0x%x 
3305,i,[ platform_bdf_and_cal.c : 202 ] QMI Platform: Cal Update remaining bytes = %d, 
3304,,[ platform_bdf_and_cal.c : 1312 ] QMI Platform: Sending FW READY ind... 
3323,IIII,[ platform_npr.c : 1942 ] invalid PCIe write access to 0x%llx, BID=0x%x, PID=0x%x, MID=0x%x 
3322,IIII,[ platform_npr.c : 1946 ] invalid PCIe read access to 0x%llx, BID=0x%x, PID=0x%x, MID=0x%x 
3321,IIII,[ platform_npr.c : 1952 ] invalid PCIe write access to 0x%llx, BID=0x%x, PID=0x%x, MID=0x%x 
3320,IIII,[ platform_npr.c : 1956 ] invalid PCIe read access to 0x%llx, BID=0x%x, PID=0x%x, MID=0x%x 
3339,ii,[ platform_tsens.c : 299 ] Invalid Threshold temp hits sensor_id = %d temp = %dDeciDegC 
3338,I,[ platform_tsens.c : 618 ] TSENS_DEF_TMR_CFG_FAILED err = 0x%x 
3337,I,[ platform_tsens.c : 400 ] TSENS_DEF_TMR_ARM_FAILED err = 0x%x 
3336,iiiIiii,[ platform_tsens.c : 239 ] TSENS_CLIENT_NOTIFY thrd_id = %d, fn_id = %d, msg_evt = %d sensor_id|temp_zone = 0x%x, curr_temp = %ddegC dc = %d temp_integral = %d 
3335,ii,[ platform_tsens.c : 655 ] TSENS_CLIENT_INSTANT_TEMP_NOTIFY client_id = %d, pdev_id = %d 
3334,,[ platform_tsens.c : 1181 ] TSENS_MEMORY_ALLOC_FAILED 
3333,iiiiiiii,[ platform_tsens.c : 1199 ] TSENS_PID_GET_CONFIG temp_thresh_1|2|3 %d %d %d kp = %d, ki = %d, kd = %d, max_temp = %d sensor = %d 
3332,iII,[ platform_tsens.c : 450 ] TSENS_RECONFIG_TEMP_THRESH_FAILED err = %d, err_bit|sensor = 0x%x 0x%x 
3331,iiiiii,[ platform_tsens.c : 1228 ] TSENS_PID_SET_CONFIG algo = %d, temp_thresh_1|2 %d %d, kp = %d, ki = %d, kd = %d 
3330,iiIIiii,[ platform_tsens.c : 1064 ] TSENS_PID_DATA temp_thresh_1|2 %d %d kp|ki = 0x%x, hyst|slope_dc = 0x%x, param_id = %d, val1 = %d, val2 = %d 
3329,,[ platform_tsens.c : 1089 ] TSENS_MEMORY_ALLOC_FAILED 
3328,iIIIIIii,[ platform_tsens.c : 1130 ] TSENS_TEMP_INFO algo = %d, err_info = 0x%x 0x%x 0x%x, num_client|num_sensor = 0x%x, temp_zone|sensor_id = 0x%x, tmr_running = %d last_dc = %d 
3327,iiiiiiii,[ platform_tsens.c : 1140 ] TSENS_TEMP_OFFSET [0-7] %d %d %d %d %d %d %d %d 
3326,iiiIiI,[ platform_tsens.c : 1108 ] TSENS_PID_DATA temp_thresh_1|2|3 %d %d %d kp|ki|kd = 0x%x, max_temp = %d sensor_id|hyst|slope_dc = 0x%x 
3325,iiiiiiii,[ platform_tsens.c : 1118 ] TSENS_TEMP_DATA_DEGC [0-7] %d %d %d %d %d %d %d %d 
3324,iiiiii,[ platform_tsens.c : 1169 ] TSENS_PID_UPDATE_PARAM algo = %d, temp_thresh_1|2 %d %d, kp = %d, ki = %d, kd = %d 
3341,IIIi,[ offload_common.c : 218 ] wlan_rx_dup_chk_fail: NULL pointer passed 0x%x 0x%x 0x%x %d
 
3340,iIIII,[ offload_common.c : 248 ] wlan_rx_dup_chk_fail(%d): Dropping Duplicate Frame_info:%x Seq:%x Time:%x Last_Time:%x
 
3350,iiiiii,[ wal_powersave_ap.c : 1356 ] WAL_AP_PS_DBGID_DETECT_OUT_OF_SYNC_STA: vdev_id=%d, AssocID=%d, Timestamp=%d, OldestTxBufferedWaitingMs=%d, detect_thresh=%d, QDepeth=%d 
3349,iI,[ wal_powersave_ap.c : 648 ] wal_ps_ap_sa_thread_msg_handler: peer=%d, cmd_id:%u 
3348,ii,[ wal_powersave_ap.c : 1472 ] WAL_AP_PS_DBGID_SLEEP_STA_DEC vdev_id = %d num_sleeping_sta:%d 
3347,ii,[ wal_powersave_ap.c : 1424 ] WAL_AP_PS_DBGID_SLEEP_STA_INC vdev_id = %d num_sleeping_sta:%d 
3346,iiii,[ wal_powersave_ap.c : 384 ] WAL_AP_PS_DBGID_PSPOLL_REQ AssocID = %d Aid = %d PeerPSEnabled = %d SendNInProgress = %d 
3345,iIiI,[ wal_powersave_ap.c : 498 ] wal_ps_buf_peer_rx_event_handler(RX): aid=%d, fc=0x%x, seq=%d, timestamp_us=%u 
3344,iIiII,[ wal_powersave_ap.c : 520 ] wal_ps_buf_peer_rx_event_handler(DATA_PPDU): aid=%d, fc=0x%x, seq=%d, qos=0x%x, timestamp_us=%u 
3343,iiii,[ wal_powersave_ap.c : 1211 ] WAL_AP_PS_DBGIG_SET_PARAM vdev_id = %d AssocID = %d Param = %d Value = %d 
3342,iiII,[ wal_powersave_ap.c : 1273 ] WAL_AP_PS_DBGIG_UAPSD_CFG vdev_id = %d AssocID = %d UAPSDTriggerTids = 0x%x UAPSDDeliveryTids = 0x%x 
3361,iii,[ wal_powersave_buf_peer_sm.c : 1154 ] WAL_AP_PS_DBGID_UPDATE_TIM vdev_id = %d AssocID = %d IsTimSet = %d 
3360,iiI,[ wal_powersave_buf_peer_sm.c : 979 ] WAL_AP_PS_DBGID_START_SP vdev_id = %d AssocID = %d last_rx_trigger_time = %u 
3359,iiII,[ wal_powersave_buf_peer_sm.c : 1010 ] WAL_AP_PS_DBGID_COMPLETED_EOSP vdev_id = %d AssocID = %d tx_comp_ts = %u last_rx_trigger_time = %u 
3358,iiIIii,[ wal_powersave_buf_peer_sm.c : 1046 ] WAL_AP_PS_DBGID_SEND_COMPLETE vdev_id = %d AssocID = %d FrameCtrl = 0x%x QoSCtrl = 0x%x USPActive = %d PendingPollResp = %d 
3357,iiii,[ wal_powersave_buf_peer_sm.c : 1105 ] WAL_AP_PS_DBGID_SEND_N_COMPLETE vdev_id = %d AssocID = %d USPActive = %d PendingPollResp = %d 
3356,iiI,[ wal_powersave_buf_peer_sm.c : 759 ] WAL_AP_PS_DBGID_START_SP vdev_id = %d AssocID = %d A_MILLISECONDS = %u 
3355,iiiIIII,[ wal_powersave_buf_peer_sm.c : 480 ] WAL_AP_PS_DBGID_PSPOLL vdev_id = %d AssocID = %d Tid = %d Flags = 0x%x legacy_tidmask = 0x%x allowed_legacy_tidmask = 0x%x pending_legacy_tidmap = 0x%x 
3354,iiiII,[ wal_powersave_buf_peer_sm.c : 492 ] WAL_AP_PS_DBGID_PSPOLL_ERROR vdev_id = %d AssocID = %d TidPaused = %d AllowdLegacyTidMask = 0x%x LegacyTidMask = 0x%x 
3353,iiiiiIII,[ wal_powersave_buf_peer_sm.c : 693 ] WAL_AP_PS_DBGID_UAPSD_RESPONSE vdev_id = %d AssocID = %d Tid = %d NumMPDUToSend = %d need_extra_qnull = %d Flags = 0x%x allow_n_flags_qnull = 0x%x SPLength = 0x%x 
3352,iiIIII,[ wal_powersave_buf_peer_sm.c : 727 ] WAL_AP_PS_DBGID_UAPSD_RESPONSE_ERROR vdev_id = %d AssocID = %d Tid/Paused = 0x%x AllowedUAPSDTidMask = 0x%x PendingTidMap = 0x%x SPLength = 0x%x 
3351,iiIi,[ wal_powersave_buf_peer_sm.c : 1211 ] WAL_AP_PS_DBGID_SYNC_TIM vdev_id = %d AssocID = %d Tids = 0x%x TimSet = %d 
3364,iii,[ wal_powersave_sta.c : 318 ] EOSP %d, get_gdepth = %d, get_hw_qdepth = %d 
3363,IIi,[ wal_powersave_sta.c : 336 ] _wal_ps_sta_process_rx_event: frame_control=%0x, qos_control=%0x, thread_id=%d 
3362,,[ wal_powersave_sta.c : 351 ] wal_ps_sta_process_rx_event: leaky AP detected 
3379,i,[ wal_egap_proxy.c : 242 ] _wal_egap_disable_event invalid frame event = %d  
 
3378,iI,[ wal_egap_proxy.c : 249 ] _wal_egap_disable_event frame event = %d egap_ap_handle->event_bitmap = 0x%x 
 
3377,i,[ wal_egap_proxy.c : 204 ] _wal_egap_enable_event invalid frame event = %d  
 
3376,iI,[ wal_egap_proxy.c : 211 ] _wal_egap_enable_event frame event = %d egap_ap_handle->event_bitmap = 0x%x 
 
3375,i,[ wal_egap_proxy.c : 281 ] _wal_egap_is_event_enabled invalid frame event = %d  
 
3374,I,[ wal_egap_proxy.c : 288 ] _wal_egap_is_event_enabled egap_ap_handle->event_bitmap = 0x%x 
 
3373,ii,[ wal_egap_proxy.c : 486 ] _wal_egap_notify_sta_sleep: num_sta_asleep=%d, num_clients=%d 
3372,,[ wal_egap_proxy.c : 609 ] _wal_egap_pdev_event_handler wal_pdev is NULL  
 
3371,,[ wal_egap_proxy.c : 613 ] _wal_egap_pdev_event_handler wal_vdev is NULL 
 
3370,,[ wal_egap_proxy.c : 619 ] _wal_egap_pdev_event_handler WAL_EGAP_REG_EV_RX_PHYERR not enabled 
 
3369,I,[ wal_egap_proxy.c : 622 ] _wal_egap_pdev_event_handler event->event_type  = 0x%x  
 
3368,,[ wal_egap_proxy.c : 635 ] _wal_egap_pdev_event_handler send RT the phyerr event  
 
3367,i,[ wal_egap_proxy.c : 570 ] _wal_egap_update_peer_connections num_clients = %d 
 
3366,,[ wal_egap_proxy.c : 572 ] _wal_egap_update_peer_connections NULL wal egap hdl ! 
3365,i,[ wal_egap_proxy.c : 559 ] wal_egap_is_powersave_frame powersave_frame = %d 
 
3383,i,[ twt_protocol.c : 398 ] twt_info unexpected: resp_req(%d)!=0 
3382,i,[ twt_protocol.c : 402 ] twt_info unexpected: next_req(%d)!=0 
3381,I,[ twt_protocol.c : 471 ] twt_parse_teardown_frame(!wake_tbtt_nego): twt_flow=%u 
3380,,[ twt_protocol.c : 67 ] twt_power_2_mantissa wrong parameters  
3424,i,[ twt_ap.c : 1936 ] %d: UAPSD+TWT Not allowed 
3423,i,[ twt_ap.c : 1972 ] ap_twt_add_i_session(send_failed): status=%d 
3422,ii,[ twt_ap.c : 415 ] ap_twt_check_send_del_all_frame FAIL for peer:%d after %d attempts 
3421,iiIi,[ twt_ap.c : 450 ] ap_twt_check_send_del_frame FAIL for peer:%d session:%d flags:%x after %d attempts 
3420,ii,[ twt_ap.c : 2026 ] ap_twt_del_dialog[unknown dialog_id]: peer=%d, dialog_id=%d 
3419,i,[ twt_ap.c : 978 ] twt_ap_twt_session_t == NULL, session_id=%d 
3418,i,[ twt_ap.c : 1403 ] %d: AP TWT not initialized on this MAC 
3417,i,[ twt_ap.c : 1409 ] %d: AP TWT: disable cmd cannot find SOC handle 
3416,i,[ twt_ap.c : 993 ] twt_ap_twt_session_t == NULL, session_id=%d 
3415,i,[ twt_ap.c : 1427 ] %d: AP TWT not initialized on this MAC 
3414,i,[ twt_ap.c : 1433 ] %d: AP TWT: disable cmd cannot find SOC handle 
3413,i,[ twt_ap.c : 1010 ] twt_ap_twt_session_t == NULL, session_id=%d 
3412,iiiii,[ twt_ap.c : 363 ] ap_twt_send_del_event Error: %d %d %d %d %d 
3411,,[ twt_ap.c : 242 ] POOL ALLOC FAILURE 
3410,i,[ twt_ap.c : 706 ] %d: ap_twt_setup_tx_completion: parse_setup_frame error 
3409,ii,[ twt_ap.c : 710 ] ap_twt_setup_tx_completion: status=%d, comp_ctxt=%d 
3408,ii,[ twt_ap.c : 817 ] ap_twt_teardown_tx_completion err: status=%d, comp_ctxt=%d 
3407,i,[ twt_ap.c : 2044 ] %d: AP TWT not enabled on this vdev 
3406,i,[ twt_ap.c : 2057 ] %d: AP TWT not enabled on this peer 
3405,i,[ twt_ap.c : 2195 ] %d: AP TWT not enabled on this vdev 
3404,i,[ twt_ap.c : 2206 ] %d: AP TWT peer memory not available on this vdev 
3403,i,[ twt_ap.c : 3240 ] TWT AP Unexpected frame type %d 
3402,i,[ twt_ap.c : 2107 ] %d: AP TWT not enabled on this vdev 
3401,i,[ twt_ap.c : 2131 ] %d: AP TWT not enabled on this peer 
3400,i,[ twt_ap.c : 2255 ] %d: AP TWT not enabled on this peer 
3399,i,[ twt_ap.c : 2261 ] %d: AP TWT not enabled on this vdev 
3398,i,[ twt_ap.c : 1379 ] %d: AP TWT not initialized on this MAC 
3397,i,[ twt_ap.c : 1385 ] %d: AP TWT: disable cmd cannot find SOC handle 
3396,ii,[ twt_ap.c : 2704 ] %d: session not found: session_id=%d 
3395,i,[ twt_ap.c : 3415 ] %d: AP TWT not initialized on this MAC 
3394,i,[ twt_ap.c : 2963 ] %d: TWT AP, setup frame details is NULL 
3393,i,[ twt_ap.c : 2615 ] %d: AP TWT not enabled on this peer 
3392,i,[ twt_ap.c : 2620 ] AP TWT duplicate dialog token(%d) received 
3391,i,[ twt_ap.c : 2652 ] TWT AP Unexpected command %d 
3390,i,[ twt_ap.c : 1322 ] %d: AP TWT not initialized on this MAC 
3389,ii,[ twt_ap.c : 1332 ] %d: AP TWT disable on MAC:%d 
3388,ii,[ twt_ap.c : 1247 ] %d: AP TWT not initialized on this MAC %d 
3387,ii,[ twt_ap.c : 1257 ] %d: AP TWT enable on MAC %d 
3386,iii,[ twt_ap.c : 1183 ] %d: Mismatch between reported number ofsessions %d and actual number of sessions %d 
3385,iIii,[ twt_ap.c : 1569 ] %d: DUPLICATE REQ twt_ap_vdev_migrate for vdev:%x migrating from MAC%d to MAC%d 
3384,iIIiiI,[ twt_ap.c : 1578 ] %d: twt_ap_vdev_migrate complete, vdev:%x twt_vdev:%x migrate from MAC%d to MAC%d new_twt_pdev:%x 
3427,i,[ twt_ap_session_sm.c : 554 ] sending pause frame failed: status=%d 
3426,iiiI,[ twt_ap_session_sm.c : 443 ] ap_twt_session_state_renegotiating_event failed after %d attempts for peer=%d session:%d flags:%x 
3425,i,[ twt_ap_session_sm.c : 747 ] sending resume frame failed: status=%d 
3428,III,[ twt_ap_smartwt.c : 266 ] ap_smartwt_get_slot_idx_start_time_end_time last_slot_extra_dur_us %llu temp %llu diff_in_time %llu 
3438,IIIIIII,[ wal_ant_share.c : 192 ] WAL_COEX_HALPHY: event(%u) param(%u) total_req(%u) rej_cnt(%u) fail_cnt(%u) in_prog(%u) switch_cntr(%u) 
3437,ii,[ wal_ant_share.c : 65 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing low RSSI Threshold from BDF= %d and Actual= %d 
3436,iiI,[ wal_ant_share.c : 1017 ] COEX_MWS_REMOTE_EVENT: [DIVERSITY_ANTENNA]adv_notice:%d, dur:%d, token:0x%x  
3435,IIiI,[ wal_ant_share.c : 1032 ] COEX_MWS_ANT_DIVERSITY: msgid(0x%x), AntShState:%u, CpAntShDur:%d, Flag:0x%x 
3434,iI,[ wal_ant_share.c : 1004 ] COEX_MWS_REMOTE_EVENT: [DIVERSITY_ANTENNA_RESP] dur:%d, token:0x%x  
3433,,[ wal_ant_share.c : 966 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing coex sync resp timeout 
3432,I,[ wal_ant_share.c : 123 ] COEX_MWS_ANT_DIVERSITY: PwrOnTimer, AntShState = 0x%x  
3431,,[ wal_ant_share.c : 130 ] COEX_MWS_ANT_DIVERSITY: PA_UNMUTE on PwrOnTimer because AntShState is SWITCH_ON_WLAN 
3430,iI,[ wal_ant_share.c : 906 ] COEX_MWS_ANT_DIVERSITY: wal_coex_ant_share_update event =%d PA_Mute = %x 
3429,iii,[ wal_ant_share.c : 235 ] COEX_MWS_ANT_DIVERSITY: RSSI Threshold met. Type= %d rssi= %d, threshold= %d 
3451,ii,[ wal_ant_share_sm.c : 1792 ] COEX_MWS_ANT_DIVERSITY: ANT_SHARE_SM: %d => %d 
3450,ii,[ wal_ant_share_sm.c : 1769 ] COEX_MWS_ANT_DIVERSITY: ANT_SHARE_SM_EVENT: %d < %d
 
3449,IIIi,[ wal_ant_share_sm.c : 280 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing Updating chainmask. tx_chm=0x%x, rx_chm=0x%x, rx_nss=0x%x, defer_smps=%d 
3448,,[ wal_ant_share_sm.c : 718 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing duration_grant_entry 
3447,,[ wal_ant_share_sm.c : 1119 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing grant_async_entry 
3446,,[ wal_ant_share_sm.c : 1382 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing grant_async_timeout_entry 
3445,,[ wal_ant_share_sm.c : 564 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing grant_sync_entry 
3444,,[ wal_ant_share_sm.c : 322 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing init_grant_entry 
3443,,[ wal_ant_share_sm.c : 443 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing init_release_entry 
3442,,[ wal_ant_share_sm.c : 876 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing pre_release_entry 
3441,,[ wal_ant_share_sm.c : 1250 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing release_async_entry 
3440,,[ wal_ant_share_sm.c : 1509 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing release_async_timeout_entry 
3439,,[ wal_ant_share_sm.c : 995 ] COEX_MWS_ANT_DIVERSITY: Antenna Sharing release_sync_entry 
3453,II,[ wal_beacon.c : 1144 ] in_next_tsf 0x%x adj_next_tsf 0x%x 
3452,iii,[ wal_beacon.c : 1196 ] update_phy_rssi avt %d ast %d rssi %d 
3462,IIIIII,[ wal_swba.c : 737 ] swba_intr: misc=0x%x,period=%u,tsf=%u,tbtt-curr=%u/next=%u,diff=%u 
3461,I,[ wal_swba.c : 792 ] cur_tsf %u 
3460,II,[ wal_swba.c : 873 ] Burst beacon drift: next_beacon = %u, next_hw_tbtt = %u 
3459,III,[ wal_swba.c : 883 ] Burst beacon drift recover: next_beacon = %u,                                         beacon_period = %u, until_next_tbtt = %u 
3458,II,[ wal_swba.c : 762 ] Staggered beacon drift: next_beacon = %u, next_hw_tbtt = %u 
3457,III,[ wal_swba.c : 772 ] Staggered beacon drift recover: next_beacon = %u, beacon_period = %u, until_next_tbtt = %u 
3456,i,[ wal_swba.c : 1944 ] next_beacon_wal_swba_restore=%d 
3455,IIII,[ wal_swba.c : 1602 ] _wal_swba_set_and_fire: cur_tsf=0x%x sta_offset=0x%x next_beacon=0x%x next_beacon_slot=%u 
3454,iiii,[ wal_swba.c : 1209 ] Fils is already enabled on some other vdev. fils_period %d vdev_id %d old_fils_period %d old_vdev_id %d 
3464,II,[ wal_chain_mgmt.c : 36 ] WAL_DBGID_GET_HW_CHAINMASK  Tx:0x%x Rx:0x%x 
3463,III,[ wal_chain_mgmt.c : 132 ] WAL_DBGID_SET_HW_CHAINMASK 0x%x 0x%x 0x%x 
3465,i,[ wal_channel_change.c : 122 ] _wal_set_home_channel : num home chans = %d 
3510,IIII,[ wal_coex_main.c : 6273 ] WAL_COEX_BT5G_HARMONIC: Complete [mac0] tx:0x%x rx:0x%x, [mac1] tx:0x%x, rx:0x%x 
3509,i,[ wal_coex_main.c : 6277 ] WAL_COEX_BT5G_HARMONIC: Requeue cmd:%d 
3508,,[ wal_coex_main.c : 6355 ] WAL_COEX_BT5G_HARMONIC: Callback unregistered 
3507,i,[ wal_coex_main.c : 6365 ] WAL_COEX_BT5G_HARMONIC: Cache cmd:%d 
3506,ii,[ wal_coex_main.c : 6383 ] WAL_COEX_BT5G_HARMONIC: Feature is disabled bdf=%d host=%d  
3505,ii,[ wal_coex_main.c : 6388 ] WAL_COEX_BT5G_HARMONIC:  cmd:%d cur_cmd=%d 
3504,ii,[ wal_coex_main.c : 6392 ] WAL_COEX_BT5G_HARMONIC: Execute cmd:%d mode=%d 
3503,I,[ wal_coex_main.c : 2519 ] WAL_COEX_HYBRID: btc_hybrid [no_2g|bt_lrssi|bt_interfer|wl_lrssi|wl_txheavy|other](0x%x) 
3502,III,[ wal_coex_main.c : 1117 ] WAL_COEX_CONFIG_MGR: state(0x%x) stimulus(%u) band(%u) 
3501,IIIIIII,[ wal_coex_main.c : 1001 ] WAL_COEX_RC_CHAINMASK: pdev_id(%u) band(%u) indx(%u) bdf_chm(0x%x) nss1(%u) nss2(%u) nss3(%u) 
3500,IIIII,[ wal_coex_main.c : 4977 ] COEX_ENTER_CRITICAL_OCS: Error(0x%x) Dur(%u) Intrvl(%u) TransState(0x%x) Status(%u) 
3499,III,[ wal_coex_main.c : 3852 ] COEX_ENTER_OCS: OCSTransitionState(%u) Status(%u) DynOCSStatus(%u) 
3498,III,[ wal_coex_main.c : 5674 ] COEX_ENTER_LATENCY_MODE: OCSTransitionState(%u) Status(%u) CoexLLOCSStatus(%u) 
3497,I,[ wal_coex_main.c : 4702 ] COEX_ERR_FREQ_OCS_ENTER: ERROR: Time since since OCS exit = %u 
3496,IIIII,[ wal_coex_main.c : 4757 ] COEX_ENTER_OCS: Error(0x%x) Dur(%u) Intrvl(%u) TranState(0x%x) Status(%u) 
3495,II,[ wal_coex_main.c : 2227 ] WAL_COEX_ENTER_PSP: Error(0x%x) TX_SEND_BURST disabled (0x%x) 
3494,III,[ wal_coex_main.c : 6509 ] COEX_ENTER_SYNC_OCS: OCSTransitionState(%u) Status(%u) syncocsstate (%u) 
3493,II,[ wal_coex_main.c : 5058 ] COEX_EXIT_CRITICAL_OCS: TransState(%u) Status(%u) 
3492,II,[ wal_coex_main.c : 3769 ] COEX_EXIT_OCS: OCSTransitionState(0x%x) DynOCSStatus(%u) 
3491,III,[ wal_coex_main.c : 5773 ] COEX_EXIT_LATENCY_MODE: OCSTransitionState(%u) Status(%u) CoexLLOCSStatus(%u) 
3490,III,[ wal_coex_main.c : 4825 ] COEX_EXIT_OCS: TranState(%u) Status(%u) Exit Reason(%u) 
3489,,[ wal_coex_main.c : 2242 ] WAL_COEX_EXIT_PSP: Exit PSP is already in progress 
3488,III,[ wal_coex_main.c : 2283 ] WAL_COEX_EXIT_PSP: Error(0x%x) TX_SEND_BURST enabled (0x%x), reason:%u 
3487,I,[ wal_coex_main.c : 6468 ] COEX_EXIT_SYNC_OCS: OCSTransitionState(0x%x) 
3486,IIIIII,[ wal_coex_main.c : 658 ] WAL_COEX_CTS2S_RESULT: result(%u) pdev(%u) ts(%u) cts2s_tx_latency(%u) cts2s_max_time(%u) dut_nav(%u) 
3485,ii,[ wal_coex_main.c : 5494 ] WAL_COEX_GET_DATA: Datatype : (%d) | inparam : (%d) is NULL 
3484,II,[ wal_coex_main.c : 5194 ] WAL_COEX_BDF: Flags(0x%x) Config(0x%x) 
3483,i,[ wal_coex_main.c : 4471 ] WAL_COEX_SYNCOCS_TIMER: Incorrect wlan_dur %d 
3482,IIIIIII,[ wal_coex_main.c : 4550 ] WAL_COEX_MNGR: Error(0x%x) mac(%u) Stimulus(%u) Reason(%u) BTSMState(0x%x) SysUpdateResult(%u) ConfigMngr(0x%x) 
3481,IIIIIII,[ wal_coex_main.c : 1431 ] WAL_COEX_ALT_CHM: pdev(%u) chm(0x%x) enable_alt(%u) is_2gchan(%u) alt_chm(%u) selfgenAltChm (%u) pending(%u) 
3480,III,[ wal_coex_main.c : 2309 ] WAL_COEX_PSP: Error(0x%x) MinInterval(%u) BtIdleTime(%u) 
3479,II,[ wal_coex_main.c : 1706 ] COEX_SET_NSS: VdevId(%u) NumStreams(%u) 
3478,iIII,[ wal_coex_main.c : 861 ] COEX_SELF_GEN_MASK: Status(%d) Selfgen(%u) RFBand(%u) MaxChains(%u) 
3477,III,[ wal_coex_main.c : 3872 ] COEX_CTS2S_SEND: Dur(%u) Time2Discard(%u) CurrTime(%u) 
3476,i,[ wal_coex_main.c : 6534 ] WAL_COEX_SYNCOCS_TIMER: Incorrect bt_dur %d 
3475,i,[ wal_coex_main.c : 6548 ] WAL_COEX_SYNCOCS_TIMER: Incorrect wlan_dur %d 
3474,IIIIIIIII,[ wal_coex_main.c : 426 ] COEX_SYS_MON_BT: [bt_on|pmh|non_link|acl_int|passive_bt|ba_active](0x%06x) num_prof(%u) ACL(%u) sniff(%u) [3DD|APTX_LL|A2DP](0x%03x) HID(%u) HFP/RVP(%u) BA(%u) ISO|ASHA|LE(0x%03x) 
3473,IIIIIIIi,[ wal_coex_main.c : 433 ] COEX_SYS_MON_WLAN: mac(%u) rx_crit(%u) rx_state(0x%x) wlan0_state(0x%x) wlan1_state(0x%x) 2g_pdev_idle(%u) probe_req_def(%u) low_latency_en(%d) 
3472,IIIIIIIII,[ wal_coex_main.c : 3439 ] COEX_SYSTEM_UPDATE: status(%u) stimulus(%u) hw_mode(%u) num_chains(%u) aggr_lim(%u) 3ant[bt_sep_ant(%u) ant_iso(%u) cfg_mode(%u) run_mode(%u)] 
3471,III,[ wal_coex_main.c : 596 ] WAL_COEX_TRF_CTS2: T2NonWlan(%u) Now(%u) Now+NonWlanDuration(%u) 
3470,IIII,[ wal_coex_main.c : 5091 ] COEX_UPDATE_CRITICAL_OCS: Dur(%u) Intrvl(%u) TransState(0x%x) Status(%u) 
3469,IIII,[ wal_coex_main.c : 4857 ] COEX_UPDATE_OCS: Dur(%u) Intrvl(%u) TransState(0x%x) Status(%u) 
3468,I,[ wal_coex_main.c : 5557 ] WAL_COEX_WSI: Error(0x%x) 
3467,I,[ wal_coex_main.c : 5579 ] WAL_COEX_WSI_TMR: enable(%u) 
3466,I,[ wal_coex_main.c : 5584 ] WAL_COEX_WSI_TMR: enable(%u) 
3535,I,[ wal_coex_bt.c : 4900 ] COEX_GENERIC_ERROR: ACL Active SCO Timer expired ! AclActiveScoTimerState = 0x%x 
3534,III,[ wal_coex_bt.c : 3631 ] WAL_COEX_BTPROF_ADD: Status(%u) RemoteId(%u) ProfileType(%u) 
3533,IIII,[ wal_coex_bt.c : 1077 ] WAL_COEX_BT_ALLOC: Ret(%u) LocalId(%u) Remote_Id(%u) MinFreeLinkId(%u) 
3532,III,[ wal_coex_bt.c : 1095 ] WAL_COEX_BT_DEALLOC: LocalId(%u) Remote_Id(%u) MinFreeLinkId(%u) 
3531,iIII,[ wal_coex_bt.c : 3916 ] WAL_COEX_TRAF_STAT: traf_status(%d). TxBW(0x%08x), RxBW(0x%08x), intvl(0x%08x) 
3530,IIIIIIII,[ wal_coex_bt.c : 4028 ] WAL_COEX_SCHED_INTERVAL: Error(0x%x) Warn(0x%x) bt_grant(%u) bt_duration(%u) interval(%u) bt_traffic_status(%u) is_bt_heavy(%u) WlanScanType(%u) 
3529,,[ wal_coex_bt.c : 4928 ] WAL_COEX_LE_ADV_RX: LE Adv Rx Timer Expired 
3528,IIiII,[ wal_coex_bt.c : 3408 ] WAL_COEX_PROC_GPM: Error(0x%x) Warn(0x%x) status(%d) type(%u) subtype(%u) 
3527,II,[ wal_coex_bt.c : 642 ] COEX_MCI_RECOVER: StimulusState(0x%x) RecoveryState(0x%x) 
3526,I,[ wal_coex_bt.c : 597 ] COEX_MCI_TIMER_HANDLER: Recovery(0x%x) 
3525,II,[ wal_coex_bt.c : 424 ] COEX_WAL_PAUSE_RESUME: Pause(%u) State(0x%x) 
3524,I,[ wal_coex_bt.c : 2821 ] WAL_COEX_BTQ: Overflow(%u) 
3523,I,[ wal_coex_bt.c : 2143 ] COEX_GENERIC_ERROR: SCO/RVP link entered PWR_SAVE state. AclActiveScoTimerState = 0x%x 
3522,I,[ wal_coex_bt.c : 2156 ] COEX_GENERIC_ERROR: SCO/RVP link entered ACTIVE state. AclActiveScoTimerState = 0x%x 
3521,Ii,[ wal_coex_bt.c : 3418 ] WAL_COEX_DBG_GPM: WAR361_Status:0x%x, Reason:%d 
3520,I,[ wal_coex_bt.c : 1675 ] WAL_COEX_STATUS_UPDATE: No record for existing link (%u) 
3519,II,[ wal_coex_bt.c : 2516 ] WAL_COEX_BT_CSB: Type(%u) Id(%u) 
3518,III,[ wal_coex_bt.c : 3659 ] WAL_COEX_BTPROF_DEL: Status(%u) RemoteId(%u) ProfileType(%u) 
3517,III,[ wal_coex_bt.c : 1573 ] WAL_COEX_BT_DEL_PROF: Invalid link: Type(%u) State(0x%x), id(%u) 
3516,IIIII,[ wal_coex_bt.c : 3563 ] COEX_BT_INTERVAL_START: Error(0x%x) Warn(0x%x) bt_intrvl_cnt(%u) duration(%u) enable_bt_bw_lim(%u) 
3515,II,[ wal_coex_bt.c : 3600 ] COEX_WLAN_POSTPAUSE_INTERVAL_START: Dur(%u) Wght(%u) 
3514,IIII,[ wal_coex_bt.c : 3582 ] COEX_WLAN_INTERVAL_START: Error(0x%x) Warn(0x%x) wlan_intrvl_cnt(%u) duration(%u) 
3513,IIII,[ wal_coex_bt.c : 478 ] COEX_UPDATE_AFH: IsAdd(%u) Freq(%u), 2G(%u) HT20(%u) 
3512,ii,[ wal_coex_bt.c : 3826 ] COEX_BT_RXSS_THRES: NewRSSI(%d) 1 LowerThresh(%d) 
3511,III,[ wal_coex_bt.c : 1493 ] COEX_BT_PRIO_BUDGET: idle(%u) low(%u) hi(%u) 
3539,IIIIIII,[ wal_coex_btle.c : 249 ] WAL_COEX_LE_LR: status(%u) state(0x%x) cmd_status(0x%x) local_id(%u) remote_id(%u) max_tx(%u) max_rx(%u) 
3538,IIIIII,[ wal_coex_btle.c : 176 ] WAL_COEX_LE_LR: state(0x%x) write(%u) local_id(%u) remote_id(%u) max_tx(%u) max_rx(%u) 
3537,III,[ wal_coex_btle.c : 295 ] WAL_COEX_LE_ASHA: result(%u) curr(%u) prev(%u) 
3536,IIIII,[ wal_coex_btle.c : 336 ] WAL_COEX_LE_ASHA: result(%u) id(%u) offset(%u) thresh(%u) is_asha(%u)  
3635,IIIII,[ wal_coex_mws.c : 5336 ] COEX_MWS_REMOTE_EVENT: frequency:%u, group:%u, ingroup_index:%u, (%u,%u) 
3634,IIIII,[ wal_coex_mws.c : 5339 ] COEX_MWS_REMOTE_EVENT: frequency:%u, group:%u, ingroup_index:%u, (%u,%u) 
3633,iiIIIIII,[ wal_coex_mws.c : 5401 ] COEX_MWS_REMOTE_EVENT: [POTENTIAL_CONFLICT] Freqs:(%d->%d), chavd_group:0x%x, chavd_1_0:0x%x, chavd_3_2:0x%x, chavd_5_4:0x%x, chavd_7_6:0x%x, err_id:0x%x 
3632,I,[ wal_coex_mws.c : 4637 ] COEX_MWS_OTHER: Conflicts bitmap: 0x%x 
3631,IIII,[ wal_coex_mws.c : 1044 ] COEX_MWS_WWAN_STATE: [FILL_BAND_INFO] tech:%u, freq:%u, dir:%u, bw:%u 
3630,Iiiiiii,[ wal_coex_mws.c : 1104 ] COEX_MWS_WWAN_STATE: [err_id:0x%x] Fill band info failed, tech_info[] full: %d, %d, %d, %d, %d,%d 
3629,,[ wal_coex_mws.c : 940 ] COEX_MWS_OTHER: [SAP_CHAVD_DEBUG] CoexFreqAvoid reported 
3628,,[ wal_coex_mws.c : 943 ] COEX_MWS_OTHER: [SAP_CHAVD_DEBUG] CoexFreqAvoid function was NULL 
3627,,[ wal_coex_mws.c : 2389 ] COEX_MWS_OTHER: Modem is considered offline, as there is no response to Active conflict req 
3626,,[ wal_coex_mws.c : 795 ] COEX_MWS_ERROR: [ERR] Trying to update conflict with no connected LTE sub 
3625,,[ wal_coex_mws.c : 1209 ] COEX_MWS_ERROR: [War] WCI2 is not ready.. init once again.. 
3624,,[ wal_coex_mws.c : 1212 ] COEX_MWS_ERROR: [War] WCI2 init failed.. 
3623,,[ wal_coex_mws.c : 1242 ] COEX_MWS_ERROR: [Err] WCI2 is not ready.. YET..WCI-2 Msg not Send 
3622,I,[ wal_coex_mws.c : 1251 ] COEX_MWS_ENCODE_SEND: [Err] Code=0x%x 
3621,II,[ wal_coex_mws.c : 1502 ] COEX_MWS_SAR: Reason=0x%x ErrCode=0x%x 
3620,I,[ wal_coex_mws.c : 1990 ] COEX_MWS_ENCODE_SEND: [Err] BLER_FillTX : Unknown cmd(0x%x) 
3619,I,[ wal_coex_mws.c : 1792 ] COEX_MWS_OTHER: [Error] unknown SINR command %u when sending to modem 
3618,I,[ wal_coex_mws.c : 1837 ] COEX_MWS_OTHER: [Error] unknown SINR command %u when sending to modem 
3617,IIIiiii,[ wal_coex_mws.c : 1621 ] COEX_MWS_OTHER: [DETECT_TIMER] TxThr:%u,Flags:0x%x,Curr:%u,TDM = %d,RSSI_TDM:%d,SINR_TDM:%d,low rx rate = %d 
3616,,[ wal_coex_mws.c : 1630 ] COEX_MWS_OTHER: [DETECT_TIMER] Modem is considered offline by WLAN now 
3615,ii,[ wal_coex_mws.c : 3020 ] COEX_MWS_PWB: [LPL] SUB %d is entering TXB - wlanid %d 
3614,ii,[ wal_coex_mws.c : 3066 ] COEX_MWS_PWB: [LPL] SUB %d is exiting TXB - wlanid %d 
3613,I,[ wal_coex_mws.c : 7961 ] COEX_MWS_ERROR: Grant value should not be 0, wlan_id:%u 
3612,I,[ wal_coex_mws.c : 6212 ] COEX_MWS_ERROR: msgid(0x%x) 
3611,Iii,[ wal_coex_mws.c : 1365 ] COEX_MWS_CP_UNFRAME: Ret(%u), CRC [Err] (rcvd:%d,Calc:%d) 
3610,I,[ wal_coex_mws.c : 1368 ] COEX_MWS_CP_UNFRAME: Ret(%u) 
3609,ii,[ wal_coex_mws.c : 3130 ] COEX_MWS_ERROR: SUB %d is trying to sleep but no policy to exit, current policy = %d 
3608,iII,[ wal_coex_mws.c : 3166 ] COEX_MWS_ERROR: [LPL] [Err] SUB %d timer expired!, now = %u, end %u 
3607,I,[ wal_coex_mws.c : 3078 ] COEX_MWS_ERROR: [LPL][Err] Recovering because missing sleep ind (%u)ms 
3606,IIIII,[ wal_coex_mws.c : 3547 ] COEX_MWS_REMOTE_EVENT: frequency:%u, group:%u, ingroup_index:%u, (%u,%u) 
3605,I,[ wal_coex_mws.c : 8318 ] COEX_MWS_TYPE_3: Rcvd LTE Wake/Sleep Ind. Dur:%u ms  
3604,,[ wal_coex_mws.c : 1707 ] COEX_MWS_PWB_UPDATE: Event[PWB_RSSI_CHANGE] 
3603,IIii,[ wal_coex_mws.c : 5171 ] COEX_MWS_WWAN_STATE: [QMI_LTE_STATE_CC_INFO] band-idx:0x%x, dimension:%u, frame_offset:%d, tdd_config:%d 
3602,iII,[ wal_coex_mws.c : 5303 ] COEX_MWS_REMOTE_EVENT: [Err] **major** error (i:%d, band_index:0x%x, len:0x%x) 
3601,,[ wal_coex_mws.c : 2309 ] COEX_MWS_OTHER: [Err][BLER_RESP_TIMER] 
3600,iiiii,[ wal_coex_mws.c : 3382 ] COEX_MWS_PWB: [PWB_CALC] cc_id=%d, sinrWLANOFFAve=%d, sinrWLANONAve=%d, deltaN=%d, falseSinr=%d 
3599,iii,[ wal_coex_mws.c : 3417 ] COEX_MWS_PWB: [PWB_CALC] TURN ON FORCED TDM : SINR: Max_Sinr_Diff=%d, P(n)=%d, needUpdate=%d 
3598,iii,[ wal_coex_mws.c : 3426 ] COEX_MWS_PWB: [PWB_CALC] TURN ON FORCED TDM : RSSI: (RSSI[%d] + P(n)[%d]) < RSSI_Threshold[%d] 
3597,iiiiIii,[ wal_coex_mws.c : 3437 ] COEX_MWS_PWB: [PWB_CALC] Max_delta_N=%d, P(n+1):%d, P(n)=%d, P(Max)=%d, [BadAP|needUpdate]=0x%02x, F TDM = %d, RSSI:%d 
3596,II,[ wal_coex_mws.c : 3830 ] COEX_MWS_PWB: Is schedule_timer (%u) < inactivity_timer (%u)  
3595,i,[ wal_coex_mws.c : 3842 ] COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_LTE_SLEEP] SINR_ON Duration is adjusted by (%d ms) 
3594,I,[ wal_coex_mws.c : 3843 ] COEX_MWS_PWB: SINR_ON timer_val=%u 
3593,,[ wal_coex_mws.c : 3885 ] COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_DISABLE] 
3592,i,[ wal_coex_mws.c : 3912 ] COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_SCHEME_ENABLE] State[UNINIT->SINR_START] UN-BLOCK_WLAN for %d usec 
3591,,[ wal_coex_mws.c : 3873 ] COEX_MWS_PWB: [PWB_UPDATE]Event[PWB_PAUSE] State[PWB_HALTED] 
3590,ii,[ wal_coex_mws.c : 4005 ] COEX_MWS_PWB_UPDATE: State[FORCED_TDM_ENABLED] RSSI_TDM:%d, SINR_TDM:%d 
3589,iii,[ wal_coex_mws.c : 3959 ] COEX_MWS_PWB_UPDATE: Exit PWB always on state as SINR-on %d and SINR-off %d and BLER: %d 
3588,ii,[ wal_coex_mws.c : 3638 ] COEX_MWS_PWB: [PWB_Helper]:Active Conflict:0, Action:%d, Value:%d 
3587,,[ wal_coex_mws.c : 2301 ] COEX_MWS_OTHER: [Err][SINR_RESP_TIMER] 
3586,i,[ wal_coex_mws.c : 1379 ] COEX_MWS_PWB: PWB WLAN ON static power = %d 
3585,i,[ wal_coex_mws.c : 1387 ] COEX_MWS_PWB: PWB WLAN ON static power 5GNR = %d 
3584,ii,[ wal_coex_mws.c : 4138 ] COEX_MWS_PWB_UPDATE: Event[SINR_READ_Warr]: Ignore Drastic change in SINR_ON value; [Old=%d, New=%d] 
3583,I,[ wal_coex_mws.c : 4153 ] COEX_MWS_PWB_UPDATE: [Warr]Event[SINR_RESP_TIMEOUT] before SINR_UPDATE, wlan_on_resped_bitmap= 0x%x 
3582,ii,[ wal_coex_mws.c : 4220 ] COEX_MWS_PWB_UPDATE: Event[SINR_READ_Warr]: Ignore Drastic change in SINR_OFF value; [Old=%d, New=%d] 
3581,I,[ wal_coex_mws.c : 4254 ] COEX_MWS_PWB_UPDATE: [Err]Event[SINR_RESP_TIMEOUT] before SINR_UPDATE, wlan_off_resped_bitmap= 0x%x 
3580,iii,[ wal_coex_mws.c : 4375 ] COEX_MWS_PWB_UPDATE: Enter PWB always on state SINR_same: %d, old_rssi: %d, new_rssi: %d 
3579,I,[ wal_coex_mws.c : 4381 ] COEX_MWS_PWB_UPDATE: [Err]Event[SINR_RESP_TIMEOUT] before SINR_UPDATE, wlan_on_resped_bitmap= 0x%x 
3578,iiiI,[ wal_coex_mws.c : 4407 ] COEX_MWS_PWB: [PWB_UPDATE] Event=%d, State(%d->%d), Err:0x%x 
3577,IIIIIIII,[ wal_coex_mws.c : 1159 ] COEX_MWS_QMI_DUMP: %08x,%08x,%08x,%08x,%08x,%08x,%08x,%08x 
3576,iiIi,[ wal_coex_mws.c : 5487 ] COEX_MWS_REMOTE_EVENT: [Err]WAL_MWSCOEX_LTE_PHY_EXIST_FLAG:%d, Stimulus:%d, Flag:0x%x Bytes: %d 
3575,IiIII,[ wal_coex_mws.c : 5497 ] COEX_MWS_REMOTE_EVENT: stimulation:0x%x, Time_Diff:%d, Flag:0x%x, ArmTimer=0x%x, PsSavedTimer=0x%x 
3574,IIi,[ wal_coex_mws.c : 5693 ] COEX_MWS_REMOTE_EVENT: [ACTIVE_CONFLICT] valid:%u, len:%u, Conflict = %d 
3573,IiIiIII,[ wal_coex_mws.c : 5823 ] COEX_MWS_REMOTE_EVENT: [ACTIVE_CONFLICT] index:0x%x, carrier:%d, Mws_Tech:0x%x, Victim_idx:%d, Wifi_Policy:0x%x, WiFi_Fc:(%u -> %u) 
3572,IIi,[ wal_coex_mws.c : 6109 ] COEX_MWS_REMOTE_EVENT: [RT-SAR] PWR report req valid(%u) Seq(%u) Expt Seq(%d) 
3571,iii,[ wal_coex_mws.c : 6125 ] COEX_MWS_REMOTE_EVENT: [RT-SAR] Modem ACK Rx valid(%d) Seq(%d) NextSeq(%d) 
3570,I,[ wal_coex_mws.c : 6131 ] COEX_MWS_REMOTE_EVENT: err_id:0x%x 
3569,ii,[ wal_coex_mws.c : 6935 ] COEX_MWS_SAR: [RT-SAR] applied limit reason (%d) MIMO limits (%d) 
3568,iiiii,[ wal_coex_mws.c : 6761 ] COEX_MWS_SAR: [RT-SAR] mac=%d chain= %d band = %d curr_tpc=%d prev_tpc=%d 
3567,iiiiii,[ wal_coex_mws.c : 6780 ] COEX_MWS_SAR: [RT-SAR] Calc chain(%d) SUM [2.4GHz=%d 5GHz=%d] AVG[2.4GHz=%d 5GHz=%d] time_delta(%d)us 
3566,,[ wal_coex_mws.c : 6802 ] COEX_MWS_SAR: [Error] RTSAR Averages encountered error, not returning an average 
3565,IIIIiii,[ wal_coex_mws.c : 4767 ] COEX_MWS_SCHEME_UPDATE: chavd_1_0:0x%x, chavd_3_2:0x%x, tdm_pb:0x%x, Final_scheme:0x%x, High duty cycle = %d, FS[%d:%d] 
3564,IIIIi,[ wal_coex_mws.c : 7900 ] COEX_WCI2_TYPE3: [Err] Fail to send Type3_Msg:0x%x, W2G:0x%x, W5G:0x%x, W6G:0x%x, Param:%d 
3563,IIIIi,[ wal_coex_mws.c : 7908 ] COEX_WCI2_TYPE3: Sent Type3_Msg:0x%x, W2G:0x%x, W5G:0x%x, W6G:0x%x, Param:%d 
3562,iiii,[ wal_coex_mws.c : 7914 ] COEX_WCI2_TYPE3: Type3_Msg_Cnt:(Time_diff:%d), Cnt(%d->%d), Test_Flag:%d 
3561,i,[ wal_coex_mws.c : 4565 ] COEX_MWS_OTHER: CA delay timer started, interval: %d 
3560,iiii,[ wal_coex_mws.c : 6980 ] COEX_MWS_WWAN_STATE: [LPL] WLAN_FREQ: %d, WWAN_FREQ: %d, SUB_id: %d, Combo_id: %d 
3559,iiii,[ wal_coex_mws.c : 2179 ] COEX_MWS_OTHER: COEX_DBG_CMD: TDM active duration: %d, TDM pause duration: %d, CDRX: %d, VoLTE: %d 
3558,iiiii,[ wal_coex_mws.c : 7258 ] COEX_MWS_REMOTE_EVENT: [LPL] Tech: %d, Sleeping: %d, Critical: %d, RSSI: %d, Duration: %d 
3557,,[ wal_coex_mws.c : 3789 ] COEX_MWS_PWB: [Warr] static_power_limit is not define 
3556,I,[ wal_coex_mws.c : 334 ] COEX_MWS_ERROR: [ERR] Invalid TDD config is received from modem: 0x%x 
3555,Iiiii,[ wal_coex_mws.c : 7437 ] COEX_MWS_TDM: [TDM_EVENT] Status(%u) Event(%d) Type(%d) TDM Running(%d) Sticky(%d) 
3554,iIIi,[ wal_coex_mws.c : 618 ] COEX_MWS_TYPE2_TX: mws tx tdm (remain:%d,fail_retry:%u,full%u), Tx_FiFo Depth: %d, 
3553,Iiii,[ wal_coex_mws.c : 1015 ] COEX_MWS_WWAN_STATE: [FILL_TECH_INFO] tech:%u, index=%d, token_state:%d, token_token:%d 
3552,II,[ wal_coex_mws.c : 2084 ] COEX_MWS_TIMER: TimerId : %u, param:%u 
3551,II,[ wal_coex_mws.c : 4790 ] COEX_MWS_OTHER: gMwsCoex5gnrPwrLimit 0x%x, Err:%u 
3550,I,[ wal_coex_mws.c : 4796 ] COEX_MWS_OTHER: INI: gMwsCoexPccChAvdDelay 0x%x 
3549,I,[ wal_coex_mws.c : 4802 ] COEX_MWS_OTHER: INI: gMwsCoexSccChAvdDelay 0x%x 
3548,,[ wal_coex_mws.c : 2449 ] COEX_MWS_ENCODE_SEND: [WLAN_MODE_CHNL_MAP_IND] Err:vdev is NULL 
3547,i,[ wal_coex_mws.c : 2453 ] COEX_MWS_ENCODE_SEND: [WLAN_MODE_CHNL_MAP_IND] Err:unexpected vdev id: %d 
3546,IIII,[ wal_coex_mws.c : 569 ] COEX_MWS_TDM: FS:%u SUBF:%x UL_FreeUL:%x Count:%x 
3545,,[ wal_coex_mws.c : 2231 ] COEX_MWS_TYPE2_RX: Schedule read after 500us  
3544,i,[ wal_coex_mws.c : 2260 ] COEX_MWS_ERROR: excced buffer size:length=%d 
3543,iiii,[ wal_coex_mws.c : 2645 ] COEX_MWS_PWB: VDEV PAUSE/UN-PAUSE: wlan: %d, client: %d, is_allowed: %d vdevid: %d 
3542,IIiIiIII,[ wal_coex_mws.c : 5024 ] COEX_MWS_WLAN_EVENT: stimulation:%u, W_state:0x%x, WlanWorstFreq:%d, WlanToken:%u, Freq:%d, W2G:0x%x, W5G:0x%x, band_mac_map:0x%x 
3541,IIIIIIi,[ wal_coex_mws.c : 2887 ] COEX_MWS_PWB: [PWR_LIMIT_SET] PrevPwrLimit:%u, finalPwr:%u, sarPwr:%u, pwb_power:%u pwb_static_power:%u, MaxPwrLimit:%u, SPB:%d 
3540,iIiI,[ wal_coex_mws.c : 2971 ] COEX_MWS_PWB: [LPL] SUB %d is entering/exiting [%u] SPWB with PWR %d, Err: 0x%x 
3654,,[ wal_coex_utils.c : 1017 ] COEX_GENERIC_ERROR: COEX_LIST_OVERFLOW_ERROR 
3653,II,[ wal_coex_utils.c : 1563 ] COEX_GENERIC_ERROR: id(%u) isPaused(%u) 
3652,,[ wal_coex_utils.c : 1094 ] COEX_GENERIC_ERROR: COEX_ERROR_GET_RSSI 
3651,,[ wal_coex_utils.c : 1119 ] COEX_GENERIC_ERROR: COEX_ERROR_GET_RSSI_SEQ 
3650,I,[ wal_coex_utils.c : 1199 ] BTCOEX_DBG_MCI_2: wal_coex_is_vdev_scanning - ret(%u)  
3649,II,[ wal_coex_utils.c : 1806 ] WAL_COEX_GET_INTERVAL: GET: OCS_Duration(%u) OCS_Interval(%u) 
3648,IIIIIIII,[ wal_coex_utils.c : 944 ] WAL_COEX_GPM_RECV: subtype[0x%x] timer(%u) F1(0x%lx) F2(0x%lx) F3(0x%lx) F4(0x%lx) F5(0x%lx) F6(0x%lx) 
3647,IIIII,[ wal_coex_utils.c : 952 ] WAL_COEX_GPM_RECV: subtype[0x%x] F7(0x%lx) F8(0x%lx) F9(0x%lx) F10(0x%lx) 
3646,IIIIIIII,[ wal_coex_utils.c : 964 ] WAL_COEX_GPM_RECV: subtype[0x%x] timer(%u) F1(0x%lx) F2(0x%lx) F3(0x%lx) F4(0x%lx) F5(0x%lx) F6(0x%lx) 
3645,III,[ wal_coex_utils.c : 985 ] WAL_COEX_GPM_RECV: type[0x%x] subtype[0x%x] timer[%u] 
3644,IIIII,[ wal_coex_utils.c : 992 ] WAL_COEX_GPM_RECV: type[0x%x] timer[%u]: [BT 5g tx chain1]  status[0x%x] dutyCycle[%u] threshold[%u] 
3643,III,[ wal_coex_utils.c : 999 ] COEX_INVALID_GPM: type[0x%x] subtype[0x%x] timer[%u] : [Unknown GPM type subtype] 
3642,iiiiiiii,[ wal_coex_utils.c : 220 ] WAL_COEX_WGHTS: Static: W0[wl_idle(%d) sw_ctrl3(%d) sw_ctrl2(%d) sw_ctrl1(%d)] W1[sw_ctrl0(%d) wait_bcn(%d) wait_ack_cts(%d) selfgen(%d] 
3641,iiiiiiii,[ wal_coex_utils.c : 266 ] WAL_COEX_WGHTS: FES Tx: W4[null(%d) data(%d) qos(%d) rsvd(%d)] W5[om(%d) oc(%d) od(%d) oo(%d)] 
3640,iiiiiiii,[ wal_coex_utils.c : 277 ] WAL_COEX_WGHTS: FES Rx: W6[bcn(%d) conn(%d) scan(%d) ibss(%d)] W7[psp(%d) bar(%d) cts(%d) rsvd(%d)] 
3639,iiiiiiii,[ wal_coex_utils.c : 287 ] WAL_COEX_WGHTS: FES Rx: W8[null(%d) data(%d) qos(%d) rsvd(%d)] W9[om(%d) oc(%d) od(%d) oo(%d)] 
3638,iiii,[ wal_coex_utils.c : 223 ] WAL_COEX_WGHTS: Static: W10[rx_lvl3(%d) rx_lvl2(%d) rx_lvl1(%d) (%d)] 
3637,iiiiiiii,[ wal_coex_utils.c : 256 ] WAL_COEX_WGHTS: FES Tx: W2[bcn(%d) conn(%d) scan(%d) ibss(%d)] W3[psp(%d) bar(%d) cts(%d) rsvd(%d)] 
3636,II,[ wal_coex_utils.c : 1815 ] WAL_COEX_SET_INTERVAL: SET: OCS_Duration(%u) OCS_Interval(%u) 
3657,IIIIIIII,[ wal_coex_wghts.c : 1006 ] COEX_SET_COEX_WEIGHT: wght_grp(%u) reason(%u) wlan_idle(%u) [hid_con_tx_o|bcon_tx_o|bcon_rx_o](0x%03x) prio_wlan_fc(%u) flow_ctrl(0x%x) concur_tx(%u) BcnTxPrioEn(%u) 
3656,I,[ wal_coex_wghts.c : 1008 ] COEX_SET_COEX_WEIGHT: Invalid wght_grp(%u) 
3655,IiiII,[ wal_coex_wghts.c : 429 ] WAL_COEX_80211_FRAME: tx_qid(%u) type[%d] subtype[%d] pwr[%u] alt_chmask[%u] 
3681,I,[ wal_coex_wlan.c : 1043 ] COEX_CHANNEL_CHANGE: Invalid pdev_id %u was passed 
3680,IiII,[ wal_coex_wlan.c : 1263 ] WAL_COEX_TBTT_TIMERS: vdev_id(%u) time_to_next_tbtt(%d) next_tbtt(0x%x) cur_time(0x%x) 
3679,i,[ wal_coex_wlan.c : 1365 ] WAL_COEX_TBTT_TIMERS: Deinit coex STA timers for  Vdev %d  
3678,IIIII,[ wal_coex_wlan.c : 795 ] COEX_RX_RATE_THRESHOLD: RSSIType(%u) LowKbpsThresh(%u) UpperKbpsThresh(%u) NumPPDUsBelowThresh(%u) NumPPDUsAboveThresh(%u) 
3677,i,[ wal_coex_wlan.c : 1380 ] WAL_COEX_TBTT_TIMERS: Init coex STA timers for  Vdev %d  
3676,ii,[ wal_coex_wlan.c : 2940 ] COEX_MWS_ANT_DIVERSITY: Entering FAS opmode %d, vdevid %d 
3675,iii,[ wal_coex_wlan.c : 3033 ] BTCOEX_DBG_MCI_2: [MPTA Helper] tx_frame_cnt_in_period=%d rx_frame_cnt_in_period=%d, total/1000=%d 
3674,IIII,[ wal_coex_wlan.c : 870 ] COEX_RX_RATE_THRESHOLD: ChWidth(0xFF) TriggRate(%u) XputMonitorActiveNum(%u) TotalCoexIntrvls(%u) EventType(%u) 
3673,IIIII,[ wal_coex_wlan.c : 899 ] COEX_RX_RATE_THRESHOLD: ChWidth(%u) TriggRate(%u) XputMonitorActiveNum(%u) TotalCoexIntrvls(%u) EventType(%u) 
3672,i,[ wal_coex_wlan.c : 1291 ] WAL_COEX_TBTT_TIMERS: PRE TBTT handler for Vdev %d 
3671,IIIIIIII,[ wal_coex_wlan.c : 990 ] WAL_COEX_BAND_CHANGE: status(%u) band_changed(%u) single_mac(%u) mac(%u) 2x2(%u) new_freq(%u) cur_band(%u) cxc(0x%x) 
3670,,[ wal_coex_wlan.c : 2238 ] COEX_VDEV_STATE: 2g vdev not paused 
3669,,[ wal_coex_wlan.c : 2285 ] COEX_VDEV_STATE: 2g vdev not unpaused 
3668,III,[ wal_coex_wlan.c : 2033 ] BTCOEX_DBG_MCI_2: wal_coex_process_vdev_start_stop - opmode(%u) subop(%u) chan(0x%x) 
3667,III,[ wal_coex_wlan.c : 1141 ] BTCOEX_DBG_MCI_2: wal_coex_reassess_wlanstate - mac(%u) band(%u) state(0x%x) 
3666,II,[ wal_coex_wlan.c : 835 ] COEX_GENERIC_ERROR: ErrCode(%u) RSSIType(%u) 
3665,I,[ wal_coex_wlan.c : 840 ] COEX_GENERIC_ERROR: ErrCode(%u) 
3664,ii,[ wal_coex_wlan.c : 1328 ] WAL_COEX_TBTT_TIMERS: Start PRE TBTT timer  for Vdev %d isStart %d 
3663,ii,[ wal_coex_wlan.c : 1350 ] WAL_COEX_TBTT_TIMERS: Start SW BMISS timer  for Vdev %d isStart %d 
3662,i,[ wal_coex_wlan.c : 1274 ] WAL_COEX_TBTT_TIMERS: Stop Coex STA timers for Vdev %d 
3661,i,[ wal_coex_wlan.c : 1307 ] WAL_COEX_TBTT_TIMERS: SW BMISS handler for Vdev %d 
3660,II,[ wal_coex_wlan.c : 2494 ] UPDATE_SPECIFIC_AP_STATE: connected:%u, behaviour:%u 
3659,IIIIIIIII,[ wal_coex_wlan.c : 1819 ] WAL_COEX_VDEV_STATE: Error(0x%x) id(%u) stimulus(%u) vdev_state(0x%x) strict_dur_scan(%u) num_peers(%u) pdev(%u) chan(%u) [op|subop](0x%02x) 
3658,III,[ wal_coex_wlan.c : 1632 ] WAL_COEX_VDEV_STATE: Error(0x%x) stimulus(%u) status(%u) 
3699,iIIIi,[ wal_coex_sched.c : 1619 ] COEX_GET_T2BT: status(%d) t2bt(%u) sched_time(%u) curr_time(%u) duration(%d) 
3698,,[ wal_coex_sched.c : 926 ] COEX_EXIT_OCS: Error - Switching to FREE_RUN for 10msecs due to ENTER_DYNAMIC_OCS failure 
3697,,[ wal_coex_sched.c : 970 ] COEX_EXIT_OCS: Error - Switching to FREE_RUN for 10msecs due to ENTER_LOW_LATENCY_MODE failure 
3696,,[ wal_coex_sched.c : 945 ] COEX_EXIT_OCS: Error - Switching to FREE_RUN for 10msecs due to ENTER_SYNC_OCS failure 
3695,i,[ wal_coex_sched.c : 953 ] COEX_EXIT_OCS: Error - Not entering sync ocs due to invalid start time %d 
3694,,[ wal_coex_sched.c : 1176 ] COEX_EXIT_OCS: Error - Switching to FREE_RUN for 10msecs due to UPDATE_OCS failure 
3693,,[ wal_coex_sched.c : 1199 ] COEX_EXIT_OCS: Error - Switching to FREE_RUN for 10msecs due to ENTER_OCS failure 
3692,IIIIIII,[ wal_coex_sched.c : 1553 ] WAL_COEX_SCHEDULER: Error(0x%x) status(%u) sched_req(%u) mngr_policy(%u) next_intrvl(%u) coex_mac(%u) sched_algo(%u) 
3691,IIIIIIIII,[ wal_coex_sched.c : 754 ] COEX_TRF_SHAPE_OCS: interval(%u) Dur(%u) Latency(%u) VdevPauseDelay(%u) ConcurrState(0x%x) nonlinkExtraIntervals(%u) wlan_2g(%u) a2dp_crit(%u) bt_qos_pct(%u) 
3690,ii,[ wal_coex_sched.c : 2218 ] COEX_SET_WEIGHT_GROUP3: Setting coex weight group 3 BT hasn't been non-critical pCoexDev->DynamicOcsSchedReq = %d  pBtCoexWeightDev->resetWtVdevPause= %d 
3689,i,[ wal_coex_sched.c : 2230 ] COEX_SET_WEIGHT_GROUP6: Setting coex weight group six pCoexDev->DynamicOcsSchedReq %d 
3688,ii,[ wal_coex_sched.c : 2239 ] COEX_SET_WEIGHT_GROUP3: Else part pCoexDev->DynamicOcsSchedReq = %d  pBtCoexWeightDev->resetWtVdevPause= %d 
3687,IIIIII,[ wal_coex_sched.c : 357 ] COEX_TRF_FREERUN: NextIntvl(%u) SchedIntvl(%u) AllocatedBtIntervals(%u) BtIntervalCnt(%u) AllocatedWlanIntervals(%u) WlanIntervalCnt(%u) 
3686,IIII,[ wal_coex_sched.c : 99 ] COEX_TRF_FREERUN_FTM: NextIntvl(%u) SchedIntvl(%u) BtIntervalCnt(%u) WlanIntervalCnt(%u) 
3685,IIIIII,[ wal_coex_sched.c : 2349 ] COEX_TRF_LOWLATENCY_MODE: NextIntvl(%u) SchedIntvl(%u) AllocatedBtIntervals(%u) BtIntervalCnt(%u) AllocatedWlanIntervals(%u) WlanIntervalCnt(%u) 
3684,IIIII,[ wal_coex_sched.c : 573 ] COEX_TRF_SHAPE_OCS: interval(%u) Dur(%u) Latency(%u) ConcurrState(0x%x) wlan_2g(%u) 
3683,IIIIII,[ wal_coex_sched.c : 1832 ] COEX_TRF_SHAPE_PSP: Error(0x%x) NextInterval(%u) wght(%u) IntrvalDur(%u) BtTriggerRecieved(%u) IS_PSP_ALG_WLAN_CRITICAL(%u) 
3682,IIIiI,[ wal_coex_sched.c : 2423 ] COEX_TRF_SOCS: sched(%u) wlan_duration(%u) bt_duration(%u) pBtCoexSchedDev->sync_ocs_sched_req(%d) socsstate(%u) 
3720,iii,[ wal_coex_txgrant.c : 331 ] WAL_COEX_TXGRANT: Allow lock request, client=%d band=%d locked=%d 
3719,,[ wal_coex_txgrant.c : 266 ] WAL_COEX_TXGRANT: De-Reg Pre STM Crash Handler : Success 
3718,,[ wal_coex_txgrant.c : 270 ] WAL_COEX_TXGRANT: De-Reg Pre STM Crash Handler : Fail 
3717,iiii,[ wal_coex_txgrant.c : 702 ] WAL_COEX_TXGRANT: Delay req fail! client=%d band=%d crash_on_going=%d deinit=%d 
3716,i,[ wal_coex_txgrant.c : 85 ] WAL_COEX_TXGRANT: ++++TxGrant Manager dump 2.4g band. macid=%d 
3715,iI,[ wal_coex_txgrant.c : 98 ] WAL_COEX_TXGRANT: Allow lock client=%d, [lock|valid]=%08x 
3714,iIii,[ wal_coex_txgrant.c : 110 ] WAL_COEX_TXGRANT: Immed client=%d, [infinit|auto|applied|txgrant|valid]=%08x req_time=%d life_time=%d] 
3713,iIiii,[ wal_coex_txgrant.c : 123 ] WAL_COEX_TXGRANT: Delay client=%d, [infinite|auto|applied|txgrant|valid]=%08x req_time=%d life_time=%d hw_time=%d 
3712,Iii,[ wal_coex_txgrant.c : 131 ] WAL_COEX_TXGRANT: Arbiter result [infinit|txgrant|mode]%08x hw_time=%d life_time%d 
3711,i,[ wal_coex_txgrant.c : 88 ] WAL_COEX_TXGRANT: ++++TxGrant Manager dump 5g band. macid=%d 
3710,,[ wal_coex_txgrant.c : 90 ] WAL_COEX_TXGRANT: TxGrant Manager dump invalid band 
3709,ii,[ wal_coex_txgrant.c : 628 ] WAL_COEX_TXGRANT:   immed mute duplicated. client=%d band=%d 
3708,iiii,[ wal_coex_txgrant.c : 577 ] WAL_COEX_TXGRANT: Immed req fail! client=%d band=%d crash_on_going=%d, deinit=%d 
3707,iiii,[ wal_coex_txgrant.c : 581 ] WAL_COEX_TXGRANT: Immed req client=%d band=%d value=%d life_time=%d 
3706,,[ wal_coex_txgrant.c : 257 ] WAL_COEX_TXGRANT: Reg Pre STM Crash Handler : Fail 
3705,II,[ wal_coex_txgrant.c : 170 ] WAL_COEX_TXGRANT: Power event: [src|event|macid|band]=0x%08x, [5g_mac|2g_mac]=0x%08x 
3704,iii,[ wal_coex_txgrant.c : 507 ] WAL_COEX_TXGRANT: Apply error. macid=%d,band=%d,readback result=%d 
3703,ii,[ wal_coex_txgrant.c : 833 ] WAL_COEX_TXGRANT: Auto allow immed client=%d, band=%d 
3702,ii,[ wal_coex_txgrant.c : 843 ] WAL_COEX_TXGRANT: Auto allow delay client=%d, band=%d 
3701,ii,[ wal_coex_txgrant.c : 796 ] WAL_COEX_TXGRANT: Sched update band=%d timeout=%d 
3700,Iiii,[ wal_coex_txgrant.c : 552 ] WAL_COEX_TXGRANT: Arb result:[infinite|macid|band|mode]=%08x, txgrant=%d hw_time:%d, life_time:%d 
3722,IIII,[ wal_coex_policy.c : 1035 ] WAL_COEX_ALGO: algo(%u) prev_algo(%u) [ftm|sep_ant|lte|nan|a2dp|hid|aptx_ll|voice](0x%08x), [wlan_ll|asha|ba|ant|not_conn|mpta_hlpr|force_pol](0x%08x) 
3721,Ii,[ wal_coex_policy.c : 1109 ] WAL_COEX_LOW_LATENCY: num_coex_latency_mode_a2dp_profiles %u a2dpbw %d 
3725,IiI,[ wal_coex_tws.c : 469 ] WAL_COEX_TWS_GPM: error(0x%x) status(%d) tws_linkid(%u) 
3724,IiI,[ wal_coex_tws.c : 441 ] WAL_COEX_TWS_GPM: error(0x%x) status(%d) tws_linkid(%u) 
3723,IiI,[ wal_coex_tws.c : 497 ] WAL_COEX_TWS_GPM: error(0x%x) status(%d) tws_linkid(%u) 
3730,i,[ wal_coex_ftm.c : 145 ] WAL_COEX_FTM: wal_coex_ftm.c LINE=%d FTM_CAL_START 
3729,iii,[ wal_coex_ftm.c : 186 ] WAL_COEX_FTM: wal_coex_ftm.c LINE=%d FTM_TX_RX_STOP state=%d chan=%d 
3728,i,[ wal_coex_ftm.c : 154 ] WAL_COEX_FTM: wal_coex_ftm.c LINE=%d FTM_CAL_STOP 
3727,iii,[ wal_coex_ftm.c : 163 ] WAL_COEX_FTM: wal_coex_ftm.c LINE=%d FTM_TX_RX_START state=%d, chan=%d 
3726,i,[ wal_coex_ftm.c : 46 ] WAL_COEX_FTM: wal_coex_ftm.c LINE=%d FTM_INIT 
3734,IIIIII,[ wal_coex_power.c : 743 ] WAL_COEX_POWER_CHANGE: Error(0x%x) mac(%u) event_type(%u) cur_state(0x%x) new_state(0x%x) all_mac_sleeping(%u) 
3733,i,[ wal_coex_power.c : 748 ] WAL_COEX_POWER_CHANGE: Invalid wlan_id from power event, wlan_id=%d 
3732,IIIIIIII,[ wal_coex_power.c : 386 ] WAL_COEX_SLEEP: status(%u) bm_0(0x%08x) bm_1(0x%08x) [mac|vote|btc|mws|wow](0x%05x) src(%u) [orig|override]reasons(0x%08x) num_2g_vdev(%u) sleep_vote_bt_int(%u) 
3731,i,[ wal_coex_power.c : 502 ] COEX_POWER_CHANGE: PHY is ON - Coex recipe change is best effort. mac_id(%d) 
3735,,[ wal_coex_gnss.c : 42 ] COEX_MWS_REMOTE_EVENT: Received GNSS coex msg 
3740,iiiiii,[ wal_coex_stats.c : 34 ] COEX_STATS_PDG_CNTRS: COEX STATS PDG CNTRS Ant %d Mcs %d Pwr %d Bw %d TxWin %d RxWin %d 
3739,iiiiiiii,[ wal_coex_stats.c : 82 ] COEX_STATS_CONC_CNTRS:                 tx_status_fes_tx_end_cntr                 %d tx_status_fes_tx_start_cntr             %d,                 tx_flush_cntr                             %d tbtt_cntr                               %d,                 wl_in_tx_abort_cntr                       %d wl_tx_auto_resp_req_cntr                %d,                 wl_tx_req_ack_cntr                        %d wl_tx_req_cntr                          %d  
3738,i,[ wal_coex_stats.c : 88 ] COEX_STATS_BT: Invalid mac ID %d 
3737,iiiiiiii,[ wal_coex_stats.c : 54 ] COEX_STATS_CONC_CNTRS:                 bt_tx_req_cntr                            %d bt_rx_req_cntr                          %d                 concurrent_bt_rx_wl_rx_cntr               %d concurrent_bt_tx_wl_rx_cntr             %d                 concurrent_bt_rx_wl_tx_cntr               %d concurrent_bt_tx_wl_tx_cntr             %d                 tx_status_resp_tx_start_cntr              %d tx_status_fes_end_cntr                  %d  
3736,iiiiiiii,[ wal_coex_stats.c : 68 ] COEX_STATS_CONC_CNTRS:                 wl_tx_req_nack_schd_bt_reason_cntr        %d wl_tx_req_nack_current_bt_reason_cntr   %d,                wl_tx_req_nack_other_wlan_tx_reason_cntr  %d wl_tx_req_nack_lcmh_reason_cntr         %d,                tx_resp_concurrent_wlan_tx_cntr           %d tx_resp_alt_based_cntr                  %d,                tx_resp_default_based_cntr                %d tx_status_resp_tx_end_cntr              %d 
3748,iiii,[ wal_coex_init.c : 364 ] COEX_MWS_INIT: 6GHz_Coex : TxPwrThr6gToLaa:%d, TxPwrThr5gToLaa:%d, TxPwrThr5gToN79:%d, CoexFreqThr5gToN79%d 
3747,,[ wal_coex_init.c : 393 ] COEX_MWS_INIT: Switch based 2G Antenna Sharing Enabled 
3746,,[ wal_coex_init.c : 399 ] COEX_MWS_INIT: Extractor based 2G Antenna Sharing Enabled 
3745,,[ wal_coex_init.c : 403 ] COEX_MWS_INIT: 2G Antenna Sharing Disabled 
3744,i,[ wal_coex_init.c : 413 ] COEX_MWS_INIT: COEX_BT_THIRD_ANT = %d 
3743,,[ wal_coex_init.c : 710 ] COEX_MWS_INIT: MWS Init Done 
3742,iI,[ wal_coex_init.c : 381 ] COEX_MWS_INIT: LTE_PHY_EXIST = %d ;coex_flags:0x%x 
3741,I,[ wal_coex_init.c : 386 ] COEX_MWS_INIT: AntShare BDF Flags = 0x%x 
3752,I,[ wal_coex_cal.c : 298 ] COEX_POLL_BT_CAL_DONE_TIMEOUT: BtCalState(0x%x) 
3751,III,[ wal_coex_cal.c : 84 ] COEX_RX_MCI_GPM_BT_CAL_MSG: OpCode(0x%x) WlanCalState(0x%x) BtCalState(0x%x) 
3750,IIII,[ wal_coex_cal.c : 245 ] COEX_WLAN_CAL_END: caltype: %u, BtCalState(0x%x) WlanCalState(0x%x), mhz: %u 
3749,IIII,[ wal_coex_cal.c : 186 ] COEX_WLAN_CAL_START: caltype: %u, BtCalState(0x%x) WlanCalState(0x%x), mhz: %u 
3783,III,[ wal_coex_gpm.c : 222 ] WAL_MCI_GPM_SENT: UpdatePendingFlag - pending_msg_bm (0x%08x), QFlags (0x%08x) gpm_ack_bm (0x%08x) 
3782,IIIIIII,[ wal_coex_gpm.c : 554 ] WHAL_MCI_GPM_SENT: WLAN Conn Status Report : 5g_ch_3_2_1_0(0x%08x), 2g_ch_1_0(0x%04x) operating_mode(0x%x) wlm(0x%x) coexLL(%u), war361(0x%x), dbam(%u) 
3781,IIII,[ wal_coex_gpm.c : 694 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - WLAN set ACL Inactivity Report : InactivityThresh(0x%x) LinkID(0x%x) 
3780,IIIIIII,[ wal_coex_gpm.c : 570 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x]- WLAN Unused channels : 0x%x 0x%x 0x%x 0x%x 0x%x 
3779,IIII,[ wal_coex_gpm.c : 1142 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - ASD Status Indication: grant(%u) reason(%u) 
3778,III,[ wal_coex_gpm.c : 1048 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Start BT RSSI Reporting: period(0x%x)second 
3777,IIII,[ wal_coex_gpm.c : 914 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - BT Airtime Stats Req: NumOfDelivery(0x%x) TestInterval(0x%x) 
3776,IIII,[ wal_coex_gpm.c : 644 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - BT Update flags : Opcode(0x%x) BT Flags(0x%x) 
3775,III,[ wal_coex_gpm.c : 1027 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Limit BT Max TX power : power(0x%x)dbm 
3774,IIIII,[ wal_coex_gpm.c : 674 ] WAL_MCI_GPM_SENT: OBSOLETE[0x%x] [0x%x] - BT Pause profile : PauseSlot(0x%x) ProfileBitmap(0x%x) Data(0x%x) 
3773,IIIII,[ wal_coex_gpm.c : 722 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - BT remote registry write : Address(0x%x) Value(0x%x) Op(0x%x) 
3772,II,[ wal_coex_gpm.c : 740 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Query BT RXSS Minimum Threshold 
3771,III,[ wal_coex_gpm.c : 761 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Set BT RXSS Minimum Threshold : Threshold(0x%x) 
3770,IIIIII,[ wal_coex_gpm.c : 596 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x]- Status Query : WLAN QueryType(0x%x) Source 0x%x pending_msg_bm (0x%x) pending_msg_ack_bm (0x%x) 
3769,III,[ wal_coex_gpm.c : 1006 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Read BT TX power : LinkId(0x%x) 
3768,I,[ wal_coex_gpm.c : 460 ] WAL_MCI_GPM_SENT: [0x%x] - CAL DONE 
3767,Ii,[ wal_coex_gpm.c : 427 ] WAL_MCI_GPM_SENT: [0x%x] - CAL GRANT, ret= %d 
3766,I,[ wal_coex_gpm.c : 443 ] WAL_MCI_GPM_SENT: GPM Sent [0x%x] -  CAL REQ 
3765,IIIIII,[ wal_coex_gpm.c : 1163 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Coex Policy Indication: policy(%u), grant_bt(%u) wlan_dur(%u), bt_dur(%u) 
3764,III,[ wal_coex_gpm.c : 1070 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - concurrent TX on chain0(%u) 
3763,IIII,[ wal_coex_gpm.c : 886 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Send group priority config : Op(0x%x) Priority(0x%x) 
3762,III,[ wal_coex_gpm.c : 617 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Disable BT GPM : State(0x%x) 
3761,IIIIII,[ wal_coex_gpm.c : 1231 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - ISO Priority Update : grpid(%u) config(%u) priority_bmap(%u) mci_prio(0x%x) 
3760,IIII,[ wal_coex_gpm.c : 1252 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - ISO Subevent Mask : linkid(%u) mask(0x%x) 
3759,IIIIII,[ wal_coex_gpm.c : 938 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - LE Data Len Req : op(%u) id(%u) max_tx(%u) max_rx(%u) 
3758,IIIII,[ wal_coex_gpm.c : 822 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Send priority config : Op(0x%x) Priority(0x%x) IsRead(0x%x) 
3757,IIIIII,[ wal_coex_gpm.c : 792 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - Sched info trigger : TriggerEnaNum(0x%x) TriggerType(0x%x) LowerBound(0x%x) UpperBound(0x%x) 
3756,IIIIIII,[ wal_coex_gpm.c : 489 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x]- Version query Major(0x%x) Minor(0%x) Cap_cfg(0x%x) pending_msg_bm (0x%x) pending_msg_ack_bm (0x%x) 
3755,IIIII,[ wal_coex_gpm.c : 514 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - WLAN Version resp. : Major(0x%x) Minor(0x%x) Cap_cfg(0x%x) 
3754,IIIIII,[ wal_coex_gpm.c : 1122 ] WHAL_MCI_GPM_SENT: [0x%x] [0x%x] WLAN Capabilities ctr(0x%x) cap W1(0x%x) cap W2(0x%x) cap B3(0x%x) 
3753,III,[ wal_coex_gpm.c : 986 ] WAL_MCI_GPM_SENT: [0x%x] [0x%x] - WLAN Status Update : Status(0x%x) 
3786,II,[ wal_coex_dbs.c : 118 ] WAL_COEX_BDF_INFO: coex_flags:0x%x, coex_config:0x%x 
3785,IIIIIII,[ wal_coex_dbs.c : 127 ] WAL_COEX_MODE_CHANGE: new_mode(%u) old_mode(%u) band_mac_map(0x%x) mac0_settings(0x%x) mac1_settings(0x%x) mac0_2x2(%u) mac1_2x2(%u) 
3784,III,[ wal_coex_dbs.c : 237 ] WAL_COEX_VDEV_STATE: COEX_VDEV_MIGRATE: old_mac_id %u, new_mac_id %u, old_mac_pwr_state %u 
3787,Ii,[ wal_coex_asd.c : 79 ] WAL_COEX_ASD: Status mismatch: bt_status(0x%x) prev_grant(0x%d) 
3797,I,[ wal_coex_sar.c : 182 ] COEX_MWS_SAR: mode update [test|2G|5G|6G|BT|old|new]=0x%08x 
3796,,[ wal_coex_sar.c : 75 ] COEX_MWS_SAR: SAR context is not initialized 
3795,iiii,[ wal_coex_sar.c : 79 ] COEX_MWS_SAR: cmd=%d, rows=%d, commit=%d, version=%d 
3794,i,[ wal_coex_sar.c : 96 ] COEX_MWS_SAR: SAR version:%d doesn't support 
3793,i,[ wal_coex_sar.c : 479 ] COEX_MWS_SAR: [Error] invalid active index set (%d) 
3792,iiiii,[ wal_coex_sar.c : 528 ] COEX_MWS_SAR: [SAR][Error] counted more SAR limit rows (%d) than recorded (%d) band(%d) mod(%d) chain(%d) 
3791,iiiIII,[ wal_coex_sar.c : 547 ] COEX_MWS_SAR: [SAR] %d get sar_limits[%d](chain,band, mod, limit)=(%d,0x%x,0x%x,0x%x) 
3790,iiiII,[ wal_coex_sar.c : 554 ] COEX_MWS_SAR: Returning from get_sar_limit_rows (%d),num_limit_rows:%d,sar_num_limits:%d,active_index:%u,Err:0x%x 
3789,iI,[ wal_coex_sar.c : 574 ] COEX_MWS_SAR: SAR_GET : index=%d, err=0x%x 
3788,III,[ wal_coex_sar.c : 285 ] COEX_MWS_SAR: chain0=%x, chain1=%x, result=%x 
3824,IIIII,[ wal_coex_iso.c : 2410 ] WAL_COEX_ISO_GET_PRIO_THRESH: status(%u) loc_profile_type(%u) cp_perc_thresh(%u) hp_perc_thresh(%u) mp_perc_thresh(%u) 
3823,IIII,[ wal_coex_iso.c : 1919 ] WAL_COEX_APTX_HQ_ISO_GET_SUBEVENT_MASK: total_nse(%u) bt_bw_nse(%u) mask(0x%x) is_mask_valid(%u) 
3822,III,[ wal_coex_iso.c : 1726 ] WAL_COEX_ISO_DETECT_PROFILE_TYPE: loc_profile_type(%u) iso_codec(%u) latency_ms(%u) 
3821,II,[ wal_coex_iso.c : 219 ] WAL_COEX_ISO_PROC_LINK: error(0x%x) status(0x%x) 
3820,IIII,[ wal_coex_iso.c : 1206 ] WAL_CEOX_ISO_INT_BM: status(%u) intvl_bm(0x%x) bt_dur(%u) wlan_dur(%u) 
3819,IIIIII,[ wal_coex_iso.c : 797 ] WAL_COEX_ISO_ACT_BM: status(0x%x) nearest_bt_start_time(%u) curr_bt_start_time(%u) curr_bt_dur(%u), curr_interval(%u) bt_bm(0x%x) 
3818,iIIIIIIII,[ wal_coex_iso.c : 1395 ] WAL_COEX_ISO_BT_TSF: status(%d) sched_start(%u) sched_stop(%u) now(%u) eff_bt(%u) eff_wlan(%u) bt(%u) wlan(%u) bt_tsf(%u) 
3817,iIIIIIII,[ wal_coex_iso.c : 1428 ] WAL_COEX_ISO_BT_TSF: status(%d) sched_start(%u) now(%u) delta(%u) eff_bt(%u) eff_wlan(%u) bt_tsf(%u) dur(%u) 
3816,II,[ wal_coex_iso.c : 1287 ] WAL_COEX_ISO_EFF_INTRVL: WLAN(%u) BT(%u) 
3815,IIIIIIII,[ wal_coex_iso.c : 1271 ] WAL_COEX_ISO_NET_ALGO: int_bm(0x%x) algo_bm(0x%x) net_policy_bm(0x%x) policy(%u) legacy_policy(%u) wlan_intrvl(%u) bt_intrvl(%u) total_active_iso_dc(%u) 
3814,IIII,[ wal_coex_iso.c : 651 ] WAL_COEX_ISO_SCHED_INFO: link_id(%u) nearest_bt_start_time(%u) sched_entry_start_ts(%u) curr_wb_time(%u) 
3813,iiiiii,[ wal_coex_iso.c : 1092 ] WAL_CEOX_ISO_BT_TSF: next_bt_tsf(%d) intrvl(%d) now(%d) time_elapsed(%d) intrvl_elapsed(%d) iso.eff_wlan_dur(%d) 
3812,II,[ wal_coex_iso.c : 826 ] WAL_COEX_ISO_ERR_PATTERN: length(%u) st_idx(%u) 
3811,IIIIIII,[ wal_coex_iso.c : 964 ] WAL_COEX_ISO_SCHED_ML: status(0x%x) bt_start_time(%u) hp_dur(%u) merging_done(%u) indx(0x%x)) bitrate_mode(%u) dbr_sdu_size(%u) 
3810,IIIIIIII,[ wal_coex_iso.c : 2081 ] WAL_COEX_HQ_ISO_GET_APTX_SCHEDULE: start_ts_set(%u) curr_start_ts(%u) sch_start_ts(%u) sync_ts(%u) cur_intvl_delta(%u) num_skip_iso_intvl(%u) bt_dur(%u) now(%u) 
3809,IIIIIIII,[ wal_coex_iso.c : 2156 ] WAL_COEX_HQ_ISO_GET_LC3_SCHEDULE: start_ts_set(%u) curr_start_ts(%u) sch_start_ts(%u) sync_ts(%u) cur_intvl_delta(%u) num_skip_iso_intvl(%u) bt_dur(%u) now(%u) 
3808,IIII,[ wal_coex_iso.c : 2287 ] WAL_COEX_ISO_GET_SCHEDULE_Q2Q: loc_profile_type(%u) schedule_start_time(%u) bt_duration(%u) wl_duration(%u) 
3807,IIII,[ wal_coex_iso.c : 2381 ] WAL_COEX_ISO_GET_SCHEDULE_UCAST_VOICE: loc_profile_type(%u) schedule_start_time(%u) bt_duration(%u) wl_duration(%u) 
3806,IIII,[ wal_coex_iso.c : 2297 ] WAL_COEX_ISO_GET_SCHEDULE_APTX_HQ: loc_profile_type(%u) schedule_start_time(%u) bt_duration(%u) wl_duration(%u) 
3805,IIII,[ wal_coex_iso.c : 2325 ] WAL_COEX_ISO_GET_SCHEDULE_LC3_HQ: loc_profile_type(%u) schedule_start_time(%u) bt_duration(%u) wl_duration(%u) 
3804,IIII,[ wal_coex_iso.c : 1969 ] WAL_COEX_LC3_HQ_ISO_GET_SUBEVENT_MASK: total_nse(%u) bt_bw_nse(%u) mask(0x%x) is_mask_valid(%u) 
3803,iiiii,[ wal_coex_iso.c : 1022 ] WAL_COEX_ISO_LU_OV: iso_wlan_intrvl(%d) iso_bt_intrvl(%d) bt_intrvl(%d) wlan_intrvl(%d) policy(%d)) 
3802,IIIIIIIIi,[ wal_coex_iso.c : 1529 ] WAL_COEX_ISO_PRIO_MASK: result(%u) link_id(%u) sdu_size(%u) piconet_clk(%u) stream_idx(%u) prio_mask(0x%x) prev_hp_dur(%u) curr_hp_dur(%u) hp_dc(%d) 
3801,IIIIIIIII,[ wal_coex_iso.c : 1459 ] WAL_COEX_QOS_ISO_INFO: group_id(%u) reason(%u) codec_info(%u) M2S_SDU_size(%u) S2M_SDU_size(%u) tx_flush_to(%u) rx_flush_to(%u) latency_ms(%u) vbc(%u) 
3800,III,[ wal_coex_iso.c : 2003 ] WAL_COEX_ISO_RESET_BT: now(%u) sync_ts(%u) delta(%u) 
3799,IIIIIII,[ wal_coex_iso.c : 1788 ] WAL_COEX_ISO_SET_LOC_PROFILE_TYPE: profile_type(%u) loc_profile_type(%u) iso_codec(%u) latency_ms(%u) iso_interval_slots(%u) min_ft(%u) min_hp_dc(%u) 
3798,II,[ wal_coex_iso.c : 1646 ] WAL_COEX_ISO_LEGACY_PROFILE: grpid(%u) loc_profile_type(%u) 
3831,,[ wal_cold_boot_cal.c : 478 ] cold boot cal start 
3830,ii,[ wal_cold_boot_cal.c : 546 ] Cold Boot Cal, 8 second timeout: actual time taken = %d, coexFlags = %d 
3829,iiiii,[ wal_cold_boot_cal.c : 603 ] CBC:: pdev %d phy_mode %d mhz %d freq1 %d freq2 %d 
3828,I,[ wal_cold_boot_cal.c : 666 ] CBC:: Total time taken for CBC = %u us 
3827,iI,[ wal_cold_boot_cal.c : 529 ] CBC:: phy mode %d cal duration so far %u us 
3826,ii,[ wal_cold_boot_cal.c : 538 ] Cold Boot Cal, 4 second timeout: actual time taken = %d, coexFlags = %d 
3825,i,[ wal_cold_boot_cal.c : 271 ] cold_boot_cal start time in USecs: %d 
3841,iiiIIII,[ wal_concurrency.c : 535 ] tsf_alloc: pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
3840,iiIIIiII,[ wal_concurrency.c : 996 ] staid_alloc: pdev_id = %d vdev_id = %d (%x.%x.%x) type = %d sta_id = 0x%x pdev_sta_id_map = 0x%x 
3839,iiIIIiII,[ wal_concurrency.c : 1108 ] staid_free: pdev_id = %d vdev_id = %d (%x.%x.%x) type = %d sta_id = 0x%x pdev_sta_id_map = 0x%x 
3838,iiiIIII,[ wal_concurrency.c : 844 ] tsf_free: pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
3837,iiIII,[ wal_concurrency.c : 1549 ] wal_vdev_add_random_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x 
3836,iiIII,[ wal_concurrency.c : 1591 ] wal_vdev_del_random_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x 
3835,IiiiIIII,[ wal_concurrency.c : 626 ] tsf_realloc (flag=0x%x): pdev_id = %d vdev_id = %d type = %d tsf_id = 0x%x bss_id = 0x%x pdev_tsf_id_map = 0x%x pdev_bss_id_map = 0x%x 
3834,iiiII,[ wal_concurrency.c : 1479 ] wal_vdev_restore_mac: pdev_id = %d vdev_id = %d spoof_type = %d sta_id = 0x%x spoof_sta_id=0x%x 
3833,iiIIIIII,[ wal_concurrency.c : 1498 ] wal_vdev_set_mac_addr: pdev_id = %d vdev_id = %d mac=%02x:%02x:%02x:%02x:%02x:%02x 
3832,iiIIIiII,[ wal_concurrency.c : 1399 ] wal_vdev_set_spoofed_mac_addr: pdev_id = %d vdev_id = %d spoof_mac=%x.%x.%x spoof_type=%d sta_id = 0x%x spoof_sta_id=0x%x 
3870,IIIiiI,[ ar_wal_phy_dev.c : 1576 ] _wal_dev_reset: mode=%x,c0=%lx,c1=%lx,inprog=%d,dis=%d,en=%x 
3869,iii,[ ar_wal_phy_dev.c : 533 ] DATA_STALL: Type=%d FAIL_CNT[%d]=%d 
3868,i,[ ar_wal_phy_dev.c : 314 ] DATA_STALL detection: PAUSE, pdev_id:%d 
3867,iii,[ ar_wal_phy_dev.c : 763 ] DATA_STALL monitor: TIMEOUT, pdev_id:%d pause_countdown:%d active_vdev_cnt:%d 
3866,IIIIII,[ ar_wal_phy_dev.c : 5777 ] DISPLAY_TPC_STATS: ctl_array_type is %lu ctl_array_len is %lu d1 is %lu d2 is %lu d3 is %lu d4 is %lu 
3865,,[ ar_wal_phy_dev.c : 5806 ] DISPLAY_TPC_STATS: CTL array contents do not match! 
3864,,[ ar_wal_phy_dev.c : 5831 ] DISPLAY_TPC_STATS: CTL array contents do not match! 
3863,II,[ ar_wal_phy_dev.c : 5649 ] DISPLAY_TPC_STATS: rate_array_type is %lu rate_array_len is %lu 
3862,,[ ar_wal_phy_dev.c : 5673 ] DISPLAY_TPC_STATS: Rates array contents do not match! 
3861,I,[ ar_wal_phy_dev.c : 5436 ] DISPLAY_TPC_STATS: wal_pdev_get_ctl_array_len totalSize = %lu 
3860,I,[ ar_wal_phy_dev.c : 5461 ] DISPLAY_TPC_STATS: wal_pdev_get_rates_array_len:  totalSize = %lu 
3859,ii,[ ar_wal_phy_dev.c : 331 ] DATA_STALL: rssi:%d vdev_id:%d 
3858,IIIIII,[ ar_wal_phy_dev.c : 5530 ] DISPLAY_TPC_STATS: reg_power_type is %lu reg_power_array_len is %lu d1 is %lu d2 is %lu d3 is %lu d4 is %lu 
3857,,[ ar_wal_phy_dev.c : 5556 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
3856,,[ ar_wal_phy_dev.c : 5571 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
3855,,[ ar_wal_phy_dev.c : 5588 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
3854,,[ ar_wal_phy_dev.c : 5605 ] DISPLAY_TPC_STATS: Regulatory array contents do not match! 
3853,III,[ ar_wal_phy_dev.c : 5387 ] DISPLAY_TPC_STATS: wmi_tpc_config tlv header is %lu, chanFreq is %lu, phyMode is %lu 
3852,IIiIIIII,[ ar_wal_phy_dev.c : 5389 ] DISPLAY_TPC_STATS: maxAntennaGain is %lu twiceMaxRDPower is %lu userAntennaGain is %d powerLimit is %lu rateMax is %lu numTxChain is %lu cfgctl is %lu flags is %lu 
3851,IIIIIIIII,[ ar_wal_phy_dev.c : 729 ] DTSD:PVDEV_PEER:%08X,TX_FLG:%08X,VFLGS:%08X,TID_SCH:%08X,MSDU_MPDU:%08X,FLGS:%08X %08X,TICKLE:%08X,NEMPTY:%08X 
3850,IiII,[ ar_wal_phy_dev.c : 743 ] DTSD:peer(%u),tid(%d) no-sched for %uS,CUR(%08X) 
3849,iII,[ ar_wal_phy_dev.c : 2674 ] WAL_DBGID_SET_POWER_STATE pdev = %d current = 0x%x desired = 0x%x 
3848,iiiI,[ ar_wal_phy_dev.c : 2701 ] umac recp_up_dur %d pcie_up_dur %d spm_up_dur %d umac_up_pf %x 
3847,iiii,[ ar_wal_phy_dev.c : 2779 ] pre_pwr_pf %d pwr_chg_pf %d post_pwr_pf %d new_st %d 
3846,iiii,[ ar_wal_phy_dev.c : 2783 ] pre_pwr_dur %d pwr_chg_dur %d post_pwr_dur %d new_st %d 
3845,iiiI,[ ar_wal_phy_dev.c : 2699 ] umac recp_down_dur %d pcie_down_dur %d spm_down_dur %d umac_down_pf %x 
3844,i,[ ar_wal_phy_dev.c : 4591 ] BiosDataType %d 
3843,iiI,[ ar_wal_phy_dev.c : 3287 ] SET_PDEV_PARAM: pdev_id=%d: param=%d value=0x%x 
3842,i,[ ar_wal_phy_dev.c : 3851 ] SET_PDEV_PARAM: DATA_STALL flag param=%d 
3918,i,[ ar_wal_vdev.c : 909 ] start hwbmiss delay wake tmr, timeout:%d 
3917,I,[ ar_wal_vdev.c : 4572 ] %s: NULL pointer 
 
3916,I,[ ar_wal_vdev.c : 4577 ] %s: invalid addr_type 
 
3915,I,[ ar_wal_vdev.c : 4603 ] %s: no buf in pool 
 
3914,I,[ ar_wal_vdev.c : 4623 ] %s: no buf in pool 
 
3913,i,[ ar_wal_vdev.c : 3998 ] SW_DTIM: Improper Beacon due to invalid usRemBufLen 1 for vdev:%d 
3912,iii,[ ar_wal_vdev.c : 4004 ] SW_DTIM: Improper Beacon due to invalid usRemBufLen (%d<%d) for vdev:%d 
3911,iii,[ ar_wal_vdev.c : 4016 ] SW_DTIM: Improper Beacon line due to invalid Dtim count (%d) and period (%d) for vdev :%d 
3910,IiI,[ ar_wal_vdev.c : 4037 ] sw_dtim_power_msg_handler: mac=%u, Beacon RX for vdev=%d, DTIM_set=%u 
3909,,[ ar_wal_vdev.c : 4041 ] sw_dtim_power_msg_handler: Beacon RX but vdev is NULL 
3908,I,[ ar_wal_vdev.c : 4654 ] %s: Invalid addr_type 
 
3907,I,[ ar_wal_vdev.c : 4659 ] %s: List is empty
 
3906,iiiIi,[ ar_wal_vdev.c : 2287 ] wal_vdev_down pdev_id %d vdev_id %d vdev_type %d flags 0x%x cnt_per_opmode %d 
3905,I,[ ar_wal_vdev.c : 4544 ] %s: NULL pointer 
 
3904,II,[ ar_wal_vdev.c : 382 ] flow_config:0x%x 0x%x 
3903,iii,[ ar_wal_vdev.c : 6644 ] vdev_id:%d, prev_channel:%d, current_channel=%d 
3902,I,[ ar_wal_vdev.c : 4760 ] %s: NULL pointer 
 
3901,I,[ ar_wal_vdev.c : 4765 ] %s: Invalid addr_type 
 
3900,I,[ ar_wal_vdev.c : 4770 ] %s: List is empty
 
3899,iIiiii,[ ar_wal_vdev.c : 5462 ] wal_vdev_migrate (%d, 0x%x): pdev %d->%d, active=%d/%d 
3898,ii,[ ar_wal_vdev.c : 5283 ] _wal_vdev_migrate_bring_up: vdev_id = %d rssi_beacon = %d 
3897,iIII,[ ar_wal_vdev.c : 5319 ] _wal_vdev_migrate_bring_up: vdev_id = %d cur_tsf_64 = 0x%x sta_bss_tstamp = 0x%x time_at_sta_bss_tstamp = 0x%x 
3896,ii,[ ar_wal_vdev.c : 5198 ] _wal_vdev_migrate_tear_down: vdev_id = %d rssi_beacon = %d 
3895,iII,[ ar_wal_vdev.c : 5213 ] _wal_vdev_migrate_tear_down: vdev_id = %d sta_bss_tstamp = 0x%x time_at_sta_bss_tstamp = 0x%x 
3894,iIi,[ ar_wal_vdev.c : 348 ] wal_vdev_event_handler: vdev_id=%d event_type=0x%x remote_peer_count=%d 
3893,ii,[ ar_wal_vdev.c : 5145 ] wal_vdev_post_migrate - old_pdev is %d, new_pdev is = %d 
3892,ii,[ ar_wal_vdev.c : 5019 ] wal_vdev_pre_migrate - old_pdev is %d, new_pdev is = %d 
3891,ii,[ ar_wal_vdev.c : 1287 ] wal_vdev_reconfig vdev_id %d  tsf_id is %d 
3890,iII,[ ar_wal_vdev.c : 2486 ] [ERP_PROTECTION]: param_val %d default profile 0x%x new profile 0x%x 
3889,iII,[ ar_wal_vdev.c : 2616 ] vdev_param_he_bss_color_disable: enable bss_color_en on HE assoc, param:%d c:%x:%x 
3888,iII,[ ar_wal_vdev.c : 2623 ] vdev_param_he_bss_color_disable: disable bss_color_en on non-HE assoc, param:%d c:%x:%x 
3887,iII,[ ar_wal_vdev.c : 2642 ] vdev_param_he_bss_color_disable: disable bss_color_en on non-HE assoc/inv_bssid, param:%d c:%x:%x 
3886,iII,[ ar_wal_vdev.c : 2646 ] vdev_param_he_bss_color_disable: enable bss_color_en on HE assoc/inv_bssid, param:%d c:%x:%x 
3885,ii,[ ar_wal_vdev.c : 2686 ] WAL_VDEV_PARAM_HE_RTS_THRESHOLD_TU: new_rts_thres=%d vdev_id=%d 
3884,i,[ ar_wal_vdev.c : 2901 ] #### vdev->packet_capture_mode %d #### 
3883,iiii,[ ar_wal_vdev.c : 1712 ] wal_vdev_start vdev_id %d vdev_type %d vdev's mac %dbss_peer %d 
3882,,[ ar_wal_vdev.c : 6052 ] _wal_vdev_state_publish: Entry  
3881,ii,[ ar_wal_vdev.c : 6094 ] _wal_vdev_state_publish: vdev_type_state is %d, vdev_id_state = %d  
3880,iiiiii,[ ar_wal_vdev.c : 6103 ] _wal_vdev_state_publish: mac_address is %d:%d:%d:%d:%d:%d  
3879,,[ ar_wal_vdev.c : 6108 ] _wal_vdev_state_publish: Exit  
3878,ii,[ ar_wal_vdev.c : 6056 ] _wal_vdev_state_publish: bytes is %d, less than output size = %d  
3877,i,[ ar_wal_vdev.c : 6063 ] _wal_vdev_state_publish: vdev_id_map %d  
3876,i,[ ar_wal_vdev.c : 6068 ] _wal_vdev_state_publish: vdev  %d  
3875,i,[ ar_wal_vdev.c : 1840 ] Spectral disabled as vdevs are zero: pdev:%d  
3874,ii,[ ar_wal_vdev.c : 1857 ] wal_vdev_stop vdev_id %d vdev_type %d 
3873,i,[ ar_wal_vdev.c : 2078 ] wal_vdev_up: force enable bss_color_en on HE assoc, color:%d 
3872,iiiIi,[ ar_wal_vdev.c : 2227 ] wal_vdev_up: pdev_id %d vdev_id %d, vdev_type %d flags 0x%x cnt_per_opmode %d 
3871,IIIIII,[ ar_wal_vdev.c : 2131 ] pdev(%x)peer %x,vdev-up for tidLen update,refcnt=%x,htc=%x,remap=%x,security=%x 
3922,ii,[ ar_wal_soc_dev.c : 720 ] wal_soc_set_mac_active: nss applied for mac0 -  %d and %d 
3921,iiiii,[ ar_wal_soc_dev.c : 758 ] wal_soc_set_mac_active: mhz=%d mac_id=%d  tx_resumed=%d last_pdev_state=%d dpd_cal=%d 
3920,i,[ ar_wal_soc_dev.c : 1071 ] wal_soc_switch_mode: Start switching to mode = %d 
3919,iiii,[ ar_wal_soc_dev.c : 1095 ] wal_soc_switch_mode: mac_id=%d Tx/Rx chainmask: %d %d pdev_state = %d 
3923,,[ ar_wal_dev_init.c : 1143 ] wal_coex_init() 
3925,ii,[ wal_dfs.c : 326 ] WAL_DFS_SCHED_SUSPEND_HNDLR thrd_id = %d pdev_id = %d 
3924,II,[ wal_dfs.c : 344 ] %s: thread_id=%lx received DFS_SUSPEND msg
 
3972,II,[ ar_wal_connection_pause.c : 4058 ] module_id:%x,pause_id:%x 
3971,Ii,[ ar_wal_connection_pause.c : 1989 ] Tx_Pause: WAL_PEER_EVENT_SEND_N_COMPLETE sent: peer:0x%x, tid_num:%d 
3970,,[ ar_wal_connection_pause.c : 3037 ] Tx_Pause: ar_wal_tx_pause_check_pending_pdev_cmd_completions: (qpeer == NULL) 
3969,,[ ar_wal_connection_pause.c : 3708 ] Tx_Pause: ar_wal_tx_pause_no_resp_req_handler: (qpeer == NULL) 
3968,IiiI,[ ar_wal_connection_pause.c : 3725 ] Tx_Pause: WAL_PEER_SEND_N_REQ rcvd: peer:0x%x, tidno:%d, num_frames:%d, flags:0x%x [No_Resp] 
3967,,[ ar_wal_connection_pause.c : 3757 ] Tx_Pause: ar_wal_tx_pause_no_resp_req_handler: (qpeer == NULL) 
3966,IiiI,[ ar_wal_connection_pause.c : 3768 ] Tx_Pause: WAL_PEER_PS_PRE_REQ rcvd: peer:0x%x, force_ps:%d, pm_ts:%d, paused_tidmask:0x%x  [No_Resp] 
3965,i,[ ar_wal_connection_pause.c : 3778 ] Tx_Pause: WAL_VDEV_TX_PAUSE_RESET_IND rcvd: vdev_id:%d [No_Resp] 
3964,Ii,[ ar_wal_connection_pause.c : 3789 ] Tx_Pause: WAL_TX_PAUSE_TID_CREATE rcvd: peer:0x%x, tid_num:%d [No_Resp] 
3963,i,[ ar_wal_connection_pause.c : 3799 ] Tx_Pause: WAL_TX_PAUSE_VDEV_CREATE rcvd: vdev_id:%d [No_Resp] 
3962,I,[ ar_wal_connection_pause.c : 3809 ] Tx_Pause: WAL_TX_PAUSE_PEER_RESET rcvd: peer:0x%x [No_Resp] 
3961,i,[ ar_wal_connection_pause.c : 3819 ] Tx_Pause: WAL_TX_PAUSE_HWQ_EMPTY rcvd: tid_num:%d [No_Resp] 
3960,i,[ ar_wal_connection_pause.c : 3829 ] Tx_Pause: WAL_CHECK_PENDING_CMDS_VDEV rcvd: vdev_id:%d [No_Resp] 
3959,i,[ ar_wal_connection_pause.c : 3839 ] Tx_Pause: WAL_CHECK_PENDING_CMDS_PDEV rcvd: pdev_id:%d [No_Resp] 
3958,i,[ ar_wal_connection_pause.c : 3847 ] Tx_Pause: unsupported no-resp request id:%d 
3957,iiii,[ ar_wal_connection_pause.c : 3389 ] Tx_Pause: WAL_PDEV_TX_PAUSE_REQ rcvd: pdev_id:%d, module_id:%d, block:%d, filter:%d 
3956,iii,[ ar_wal_connection_pause.c : 3418 ] Tx_Pause: WAL_PDEV_TX_UNPAUSE_REQ rcvd: pdev_id:%d, module_id:%d, block:%d 
3955,i,[ ar_wal_connection_pause.c : 3438 ] Tx_Pause: unsupported pdev request id:%d 
3954,I,[ ar_wal_connection_pause.c : 3603 ] Tx_Pause: ar_wal_tx_pause_peer_req_handler: (qpeer == NULL), mod=%u 
3953,IiIIi,[ ar_wal_connection_pause.c : 3620 ] Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_REQ rcvd: peer:0x%x, module_id:%d, tids_to_block:0x%x, tids_to_unblock:0x%x, filter:%d 
3952,IiIIi,[ ar_wal_connection_pause.c : 3662 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_EXT_REQ rcvd: 1st_peer:%u, module_id:%d, tids_to_pause:0x%x, tids_to_unpause:0x%x, filter:%d 
3951,i,[ ar_wal_connection_pause.c : 3681 ] Tx_Pause: unsupported peer request id:%d 
3950,IiII,[ ar_wal_connection_pause.c : 2553 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_COMPLETE sent: peer:0x%x, module_id:%d, tids_to_pause:0x%x, tids_to_unpause:0x%x 
3949,IiII,[ ar_wal_connection_pause.c : 2584 ] Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_COMPLETE sent: peer:0x%x, module_id:%d, tids_to_block:0x%x, tids_to_unblock:0x%x 
3948,iii,[ ar_wal_connection_pause.c : 2612 ] Tx_Pause: WAL_VDEV_TX_PAUSE_COMPLETE sent: vdev_id:%d, module_id:%d, block:%d 
3947,iii,[ ar_wal_connection_pause.c : 2639 ] Tx_Pause: WAL_VDEV_TX_UNPAUSE_COMPLETE sent: vdev_id:%d, module_id:%d, block:%d 
3946,iii,[ ar_wal_connection_pause.c : 2666 ] Tx_Pause: WAL_PDEV_TX_PAUSE_COMPLETE sent: pdev_id:%d, module_id:%d, block:%d 
3945,iii,[ ar_wal_connection_pause.c : 2693 ] Tx_Pause: WAL_PDEV_TX_UNPAUSE_COMPLETE sent: pdev_id:%d, module_id:%d, block:%d 
3944,IiII,[ ar_wal_connection_pause.c : 2725 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_EXT_COMPLETE sent: 1st_peer:0x%x, module_id:%d, tids_to_pause:0x%x, tids_to_unpause:0x%x 
3943,IiII,[ ar_wal_connection_pause.c : 2770 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_REQ comp: peer:0x%x, module_id:%d, tids_to_pause:0x%x, tids_to_unpause:0x%x 
3942,IiII,[ ar_wal_connection_pause.c : 2783 ] Tx_Pause: WAL_PEER_TX_BLOCK_UNBLOCK_REQ comp: peer:0x%x, module_id:%d, tids_to_block:0x%x, tids_to_unblock:0x%x 
3941,iii,[ ar_wal_connection_pause.c : 2794 ] Tx_Pause: WAL_VDEV_TX_PAUSE_REQ comp: vdev_id:%d, module_id:%d, block:%d 
3940,iii,[ ar_wal_connection_pause.c : 2805 ] Tx_Pause: WAL_VDEV_TX_UNPAUSE_REQ comp: vdev_id:%d, module_id:%d, block:%d 
3939,iii,[ ar_wal_connection_pause.c : 2816 ] Tx_Pause: WAL_PDEV_TX_PAUSE_REQ comp: pdev_id:%d, module_id:%d, block:%d 
3938,iii,[ ar_wal_connection_pause.c : 2827 ] Tx_Pause: WAL_PDEV_TX_UNPAUSE_REQ comp: pdev_id:%d, module_id:%d, block:%d 
3937,IiII,[ ar_wal_connection_pause.c : 2841 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_EXT_REQ comp: 1st_peer:%u, module_id:%d, tids_to_pause:0x%x, tids_to_unpause:0x%x 
3936,iiii,[ ar_wal_connection_pause.c : 3461 ] Tx_Pause: WAL_VDEV_TX_PAUSE_REQ rcvd: vdev_id:%d, module_id:%d, block:%d, filter:%d 
3935,iii,[ ar_wal_connection_pause.c : 3481 ] Tx_Pause: WAL_VDEV_TX_UNPAUSE_REQ rcvd: vdev_id:%d, module_id:%d, block:%d 
3934,i,[ ar_wal_connection_pause.c : 3492 ] Tx_Pause: unsupported vdev request id:%d 
3933,iiiI,[ ar_wal_connection_pause.c : 4112 ] tid_pause_data_stall tid_num:%d pause_module_id_map:%d block_module_id_map:%d peer:0x%x 
3932,I,[ ar_wal_connection_pause.c : 3518 ] Tx_Pause: ar_wal_peer_pause_unpause_req_handler: (qpeer == NULL), mod=%u 
3931,IiIIi,[ ar_wal_connection_pause.c : 3537 ] Tx_Pause: WAL_PEER_TX_PAUSE_UNPAUSE_REQ rcvd: peer:0x%x, module_id:%d, tids_to_pause:0x%x, tids_to_unpause:0x%x, filter:%d 
3930,I,[ ar_wal_connection_pause.c : 127 ] Tx_Pause: conn_pause_get_qpeer_from_id: (qpeer == NULL): sw_peer_id=%u 
3929,I,[ ar_wal_connection_pause.c : 2373 ] Tx_Pause: Pdev event PEER_CREATE for peer:0x%x rcvd 
3928,II,[ ar_wal_connection_pause.c : 748 ] Tx_Pause: wal_connection_pause_en_dis_ext: NULL peer list, mod=%u, is_en=%u 
3927,II,[ ar_wal_connection_pause.c : 755 ] Tx_Pause: wal_connection_pause_en_dis_ext: (qpeer == NULL), mod=%u, is_en=%u 
3926,i,[ ar_wal_connection_pause.c : 3893 ] Tx_Pause: unsupported request id:%d 
3973,i,[ wal_early_rx.c : 62 ] actual min early_rx:%d 
4036,ii,[ wal_wmac_pm.c : 662 ] correct_tsf_for_go:cur(%d)<(%d) 
4035,iiIi,[ wal_wmac_pm.c : 708 ] ch_imbalance: min:%d max:%d chmsk:0x%x thr:%d 
4034,iiiI,[ wal_wmac_pm.c : 2196 ] cur_sm=%d new_pwr_state=%d force_swdtim=%d reason=%x 
4033,iII,[ wal_wmac_pm.c : 2281 ] mac:%d total_time_left=%lu wmac power_level %x 
4032,i,[ wal_wmac_pm.c : 2303 ] invalid TSF id:%d 
4031,i,[ wal_wmac_pm.c : 2314 ] Sleep Aborted:%dus close to target wake time
 
4030,,[ wal_wmac_pm.c : 2331 ] wpm_eval ACTIVE to HWDTIM 
4029,,[ wal_wmac_pm.c : 2361 ] wpm_eval ACTIVE to IMPS 
4028,,[ wal_wmac_pm.c : 2370 ] wpm_eval ACTIVE to SWDTIM 
4027,,[ wal_wmac_pm.c : 2207 ] wpm_eval IMPS to ACTIVE 
4026,,[ wal_wmac_pm.c : 2209 ] wpm_eval HWDTIM to ACTIVE 
4025,i,[ wal_wmac_pm.c : 3268 ] exit_hwdtim_awake mac:%d 
4024,ii,[ wal_wmac_pm.c : 4711 ] wal_pm_get_ocl_rssi_threshold: %d, pdev_id %d 
4023,i,[ wal_wmac_pm.c : 4541 ] wal_pm_get_sap_xlna_bypass: %d 
4022,iii,[ wal_wmac_pm.c : 4552 ] get_xlna_rssi_threshold: low %d high %d pdev_id %d 
4021,ii,[ wal_wmac_pm.c : 4576 ] get_xlna_status: status %d pdev_id %d 
4020,i,[ wal_wmac_pm.c : 4566 ] wal_pm_is_xlna_bypass_enabled: enable %d 
4019,iii,[ wal_wmac_pm.c : 5005 ] wal_lower_gtc_gain pdev_id %d lower:%d cur:%d 
4018,ii,[ wal_wmac_pm.c : 4626 ] wal_pm_set_xlna: xlna %d pdev_id %d 
4017,ii,[ wal_wmac_pm.c : 4636 ] set_xlna: xlna %d pdev_id %d 
4016,iiiIi,[ wal_wmac_pm.c : 4040 ] wpm_change_req id:%d mac:%d pwr_state:%d f:%p l:%d 
4015,IiI,[ wal_wmac_pm.c : 900 ] active_entry_ts:%lu mac:%d cnt:%lu 
4014,ii,[ wal_wmac_pm.c : 924 ] mac:%d HW DTIM AWAKE fw trig wake %d 
 
4013,ii,[ wal_wmac_pm.c : 929 ] mac:%d HW DTIM AWAKE resume tx %d 
 
4012,ii,[ wal_wmac_pm.c : 962 ] mac:%d IMPS trans to fw control %d 
 
4011,ii,[ wal_wmac_pm.c : 987 ] mac:%d IMPS fw trig wake %d 
 
4010,ii,[ wal_wmac_pm.c : 992 ] mac:%d IMPS resume tx %d 
 
4009,ii,[ wal_wmac_pm.c : 997 ] mac:%d IMPS post trans to fw control %d 
 
4008,ii,[ wal_wmac_pm.c : 1017 ] mac:%d PARTIAL fw trig wake %d 
 
4007,ii,[ wal_wmac_pm.c : 1022 ] mac:%d PARTIAL resume tx %d 
 
4006,Ii,[ wal_wmac_pm.c : 1387 ] hw_dtim_awake_entry_ts:%lu mac:%d 
4005,ii,[ wal_wmac_pm.c : 1401 ] mac:%d HW DTIM h2s grant %d 
 
4004,ii,[ wal_wmac_pm.c : 1407 ] mac:%d HW DTIM trans to fw control %d 
 
4003,ii,[ wal_wmac_pm.c : 1426 ] mac:%d HW DTIM post trans to fw control %d 
 
4002,IiI,[ wal_wmac_pm.c : 1171 ] hw_dtim_entry_ts:%lu mac:%d cnt:%lu 
4001,ii,[ wal_wmac_pm.c : 1207 ] mac:%d ACTIVE hwdtim fw assist sleep %d 
 
4000,ii,[ wal_wmac_pm.c : 1222 ] mac:%d PARTIAL hwdtim fw assist sleep %d 
 
3999,Ii,[ wal_wmac_pm.c : 1348 ] hw_dtim_exit_ts:%lu mac:%d 
3998,IiI,[ wal_wmac_pm.c : 1703 ] imps_entry_ts:%lu mac:%d cnt:%lu 
3997,ii,[ wal_wmac_pm.c : 1722 ] mac:%d imps fw assist sleep %d 
 
3996,Ii,[ wal_wmac_pm.c : 1820 ] imps_exit_ts:%lu mac:%d 
3995,ii,[ wal_wmac_pm.c : 1873 ] mac:%d HW DTIM h2s grant %d 
 
3994,ii,[ wal_wmac_pm.c : 1879 ] mac:%d HW DTIM trans to fw control %d 
 
3993,Ii,[ wal_wmac_pm.c : 1570 ] sw_dtim_entry_ts:%lu mac:%d 
3992,Ii,[ wal_wmac_pm.c : 4360 ] swdtim_rt_msg_handler mac:%u msg_id:%d 
3991,iiIi,[ wal_wmac_pm.c : 4787 ] wlan_ocl_update_vdev_rssi: min:%d max:%d idx:0x%x thres:%d 
3990,i,[ wal_wmac_pm.c : 417 ] update_spm param:%d 
3989,iII,[ wal_wmac_pm.c : 2748 ] WDOG mac:%d glb_cnt:0x%08x_%08x
 
3988,iII,[ wal_wmac_pm.c : 2750 ] WDOG mac:%d cur_tsf:0x%08x_%08x
 
3987,i,[ wal_wmac_pm.c : 4962 ] wal_pm_wlm_ani_level lvl:%d 
3986,iiiii,[ wal_wmac_pm.c : 4992 ] wal_pm_wlm_ull_set_ani_period_step mode=:%d poll:%d listen:%d inc setp:%d dec step:%d 
3985,ii,[ wal_wmac_pm.c : 4904 ] wpm_assert_phy_off pdev_id %d sm_state:%d 
3984,i,[ wal_wmac_pm.c : 3649 ] do async reset: cnt %d 
3983,i,[ wal_wmac_pm.c : 2603 ] Sleep Aborted:%dus close to target wake time
 
3982,iii,[ wal_wmac_pm.c : 2613 ] mac:%d ACTIVE validate imps %d pf %d
 
3981,i,[ wal_wmac_pm.c : 4934 ] wpm_wmac_phy_release_off pdev_id %d 
3980,i,[ wal_wmac_pm.c : 2520 ] mac:%d fake TSF OOR 
3979,iIIIII,[ wal_wmac_pm.c : 2525 ] mac:%d cur_tsf:0x%08x_0x%08x next_tbtt:0x%08x_0x%08x dtim_period:%0x 
3978,i,[ wal_wmac_pm.c : 2547 ] Sleep Aborted:%dus close to target wake time
 
3977,iii,[ wal_wmac_pm.c : 2559 ] mac:%d ACTIVE validate sleep %d pf %d
 
3976,i,[ wal_wmac_pm.c : 3554 ] consective_wow_awake_to_cnt:%d 
3975,,[ wal_wmac_pm.c : 3567 ] long mac awake 
3974,i,[ wal_wmac_pm.c : 3575 ] null_check_failure_thr_cnt:%d 
4048,iiii,[ wal_avg_bmiss.c : 58 ] whal_wmac_get_bcn_stats mac id %d bcn_cnt:%d, bmiss_cnt:%d, flag %d 
4047,I,[ wal_avg_bmiss.c : 65 ] b:0x%08x 
4046,I,[ wal_avg_bmiss.c : 68 ] whal_wmac_get_bcn_stats failed 0x%x 
4045,Iii,[ wal_avg_bmiss.c : 142 ] %p bcn_cnt:%d, bmiss_cnt:%d
 
4044,I,[ wal_avg_bmiss.c : 144 ] b:0x%08x
 
4043,I,[ wal_avg_bmiss.c : 160 ] %p can't find vdev
 
4042,I,[ wal_avg_bmiss.c : 166 ] %p enter high bmiss mode 
4041,I,[ wal_avg_bmiss.c : 98 ] whal_wmac_set_bcn_stats failed 0x%x 
4040,Iii,[ wal_avg_bmiss.c : 197 ] %p bcn_cnt:%d, bmiss_cnt:%d
 
4039,I,[ wal_avg_bmiss.c : 199 ] b:0x%08x
 
4038,I,[ wal_avg_bmiss.c : 217 ] %p can't find vdev
 
4037,I,[ wal_avg_bmiss.c : 225 ] %p enter low bmiss mode 
4065,i,[ wal_spm.c : 1331 ] wal_spm_css_state_change_notify: ccpm_request_wlan_pwr failed with error code: %d 
4064,i,[ wal_spm.c : 1337 ] wal_spm_css_state_change_notify :ccpm_request_wlan_ccvs failed with error code: %d 
4063,i,[ wal_spm.c : 1351 ] wal_spm_css_state_change_notify :ccpm_request_wlan_ccvs failed with error code: %d 
4062,i,[ wal_spm.c : 1357 ] _wal_spm_css_pwr_down : ccpm_request_wlan_pwr failed with error code: %d 
4061,i,[ wal_spm.c : 1727 ] _wal_spm_init : ccpm_request_wlan_pwr failed with error code: %d 
4060,i,[ wal_spm.c : 1088 ] _wal_spm_set_wpm_params_cfg : ccpm_request_wlan_pwr failed with error code: %d 
4059,ii,[ wal_spm.c : 563 ] wal_spm_aggr_dcvs_level: m0 lvl %d m1 lvl %d 
4058,iii,[ wal_spm.c : 575 ] wal_spm_aggr_dcvs_level: m0 lvl %d m1 lvl %d aggr %d 
4057,iiiiiii,[ wal_spm.c : 492 ] wal_spm_bw_mode_change: mac %d dcvs %d pend lvl %d swt %d last lvl %d swt %d bwm %d 
4056,iiiiii,[ wal_spm.c : 731 ] wal_spm_bw_mode_change_internal: dcvs %d pend lvl %d swt %d last lvl %d swt %d bwm %d 
4055,ii,[ wal_spm.c : 800 ] wal_spm_dcvs_disable: DCVS disable ref count %d, module id %d 
4054,ii,[ wal_spm.c : 822 ] wal_spm_dcvs_enable: DCVS enable ref count %d, module id %d 
4053,iiiii,[ wal_spm.c : 657 ] wal_spm_post_channel_change_cb: dcvs %d pend lvl %d swt %d last lvl %d swt %d 
4052,iiii,[ wal_spm.c : 596 ] wal_spm_pre_channel_change_cb: phymode %d mhz %d freq1 %d freq2 %d 
4051,iiiiiii,[ wal_spm.c : 615 ] wal_spm_pre_channel_change_cb: dcvs %d pend lvl %d swt %d last lvl %d swt %d nbw %d mid %d 
4050,ii,[ wal_spm.c : 629 ] wal_spm_pre_channel_change_cb: cur %d aggr %d 
4049,iiiiii,[ wal_spm.c : 605 ] wal_spm_pre_channel_change_cb: 20mhz %d 40mhz %d 80mhz %d 160mhz %d he8080mhz %d vht8080mhz %d 
4066,,[ wal_pm_arbiter.c : 278 ] wal_pm_arbiter_req double sleep req 
4072,iii,[ wal_power_debug.c : 374 ]   wal_pm_lock_stats holding by WAL(MAC#0) request : %d, pm_requester :%d, ref_cnt %d
 
4071,I,[ wal_power_debug.c : 390 ] wal_pm_lock_stats holding by WAL(MAC#1) func_requested :%p
 
4070,I,[ wal_power_debug.c : 375 ] wal_pm_lock_stats holding by WAL(MAC#0) func_requested :%p
 
4069,iii,[ wal_power_debug.c : 388 ]   wal_pm_lock_stats holding by WAL(MAC#1) request : %d, pm_requester :%d, ref_cnt %d
 
4068,i,[ wal_power_debug.c : 1141 ] wal_power_debug_pf_log_cmd: config %d 
4067,ii,[ wal_power_debug.c : 1093 ] gtc_gain_adj_step %d for MAC%d 
4074,II,[ wal_sw_dtim.c : 323 ] ar_wal_vdev_sw_dtim_multicast_rx: DATA, fc:%0x, more:%u 
4073,ii,[ wal_sw_dtim.c : 333 ] ar_wal_vdev_sw_dtim_multicast_rx: Unexpeted unicast packet received for vdev=%d in state=%d 
4085,ii,[ wal_sw_dtim_wmac_sm.c : 1123 ] wal_sw_dtim_assert_phy_off pdev_id %d sm_state:%d 
4084,i,[ wal_sw_dtim_wmac_sm.c : 614 ] fail: !vdev_is_safe_to_sleep(%d) 
4083,II,[ wal_sw_dtim_wmac_sm.c : 639 ] fail: min_time_till_tbtt=%u back_off=%u 
4082,i,[ wal_sw_dtim_wmac_sm.c : 51 ] wal_sw_dtim_wmac_post_msg: msg_id %d 
4081,II,[ wal_sw_dtim_wmac_sm.c : 65 ] sw_dtim_wmac_power_req mac=%u cmd_id=%u 
4080,i,[ wal_sw_dtim_wmac_sm.c : 559 ] Sleep Aborted %dus close to target wake time
 
4079,,[ wal_sw_dtim_wmac_sm.c : 236 ] fail:unsupport vdev 
4078,,[ wal_sw_dtim_wmac_sm.c : 378 ] fail: validate_imps_swdtim 
4077,III,[ wal_sw_dtim_wmac_sm.c : 504 ] success: timeout=%u min_tbtt=%u sleep_exit_sys_time=%u 
4076,,[ wal_sw_dtim_wmac_sm.c : 249 ] fail:start reeval timer 
4075,,[ wal_sw_dtim_wmac_sm.c : 280 ] fail: close to tbtt 
4090,i,[ wal_sw_dtim_vdev_sm.c : 72 ] sw_dtim_be_msg_handler: msg_id %d 
4089,iii,[ wal_sw_dtim_vdev_sm.c : 338 ] sw_dtim_vdev_is_safe_to_sleep(FALSE): vdev_id=%d, cur_state:%d, next_state:%d 
4088,iI,[ wal_sw_dtim_vdev_sm.c : 353 ] sw_dtim_vdev_is_safe_to_sleep(TRUE): vdev_id=%d time_till_TBTT=%u 
4087,IIi,[ wal_sw_dtim_vdev_sm.c : 274 ] sw_dtim_vdev_start_sm: tbtt=%0x < tsf=%0x for vdev=%d 
4086,iIi,[ wal_sw_dtim_vdev_sm.c : 155 ] sw_dtim_vdev_start_tbtt_timer: vdev_id=%d time_till_TBTT=%u TSF more than TBTT count: %d 
4098,ii,[ wal_rc_peer.c : 2380 ] rx cck Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4097,ii,[ wal_rc_peer.c : 2211 ] rx mcs 3d Stats publish :: input buffer size = %d 3d stats buffer size = %d 
4096,iiI,[ wal_rc_peer.c : 2307 ] rx mcs Stats publish :: input buffer size = %d mcs stats buffer size = %d, nss:8/bw:8 0x%08x 
4095,ii,[ wal_rc_peer.c : 2344 ] rx ofdm Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4094,ii,[ wal_rc_peer.c : 2452 ] tx cck Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4093,ii,[ wal_rc_peer.c : 2169 ] tx mcs 3d Stats publish :: input buffer size = %d 3d stats buffer size = %d 
4092,iiI,[ wal_rc_peer.c : 2260 ] tx mcs Stats publish :: input buffer size = %d mcs stats buffer size = %d, nss:8/bw:8 0x%08x 
4091,ii,[ wal_rc_peer.c : 2416 ] tx ofdm Stats publish :: input buffer size = %d ofdm stats buffer size = %d 
4100,II,[ wal_rc_vdev.c : 612 ] RATECTRL_DBGID_WAL_SET_VDEV_DATA_RX: rc=0x%x data_rc=0x%x 
4099,II,[ wal_rc_vdev.c : 125 ] RATECTRL_DBGID_WAL_SET_VDEV_DATA_RX  rc=0x%x data_rc=0x%x 
4105,iii,[ wal_rc_pdev.c : 2655 ] limit_tx_chain_6g_lpi %d vdev_id %d rssi %d 
4104,iiIII,[ wal_rc_pdev.c : 1811 ] RC_QUERY : tid_num %d, sw_retry %d secondary_rc 0x%x tid_flags 0x%x %x 
4103,Iii,[ wal_rc_pdev.c : 2003 ] rate_sched:bw_mask:8/max_bw:8=0x%08x,flags=%d rix=%d 
4102,IiII,[ wal_rc_pdev.c : 2086 ] update ratecode data_rc=0x%x nss=%d tx_chain_mask[0]=0x%x tx_mask=0x%x 
4101,iii,[ wal_rc_pdev.c : 737 ] SET tx_chain_mask[%d]: new=%d old=%d 
4152,iii,[ wal_rtt.c : 169 ] Detected Outlier. i: %d rtt: %d bw: %d 
4151,iiii,[ wal_rtt.c : 234 ] chain: %d cumilative_rtt_per_chain: %d, num_samples: %d min_mean_rtt: %d 
4150,ii,[ wal_rtt.c : 2168 ] _wal_collect_report_info: pre %d bw %d 
4149,IIi,[ wal_rtt.c : 1669 ] _wal_report_type2_buffer_done() buff = %p, curr: %p len: %d 
4148,IIii,[ wal_rtt.c : 1652 ] _wal_report_type2_buffer_init buff = %p cur_p = %p chan = %d report_type = %d 
4147,iiiiii,[ wal_rtt.c : 2346 ] _wal_report_type2_collect_report_info:  total_time = %d num_frms = %d info1 = %d info2 = %d info3 = %d start_ts = %d 
4146,IIi,[ wal_rtt.c : 2397 ] RTT_INITR_TSTAMP: t2= 0x%08x%08x fac= %d 
4145,iIiiIIII,[ wal_rtt.c : 2457 ] _wal_report_type2_collect_report_info: rtt_ps: %d rssi=0x%x tx_preamble=%d tx_bw=%d tx_rate_info1 = 0x%x tx_rate_info2= 0x%x rx_rate_info1=0x%x, rx_rate_info2 = 0x%x 
4144,IIiIIiiiI,[ wal_rtt.c : 2487 ] RTT_INITR_TSTAMP: t2=%u, t3=%u  t3_del=%d t1=%u t4=%u t4_del=%d rtt=%d meas_count=%d num_rtt_per_frame_info_saved: %u 
4143,IIII,[ wal_rtt.c : 2509 ] _wal_report_type2_collect_report_info:  tx_rate_info1=0x%x, tx_rate_info2 =0x%x, rx_rate_info1=0x%x, rx_rate_info2=0x%x 
4142,IIiIII,[ wal_rtt.c : 2535 ] RTT_INITR_TSTAMP: t2= 0x%08x%08x fac= %d rx_preamble=%u, rx_bw=%u rssi = 0x%x  
4141,,[ wal_rtt.c : 2379 ] DISCARDING MEASUREMENT!! T3 not captured 
4140,I,[ wal_rtt.c : 1863 ] _wal_report_type2_update_start_ts: start_ts(rtt_ctxt) start_ts(peer_head) %u 
4139,III,[ wal_rtt.c : 1445 ] _wal_rtt_attach() pdev = %p rtt_pdev_ctxt = %p wal_rtt_ctxt = %p 
4138,iiii,[ wal_rtt.c : 339 ] rtt_compute_distance num_meas: %d mean_rtt: %d median_rtt: %d distance_cm: %d 
4137,iiiiiii,[ wal_rtt.c : 1949 ] wal_rtt_ctxt_clean: rxoffld_under_cnt: %d rxoffld_alloc_cnt: %d rxind_under_cnt: %d rxind_alloc_cnt: %d tm_rx_comp_cnt: %d rxoffld_drop_cnt: %d rxind_drop_cnt: %d 
4136,iiiiII,[ wal_rtt.c : 1601 ] _wal_rtt_ctxt_init() :freq: %d is_qca: %d force_legacy_ack: %d enable_ht_vht_ack :%d self_mac: %08x%04x 
4135,IIIIII,[ wal_rtt.c : 502 ] _wal_rtt_get_buffer_ptr:max_len:0x%x rem_len:0x%x reqd_len:0x%x buff:0x%x buf_p:0x%x cur_p:0x%x 
4134,iIIIi,[ wal_rtt.c : 1475 ] _wal_rtt_init() pdev_id = %d rtt_ctxt: %p  alloc_buff = %p buff = %p max_buff_len = %d 
4133,I,[ wal_rtt.c : 2001 ] rtt_local_send() Not a valid rtt frame type, retrun error! txrx_cb_flags: 0x%x 
4132,iIIIi,[ wal_rtt.c : 2054 ] _wal_rtt_local_frame_send_with_rate: acks%d tid_num 0x%x rate_info 0x%08x%08x report %d 
4131,IIiiI,[ wal_rtt.c : 3619 ] _wal_rtt_mt_cb: msg:0x%x id:0x%x s_thr:%d d_thr:%d ticks:0x%x 
4130,,[ wal_rtt.c : 2584 ] TX completion message was dropped. Report failure 
4129,,[ wal_rtt.c : 2590 ] _wal_rtt_null_ack_hdl() is called after RTT session is completed !!! 
4128,II,[ wal_rtt.c : 2597 ] Ignore NULL ack for stale entry: ath_buf: %p: last queued NULL frame ath_buf: %p 
4127,iiiiiiii,[ wal_rtt.c : 375 ] index: %d count: %d rtt_ps: %d sum_rtt: %d tx_bw: %d, rx_bw: %d tx_ch_idx: %d rx_ch_idx: %d 
4126,,[ wal_rtt.c : 2643 ] TX completion message was dropped. Report failure 
4125,,[ wal_rtt.c : 2649 ] _wal_rtt_tm_ack_hdl() is called after RTT session is completed !!! 
4124,II,[ wal_rtt.c : 2656 ] Ignore TM ack for stale entry: ath_buf: %p: last queued TM frame ath_buf: %p 
4123,,[ wal_rtt.c : 2926 ] _wal_rtt_tm_rx_hdl: TM frame not directed to me. Don't process 
4122,,[ wal_rtt.c : 2938 ] _wal_rtt_tm_rx_hdl: Not a valid TM frame. Don't process 
4121,III,[ wal_rtt.c : 3045 ] _wal_rtt_tm_rx_hdl: rx_ts %10u now_ts %10u rx_proc_delay %10u 
4120,i,[ wal_rtt.c : 3119 ] _wal_rtt_tm_rx_hdl: HT_VHT ack enable RTT_TM_FTM1 %d 
4119,iii,[ wal_rtt.c : 3124 ] _wal_rtt_tm_rx_hdl:  expect_token=%d, dia_token=%d, follow_token=%d 
4118,IIII,[ wal_rtt.c : 3224 ] _wal_rtt_tm_rx_hdl:  t1_32=0x%x, t1_0=0x%x, t4_32=0x%x, t4_0=0x%x 
4117,II,[ wal_rtt.c : 3245 ] CFR/CIR report queue full; CFR/CIR data at 0x%04x%04x will be dropped 
4116,i,[ wal_rtt.c : 3249 ] no CFR/CIR pending for report type %d 
4115,iII,[ wal_rtt.c : 3256 ] CFR/CIR pending for report type %d; CFR/CIR data at 0x%04x%04x will be dropped 
4114,,[ wal_rtt.c : 3399 ] wal_rtt_tx_ppdu_done(): rx_location_info is found to be invalid 
4113,IIIIIIIIi,[ wal_rtt.c : 3604 ] _wal_rtt_tx_ppdu_done(%u-sided): abf: 0x0 tx_preamble=%u, retries=%u tod_32=%u tod_0=%u toa_32=%u toa_0=%u fac_valid: %u fac=%d 
4112,II,[ wal_rtt.c : 3451 ] CFR/CIR report queue full; CFR/CIR data at 0x%04x%04x will be dropped 
4111,i,[ wal_rtt.c : 3455 ] no CFR/CIR pending for report type %d 
4110,iII,[ wal_rtt.c : 3462 ] CFR/CIR pending for report type %d; CFR/CIR data at 0x%04x%04x will be dropped 
4109,II,[ wal_rtt.c : 3508 ] CFR/CIR report queue full; CFR/CIR data at 0x%04x%04x will be dropped 
4108,i,[ wal_rtt.c : 3512 ] no CFR/CIR pending for responder report type %d 
4107,iII,[ wal_rtt.c : 3519 ] CFR/CIR pending for responder report type %d; CFR/CIR data at 0x%04x%04x will be dropped 
4106,ii,[ wal_rtt.c : 3747 ] wal_rtt_unit_test: debug_cnt[%d] = %d 
4154,iII,[ wal_rtt_init.c : 83 ] _wal_rtt_psoc_init() wal_rtt_ctxt idx in rtt_psoc_handle: %d rtt_ctxt: %p alloc_buff_p: %p 
4153,Iiii,[ wal_rtt_init.c : 92 ] _wal_rtt_psoc_init() psoc_rtt handle: %p sizes rtt_tx_pool: %d rtt_rx_pool handle: %d, rtt_rx_ofld_pool: %d 
4156,iIIi,[ wal_cfir.c : 44 ] wal_cfir_resolve: pdev %d cfg 0x%08x => 0x%08x status %d 
4155,I,[ wal_cfir.c : 87 ] wal_cfir_req_unregister: req %p already unregistered 
4166,ii,[ wal_spectral.c : 375 ] Pdev id : %d WMI event with reset_delay %d 
4165,iIIi,[ wal_spectral.c : 454 ] <%d>: WMI event called %p with %u buffers for module %d  
4164,ii,[ wal_spectral.c : 512 ] out_ring reap : Before read shadow_tail_idx %d & After read shadow_tail_idx %d 
4163,ii,[ wal_spectral.c : 544 ] SSCAN: cfg.ScanCountCopy %d cfg.ScanCount %d 
4162,i,[ wal_spectral.c : 751 ] pdev_id = %d: spectral sig handler 
4161,i,[ wal_spectral.c : 774 ] pdev_id = %d: spectral sig handler 
4160,i,[ wal_spectral.c : 801 ] pdev_id = %d: spectral sig handler 
4159,i,[ wal_spectral.c : 641 ] Resume SSCAN : pending elements in out_ring %d 
4158,iiii,[ wal_spectral.c : 161 ] SSCAN_DUMP mac_id = %d: trigger = %d enable = %d scan_mode = %d 
4157,I,[ wal_spectral.c : 173 ] SSCAN_DUMP: wal_spectral_scan_get_config  called %p 
4168,i,[ direct_dma_wmi.c : 213 ] pdev_id = %d: DMA is not attached 
4167,i,[ direct_dma_wmi.c : 236 ] pdev_id = %d: DMA is not attached 
4180,Iiii,[ wal_tx_common.c : 635 ] wal_peer_wow_null_per_stats_update: stats_start_time = 0x%x null_success = %d, null_fail = %d, cumulative_wake_time_ps_sta_ms = %d  
4179,Ii,[ wal_tx_common.c : 42 ] WAL_DBGID_STA_KICKOUT:                     peer=0x%x consecutive_null_failure=%d 
4178,iii,[ wal_tx_common.c : 46 ] WAL_DBGID_STA_KICKOUT:                     null_ppdu_fail_time:%dms delta:%dms vdev_type:%d 
4177,iIiIIIIII,[ wal_tx_common.c : 699 ] WAL_DBGID_STA_KICKOUT: KICKOUT_REASON_NULL_PER_CHECK_FAILURE_TH null_per= %d% wake_per= %d% null_fail_count= 0x%x, null_pass_count= 0x%x cumulative_wake_time_ps_sta_ms= 0x%x , null_per_stats_start_time = 0x%x, curr_time= 0x%x  
4176,iiIIIi,[ wal_tx_common.c : 169 ] consecutive_failure_reset : pdev=%d, vdev=%d, peer=0x%x, tid=0x%x (flags=0x%x), failure=%d -> 0 
4175,Iii,[ wal_tx_common.c : 341 ] SEC_RETRY ptid %x tid_num %d in AGGR Seq, enable tid for sw_retry %d
 
4174,IIIIiiIIi,[ wal_tx_common.c : 377 ] pdev_vdev_id=0x%x, peer=0x%x,tid=0x%x (flags=0x%x), consecutive failure=%d, kickout thresh=%d rate_code=0x%x, tsRate flags=0x%x, ppdu_mprot_type:%d 
4173,IIIIIii,[ wal_tx_common.c : 381 ] pdev:8/vdev:8 =0x%08x, peer=0x%x,tid=0x%x (flags=0x%x %x), consecutive failure=%d, kickout thresh=%d  
4172,IIiIIII,[ wal_tx_common.c : 415 ] pdev:8/vdev:8 0x%08x peer=0x%x consecutive_failure:%d cur_time:%x elapsed_ppdu_fail_time:%x tid_retryfailure:%x vdevtype:%x 
4171,II,[ wal_tx_common.c : 505 ] WAL_DBGID_STA_KICKOUT  0x%x 0x%x 
4170,IIII,[ wal_tx_common.c : 509 ] ppdu_fail_time:%x current_time:%x delta:%x type:%x  
4169,III,[ wal_tx_common.c : 282 ] WAL_DBGID_XCESS_FAILURES  %p 0x%x MAC:%x 
4194,III,[ wal_wmm.c : 36 ] WMMAC_PAUSE_CB: peer=0x%x blocked tids=0x%x/0x%x 
4193,Iiii,[ wal_wmm.c : 65 ] WMMAC_Q_REPRIO: peer=0x%x tid=%d qid:%d->%d 
4192,iI,[ wal_wmm.c : 71 ] WMMAC_PAUSE_CB: unblock tid(%d)=0x%x 
4191,Iiii,[ wal_wmm.c : 340 ] WMMAC_Q_DEPRIO: peer=0x%x tid=%d qid:%d->%d 
4190,IiI,[ wal_wmm.c : 350 ] WMMAC_Q_DROP: peer=0x%x tid(%d)=0x%x 
4189,Iiiiii,[ wal_wmm.c : 393 ] WMMAC_STATUS: peer=0x%x, used=%d, admitted=%d, txq_sts=%d/%d, downgrade=%d 
4188,iIiii,[ wal_wmm.c : 424 ] WMMAC_TXQ_STATUS ac=%d txq_status=0x%02x used=%d admitted=%d downgrade=%d 
4187,iiiII,[ wal_wmm.c : 108 ] WMMAC_ADD_DELTS: ac=%d admitted=%d acm=%d block=0x%x downgrade=0x%x 
4186,iii,[ wal_wmm.c : 156 ] WMMAC_UPDATE: used_time=%d admitted_time=%d, downgrade=%d 
4185,IIII,[ wal_wmm.c : 462 ] WMMAC_PERIODIC_UPDATE 0x%x 0x%x 0x%x 0x%x 
4184,I,[ wal_wmm.c : 472 ] WMMAC_NO_DOWNGRADE: unblock tid mask=0x%x 
4183,Iii,[ wal_wmm.c : 493 ] WMMAC_PERIODIC_UPDATE (VO): peer=0x%x, used=%d, admitted=%d 
4182,Iii,[ wal_wmm.c : 503 ] WMMAC_PERIODIC_UPDATE (VI): peer=0x%x, used=%d, admitted=%d 
4181,iii,[ wal_wmm.c : 181 ] WMMAC_USED_TIME_EXCEED: used=%d admitted=%d wmmac_q=%d 
4208,ii,[ wlan_buf.c : 1046 ] MGMT buf get failure: mgmtbufCnt = %d, bsmall = %d 
4207,I,[ wlan_buf.c : 1104 ] MGMT buf abf at start : 0x%x 
4206,iii,[ wlan_buf.c : 1109 ] MGMT buf abf failure: smgmtbufCnt = %d, bsmall = %d mgmtBufCnt = %d 
4205,Ii,[ wlan_buf.c : 1116 ] Remove MGMT buf from start abf : 0x%x, mgmtBufCnt : %d 
4204,IiiiI,[ wlan_buf.c : 1133 ] MGMT buf get success: abf = 0x%x  mgmtBufCnt =%d smgmtbuffcnt = %d bsmall = %d,flags = 0x%x 
4203,ii,[ wlan_buf.c : 1074 ] MGMT buf get beacon: mac_id:%d, rsvd:%d 
4202,,[ wlan_buf.c : 1222 ] wlan_buf_mac_buffer_dispatcher no buffers available in chain 
4201,,[ wlan_buf.c : 1238 ] wlan_buf_mac_buffer_dispatcher oops 
4200,,[ wlan_buf.c : 1250 ] wlan_buf_mac_buffer_dispatcher oops 
4199,Ii,[ wlan_buf.c : 486 ] MGMT buf allocation auth_buf :0x%x , mgmtBufCnt : %d 
4198,IiI,[ wlan_buf.c : 826 ] buf free: free the reused abf:0x%x, thread:%d, cb flags:0x%x 
4197,IiIi,[ wlan_buf.c : 834 ] free beacon abf:0x%x, thread:%d, cb flags:0x%x,rsvd:%d 
4196,,[ wlan_buf.c : 1288 ] wlan_buf_mac_buffer_dispatcher oops 
4195,,[ wlan_buf.c : 1314 ] wlan_buf_mac_buffer_dispatcher oops 
4209,,[ aes_gcm.c : 318 ] GCM: Tag mismatch 
4210,III,[ cmnos_intmux.c : 97 ] cmnos_intmux_dsr_attach error: handler = %p, pinum = %p, pparg=%p 
4217,IIII,[ cmnos_allocram.c : 560 ] unknown proxy_flag:0x%x, ret:0x%x, ret1:0x%x,ret2:0x%x 
4216,IiII,[ cmnos_allocram.c : 254 ] arena_flags: 0x%x, bytes:%d, call1:0x%x, call2:0x%x
 
4215,,[ cmnos_allocram.c : 625 ] BEGIN: cmnos_allocram_info_dump() 
4214,,[ cmnos_allocram.c : 656 ] HEX_DUMP: 
4213,,[ cmnos_allocram.c : 666 ] END: cmnos_allocram_info_dump() 
4212,iIIiii,[ cmnos_allocram.c : 628 ] arena: %d, start: 0x%p, current: 0x%p, used = %d, remaining: %d, num_allocs: %d
 
4211,iiiii,[ cmnos_allocram.c : 654 ] max: %d, idx: %d, total_num: %d, total_bytes: %d, length: %d 
4230,II,[ cmnos_thread.c : 4600 ] assert:r0=0x%x, r1=0x%x
 
4229,II,[ cmnos_thread.c : 4749 ] assert:r0=0x%x, r1=0x%x
 
4228,IIi,[ cmnos_thread.c : 4636 ] assert:r0=0x%x, r1=0x%x line#%d 
4227,II,[ cmnos_thread.c : 4719 ] assert:r0=0x%x, r1=0x%x
 
4226,III,[ cmnos_thread.c : 2994 ] thread exit exception:r0=0x%x, r1=0x%x, line:0x%x
 
4225,iii,[ cmnos_thread.c : 1891 ] APP THREAD ID %d thread stack: %dB used, %dB unused
 
4224,,[ cmnos_thread.c : 1725 ] cmnos_threads_delete
 
4223,I,[ cmnos_thread.c : 1745 ] cmnos_threads_delete: wait for thread app id 0x%x to exit
 
4222,I,[ cmnos_thread.c : 1748 ] cmnos_threads_delete: thread app id 0x%x is done
 
4221,,[ cmnos_thread.c : 1800 ] cmnos_threads_delete: clean up mutex locks
 
4220,,[ cmnos_thread.c : 1809 ] cmnos_threads_delete: clean up thread barriers
 
4219,,[ cmnos_thread.c : 1820 ] cmnos_threads_delete: do global cleanups
 
4218,I,[ cmnos_thread.c : 1732 ] cmnos_threads_delete: send exit to 0x%x thread app id
 
4234,,[ platform_init.c : 55 ] WLAN Platform: Starting wlan tasks... 
4233,,[ platform_init.c : 241 ] QMI Platform: Sending msg to RT thread to do cold cal init... 
4232,i,[ platform_init.c : 84 ] WLAN Adrastea/MSL HW init, enable_hw_debug =%d 
4231,,[ platform_init.c : 139 ] QMI Platform: Starting wlan tasks... 
4236,,[ platform_deinit.c : 33 ] QMI Platform: Deinit started... 
4235,,[ platform_deinit.c : 80 ] QMI Platform: Threads killed... 
4237,ii,[ platform_common.c : 151 ] plat_set_one_ce_service_map_cfg: ERROR - idx %d > PIPE_TO_CE_MAP_CNT %d 
4243,,[ platform_athdiag.c : 229 ] plat_athdiag_proc_read_req: Sending msg to RT thread to do athdiag read 
4242,,[ platform_athdiag.c : 178 ] plat_athdiag_white_list_add: only support limited security area 
4241,,[ platform_athdiag.c : 335 ] platform_proc_athdiag_read_req: can't access restrict area 
4240,IIi,[ platform_athdiag.c : 357 ] QMI Platform: Athdiag read REQ received...offset = 0x%x | mem_type = 0x%x | data_len = %d 
4239,,[ platform_athdiag.c : 410 ] platform_proc_athdiag_write_req: can't access restrict area 
4238,IIi,[ platform_athdiag.c : 432 ] QMI Platform: Athdiag write REQ received...offset = 0x%x | mem_type = 0x%x | data_len = %d 
4312,II,[ qmi_platform.c : 845 ] Error code 0x%x in msg_id 0x%x 
4311,IIiII,[ qmi_platform.c : 2765 ] platform_fill_host_twt_config_req twt_start_time=0x%08x%08x interval=%d twt_sta_upo=%ld twt_sta_dl=%ld 
4310,i,[ qmi_platform.c : 2357 ] platform_proc_qdss_cfg_download_req: QDSS cfg download curr_size = %d, 
4309,i,[ qmi_platform.c : 2373 ] platform_proc_qdss_cfg_download_req: QDSS cfg download done, current_size = %d, 
4308,IIII,[ qmi_platform.c : 494 ] qmi_event_history_log: msg_id = 0x%x, client_handle = 0x%x, event = 0x%x, tick = 0x%x 
4307,i,[ qmi_platform.c : 163 ] qmi_plat_check_state: error - received HOST_CAP_REQ at wrong state %d 
4306,iI,[ qmi_platform.c : 192 ] qmi_plat_check_state: ERROR: wrong state %d to receive msg_id 0x%x 
4305,i,[ qmi_platform.c : 203 ] qmi_plat_check_state: error - received MSA INFO REQ at wrong state %d 
4304,i,[ qmi_platform.c : 212 ] qmi_plat_check_state: error - received MSA READY REQ at wrong state %d 
4303,i,[ qmi_platform.c : 221 ] qmi_plat_check_state: error - sending MSA READY IND at wrong state %d 
4302,i,[ qmi_platform.c : 231 ] qmi_plat_check_state: error - received CAPABILITY REQ at wrong state %d 
4301,i,[ qmi_platform.c : 255 ] qmi_plat_check_state: error - received CAPABILITY REQ at wrong state %d 
4300,i,[ qmi_platform.c : 288 ] qmi_plat_check_state: error - received BDF DOWNLOAD REQ at wrong state %d 
4299,i,[ qmi_platform.c : 174 ] qmi_plat_check_state: WARNING: wrong state to send remote ddr mem cfg indication, state = %d 
4298,i,[ qmi_platform.c : 298 ] qmi_plat_check_state: error - received CAL_REPORT REQ at wrong state %d 
4297,i,[ qmi_platform.c : 308 ] qmi_plat_check_state: error - received M3_INFO REQ at wrong state %d 
4296,i,[ qmi_platform.c : 318 ] qmi_plat_check_state: error - send FW ready at wrong state %d 
4295,Ii,[ qmi_platform.c : 353 ] qmi_plat_check_state: error - Try to send FW Ready ind at wrong mode 0x%x and wrong state %d 
4294,i,[ qmi_platform.c : 363 ] qmi_plat_check_state: error - received CFG REQ at wrong state %d 
4293,Ii,[ qmi_platform.c : 381 ] qmi_plat_check_state: error - received MODE REQ w/ mode = 0x%x at wrong state %d 
4292,Ii,[ qmi_platform.c : 395 ] qmi_plat_check_state: error - received MODE REQ w/ mode = 0x%x at wrong state %d 
4291,Ii,[ qmi_platform.c : 418 ] qmi_plat_check_state: error - received MODE REQ w/ mode = 0x%x at wrong state %d 
4290,i,[ qmi_platform.c : 432 ] qmi_plat_check_state: error - Try to send CAL Done Ind at wrong state %d 
4289,Ii,[ qmi_platform.c : 440 ] qmi_plat_check_state: error - Try to send Cal Done Ind at wrong mode 0x%x and wrong state %d 
4288,iI,[ qmi_platform.c : 183 ] qmi_plat_check_state: ERROR: wrong state %d to receive msg_id 0x%x 
4287,i,[ qmi_platform.c : 452 ] qmi_plat_check_state: error - Try to send SOC WAKE at wrong state %d 
4286,i,[ qmi_platform.c : 466 ] qmi_plat_check_state: error - Try to send SOC WAKE at wrong state %d 
4285,I,[ qmi_platform.c : 694 ] Client with handle 0x%x connected 
4284,I,[ qmi_platform.c : 725 ] Client with handle 0x%x disconnected 
4283,,[ qmi_platform.c : 1904 ] QMI Platform: sending QMI_WLFW_FILE_SAVE_IND_V01 
4282,I,[ qmi_platform.c : 1868 ] QMI Platform: BDF download REQ received, seg_id 0x%x 
4281,,[ qmi_platform.c : 2127 ] QMI Platform: Cal report REQ received 
4280,,[ qmi_platform.c : 2102 ] QMI Platform: Cap REQ received 
4279,ii,[ qmi_platform.c : 1929 ] QMI Platform: QMI_WLFW_FILE_DATA_REQ_V01 received, invalid parameter, req_id %d, cur_seg_id %d 
4278,,[ qmi_platform.c : 1940 ] QMI Platform: QMI_WLFW_FILE_DATA_REQ_V01 received, cur_seg_id 
4277,ii,[ qmi_platform.c : 1968 ] QMI Platform: QMI_WLFW_FILE_DATA_RESP_V01 sent,  data %d, end %d 
4276,II,[ qmi_platform.c : 1017 ] wlfw_handle_host_cap_req: num_clients=%x, nm_modem=%x 
4275,,[ qmi_platform.c : 2682 ] wlfw_handle_host_ims_wfc_req invalid data received 
4274,IIIii,[ qmi_platform.c : 2734 ] wlfw_handle_host_ims_wfc_req twt_start_time=0x%08x%08x media_quality=%ld wfc_call_active=%d call held=%d emergency 
4273,,[ qmi_platform.c : 1178 ] QMI Platform: Ind register REQ received 
4272,I,[ qmi_platform.c : 1212 ] Client with unique ID 0x%x registering 
4271,I,[ qmi_platform.c : 1217 ] Client with unique ID 0x%x found in client_list 
4270,i,[ qmi_platform.c : 1749 ] QMI Platform: INI REQ received, debug mode = %d 
4269,ii,[ qmi_platform.c : 1767 ] QMI Platform: recieved INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
4268,ii,[ qmi_platform.c : 1771 ] QMI Platform: recieved INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
4267,ii,[ qmi_platform.c : 1778 ] QMI Platform: recieved INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
4266,ii,[ qmi_platform.c : 1782 ] QMI Platform: Did not recieve INI REQ, enablefwlog_valid = %d, enablefwlog = %d 
4265,Ii,[ qmi_platform.c : 2090 ] QMI Platform: M3 download REQ received, paddr = %ul, size = %d 
4264,,[ qmi_platform.c : 2148 ] QMI Platform: MAC addr REQ received 
4263,IIIIII,[ qmi_platform.c : 2195 ] Valid mac addr received from modem NV: %x : %x : %x : %x : %x : %x 
4262,,[ qmi_platform.c : 1974 ] I shouldn't have been called F 
4261,,[ qmi_platform.c : 2576 ] QDSS mem info REQ received 
4260,I,[ qmi_platform.c : 2472 ] QDSS mode REQ received, mode = 0x%x 
4259,i,[ qmi_platform.c : 1286 ] wlfw_handle_remote_ddr_mem_req: INFO: num_mem_cfg = %d 
4258,,[ qmi_platform.c : 2272 ] QMI Platform: Shutdown req recvd 
4257,i,[ qmi_platform.c : 2292 ] QMI Platform: platform state %d 
4256,,[ qmi_platform.c : 1607 ] QMI Platform: Wlan Cfg REQ received 
4255,i,[ qmi_platform.c : 1694 ] wlfw_handle_wlan_cfg_req: svc_cfg_len - %d 
4254,I,[ qmi_platform.c : 1353 ] QMI Platform: Wlan mode REQ received, mode = 0x%x 
4253,,[ qmi_platform.c : 1380 ] wlfw_handle_wlan_mode_req: hw_debug_valid = d, hw_debug = d 
4252,,[ qmi_platform.c : 2031 ] WHY DID YOU CALL ME 
4251,,[ qmi_platform.c : 921 ] QMI Platform: sending QMI_WLFW_RESPOND_GET_INFO_IND_V01 
4250,II,[ qmi_platform.c : 585 ] Ind with id 0x%x sent to client handle 0x%x 
4249,II,[ qmi_platform.c : 614 ] Ind with id 0x%x not sent to client handle 0x%x 
4248,II,[ qmi_platform.c : 596 ] Setting fw_status_mask in handle 0x%x with FW READY; new value = 0x%x 
4247,II,[ qmi_platform.c : 603 ] Handle 0x%x, fw_status_mask = 0x%x 
4246,II,[ qmi_platform.c : 609 ] Indication sent failed. Err code = 0x%x id = 0x%x 
4245,,[ qmi_platform.c : 915 ] QMI Platform: sending QMI_WLFW_QDSS_TRACE_FREE_IND_V01 
4244,,[ qmi_platform.c : 893 ] QMI Platform: sending QMI_WLFW_QDSS_TRACE_SAVE_IND_V01 
4313,I,[ pool_mgr_api.c : 150 ] product resulting in buffer overflow: num_of_elem * elem_sz = 0x%x 
4315,i,[ latency_profile.c : 458 ] profile_report: #profiles enabled > WMI limit (=%d) 
4314,i,[ latency_profile.c : 494 ] profile_report: could not alloc, size=%d 
4321,IIIi,[ sm.c : 357 ] SM: %x:%x:%p : allocation from event pool failed for event %d 
4320,IIIi,[ sm.c : 240 ] SM: %x:%x:%p : invalid event %d 
4319,iiIIiIIII,[ sm.c : 290 ] [SM:RcvEvt] Evt:%d not handled in CurS:%d mod_id=%x instance=%x vapid =%d make_sm = 0x%x extra = 0x%x extra2 = 0x%x extra3 = 0x%x 
4318,IIIiIII,[ sm.c : 265 ] [SM:RcvEvt] CurS:%x<-Evt:%x mod_id/inst/evt_q=%x vapid =%d ext1/2/3=0x%x/0x%x/0x%x 
4317,IIIii,[ sm.c : 274 ] SM: %x :%x :%p : event %d not handled in state %d 
4316,IIIiIII,[ sm.c : 413 ] [SM:ChgSta] CurS:%x->NxtS:%x mod_id/inst/evt_q=%x vapid=%d ext1/2/3=0x%x/0x%x/0x%x 
4355,,[ wlan_stats.c : 2045 ] PS_STA_AVG_CHANNEL_CONGESTION(ERROR0):total_awake_period == 0 
4354,II,[ wlan_stats.c : 2064 ] PS_STA_AVG_CHANNEL_CONGESTION(ERROR1):diff_all(%u) < diff_tx(%u) 
4353,I,[ wlan_stats.c : 2082 ] PS_STA_AVG_CHANNEL_CONGESTION(ERROR2): chan_activity(%u) > 100 
4352,,[ wlan_stats.c : 2178 ] wlan_clear_vdev_stats_BEThread: Fail to allocate clearLLStatsMsg buffer 
4351,iii,[ wlan_stats.c : 530 ] wlan_stats_processor:vdev_id:%d ch%d_snr:%d 
4350,,[ wlan_stats.c : 2334 ] _wlan_iface_link_stats_process: vdev is NULL 
4349,,[ wlan_stats.c : 2345 ] _wlan_iface_link_stats_process: wal_vdev is NULL 
4348,,[ wlan_stats.c : 3814 ] wlan_link_stats_init, ftm mode, will not initialize p_link_layer_stats_ctxt 
4347,ii,[ wlan_stats.c : 5438 ] iface_stats: vdev_id:%d af_avg:%d 
4346,,[ wlan_stats.c : 4659 ] Failed to get peer_stats_info_ctxt from stats_handle 
4345,i,[ wlan_stats.c : 4674 ] Failed to allocate peer_stats_info report evt buf %d 
4344,iI,[ wlan_stats.c : 3794 ] RADIO_LINK_STATS process started, num_radio = %d pending_bitmask = 0x%x 
4343,,[ wlan_stats.c : 3634 ] RADIO_LINK_STATS the last buffer is in process on one of the radios 
4342,i,[ wlan_stats.c : 3656 ] RADIO_LINK_STATS WMI Event Alloc failure, ev_length:%d 
4341,iii,[ wlan_stats.c : 3691 ] RADIO_LINK_STATS process cur_pwr_state:%d next_pwr_state:%d radio_id:%d 
4340,,[ wlan_stats.c : 3731 ] RADIO_LINK_STATS rx_time greater than cca_busy_time 
4339,,[ wlan_stats.c : 4917 ] BIGDATA ERR: mem alloc failed  
4338,iiiiiii,[ wlan_stats.c : 4958 ] BIGDATA STATS: vdev_id=%d tsf_out_of_sync=%d ani=%d data_tx_pwr=%d tx_pwr[dss,ofdm]=%d,%d kbps=%d 
4337,ii,[ wlan_stats.c : 429 ]  PS_STA_AVG_CHANNEL_CONGESTION BusyChanRunningAvg = %d %d 
4336,I,[ wlan_stats.c : 1002 ] vdev_id=%u is NULL 
4335,ii,[ wlan_stats.c : 1194 ] wlan_stats_processor:vdev_id:%d invalid_snr:%d 
4334,ii,[ wlan_stats.c : 1205 ] wlan_stats_processor:vdev_id:%d bcn_snr:%d 
4333,iii,[ wlan_stats.c : 1343 ] wlan_stats_processor: peer_stats->peer_tx_rate = %d rx_rate = %d rssi = %d 
4332,iII,[ wlan_stats.c : 1437 ] wlan_stats_processor: rx_mc_bc_cnt = %d peer_macaddr31to0 = 0x%x peer_macaddr47to32 = 0x%x 
4331,ii,[ wlan_stats.c : 1445 ] wlan_stats_processor: rx_duration = %d rx_duration_u32 = %d  
4330,,[ wlan_stats.c : 1649 ] wlan_stats_processor: Ran out of buffers; Aborting Report generation;               Sending Report to Host  
4329,iI,[ wlan_stats.c : 1006 ] vdev free=%d, pmf_vdev_ctxt=%u 
4328,ii,[ wlan_stats.c : 1170 ] wlan_stats_processor:vdev_id:%d mac_snr:%d 
4327,iI,[ wlan_stats.c : 2982 ] clear radio stats, i %d, wal_pdev 0x%x 
4326,,[ wlan_stats.c : 4744 ] _wlan_wlm_stats_process: vdev is NULL 
4325,,[ wlan_stats.c : 4752 ] _wlan_wlm_stats_process: wal_vdev is NULL 
4324,i,[ wlan_stats.c : 4757 ] _wlan_wlm_stats_process: cmd->vdev_id:%d is not up or sta 
4323,iiI,[ wlan_stats.c : 3492 ] RADIO_LINK_STATS tx power level offset done, radio idx = %d num_radio = %d pending_bitmask = 0x%x 
4322,iiI,[ wlan_stats.c : 3528 ] RADIO_LINK_STATS tx power level wmi_evt alloc NULL, radio idx = %d num_radio = %d pending_bitmask = 0x%x 
4361,I,[ wlan_wmi_ctrl_path_stats.c : 443 ] cp_stats print stats for pdev_id =0x%X 
4360,I,[ wlan_wmi_ctrl_path_stats.c : 114 ] cp_stats event_send_complete & released buffer= 0x%X  
4359,IIi,[ wlan_wmi_ctrl_path_stats.c : 739 ] cp_stats Reeived cp stats_req with stats_id_mask =0x%X  action =0x%X req_id %d 
4358,,[ wlan_wmi_ctrl_path_stats.c : 148 ] cp_stats calling send event 
4357,II,[ wlan_wmi_ctrl_path_stats.c : 178 ] cp_stats send wmi event with more data = 0x%X  event_status = 0x%X 
4356,I,[ wlan_wmi_ctrl_path_stats.c : 716 ] cp_stats call send event with more data = 0x%X  
4370,iiiiiiii,[ wlan_traffic_mon.c : 303 ] TRAFFIC_INFORM_CLIENT vdev_id = %d req_id = %d rx_status_chng = %d rx_thrsh = %d rx_throughput = %d, tx_status_chng = %d tx_thrsh = %d tx_throughput = %d 
4369,I,[ wlan_traffic_mon.c : 317 ] TRAFFIC_MEMORY_CORRUPTED 0x%x 
4368,ii,[ wlan_traffic_mon.c : 96 ] TRAFFIC_DATA_RESET_ERROR vdev_id = %d, mac_id = %d 
4367,iiI,[ wlan_traffic_mon.c : 101 ] TRAFFIC_DATA_RESET_1 mac_id = %d, vdev_id = %d, vdev_bitmap = 0x%x 
4366,i,[ wlan_traffic_mon.c : 367 ] TRAFFIC_STA_CONN_STATE_FAILED state = %d 
4365,iiiiiiI,[ wlan_traffic_mon.c : 385 ] TRAFFIC_STA_CONN_STATE vdev_id = %d, mac_id = %d, state = %d is_associated = %d  is_running = %d is_enabled = %d vdev_bitmap = 0x%x 
4364,iiiii,[ wlan_traffic_mon.c : 177 ] wlan_traffic_change_thres vdev _id = %d, old rx_thres = %d, new rx_thres = %d, old tx_thres = %d, new tx_thres = %d 
4363,iiii,[ wlan_traffic_mon.c : 572 ] TRAFFIC_MON_PRE_PWR_CHNG vdev_id = %d, macid = %d, is_suspend = %d, mon_time = %d 
4362,iiii,[ wlan_traffic_mon.c : 619 ] TRAFFIC_MON_POST_PWR_CHNG vdev_id = %d, macid = %d, is_suspend = %d, mon_time = %d 
4378,IIII,[ wlan_estimate_linkspeed.c : 441 ] wlan_est_linkspeed_chan_time_end chan_mhz 0x%x chan_dur_us 0x%x busy_time_us 0x%x accu_idle_dur_us 0x%x 
4377,II,[ wlan_estimate_linkspeed.c : 299 ] wlan_est_linkspeed_indicate_home_chan_update chan_mhz 0x%x home_chan_added 0x%x 
4376,iI,[ wlan_estimate_linkspeed.c : 365 ] wlan_est_linkspeed_vdev_en_dis vdev_id = %d 0x%x 
4375,II,[ wlan_estimate_linkspeed.c : 42 ] wlan_est_linkspeed_vdev_evt_handler vdev_id = 0x%x, evt = 0x%x 
4374,III,[ wlan_estimate_linkspeed.c : 75 ] wlan_est_linkspeed_wal_pdev_evt_handler event 0x%x, new_power_state 0x%x, cur_power_state 0x%x 
4373,III,[ wlan_estimate_linkspeed.c : 99 ] wlan_est_linkspeed_wal_pdev_evt_handler event 0x%x, new_power_state 0x%x, cur_power_state 0x%x 
4372,iIIIII,[ wlan_estimate_linkspeed.c : 200 ] wlan_peer_calc_est_linkspeed vdev_id %d, est_link_speed_kbps 0x%x, idle_time 0x%x, sample_time 0x%x, tx_bytes 0x%x, tx_time 0x%x 
4371,III,[ wlan_estimate_linkspeed.c : 204 ] wlan_peer_calc_est_linkspeed2 goodput 0x%x, inst_linkspeed 0x%x, inst_linkspeed_kbps 0x%x 
4384,iIiIiIii,[ wlan_rssi_monitor.c : 311 ] RSSI_MONITOR_ARBITER_CONFIG_HW: vdevid=%d, configure_low_rssi_thresh=%u, final_low_rssi_thresh=%d, configure_high_rssi_thresh=%u, final_high_rssi_thresh=%d, rssi_weight=%u low client:%d high client:%d 
4383,iI,[ wlan_rssi_monitor.c : 391 ] RSSI_MONITOR_ENABLE_THRESHOLDS_CLIENT_REQ_ERR(!client_data): vdevid=%d, client=%u 
4382,iii,[ wlan_rssi_monitor.c : 52 ] RSSI_MONITOR_GET_BEACON_RSSI_AVG: vdevid=%d, rssi_avg=%d, mac_id=%d 
4381,iI,[ wlan_rssi_monitor.c : 461 ] RSSI_MONITOR_HW_EVENT: vdevid=%d, event_type=%x 
4380,iIIiii,[ wlan_rssi_monitor.c : 119 ] RSSI_MONITOR_UPDATE_BEACON_RSSI: vdevid=%d, mac_id=%u, rssi_last=%u, rssi_avg_last=%d rssi_new=%d rssi_avg_new=%d 
4379,iI,[ wlan_rssi_monitor.c : 512 ] RSSI_MONITOR_VDEV_EVENT: vdevid=%d, notif=%u 
4391,ii,[ wlan_pm_arbiter.c : 497 ] wlan_pm_arbiter_dump_wake_stats: mac_id=%d, ModuleID=%d 
4390,iii,[ wlan_pm_arbiter.c : 482 ] wlan_pm_arbiter_req_migration: vdevid=%d, old_mac_id=%d, new_mac_id=%d 
4389,IIIII,[ wlan_pm_arbiter.c : 345 ] PS_STA_PM_ARB_RESOLVE: mac/power_state/request/mod_id = 0x%x bitmask[0]=0x%x, bitmask[1]=0x%x, bitmask[2]=0x%x, bitmask[3]=0x%x 
4388,ii,[ wlan_pm_arbiter.c : 649 ] wake_monitor mac:%d win_len:%dms 
4387,iiiiii,[ wlan_pm_arbiter.c : 672 ] wake_monitor mac:%d w_list mod:%d vdev:%d total_time:%dms total_cnt:%d max_time:%dms 
4386,iiiiii,[ wlan_pm_arbiter.c : 693 ] wake_monitor mac:%d s_list mod:%d vdev:%d total_time:%dms total_cnt:%d max_time:%dms 
4385,iii,[ wlan_pm_arbiter.c : 433 ] wlan_pm_arbiter_vdev_migration: vdevid=%d, old_mac_id=%d, new_mac_id=%d 
4398,iII,[ wlan_powersave.c : 505 ] wlan_ps_add_rogue_ap_by_bssid: RAP: total rap=%d, rap bssid=0x%x 0x%x 
4397,ii,[ wlan_powersave.c : 482 ] wlan_ps_check_if_rogue_ap_is_connected: RAP: is_rogeu_ap=%d, num_of_rap=%d 
4396,i,[ wlan_powersave.c : 453 ] wlan_ps_set_fake_rap_detection: RAP: fake_rap_detection=%d 
4395,i,[ wlan_powersave.c : 464 ] wlan_ps_set_force_rap_info_event: RAP: force_rap_info_event=%d 
4394,i,[ wlan_powersave.c : 339 ] wlm pcie l11 disable: %d 
4393,i,[ wlan_powersave.c : 368 ] wlm phyrf powersave disable: %d 
4392,ii,[ wlan_powersave.c : 524 ] wlan_ps_wmi_pdev_set_rap_config: RAP: is_enabled=%d, num_of_rap=%d 
4403,iiiIi,[ wlan_powersave_ap.c : 2373 ] AP_PS_DBGID_DELIVER_CAB vdev_id = %d Tid = %d NumMPDU = %d Flags = 0x%x RetryOther = %d 
4402,i,[ wlan_powersave_ap.c : 2311 ] AP_PS_DBGID_CAB_FINISH vdev_id = %d 
4401,i,[ wlan_powersave_ap.c : 2464 ] AP_PS_DBGID_START_CAB vdev_id = %d 
4400,i,[ wlan_powersave_ap.c : 3155 ] AP_PS_DBGID_VDEV_CREATION_FAILURE AP PS:vdev_id = %d vdev alloc failed 
4399,Ii,[ wlan_powersave_ap.c : 3362 ] AP_PS_DBGID_HOST_TX_PAUSE vdev_map = %0x, pause: %d 
4426,Iii,[ wlan_powersave_sta.c : 945 ] wlan_ps_sta_check_data_stall_detected: current_index=%0x, notxrx_count=%d, notxrx_max_count=%d 
4425,ii,[ wlan_powersave_sta.c : 3480 ] wlan_ps_sta_check_long_inactive_duration: is_enabled=%d, duration_ms=%d 
4424,Ii,[ wlan_powersave_sta.c : 3330 ] wlan_ps_sta_check_low_rssi_is_detected: rssi_avg=%0d, low_rssi_is_detected=%d 
4423,IIIIII,[ wlan_powersave_sta.c : 3363 ] wlan_ps_sta_check_vendor_specific_ie: AP: specific_code=%x:%x:%x:%x:%x:%x 
4422,iiiiiI,[ wlan_powersave_sta.c : 2793 ] PS_STA_PSPOLL_SEQ_DONE vdev_id = %d QueueTime = %d CompleteTime = %d ResponseTime = %d ResponseDuration = %d ResponseFrameCtrl/QosCtrl = 0x%x 
4421,iii,[ wlan_powersave_sta.c : 1921 ] PS_STA_DELIVER_EVENT vdev_id = %d EventType = %d Statue = %d 
4420,iI,[ wlan_powersave_sta.c : 3056 ] STA PS: wlan_ps_sta_health_monitor_timeout: vdev_id=%d sta_flags=0x%X 
4419,,[ wlan_powersave_sta.c : 3455 ] wlan_ps_sta_long_inactive_monitor_timeout: start timer again 
4418,iII,[ wlan_powersave_sta.c : 1757 ] wlan_ps_sta_pause: vdev_id=%d, module_id=%u, timeout_us=%u 
4417,iiIIII,[ wlan_powersave_sta.c : 1068 ] PS_STA_RESYNC vdev_id = %d VDevUpCnt = %d IsBTConnected = 0x%x Flags = 0x%x VDevSubMode = 0x%x BitMap = 0x%x 
4416,ii,[ wlan_powersave_sta.c : 2663 ] PS_STA_COEX_MODE vdev_id = %d Enable = %d 
4415,ii,[ wlan_powersave_sta.c : 2674 ] PS_STA_WOW_MODE vdev_id = %d Enable = %d 
4414,iII,[ wlan_powersave_sta.c : 1996 ] PS_STA_SET_PARAM vdev_id = %d param = 0x%x value = 0x%x 
4413,i,[ wlan_powersave_sta.c : 2138 ] WLAN_PS_STA_PARAM_POWER_ENABLE =%d 
4412,i,[ wlan_powersave_sta.c : 771 ] STA PS vdev_id = %d, No buffers available for null frames 
4411,,[ wlan_powersave_sta.c : 893 ] wlan_ps_sta_txrx_inactivity_check extend2 
4410,iiI,[ wlan_powersave_sta.c : 874 ] wlan_ps_sta_txrx_inactivity_check extend: num_of_no_rx_with_tim=%d, inactive_time_us=%d, verdor_spec_info=%b 
4409,ii,[ wlan_powersave_sta.c : 882 ] wlan_ps_sta_txrx_inactivity_check extend: override_ito_us=%d, inactive_time_us=%d 
4408,iI,[ wlan_powersave_sta.c : 1806 ] wlan_ps_sta_unpause: vdev_id=%d, mod_id=%u 
4407,Iiii,[ wlan_powersave_sta.c : 2977 ] STA PS: VOWiFi: voip_notify: vdev_id=%u, vo_call_start=%d, intvl_ms=%d media_quality=%d 
4406,i,[ wlan_powersave_sta.c : 383 ] STA PS vdev_id = %d, QoS Null Pending but no pending frame in queue ???  
4405,ii,[ wlan_powersave_sta.c : 2511 ] PS_STA_UAPSD_AUTO_TRIG VdevID = %d NumAC = %d 
4404,iiiiii,[ wlan_powersave_sta.c : 2532 ] PS_STA_UAPSD_AUTO_TRIG_PER_AC vdev_id = %d WMM_AC = %d UserPriority = %d SrvIntl = %d SuspIntl = %d DelayIntl = %d 
4437,ii,[ wlan_powersave_sta_sm.c : 722 ] wlan_ps_sta_data_activity_pending: vdev_id=%d, inactive_time_us=%d 
4436,III,[ wlan_powersave_sta_sm.c : 350 ] wlan_ps_sta_null_tx_completion_base: flags=%x, flags_2=%x, flags_3=%x 
4435,,[ wlan_powersave_sta_sm.c : 935 ] wlan_ps_sta_state_active_entry: cancel long_inactive_monitor_timer 
4434,ii,[ wlan_powersave_sta_sm.c : 1415 ] wlan_ps_sta_state_pause_event: vdev id = %d, pause_stat_rx_frms_leaked = %d 
4433,iii,[ wlan_powersave_sta_sm.c : 3443 ] SPEC_PSPOLL_TIMEOUT: vdevid=%d, spec=%d, timeout=%d 
4432,iiii,[ wlan_powersave_sta_sm.c : 2905 ] sleep_awake_event_rx: MD=%d, pspoll_count=%d, is_qos_null:%d, nodata_count=%d 
4431,iiii,[ wlan_powersave_sta_sm.c : 2910 ] sleep_awake_event_rx: is_qos_null:%d, wakeup_dur=%d, nodata_count=%d, max_count=%d 
4430,,[ wlan_powersave_sta_sm.c : 3154 ] total_spec_pspoll_count reaches MAX: reset it 
4429,,[ wlan_powersave_sta_sm.c : 2137 ] wlan_ps_sta_state_active_entry: start long_inactive_monitor_timer 
4428,iIIiI,[ wlan_powersave_sta_sm.c : 402 ] wlan_ps_sta_tx_sent_send_nullfunc: vdevid=%d, force_ps=0X%x, sta_handle=%p, peer_type=%d, blocked_tids=0X%x 
4427,ii,[ wlan_powersave_sta_sm.c : 1897 ] PS_STA_SPECPOLL_TIMER_STARTED vdev_id = %d SpecPsPollNoDataCnt = %d 
4447,IIi,[ wlan_qpower.c : 429 ] wlan_qpower_check_if_higher_ITO_required: flag=0x%x, flag_2=0x%x, busy_chan_running_avg=%d 
4446,i,[ wlan_qpower.c : 440 ] current wake window exceeded observation window curr_wake_time_ms = %d  
4445,iIIII,[ wlan_qpower.c : 598 ] wlan_power_check_if_rogue_ap_is_detected: vdev_id=%d flags=0x%x flags2=0x%x num_entries=%0d num_no_rx_with_tim=%0d 
4444,iIIIIIII,[ wlan_qpower.c : 693 ] wlan_power_check_traffic_history during voip: vdev_id = %d num_entries = 0x%x total_rx_bytes = 0x%0x first_entry_timestamp:%0x%0x current_time:%0x%0x spec_wakeup_needed:%0x 
4443,iIIIIIII,[ wlan_qpower.c : 723 ] wlan_power_check_traffic_history: vdev_id=%d, current_index=%u, num_wakeups_with_tx=%u, num_wakeups_with_rx=%u, total_duration=%u, rx_throughput=%u, tx_throughput=%u, spec_wakeup_needed=%u 
4442,IIIIII,[ wlan_qpower.c : 717 ] wlan_power_check_traffic_history(d): total_rx_bytes=%u, total_tx_bytes=%u, last_exit_timestamp=%u:%u, first_entry_timestamp=%u%u 
4441,i,[ wlan_qpower.c : 300 ] wlan_ps_sta_txrx_inactivity_check is_tim_war_enabled wal_vdev id : %d  
4440,iIIIIIII,[ wlan_qpower.c : 902 ] wlan_power_is_spec_wakeup_needed: vdev_id=%d, active_duration=%u, current_ito_us=%u, congestion=%u, thresh=%u, voip_in_progress=%u, specIto=%u, spec_wakeup=%u 
4439,IIIIIII,[ wlan_qpower.c : 348 ] wlan_record_end: current_index = %0x exit_timestamp:%0x:%0x entry_timestamp:%0x:%0x total_rx=%u, total_tx=%u 
4438,IIIII,[ wlan_qpower.c : 269 ] wlan_record_start: current_index=%u, entry_timestamp=%u:%u, total_rx=%u, total_tx=%u 
4496,i,[ wlan_egap.c : 2935 ] registering wlan_egap_vdev_notif_handler AP nResult = %d 
 
4495,i,[ wlan_egap.c : 2937 ] registering wlan_egap_vdev_notif_handler Non AP nResult = %d 
 
4494,,[ wlan_egap.c : 2979 ] egap_delete_vdev_instance unregistering wlan_egap_vdev_notif_handler non AP 
 
4493,,[ wlan_egap.c : 3463 ] egap_init 
4492,II,[ wlan_egap.c : 3518 ] WLAN_MAC_EGAP_F_IS_SINGLE_CHM_SET :0x%x, rx_chainmask:0x%x
 
4491,,[ wlan_egap.c : 3549 ] Failed EGAP init 
4490,,[ wlan_egap.c : 2188 ] wlan_egap_notify_sta_sleeping: egap_pdev_ctxt or egap_ap_vdev_ctxt is invalid !! 
4489,,[ wlan_egap.c : 2194 ] wlan_egap_notify_sta_sleeping: egap_mac_ctxt is invalid !! 
4488,iiii,[ wlan_egap.c : 2200 ] wlan_egap_notify_sta_sleeping: vdev->id=%d, egap_mac_ctxt->flags=%d, remote_peer_cnt=%d, num_sleeping_sta=%d 
4487,iIiI,[ wlan_egap.c : 2056 ] wlan_egap_pause_egap: vdev_id=%d, egap_mac_ctxt->flags=0x%x, pause_id=%d, pause_bitmap=0x%x 
4486,,[ wlan_egap.c : 2629 ] egap_pdev_phyerr_event_handler egap handle NULL 
4485,i,[ wlan_egap.c : 2636 ] egap_pdev_phyerr_event_handler : PHYERR sm_get_curstate = %d 
 
4484,iIiI,[ wlan_egap.c : 2089 ] wlan_egap_resume_egap: vdev_id=%d, egap_mac_ctxt->flags=0x%x, pause_id=%d, pause_bitmap=0x%x 
4483,ii,[ wlan_egap.c : 3112 ] egap_set_param_handler:AP_PS_DBGID_EGAP_SET_PARAM paramid = %d , param_value = %d 
 
4482,,[ wlan_egap.c : 3117 ] egap_set_param_handler: egap_pdev_ctxt = NULL  
 
4481,,[ wlan_egap.c : 3148 ] WLAN_EGAP_PARAM_IS_PWRSAVE_BY_INACTIVITY_ENABLED 
 
4480,i,[ wlan_egap.c : 463 ] egap_thread_comm_msg_handler cmd= %d 
4479,,[ wlan_egap.c : 476 ] egap_thread_comm_msg_handler :WLAN_EGAP_THREAD_COMM_CMD_EVENT_STA_POWERSAVE null peer  
4478,iiiiiI,[ wlan_egap.c : 2309 ] wlan_egap_vdev_notif_handler: type=%d, mac_id=%d, vdev_id=%d, ic_opmode=%d, ic_subopmode=%d, egap_pdev_flags=0x%x 
4477,iiI,[ wlan_egap.c : 2317 ] wlan_egap_vdev_notif_handler: egap_mac_ctxt: num_ap_vdevs=%d, num_non_ap_vdevs=%d, flags = 0x%x 
4476,ii,[ wlan_egap.c : 2347 ] egap_vdev_notif_handler : VDEV_STOP num_non_ap_vdevs = %d num_ap_vdevs = %d 
 
4475,,[ wlan_egap.c : 2428 ] egap_mac_ctxt->ap_vdev_ctxt==NULL 
 
4474,ii,[ wlan_egap.c : 2502 ] egap_vdev_notif_handler egap_ap_vdev_ctxt->mac_id = %d vdev->e_mac_id = %d 
 
4473,i,[ wlan_egap.c : 2516 ] Not handled event in _wlan_egap_vdev_notif_handler notif->type = %d 
 
4472,,[ wlan_egap.c : 2552 ] egap_wal_pdev_event_handler egap handle NULL 
4471,,[ wlan_egap.c : 2568 ] egap_wal_pdev_event_handler peer NULL 
4470,iI,[ wlan_egap.c : 2576 ] egap_wal_pdev_event_handler sm_get_curstate(&(egap_pdev_ctxt->sm)) = %d event->event_type  = 0x%x  
 
4469,,[ wlan_egap.c : 3307 ] egap_wmi_dispatch_cmds 
 
4468,,[ wlan_egap.c : 3310 ] egap_wmi_dispatch_cmds !egap_pdev_ctxt 
 
4467,i,[ wlan_egap.c : 946 ] EGAP Chainmask update silent_num_chains = %d 
4466,iII,[ wlan_egap.c : 277 ] wlan_egap_configure_egap_mac_hdl: mac_id=%d, vdev=%x, egap_ap_vdev_ctxt=%x
 
4465,,[ wlan_egap.c : 2843 ] egap_create_ap_vdev_instance 
 
4464,,[ wlan_egap.c : 2879 ] egap_delete_ap_vdev_instance unregistering wlan_egap_vdev_notif_handler AP 
 
4463,i,[ wlan_egap.c : 1287 ] egap_is_traffic_pending = %d  
4462,iiIi,[ wlan_egap.c : 2268 ] VDEV_POST_MIGRATION new_egap_pmac_hdl->num_ap_vdevs = %d new_egap_pmac_hdl->num_non_ap_vdevs = %d new_egap_pmac_hdl->flags = 0x%x new_mac_id = %d 
 
4461,iiI,[ wlan_egap.c : 2106 ] wlan_egap_scan_evt_handler[SCAN_STARTED]: scan_id=%d, vdev_id=%d, egap_mac_ctxt->flags=0x%x 
4460,iiI,[ wlan_egap.c : 2118 ] wlan_egap_scan_evt_handler[SCAN_COMPLETED]: scan_id=%d, vdev_id=%d, egap_mac_ctxt->flags=0x%x 
4459,ii,[ wlan_egap.c : 580 ] egap_sendcomplete_evt_handler frame_control type = %d frame subtype = %d  
 
4458,i,[ wlan_egap.c : 784 ] egap_set_event_handlers: new_mask = %d 
4457,i,[ wlan_egap.c : 818 ] egap_set_event_handler registration error : Result = %d SWBA  
4456,i,[ wlan_egap.c : 827 ] egap_set_event_handler deregistration error : Result = %d SWBA 
4455,i,[ wlan_egap.c : 846 ] egap_set_event_handler registration error : Result = %d PHYERR  
4454,i,[ wlan_egap.c : 862 ] egap_set_event_handler deregistration error: Result = %d PHYERR 
4453,,[ wlan_egap.c : 1942 ] egap_sm_unable_to_start not idle 
 
4452,,[ wlan_egap.c : 1957 ] egap_sm_start  
 
4451,I,[ wlan_egap.c : 1960 ] egap_sm_unable_to_start egap_mac_ctxt->flags = 0x%x 
 
4450,,[ wlan_egap.c : 1538 ] egap_sm_state_pwrsave_off_exit  
 
4449,,[ wlan_egap.c : 1994 ]  egap_sm_stop 
 
4448,iiiiI,[ wlan_egap.c : 3221 ] wlan_wmi_egap_param_cmd: enable=%d, inactivity_time=%d, wait_time=%d, flags=%d, reduced_txrx_chainmask=0x%x 
4546,iiii,[ wlan_pgap.c : 187 ] wlan_pgap_ap_rps_update_ap_vdev_config: flags=%d, ipps=%d, npkt_slots=%d, percent=%d 
4545,,[ wlan_pgap.c : 500 ] wlan_pgap_check_if_phase_off_tx_is_allowed: no HOLD_PHASE_OFF flag 
4544,iii,[ wlan_pgap.c : 528 ] wlan_pgap_check_if_phase_off_tx_is_allowed: %d: remaining_quota=%d, total_lantency=%d 
4543,i,[ wlan_pgap.c : 765 ] wlan_pgap_check_if_txrx_over_ipps: is_over_ipps=%d 
4542,i,[ wlan_pgap.c : 730 ] wlan_pgap_check_if_txrx_under_ipps: is_under_ipps=%d 
4541,i,[ wlan_pgap.c : 1990 ] pgap_create_ap_vdev_instance: wrong ap_vdev_up_count=%d 
4540,I,[ wlan_pgap.c : 2009 ] pgap_create_ap_vdev_instance: pgap_ap_vdev_ctxt=%p 
4539,I,[ wlan_pgap.c : 2108 ] wlan_pgap_create_vdev_instance: pgap_vdev_ctxt=%p 
4538,,[ wlan_pgap.c : 2041 ] pgap_delete_ap_vdev_instance: pgap_ap_vdev_ctxt 
4537,I,[ wlan_pgap.c : 2138 ] pgap_delete_vdev_instance: pgap_vdev_ctxt=%p 
4536,iiii,[ wlan_pgap.c : 119 ] wlan_pgap_get_interval_to_next_tbtt: cur_tsf=%d, next_tbtt=%d, interval=%d, bi=%d 
4535,ii,[ wlan_pgap.c : 545 ] wlan_pgap_get_phase_quota: bi_us=%d, phase_off_quota=%d 
4534,ii,[ wlan_pgap.c : 698 ] wlan_pgap_get_vdev_tx_rx_stats: rx_cnt=%d, tx_cnt=%d 
4533,i,[ wlan_pgap.c : 2617 ] wlan_pgap_init: is_enabled=%d 
4532,,[ wlan_pgap.c : 2352 ] wlan_pgap_oem_data_get_ap_rps_cmd: Err: Vdev OR pgap_vdev_ctx is NULL  
4531,ii,[ wlan_pgap.c : 2376 ] wlan_pgap_oem_data_get_ap_rps_cmd: max event size exceeded %d, max_limit %d 
4530,i,[ wlan_pgap.c : 2387 ] wlan_pgap_oem_data_get_ap_rps_cmd: memory allocation failed, %d 
4529,,[ wlan_pgap.c : 2290 ] wlan_pgap_oem_data_set_ap_bw_cmd: read header TLV failed 
4528,,[ wlan_pgap.c : 2305 ] wlan_pgap_oem_data_set_ap_suspend_cmd: warning: wrong TLV type 
4527,,[ wlan_pgap.c : 2175 ] wlan_pgap_oem_data_set_ap_rps_cmd: read header TLV failed 
4526,,[ wlan_pgap.c : 2207 ] wlan_pgap_oem_data_set_ap_rps_cmd: warning: wrong TLV type 
4525,Ii,[ wlan_pgap.c : 593 ] wlan_pgap_phase_timer_handler: flags=0x%x, cur_state=%d 
4524,II,[ wlan_pgap.c : 638 ] wlan_pgap_phase_timer_start: PHASE_ON : interval_us=%u, phase_us=%u 
4523,II,[ wlan_pgap.c : 655 ] wlan_pgap_phase_timer_start: PHASE_OFF: interval_us=%u, wakeup_us=%u 
4522,Ii,[ wlan_pgap.c : 664 ] wlan_pgap_phase_timer_start: flags=0x%x, to_us=%d 
4521,i,[ wlan_pgap.c : 428 ] wlan_pgap_set_event_handlers: new_mask = %d 
4520,iiii,[ wlan_pgap.c : 854 ] wlan_pgap_slot_timer_handler: cur_index=%d, num_slots=%d, totol_pkt=%d, over_ipps=%d 
4519,iiii,[ wlan_pgap.c : 912 ] wlan_pgap_slot_timer_start: cur_index=%d, num_slots=%d, max_off_num=%d, max_on_num=%d 
4518,,[ wlan_pgap.c : 1637 ] send EV_PWRSAVE_OFF, PGAP SM to active 
4517,,[ wlan_pgap.c : 1625 ] send EV_PWRSAVE_ON, PGAP SM to phase on 
4516,,[ wlan_pgap.c : 1549 ] pgap_sm_unable_to_start: no UP AP vdev 
4515,I,[ wlan_pgap.c : 1555 ] pgap_sm_unable_to_start: isn't enabled, ap_vdev_flag=0x%x 
4514,I,[ wlan_pgap.c : 1562 ] pgap_sm_unable_to_start: sta is connected, ap_vdev_flag=0x%x 
4513,I,[ wlan_pgap.c : 1568 ] pgap_sm_unable_to_start: mac_flag=0x%x 
4512,,[ wlan_pgap.c : 1573 ] pgap_sm_unable_to_start: sm is not idle 
4511,,[ wlan_pgap.c : 1580 ] send EV_START, PGAP SM to start 
4510,,[ wlan_pgap.c : 1606 ] send EV_STOP, PGAP SM to stop 
4509,ii,[ wlan_pgap.c : 297 ] wlan_pgap_update_pgap_mac_context: mac_id mismatch %d!=%d 
4508,iiiii,[ wlan_pgap.c : 1707 ] pgap_vdev_notif_handler: type=%d, mac_id=%d, vdev_id=%d, opmode=%d, submode=%d 
4507,,[ wlan_pgap.c : 1786 ] pgap_vdev_notif_handler: ERR! pgap_ap_vdev_ctxt is NULL during CONN_PEER 
4506,,[ wlan_pgap.c : 1809 ] pgap_vdev_notif_handler: ERR! pgap_ap_vdev_ctxt is NULL during DELETE_PEER 
4505,iiii,[ wlan_pgap.c : 1831 ] pgap_vdev_notif_handler: old_mac_id=%d, new_mac_id=%d, pgap's mac_id=%d, vdev's mac_id=%d 
4504,i,[ wlan_pgap.c : 1853 ] pgap_vdev_notif_handler: Not handled evt. type=%d 
4503,IIii,[ wlan_pgap.c : 1748 ] pgap_vdev_notif_handler: VDEV_STOP: mac flags=0x%x, ap vdev flags=0x%x, mac_vdev_up = %d , ap_vdev =%d 
4502,IIii,[ wlan_pgap.c : 1775 ] pgap_vdev_notif_handler: VDEV_UP: mac flags=0x%x, ap vdev flags=0x%x mac_vdev = %d, ap_vdev = %d,  
4501,iii,[ wlan_pgap.c : 221 ] pgap_vdev_set_params: vdev_id=%d, param_id=%d, param_value=%d 
4500,i,[ wlan_pgap.c : 264 ] pgap_vdev_set_params: invalid param id=%d 
4499,,[ wlan_pgap.c : 1923 ] wlan_pgap_wal_peer_event_pre_send: null peer 
4498,,[ wlan_pgap.c : 1873 ] wlan_pgap_wal_peer_event_pre_send: null peer 
4497,II,[ wlan_pgap.c : 1884 ] wlan_pgap_wal_peer_event_pre_send: mac_flags=0x%x, frame_control=0x%x 
4617,iiiiiii,[ wlan_smps.c : 2412 ] STA_SMPS_VHT_OP_MODE_NOTIF_PEER_COMPLETE : vdevid = %d peerid = %d completion_status = %d peer_smps_frames_sent_mask = %d vedevNotif = %dsm_power_control = %d, vcLastSMpwrCntrl = %d 
4616,i,[ wlan_smps.c : 2481 ] SMPS Action TX frame not sent, attemps:%d 
4615,ii,[ wlan_smps.c : 2488 ] SMPS action frame attempt mask %d smps_power_control %d 
4614,,[ wlan_smps.c : 2654 ] SMPS_AP Action frame could not send BW OMN notification connection is not VHT 
4613,i,[ wlan_smps.c : 2695 ] SMPS Action TX frame not sent, attemps:%d 
4612,iii,[ wlan_smps.c : 2542 ] STA_SMPS_SEND_VHT_OPMODE_NOTIF_FRAME_TO_PEER vdevid = %d peerid = %d ret_value = %d 
4611,i,[ wlan_smps.c : 4323 ] SMPS Build Operation mode notification IE: enable = %d 
4610,,[ wlan_smps.c : 3462 ] wlan_smps_cfg_change_timeout 
 
4609,iii,[ wlan_smps.c : 3604 ] wlan_smps_cfg_notify_done: status:%d, stage:%d->0 smps_cfg_notify_compl_args.ctxt=%d  
4608,iiiIi,[ wlan_smps.c : 3638 ] wlan_smps_chainmask_change_handle_done: status:%d, stage:%d->0,smps_cfg_notify_compl_args.ctxt=%d cur_chain_h16/next_chain=0x%x,smstate:%d 
4607,,[ wlan_smps.c : 3293 ] wlan_smps_vc_cfg_notify queued cfg 
 
4606,iI,[ wlan_smps.c : 4347 ] SMPS get Operation mode notification IE length %d %p 
4605,ii,[ wlan_smps.c : 1299 ] wlan_smps_get_peer_bandwidth channel_width = %d, peer_bw = %d 
4604,i,[ wlan_smps.c : 4764 ] vdev id greater than max supported vdev vdev_id = %d 
4603,i,[ wlan_smps.c : 4775 ] vdev is NULL or vdev_not_up for id vdev_id = %d 
4602,,[ wlan_smps.c : 4796 ] smps_vdev_handle is NULL 
4601,iI,[ wlan_smps.c : 4822 ] sta duplicate/invalid rxx nss for vdev_id = %d requested_rxnss = %x 
4600,iII,[ wlan_smps.c : 4834 ] frame was not sent since rx chainmask is allready on same configuraion vdev_id = %d requested_rxnss = %x curr_vc_rxchain_mode = %x 
4599,iII,[ wlan_smps.c : 4849 ] frame was not sent since rx chainmask is 1x1 vdev_id = %d requested_rxnss = %x curr_vc_rxchain_mode = %x 
4598,iiiiI,[ wlan_smps.c : 4881 ] sta Sending smps frame for rx nss change request vdev_id = %d req_rxnss = %d, applied_rxnss =%d, sm_power_control = %d, curreVCrxnss = 0x%x 
4597,,[ wlan_smps.c : 4890 ] No action on frame tx 
4596,ii,[ wlan_smps.c : 2783 ] STA_SMPS_CREATE_NON_STA_INSTANCE vdevid = %d smps_handle = %d 
4595,ii,[ wlan_smps.c : 2794 ] STA_SMPS_DELETE_NON_STA_INSTANCE : vdevid = %d smps_handle = %d  
4594,,[ wlan_smps.c : 2749 ] SMPS_DEBUG applied rxnss reset is done 
4593,iii,[ wlan_smps.c : 2052 ] STA_SMPS_DTIM_CHMASK_UPDATE_AWAKE : tx_chainmask = %d rx_chainmask = %d orig_rx_chainmask = %d 
4592,ii,[ wlan_smps.c : 2057 ] DTIM_UPDATE_CHAIN_ON_AWAKE: update chain in single chain, hwchain=%d, new=%d 
4591,i,[ wlan_smps.c : 2024 ] wlan_smps_pdev_update_dtim_chmask_on_sleep RSSI_INDICATION = %d 
4590,ii,[ wlan_smps.c : 4726 ] Per vdev reqest active on vdev %d current vdev = %d , hence rejecting request 
4589,,[ wlan_smps.c : 4972 ] returning vdev is NULL 
4588,IIII,[ wlan_smps.c : 5006 ] sta smps rxnss vdev level notification applied and stored for vdev_id = 0x%x flag = %x, Req rxnss = 0x%x applied rxnss = 0x%x 
4587,III,[ wlan_smps.c : 5016 ] sta smps rxnss vdev level notification failed for vdev_id = 0x%x, flag = %xapplied rxnss = 0x%x 
4586,IIII,[ wlan_smps.c : 5038 ] nsta smps rxnss vdev level notification applied and stored for vdev_id = 0x%x flag = %x, Req rxnss = 0x%x applied rxnss = 0x%x 
4585,II,[ wlan_smps.c : 5048 ] nsta smps rxnss vdev level notification failed for vdev_id = 0x%x, flag = %x 
4584,I,[ wlan_smps.c : 3563 ] wlan_smps_set_current_cfg vdev level notification hence no update vdev_map = 0x%x 
4583,i,[ wlan_smps.c : 2312 ] STA_SMPS_CREATE_STA_INSTANCE : sta_handle = %d 
4582,i,[ wlan_smps.c : 2335 ] STA_SMPS_DELETE_STA_INSTANCE : sta_handle = %d 
4581,,[ wlan_smps.c : 1451 ] SMPS_STA Action frame could not send BW OMN/OMI notification connection is not VHT 
4580,,[ wlan_smps.c : 1496 ] SMPS_STA Action frame could not send BW OMN/OMI notification wrong rx NSS 
4579,,[ wlan_smps.c : 1506 ] SMPS_STA Action frame could not send BW OMN/OMI notification wrong tx NSS 
4578,,[ wlan_smps.c : 1511 ] wlan_smps_sta_send_action_frame IEEE80211_NODE_HE 
4577,ii,[ wlan_smps.c : 1549 ] SMPS_STA Action frame send power_control: %d ret_value:%d 
4576,iiiii,[ wlan_smps.c : 2107 ] wlan_smps_sta_vdev_notif_handler notif->type = %d smps_handle->applied_rxnss = %d smps_handle->requested_rxnss = %d smps_handle->flag = %d, vdev->preferred_rx_streams =%d 
4575,,[ wlan_smps.c : 2115 ] SMPS_DEBUG applied rxnss reset is done 
4574,i,[ wlan_smps.c : 2125 ] Not handled event in wlan_smps_sta_vdev_notif_handler notif->type = %d 
 
4573,iIIiIi,[ wlan_smps.c : 4049 ] wlan_smps_vc_cfg_notify : arg %d req rx_chainmask = 0x%x currVCrxnss = 0x%xnew_channel_width = %d , updatecfg= 0x%x, is_vdev_notif = %d 
4572,I,[ wlan_smps.c : 4063 ] SMPS not supported on current channel 0x%x 
4571,iIi,[ wlan_smps.c : 4071 ] wlan_smps_vc_cfg_notify vc_handle->cfg_change_stage=%d, new_cfg.update_cf=%x, new_cfg.vdev_map = %d 
4570,,[ wlan_smps.c : 4085 ] wlan_smps_rejecting_queuing, something is already queued 
 
4569,Ii,[ wlan_smps.c : 4108 ] wlan_smps_vc_cfg_notify queued cb = 0x%x, ret = %d 
4568,i,[ wlan_smps.c : 4118 ] invalid smps cfg notification value new_cfg.channel_width = %d 
4567,,[ wlan_smps.c : 4158 ] SMPS_CFG_CHANGE_NOTIFY: rejected due to duplicate request 
4566,IiI,[ wlan_smps.c : 4243 ] SMPS_CFG_CHANGE_NOTIFY: ONLY CFG PARAM CHANGE mhz: 0x%x, ret = %d, Notification mask = 0x%x 
4565,Iiiii,[ wlan_smps.c : 4254 ] SMPS_CFG_CHANGE_NOTIFY:  mhz: 0x%x, ret = %d, prev_vc_rx_chain_mode: %d, next_vc_rx_chain_mode: %d, chain_mask_change_stage: %d  
4564,I,[ wlan_smps.c : 4256 ] SMPS_CFG_CHANGE_NOTIFY: Invalid VC handle %p 
4563,iiIIII,[ wlan_smps.c : 3894 ] invalid smps cfg notification requested ul_disablemu = %d, channel_width = %d rx_chainmask = 0x%x, tx_chainmask = 0x%x, update cfg = %x, vdev map = %x 
4562,I,[ wlan_smps.c : 3973 ] vdev level notification is requested  = 0x%x 
4561,iiiii,[ wlan_smps.c : 891 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL_OLD_DBG : power control = %d vc_handle->last_frame_sm_pwr_ctrl = %d completion status = %d current_state = %d vc_handle->cfg_change_stage = %d  
4560,iI,[ wlan_smps.c : 895 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL Additional params: prev_forced_mode = %d channel mhz = 0x%x 
4559,,[ wlan_smps.c : 993 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL : incorrect state readjustment 
 
4558,,[ wlan_smps.c : 1024 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL : fallback on legacy SMPS configuration 
 
4557,i,[ wlan_smps.c : 1086 ] STA_SMPS_VC_ACTION_FRAME_TX_COMPL : action_valid = %d 
 
4556,,[ wlan_smps.c : 1098 ] wlan_smps_vc_cfg_notify queued cfg 
 
4555,i,[ wlan_smps.c : 2877 ] STA_SMPS_CREATE_VIRTUAL_CHAN_INSTANCE : vc_handle = %d 
4554,i,[ wlan_smps.c : 2953 ] STA_SMPS_DELETE_VIRTUAL_CHAN_INSTANCE : vc_handle = %d 
4553,ii,[ wlan_smps.c : 340 ]  STA_SMPS_VIRTUAL_CHAN_SMPS_START : vc_handle = %d, vc_handle->enabled = %d 
4552,ii,[ wlan_smps.c : 357 ] SMPSVC CHNL START : STA_SMPS_INVALID_SM_EVENT event = %d dynamicSMPSSupported = %d 
4551,ii,[ wlan_smps.c : 387 ] STA_SMPS_VIRTUAL_CHAN_SMPS_STOP : vc_handle = %d, vc_handle->enabled = %d  
4550,iiiiii,[ wlan_smps.c : 415 ] wlan_smps_virtual_chan_update : vc_handle = %d, vc_handle->enabled = %d,vc_handle->cfg_notification_mode = %d, vc_handle->fw_forced_mode =%d , vc_handle->host_forced_mode = %d, smps_cur_state = %d   
4549,,[ wlan_smps.c : 449 ] wlan_smps_virtual_chan_update : smps action frame sent  
4548,,[ wlan_smps.c : 444 ] wlan_smps_virtual_chan_update : smps restarted  
4547,i,[ wlan_smps.c : 1704 ] wlan_smps_virtual_chan_update_dtim_chmask WAL_PM_MAC_PARAM_RSSI_INDICATION = %d 
4618,ii,[ wlan_smps_sm.c : 186 ] SMPS_STATE_STATIC_EVENT: chain: %d, dropped ev:%d 
4624,ii,[ wlan_opmode.c : 76 ] WLAN_OPMODE_SET_PMAC_LATENCY: mac_id=%d, opmode_latency=%d 
4623,ii,[ wlan_opmode.c : 85 ] WLAN_OPMODE_SET_PMAC_LATENCY: mac_id=%d, opmode_latency=%d [!WAL_EOK returned] 
4622,i,[ wlan_opmode.c : 259 ] WLAN_OPMODE_VDEV_FREE: vdev_id=%d 
4621,i,[ wlan_opmode.c : 243 ] WLAN_OPMODE_VDEV_INIT: vdev_id=%d 
4620,i,[ wlan_opmode.c : 250 ] WLAN_OPMODE_VDEV_INIT: vdev_id=%d [!A_OK returned] 
4619,iI,[ wlan_opmode.c : 157 ] WLAN_OPMODE_WAL_PDEV_EVT: pmac_id=%d, event=0x%x 
4645,iiii,[ wlan_xlna_bypass.c : 191 ] wlan_arbiter_xlna_bypass: nandw %d scrq %d hxlnap %d wlm %d 
4644,ii,[ wlan_xlna_bypass.c : 215 ] wlan_arbiter_xlna_bypass: xlna %d status %d 
4643,iiii,[ wlan_xlna_bypass.c : 209 ] wlan_arbiter_xlna_bypass: acv %d lowrssi %d pausev %d pausep %d 
4642,iii,[ wlan_xlna_bypass.c : 212 ] wlan_arbiter_xlna_bypass: pid %d asvc %d axlna %d 
4641,Iiiii,[ wlan_xlna_bypass.c : 61 ] wlan_nan_xlna_bypass_dw_event_handler: pdev %p pdev_id %d band %d event %d mac_id %d 
4640,i,[ wlan_xlna_bypass.c : 71 ] wlan_nan_xlna_bypass_event_handler: event_type %d 
4639,,[ wlan_xlna_bypass.c : 822 ] wlan_wmi_set_xlna_bypass_cmd: enter 
4638,i,[ wlan_xlna_bypass.c : 850 ] wlan_wmi_xlna_bypass_dispatch_cmds: cmdid=%d 
4637,,[ wlan_xlna_bypass.c : 783 ] WMI_GET_ELNA_BYPASS_EVENT PKT NULL 
4636,,[ wlan_xlna_bypass.c : 97 ] wlan_xlna_bypass_init: enter 
4635,ii,[ wlan_xlna_bypass.c : 508 ] wlan_xlna_bypass_pdev_scan_evt_handler: scan type pid %d evt %d 
4634,i,[ wlan_xlna_bypass.c : 349 ] xlna_sap disable: remote_peer_cnt %d 
4633,i,[ wlan_xlna_bypass.c : 379 ] xlna_sap enable: remote_peer_cnt %d 
4632,,[ wlan_xlna_bypass.c : 297 ] wlan_xlna_rssi_event_handler: LOW_RSSI_THRESHOLD_MET 
4631,,[ wlan_xlna_bypass.c : 301 ] wlan_xlna_rssi_event_handler: HIGH_RSSI_THRESHOLD_MET 
4630,iii,[ wlan_xlna_bypass.c : 741 ] xlna_sap peer:%d rssi:%d min:%d 
4629,iii,[ wlan_xlna_bypass.c : 537 ] wlan_xlna_scan_evt_handler: evtt %d wvdevt %d vifUp %d 
4628,i,[ wlan_xlna_bypass.c : 650 ] xlna_swbmiss: evt->evt_type:%d 
4627,iii,[ wlan_xlna_bypass.c : 405 ] wlan_xlna_vdev_event_hdlr: vid %d pid %d type %d 
4626,i,[ wlan_xlna_bypass.c : 491 ] xlna_sap peer change: remote_peer_cnt %d 
4625,iIi,[ wlan_xlna_bypass.c : 580 ] wlan_xlna_wal_pdev_evt_handler: pdev %d type 0x%x, powerstate %d 
4664,iiiiiiii,[ wlan_ocl.c : 213 ] wlan_arbiter_ocl: hocpv %d lrssi %d arbo %d asvc %d avc %d apvd %d wlm:%d coex %d 
4663,ii,[ wlan_ocl.c : 267 ] wlan_arbiter_ocl: mode:%d cur mode:%d 
4662,ii,[ wlan_ocl.c : 285 ] wlan_arbiter_ocl: New mode:%d flag_2G:%d 
4661,iiii,[ wlan_ocl.c : 245 ] wlan_arbiter_ocl: opr %d nandw %d scrq %d hoclp %d 
4660,iiiii,[ wlan_ocl.c : 263 ] wlan_arbiter_ocl: omr %d lss %d opv %d opp %d wlm %d 
4659,iii,[ wlan_ocl.c : 391 ] wlan_ocl_event_hdlr: ifUP %d, type %d event type %d 
4658,,[ wlan_ocl.c : 439 ] ocl_event_hdlr: enter ocl 
4657,ii,[ wlan_ocl.c : 549 ] wlan_ocl_pdev_scan_evt_handler: scan type pid %d evt %d 
4656,i,[ wlan_ocl.c : 370 ] wlan_ocl_rssi_event_handler: LOW_RSSI_THRESHOLD_MET : %d 
4655,,[ wlan_ocl.c : 374 ] wlan_ocl_rssi_event_handler: HIGH_RSSI_THRESHOLD_MET 
4654,,[ wlan_ocl.c : 380 ] ocl_rssi_event_handler: enter ocl 
4653,iii,[ wlan_ocl.c : 602 ] wlan_ocl_scan_evt_handler: vdev %d pdev %d type %d 
4652,,[ wlan_ocl.c : 628 ] ocl_scan_evt_handler: enter ocl 
4651,iii,[ wlan_ocl.c : 479 ] wlan_ocl_vdev_event_hdlr: vdev_id %d type %d, ifUp %d 
4650,,[ wlan_ocl.c : 494 ] ocl_vdev_event_hdlr: stop enter ocl 
4649,,[ wlan_ocl.c : 516 ] ocl_vdev_event_hdlr: up enter ocl 
4648,,[ wlan_ocl.c : 525 ] ocl_vdev_event_hdlr: mi enter ocl 
4647,i,[ wlan_ocl.c : 815 ] wlan_wmi_ocl_dispatch_cmds: cmdid=%d 
4646,ii,[ wlan_ocl.c : 774 ] wlan_wmi_set_ocl_cmd: OCL cmd:%d vdev:%d 
4676,ii,[ wlan_ani.c : 388 ] wlan_ani_pdev_scan_evt_handler: pid %d evt %d 
4675,,[ wlan_ani.c : 303 ] wlan_ani_rssi_event_handler: LOW_RSSI_THRESHOLD_MET 
4674,,[ wlan_ani.c : 307 ] wlan_ani_rssi_event_handler: HIGH_RSSI_THRESHOLD_MET 
4673,iii,[ wlan_ani.c : 419 ] wlan_ani_scan_evt_handler: vdev %d pdev %d type %d 
4672,iii,[ wlan_ani.c : 338 ] wlan_ani_vdev_event_hdlr: vdev_id %d type %d, ifUp %d 
4671,,[ wlan_ani.c : 353 ] ani_vdev_event_hdlr: stop enter ani 
4670,,[ wlan_ani.c : 358 ] ani_vdev_event_hdlr: up enter ani 
4669,,[ wlan_ani.c : 367 ] ani_vdev_event_hdlr: mi enter ani 
4668,iIiiii,[ wlan_ani.c : 195 ] wlan_arbiter_ani: scan:%d   reason:0x%x other_vdev_cnt:%d sta_vdev_cnt:%d active_vdev:%d pdev_id:%d 
4667,iiii,[ wlan_ani.c : 280 ] wlan_arbiter_ani h:%d   l:%d cur:%d level: %d 
4666,iiii,[ wlan_ani.c : 213 ] wlan_arbiter_ani: mode_request:%d pause_vdev:%d pause_pdev:%d vote:%d 
4665,,[ wlan_ani.c : 220 ] wlan_arbiter_ani:   Normal 
4693,iiI,[ wlan_twt.c : 675 ] wlan_twt_wmi_add_dialog: vdev_id=%d, id=%d, flags=0x%x 
4692,iii,[ wlan_twt.c : 807 ] wlan_twt_wmi_add_dialog_complete_event: vdev=%d, id=%d, status=%d 
4691,iiI,[ wlan_twt.c : 890 ] wlan_twt_wmi_del_dialog: vdev_id=%d, id=%d, flags=0x%x 
4690,iii,[ wlan_twt.c : 954 ] wlan_twt_wmi_del_dialog_complete_event: vdev=%d, id=%d, status=%d 
4689,iI,[ wlan_twt.c : 357 ] wlan_twt_wmi_disable: pdev_id=%d, flags=0x%x 
4688,i,[ wlan_twt.c : 466 ] wlan_twt_wmi_disable_complete_event: pdev_id=%d 
4687,iiI,[ wlan_twt.c : 207 ] wlan_twt_wmi_enable: pdev_id=%d, sta_cong_timer_ms=%d, pdev-flags=0x%x 
4686,ii,[ wlan_twt.c : 263 ] wlan_twt_wmi_enable_complete_event: pdev_id=%d, status=%d 
4685,iiii,[ wlan_twt.c : 1311 ] wlan_twt_wmi_nudge_dialog: vdev_id=%d, id=%d, suspend_duration_ms=%d, next_twt_size=%d 
4684,iiiI,[ wlan_twt.c : 1383 ] wlan_twt_wmi_nudge_dialog_complete_event: vdev=%d, id=%d, status=%d, next_twt=0x%x 
4683,ii,[ wlan_twt.c : 1010 ] wlan_twt_wmi_pause_dialog: vdev_id=%d, id=%d 
4682,iii,[ wlan_twt.c : 1068 ] wlan_twt_wmi_pause_dialog_complete_event: vdev=%d, id=%d, status=%d 
4681,iii,[ wlan_twt.c : 1134 ] wlan_twt_wmi_resume_dialog: vdev_id=%d, id=%d, next_twt_size=%d 
4680,iii,[ wlan_twt.c : 1204 ] wlan_twt_wmi_resume_dialog_complete_event: vdev=%d, id=%d, status=%d 
4679,iiiI,[ wlan_twt.c : 526 ] wlan_twt_wmi_send_twt_ack_event: vdev=%d, id=%d, status=%d twt_cmd:%x 
4678,ii,[ wlan_twt.c : 1280 ] wlan_twt_wmi_clear_stats_dialog: vdev_id=%d, id=%d 
4677,i,[ wlan_twt.c : 1283 ] AP TWT stats not supported, vdev_id=%d  
4694,iii,[ wlan_twt_protocol.c : 236 ] wlan_twt_action_frame_handler: cat=%d, act=%d, len=%d 
4731,ii,[ wlan_twt_sta.c : 1387 ] sta_twt_del_all_session: vdev_id=%d, status=%d 
4730,ii,[ wlan_twt_sta.c : 1631 ] wlan_sta_twt_action_frame_tx_completion: vdev=%d, status=%d 
4729,iI,[ wlan_twt_sta.c : 2224 ] wlan_sta_twt_add_voip_session: vdev=%d, flags=0x%x 
4728,IiiiiI,[ wlan_twt_sta.c : 2987 ] wlan_sta_twt_congest_trigger: flags=0x%x, non_my_txrx_percent=%d, my_txrx_percent=%d, to_start=%d, to_stop=%d,pause_bitmap = 0x%x 
4727,iiii,[ wlan_twt_sta.c : 3198 ] wlan_sta_twt_duty_cycle_tune: my_tx_rx_percent=%d, wake_duration=%d, wake_interval=%d, service_period_extension=%d 
4726,I,[ wlan_twt_sta.c : 3882 ] wlan_sta_twt_fw_disable_vdev: flags=0x%x 
4725,Iii,[ wlan_twt_sta.c : 3798 ] wlan_sta_twt_fw_enable_vdev: flags=0x%x, is_host_ctrl_old=%d, is_host_ctrl_new=%d 
4724,iii,[ wlan_twt_sta.c : 3020 ] wlan_sta_twt_txrx_update retries = %d MPDU=%d AMPDU=%d 
4723,I,[ wlan_twt_sta.c : 4020 ] wlan_sta_twt_host_disable_vdev: flags=0x%x 
4722,IIIi,[ wlan_twt_sta.c : 3988 ] wlan_sta_twt_host_enable_vdev: vdev=%u, flags=0x%x, mac-flags=0x%x, is_host_ctrl=%d 
4721,i,[ wlan_twt_sta.c : 1814 ] wlan_sta_twt_initiate_setup(send_failed): status=%d 
4720,iii,[ wlan_twt_sta.c : 3604 ] wlan_sta_twt_nan_evt_handler: event_type %d,twt_nan_concurrency: %d on mac %d 
4719,iIiI,[ wlan_twt_sta.c : 2855 ] wlan_sta_twt_pause_twt: vdev_id=%d, flags=0x%x, pause_id=%d, pause_bitmap=0x%x 
4718,i,[ wlan_twt_sta.c : 587 ] wlan_sta_twt_initiate_setup(send_failed): status=%d 
4717,iIiI,[ wlan_twt_sta.c : 2933 ] wlan_sta_twt_resume_twt: vdev_id=%d, flags=0x%x, pause_id=%d, pause_bitmap=0x%x 
4716,iIii,[ wlan_twt_sta.c : 3927 ] wlan_sta_twt_resync_enablement: mac_id=%d, flags=0x%X, up_cnt=%d, bt=%d 
4715,i,[ wlan_twt_sta.c : 3941 ] wlan_sta_twt_resync_enablement: CSA in progress, mac_id=%d 
4714,ii,[ wlan_twt_sta.c : 2455 ] BT Status=%d channel=%d 
4713,,[ wlan_twt_sta.c : 2494 ] wlan_sta_twt_resync_voip: Tuning 
4712,i,[ wlan_twt_sta.c : 2532 ] wlan_sta_twt_resync_voip: Tuning VOIP duration = %d 
4711,,[ wlan_twt_sta.c : 2542 ] wlan_sta_twt_resync_voip: add VOIP 
4710,,[ wlan_twt_sta.c : 2547 ] wlan_sta_twt_resync_voip TWT NtA: delete VOIP 
4709,,[ wlan_twt_sta.c : 2553 ] wlan_sta_twt_resync_voip cmd: delete VOIP 
4708,iiiii,[ wlan_twt_sta.c : 2477 ] wlan_sta_twt_resync_voip: sta_twt_vdev->flags.host_enabled %d twt_enabled=%d voip active=%d in voip=%d TWT interval=%d 
4707,iiI,[ wlan_twt_sta.c : 3521 ] wlan_sta_twt_scan_evt_handler[SCAN_STARTED]: twt_vdev=%d, scan_vdev=%d, flags=0x%x 
4706,iiI,[ wlan_twt_sta.c : 3536 ] wlan_sta_twt_scan_evt_handler[SCAN_COMPLETED]: twt_vdev=%d, scan_vdev=%d, flags=0x%x 
4705,i,[ wlan_twt_sta.c : 1099 ] sending pause frame failed: status=%d 
4704,Iii,[ wlan_twt_sta.c : 2302 ] qmi msg nextTWT=%u dur=%d int=%d 
4703,i,[ wlan_twt_sta.c : 1143 ] sending resume frame failed: status=%d 
4702,iii,[ wlan_twt_sta.c : 3385 ] wlan_sta_twt_wmi_stats_event: vdev=%d, id=%d, event_type =%d 
4701,iiiiIII,[ wlan_twt_sta.c : 747 ] wlan_sta_twt_setup_done: is_broadcast=%d, is_unannoun=%d, is_trigger=%d, unsolicited=%d, wake_dura_us=%u, wake_intvl_us=%u, sp_offset_us=%u 
4700,i,[ wlan_twt_sta.c : 1346 ] wlan_sta_twt_setup_tx_completion: parse_setup_frame error, comp_ctxt = %d 
4699,iii,[ wlan_twt_sta.c : 2412 ] wlan_sta_twt_tune_voip_session fw_started=%d, all_paused=%d ap_control=%d 
4698,iii,[ wlan_twt_sta.c : 2418 ] wlan_sta_twt_tune_voip_session wake_duration=%d, wake_interval=%d wlan_twt_voip_sp=%d 
4697,ii,[ wlan_twt_sta.c : 3662 ] wlan_sta_twt_vdev_notif_handler: vdev_id=%d, notif=%d(3-stop, 2-DOWN) 
4696,i,[ wlan_twt_sta.c : 3680 ] wlan_sta_twt_vdev_notif_handler: vdev_id=%d, notif=UP 
4695,i,[ wlan_twt_sta.c : 3730 ] wlan_sta_twt_vdev_notif_handler: vdev_id=%d, notif=BRCM_AP_DETECTED 
4739,,[ wlan_twt_sta_sm.c : 1408 ] TWT VOIP session deleted 
4738,i,[ wlan_twt_sta_sm.c : 1348 ] sending teardown frame failed: status=%d 
4737,i,[ wlan_twt_sta_sm.c : 875 ] sending pause frame failed: status=%d 
4736,i,[ wlan_twt_sta_sm.c : 938 ] sending resume frame failed: status=%d 
4735,i,[ wlan_twt_sta_sm.c : 734 ] sending tune req frame failed: status=%d 
4734,i,[ wlan_twt_sta_sm.c : 745 ] sending renego req frame failed: status=%d 
4733,i,[ wlan_twt_sta_sm.c : 1180 ] got RESUME_REQ in resuming state %d 
4732,i,[ wlan_twt_sta_sm.c : 1198 ] sending resume frame failed: status=%d 
4740,,[ wlan_twt_sta_adaptor.c : 74 ] error on wlan_log_save_module_level 
4749,III,[ wlan_twt_ap.c : 283 ] AP TWT: Cant find peer lsb_mac=%x:%x:%x 
4748,i,[ wlan_twt_ap.c : 584 ] AP TWT: Vdev id = %d not TWT enabled 
4747,i,[ wlan_twt_ap.c : 994 ] AP TWT: Vdev id = %d not TWT enabled 
4746,i,[ wlan_twt_ap.c : 748 ] AP TWT: peer id = %d not TWT enabled 
4745,iIIi,[ wlan_twt_ap.c : 1224 ] wlan_twt_ap_req_en_dis(DIS): For mac_id=%d, Modules=%x TotalReqs=%x Host=%d 
4744,iIIi,[ wlan_twt_ap.c : 1237 ] wlan_twt_ap_req_en_dis(EN): For mac_id=%d, Modules=%x TotalReqs=%x Host=%d 
4743,i,[ wlan_twt_ap.c : 953 ] AP TWT: Vdev id = %d not TWT enabled 
4742,i,[ wlan_twt_ap.c : 1150 ] twt_stats wlan_twt_wmi_session_stats_event: twt wmi events are disabled pdev=%d 
4741,ii,[ wlan_twt_ap.c : 1160 ] twt_stats WMI_EVENT_ALLOC_FAILURE: pdev_id = %d evt_id = WMI_TWT_SESSION_STATS_EVENTID, length=%d 
4751,iii,[ wlan_powersave_sta_unit_test.c : 234 ] STA PS ITO pattern %d ito %d ms specWakeup %d ms 
4750,ii,[ wlan_powersave_sta_unit_test.c : 265 ] STA PS ITO config ito=%d ms specWakeup=%d ms 
4762,iiiiiiii,[ wlan_twt_unit_test.c : 860 ] wlan_twt_unit_test: vdev_id=%d, num_args=%d, type=%d, args:%d-%d-%d-%d-%d 
4761,i,[ wlan_twt_unit_test.c : 916 ] wlan_twt_unit_test: wrong num_args==%d, for WLAN_TWT_TEST_TYPE_ADD 
4760,i,[ wlan_twt_unit_test.c : 1041 ] unit test = %d 
4759,i,[ wlan_twt_unit_test.c : 1048 ] unit test = %d 
4758,i,[ wlan_twt_unit_test.c : 863 ] vdev == NULL: %d 
4757,i,[ wlan_twt_unit_test.c : 864 ] !vdev->ifUp, %d 
4756,ii,[ wlan_twt_unit_test.c : 797 ] wlan_twt_show_session_info: total %d session(s) in vdev%d 
4755,i,[ wlan_twt_unit_test.c : 667 ] TWT SP duration changed, early_sp_end_us=%d 
4754,i,[ wlan_twt_unit_test.c : 682 ] HostRequest: Prevent TWT to prompt ps-sm to send PM0 (1-Yes/0-No)=%d 
4753,iiIIIII,[ wlan_twt_unit_test.c : 779 ] wlan_twt_show_session_info: dialog_id=%d, session_id=%d, is_broadcast=%u,is_trigger=%u, is_unannoun=%u, responder_pm=%u, is_unsolicited=%u 
4752,IIII,[ wlan_twt_unit_test.c : 785 ] wlan_twt_show_session_info: wake_dura_us=%u, wake_intvl_us=%u,next_twt=%u, sp_offset_us=%u 
4765,,[ mu_gid_rx.c : 152 ] 11ac MU-MIMO GID MGMT: Ignoring GID MGMT message recieved while not in STA mode. 
4764,ii,[ mu_gid_rx.c : 69 ] 11ac MU-MIMO GID MGMT: Error in assigned group %d, user position %d 
4763,ii,[ mu_gid_rx.c : 75 ] 11ac MU-MIMO GID MGMT: Assigned group %d, user position %d 
4794,,[ ratectrl.c : 5423 ] RTS BL SM change RTS_11AC_AND_LEG_ALLOWED -> RTS_LEG_ALLOWED 
4793,,[ ratectrl.c : 5426 ] RTS BL SM change RTS_11AC_AND_LEG_ALLOWED -> RTS_LEG_ALLOWED_WITH_11AC_FALLBACK 
4792,,[ ratectrl.c : 5436 ] RTS BL SM change RTS_11AC_AND_LEG_ALLOWED -> RTS_DISALLOWED 
4791,,[ ratectrl.c : 5459 ] RTS BL SM change RTS_LEG_ALLOWED_WITH_11AC_FALLBACK -> RTS_DISALLOWED 
4790,,[ ratectrl.c : 5475 ] RTS BL SM change RTS_LEG_ALLOWED_WITH_11AC_FALLBACK -> RTS_11AC_AND_LEG_ALLOWED 
4789,,[ ratectrl.c : 5493 ] RTS BL SM change RTS_LEG_ALLOWED -> RTS_DISALLOWED 
4788,iii,[ ratectrl.c : 3738 ] _GetBestRate num_rates %d nss0 Rix %d nss1 Rix %d  
4787,II,[ ratectrl.c : 7330 ] rc_get_nondata_rc: %x for peer:%p  
4786,II,[ ratectrl.c : 7388 ] rc_get_ofdm_nondatarc: %x for peer:%p  
4785,iIIIiI,[ ratectrl.c : 2719 ] rc_mask_idx %d rc_mask 0x%x xretry_mask_4_nss 0x%x new_rc_mask 0x%x xretry_max_mcs_allowed %d mem: 0x%x 
4784,IIiiiII,[ ratectrl.c : 7127 ] RATECTRL_DBGID_RATE_UPDATE: cur_rate:0x%x rate_code:0x%x currPER:%d lastPER:%d Mbps:%d bw_idx:%x tpc:0x%x 
4783,iiiI,[ ratectrl.c : 7180 ] TxRetrySchedule: DYN BW : idx %d rts %d cts %d rate_info.rts_rix %x
 
4782,iIIII,[ ratectrl.c : 7527 ] pdev_id:%d rc_leg_rate_allowed=0x%x rc_legacy_mask=0x%x temp_cck_rate_bitmap=0x%x module_id=0x%x 
4781,iIIIII,[ ratectrl.c : 7557 ] FINAL: pdev_id:%d rc_leg_rate_allowed=0x%x rc_legacy_mask=0x%x  pdev->rc_legacy_mask: BT=0x%x LTE_COEX=0x%x HE_ASSOC=0x%x
 
4780,iiii,[ ratectrl.c : 3997 ] _rcRateFind bw_idx %d bestRate Rix %d (nss %d mcs %d) 
4779,,[ ratectrl.c : 5894 ] Set INVALID!!! RTS Rate Index 
4778,ii,[ ratectrl.c : 5904 ] _RATE_SetRtsCtsRate: Def RTS Rate Rix %d Alt RTS Rate Rix %d  
4777,I,[ ratectrl.c : 4674 ] SEC_RETRY skip PER update flags:0x%x 
4776,iIiiiiI,[ ratectrl.c : 4789 ] RATECTRL_DBGID_RATE_UPDATE: _rcUpdate_HT is_gtx_tx %d ptx_rc 0x%x ptx_tpc %d nFrames %d retries %d nBad %d flags 0x%x 
4775,iii,[ ratectrl.c : 4881 ] _rcUpdate_HT: Xretry : Enable RTS -- rtsForFirstSeries %d 11ac rts %d leg rts %d 
 
4774,iii,[ ratectrl.c : 4903 ] _rcUpdate_HT: Xretry Prot failure: After Toggle RTS -- rtsForFirstSeries %d --[RTS Profile %d Toggle %d]
 
4773,I,[ ratectrl.c : 4941 ] RATECTRL_DBGID_RATE_UPDATE: _rcUpdate_HT bw_idx:8/nss_idx:8/xRetry:16 0x%08x  
4772,iiiiiiii,[ ratectrl.c : 4982 ] xretry :: Rix %d (nss - %d, mcs - %d bw %d) xretry_max_mcs_allowed - %d PER-(ref = %d, new = %d) ER %d 
 
4771,ii,[ ratectrl.c : 5022 ] _rcUpdate_HT: PPDU complete/partial Success 11ac rts %d leg rts %d 
 
4770,iIiI,[ ratectrl.c : 5080 ] _rcUpdate_HT: xretry_max_mcs_allowed reset to %d (mem: 0x%x) for Rix %d (nss:8/mcs:8/bw:8 0x%08x) 
 
4769,IIIII,[ ratectrl.c : 7915 ] rc_update_rts_per: rts_rix 0x%x def_rix 0x%x alt_rix 0x%x curr_rix 0x%x ni_legacy_rate_set 0x%x 
 
4768,II,[ ratectrl.c : 2281 ] rc_validate_rateset/NON_HT:  Before mask update ni_legacy_rate_set 0x%x validTxRateMask 0x%x 
4767,II,[ ratectrl.c : 2320 ] rc_validate_rateset/NON_HT:  After mask update ni_legacy_rate_set 0x%x validTxRateMask 0x%x 
4766,iiIiiI,[ ratectrl.c : 2481 ] NSS Mismatch: 160nss %d, 160_mcs_nss_set %d, 160_mcs_nss_map %x, 80nss %d, 80_mcs_nss_set %d, 80_mcs_nss_map %x 
4801,I,[ ratectrl_if.c : 269 ] is_rc_peer_mem_optimized: peer is invalid vdev:0x%x 
4800,IIi,[ ratectrl_if.c : 2220 ] AUTORATE_RESET_USER_START_RATE: peer  phymode:8/ht:8/vht:8 : 0x%08x ni_flags 0x%x  user_start_rate %d 
4799,,[ ratectrl_if.c : 1960 ] RATE_EnableCCKRatesInHTMode: No vdev's attached to pdev, rejecting WLAN_PDEV_ENABLE_CCK_RATE !
 
4798,i,[ ratectrl_if.c : 2032 ] vdev[%d] is NULL, rejecting WLAN_PDEV_ENABLE_CCK_RATE !
 
4797,IiiIiii,[ ratectrl_if.c : 2010 ] Enabling coex restriction (pdev - 0x%x) enable %d min_rate:%d on wlan_peer:0x%x rc_mode:%d rateMax:%d bestRate:%d 
4796,IiiIiii,[ ratectrl_if.c : 2022 ] Enabling coex restriction (pdev - 0x%x) enable %d min_rate:%d on wlan_peer:0x%x rc_mode:%d rateMax:%d bestRate:%d 
4795,IIiII,[ ratectrl_if.c : 2379 ] 
org_rc_mask_null pdev_rc_mask[0]:%x pdev_rc_mask[1]:%x phymode:%d ni_legacy_rate_set:%x rc_legacy_mask_final:%llx 
4815,,[ ratectrl_debug.c : 412 ] setUnitTestcmd FAILED : SUPPORT_AUTORATE_RESET not implemented 
4814,iii,[ ratectrl_debug.c : 439 ] Number of invalid peer assoc capabilities for HT %d, VHT %d, HE %d
 
4813,i,[ ratectrl_debug.c : 467 ] g_dbg_enable_he_short_gi: %d 
 
4812,Ii,[ ratectrl_debug.c : 502 ] RTS_DEBUG: vdev id:8/rts cts type:8/rts cts profile:16 0x%08x rts_rix %d
 
4811,I,[ ratectrl_debug.c : 534 ] RT_UPDATE SU Mode, BW:8/NSS8: %08u. 
4810,I,[ ratectrl_debug.c : 537 ] RT_UPDATE MU Mode,  BW:8/NSS8: %08u. 
4809,I,[ ratectrl_debug.c : 542 ] RT_UPDATE Last Probed  BW:8/NSS:8/MCS:8 : %08u. 
4808,IIIII,[ ratectrl_debug.c : 549 ] RT_UPDATE MCS_%u: PPDU Tried: %u, PPDU ACK Failed: %u, MPDUS Tried: %u, MPDUS Failed: %u. 
4807,,[ ratectrl_debug.c : 580 ] This command is not supported in this platform. 
4806,,[ ratectrl_debug.c : 615 ] This command is not supported in this platform 
4805,i,[ ratectrl_debug.c : 153 ] _RATE_GTX_dbg: VDEV ID:%d wal_vdev is NULL 
4804,i,[ ratectrl_debug.c : 196 ] _RATE_GTX_dbg: INAVLID CMD: %d 
4803,iii,[ ratectrl_debug.c : 161 ] VDEV ID:%d PDEV ID:%d GTX STATUS:%d  
4802,II,[ ratectrl_debug.c : 166 ]  gtxPERThreshold:8/gtxPERMargin:8/gtxTPCstep:8/gtxTPCMin:8  :0x%08x   userGtxMask:8/gtxBWMask:8 0x%08x
, 
4829,,[ ratectrl_gtx.c : 420 ] RATECTRL_DBGID_GTX_UPDATE: GTX disable, Rate not found  
4828,,[ ratectrl_gtx.c : 427 ] RATECTRL_DBGID_GTX_UPDATE: GTX disable, Rate change  
4827,,[ ratectrl_gtx.c : 436 ] RATECTRL_DBGID_GTX_UPDATE: GTX disable, BW mis-match  
4826,II,[ ratectrl_gtx.c : 453 ] RATECTRL_DBGID_GTX_UPDATE: GTX disable, MAX TX Power changed, last_tpc=0x%x halphy_tpc=0x%x 
4825,IiIIIi,[ ratectrl_gtx.c : 618 ] TPC DOWN EVAL: last_tpc 0x%x tpc_step %d, curr_min_tpc 0%x gtxTPCMin 0x%x temp 0x%x packets %d 
4824,ii,[ ratectrl_gtx.c : 725 ] cur_min_tpc updated to %d for bw_idx %d
 
4823,iiii,[ ratectrl_gtx.c : 740 ] Reset pseudo_per[%d] = %d last_tpc %d updated_tpc %d
 
4822,IIiiIIII,[ ratectrl_gtx.c : 756 ] RATECTRL_DBGID_GTX_UPDATE: UP: tpc=0x%x last_tpc=0x%x curr_PPER:%d curr_RPER:%d rix=0x%x ratecode:%x bw_idx=0x%x (ER,RTS) 0x%x 
4821,IIIIIII,[ ratectrl_gtx.c : 193 ] :RATECTRL_DBGID_GTX_UPDATE:RTMask:0x%x:0x%x:0x%x:0x%x:0x%x:0x%x:0x%x 
4820,iIIII,[ ratectrl_gtx.c : 71 ] :RATECTRL_DBGID_GTX_UPDATE:MCSMask:HE20:nss_max:%d:mcsMask:0x%04X:mcs_max:%02d:validTxRateMask:0x%08X:gtxRTMask:0x%08X 
4819,iIIII,[ ratectrl_gtx.c : 159 ] :RATECTRL_DBGID_GTX_UPDATE:MCSMask:VHT160:nss_max:%d:mcsMask:0x%04X:mcs_max:%02d:validTxRateMask:0x%08X:gtxRTMask:0x%08X 
4818,iIIII,[ ratectrl_gtx.c : 175 ] :RATECTRL_DBGID_GTX_UPDATE:MCSMask:HT20:nss_max:%d:mcsMask:0x%04X:mcs_max:%02d:validTxRateMask:0x%08X:gtxRTMask:0x%08X 
4817,iIIII,[ ratectrl_gtx.c : 121 ] :RATECTRL_DBGID_GTX_UPDATE:MCSMask:HE160:nss_max:%d:mcsMask:0x%04X:mcs_max:%02d:validTxRateMask:0x%08X:gtxRTMask:0x%08X 
4816,iIIII,[ ratectrl_gtx.c : 143 ] :RATECTRL_DBGID_GTX_UPDATE:MCSMask:VHT20:nss_max:%d:mcsMask:0x%04X:mcs_max:%02d:validTxRateMask:0x%08X:gtxRTMask:0x%08X 
4853,i,[ sched_algo.c : 3001 ] STANDALONE:sched_algo_cmd_update_user_info NDPA FLAG NOT SET $$$tid_num=%d 
4852,iII,[ sched_algo.c : 10868 ] sched_algo_disable_sched_mode_bmap_update: IN: txq_id: %d, disabled_sched_mode_bmap_req: 0x%08x, disabled_sched_mode_bmap: 0x%08x 
4851,iII,[ sched_algo.c : 10895 ] sched_algo_disable_sched_mode_bmap_update: OUT: txq_id: %d, disabled_sched_mode_bmap_req: 0x%08x, disabled_sched_mode_bmap: 0x%08x 
4850,iiiIiIII,[ sched_algo.c : 5296 ] twt_dbg_eosp / ul_dbg: sched_dispatch_sched_cmd txqid=%d, sched_id=%d, posted_commands=%d,sched_cmd_flags=0x%x, is_partial=%d, tsf_low=%u, start_time=%u, end_time=%u 
 
4849,IiiIII,[ sched_algo.c : 9486 ] twt_dbg_eosp: sched_algo_dl_eligible_check peer_id=%u, is_announced=%d, is_ul_received=%d,tidq->tid_num=%u, tid_ext_flags=0x%x, eosp_state=%u 
4848,ii,[ sched_algo.c : 4245 ] TTL dropped count:%d, tid:%d 
4847,iiiii,[ sched_algo.c : 10656 ] pdev_id:%d tx_send_lp_pcie_state_change %d->%d            cur_time_ms:%d last_pcie_tx_activity_ms:%d  
4846,ii,[ sched_algo.c : 10679 ] tx pdev_id:%d pcie lp state changed to active mode counter part state:%d 
4845,ii,[ sched_algo.c : 10706 ] tx pdev_id:%d pcie lp state changed to sleep mode counter part state:%d 
4844,III,[ sched_algo.c : 8195 ] migrate peer in delete prog %p, flags:%x, sw_peer_id:%x 
4843,iII,[ sched_algo.c : 8225 ] migrate peer %d, already on MAC(%u %u) 
4842,IIiiiII,[ sched_algo.c : 3572 ] PPDU Duration debug: sched_id=0x%x sched_seq_type=0x%x txop_us=%d txtime_us=%d max_ppdus=%d flags=0x%x 0x%x 
4841,IIIII,[ sched_algo.c : 7031 ] discard trigger msg as pdev mismatch peer_id=%x,tid=%x,pdev=%x:%x,flag=%x 
4840,i,[ sched_algo.c : 8742 ] sched_algo_req_handler: unsupported msg type:%d 
4839,iiiiii,[ sched_algo.c : 2447 ] twt_dbg: twt_sched_algo_return (slot ended):txqid=%d, tsf_now_msb=%d, lsb=%d, curr_slot_end msb=%d, lsb=%d slot_valid:%d 
4838,iiI,[ sched_algo.c : 2579 ] twt_dbg: twt_sched_algo_run_policy: txqid=%d, sched_cmd_space=%d, flags=%x 
4837,iiII,[ sched_algo.c : 6109 ] TTL tid:%d txq_id:%d, flg-clr:%x %x 
4836,ii,[ sched_algo.c : 286 ] STANDALONE : SEND MESSAGE TO SCHEDULER %d thread id %d  
4835,ii,[ sched_algo.c : 1582 ] ul_dbg_sched_algo_tid_register: num_frames=%d, tid_num=%d 
4834,iiiIi,[ sched_algo.c : 1620 ] TID REG:peer %d tidnum %d txqid %d flags %x num active %d
 
4833,ii,[ sched_algo.c : 1709 ] ul_dbg_sched_algo_tid_unregister: num_frames=%d, tid_num=%d 
4832,iiiIii,[ sched_algo.c : 1763 ] TID UNREG:peer %d tidnum %d txq %d flags %x num active %d, pause_tid:%d 
4831,II,[ sched_algo.c : 2861 ] sched_algo_cmd_update_user_info: g_qnull_peer_id%x %x 
4830,,[ sched_algo.c : 2867 ] NEW_STATS: qnull set 
4854,ii,[ sched_algo_rr.c : 296 ] twt_dbg: sched_algo_run_rr_scheduler_tidq0 skip tid tid:%d elgble: %d 
4886,ii,[ sched_algo_dbg.c : 196 ] STANDALONE : TICKLE SCHEDULER %d thread id %d  
4885,i,[ sched_algo_dbg.c : 2504 ] SCHED_RU_ALLOC_DBG: g_sched_algo_cfg.dbg.cnt.dl_mode_allocation_failed: %d 
4884,I,[ sched_algo_dbg.c : 4359 ] CV_UPLOAD cv_dma_timeout_err  : %u 
4883,I,[ sched_algo_dbg.c : 4362 ] CV_UPLOAD cv_nc_idx_mismatch  : %u 
4882,I,[ sched_algo_dbg.c : 4365 ] CV_UPLOAD cv_expiry_in_update : %u 
4881,I,[ sched_algo_dbg.c : 4368 ] CV_UPLOAD cv_update_failed    : %u 
4880,I,[ sched_algo_dbg.c : 4371 ] CV_UPLOAD cv_pkt_bw_exceed    : %u 
4879,i,[ sched_algo_dbg.c : 2796 ] pdev %d not initialized 
 
4878,II,[ sched_algo_dbg.c : 5063 ] DYN_MIMO_PS sw_peer_id: %u, dyn_mimo_ps_enabled: %u. 
4877,ii,[ sched_algo_dbg.c : 2800 ] pdev %d rx_ps_fifo_drop %d 
 
4876,iii,[ sched_algo_dbg.c : 3661 ] STANDALONE INVALID SW PEER ID cmd num %d pdev id %d sw peer id %d 
4875,iii,[ sched_algo_dbg.c : 3664 ] STANDALONE  cmd num %d pdev id %d sw peer id %d  
4874,I,[ sched_algo_dbg.c : 3708 ] effective_tput_gain_factor: %u. 
4873,II,[ sched_algo_dbg.c : 3803 ] PARTIAL_SND_STATS: : MU2  1:%u 2:%u  
4872,III,[ sched_algo_dbg.c : 3808 ] PARTIAL_SND_STATS: : MU3  1:%u 2:%u 3:%u 
4871,i,[ sched_algo_dbg.c : 2508 ] SCHED_RU_ALLOC_DBG: g_sched_algo_cfg.dbg.cnt.ul_mode_allocation_failed: %d 
4870,IIII,[ sched_algo_dbg.c : 3814 ] PARTIAL_SND_STATS: : MU4  1:%u 2:%u 3:%u 4:%u 
4869,II,[ sched_algo_dbg.c : 3935 ] dl_mu_mimo_my_cv_sync g_dbg_mu_cv_sync_counter: %u, g_dbg_mu_cv_sync_counter_invalid_idx: %u. 
4868,,[ sched_algo_dbg.c : 4109 ] SU_STATS_DBG: usage: wifitool athX setUnitTestCmd 0x47 3 258 < 0 / 1 > 
4867,,[ sched_algo_dbg.c : 4133 ] SU_STATS_DBG: ---Cleared all SU Multi Destination and SU Only stats--- 
4866,iiii,[ sched_algo_dbg.c : 4139 ] SU_STATS_DBG: num_su_multi_dest_scheduled: BK: %d | BE = %d | VI = %d | VO = %d 
4865,iiii,[ sched_algo_dbg.c : 4145 ] SU_STATS_DBG:       num_su_only_scheduled: BK: %d | BE = %d | VI = %d | VO = %d 
4864,i,[ sched_algo_dbg.c : 4207 ] STANDALONE INVALID SW PEER ID %d 
4863,,[ sched_algo_dbg.c : 4213 ] STANDALONE SEND MSG SUCCESSFUL 
4862,,[ sched_algo_dbg.c : 4215 ] STANDALONE SEND MSG FAILED  
4861,iiii,[ sched_algo_dbg.c : 4237 ] AC_DBG: Requests BE: %d, BK: %d, VI: %d, VO: %d 
4860,ii,[ sched_algo_dbg.c : 2517 ] SCHED_RU_ALLOC_DBG: g_sched_algo_cfg.dbg.cnt.sched_mode_disabled[%d]: %d 
4859,iiii,[ sched_algo_dbg.c : 4238 ] AC_DBG: Counters Data Txq : %d, Other Txq: %d, i/p max_sched_cmd < pending sched_cmds: %d, default %d 
4858,I,[ sched_algo_dbg.c : 4347 ] CV_UPLOAD cv_fcs_err          : %u 
4857,I,[ sched_algo_dbg.c : 4350 ] CV_UPLOAD cv_frag_idx_mimatch : %u 
4856,I,[ sched_algo_dbg.c : 4353 ] CV_UPLOAD cv_invalid_peer_id  : %u 
4855,I,[ sched_algo_dbg.c : 4356 ] CV_UPLOAD cv_dma_not_done_err : %u 
4898,IIiII,[ sched_algo_twt.c : 49 ] twt_dbg: twt_scheduler_timer1: tsf_now_msb=%u, lsb=%u, curr_slot_idx=%d, curr_slot_start msb=%u, lsb=%u 
4897,iiII,[ sched_algo_twt.c : 56 ] twt_dbg: twt_scheduler_timer1: 5ghz=%d, next_slot_idx=%d, next_slot_start msb=%u, lsb=%u 
4896,IIIi,[ sched_algo_twt.c : 91 ] twt_dbg: twt_scheduler_timer:peer_id=%u, peer_end_tsf msb=%u, lsb=%u, twt_qid=%d 
4895,IIIIIIII,[ sched_algo_twt.c : 930 ] twt_dbg_eosp: check_eosp_eligibility:tid_num=%u, inactivity_time_us=%u, last_activity_ts=%u, frms_swq=%u, frms_hwq=%u, is_eosp_eligible=%u,elapsed_time=%u, remaining_time=%u
 
4894,Iiiiii,[ sched_algo_twt.c : 361 ] twt_dbg: sched_algo_twt_get_next_tid1 overlapping peer_id=%u tsf_low=%d sp-start=%d sp-end=%d sw-q=%d hw-q=%d 
4893,Iii,[ sched_algo_twt.c : 408 ] twt_dbg: sched_algo_twt_get_next_tid2 chosen peer_id=%u TID:%d Eligible:%d 
4892,Iii,[ sched_algo_twt.c : 417 ] twt_dbg: sched_algo_twt_get_next_tid3 ineligible peer_id=%u TID:%d Eligible:%d 
4891,II,[ sched_algo_twt.c : 619 ] twt_dbg: twt_peer_register peer_id=%u, twt_peer_count=%u 
4890,III,[ sched_algo_twt.c : 668 ] twt_dbg: twt_peer_unregister peer_id=%u, twt_peer_count=%u, peer_twt_state=0x%x 
4889,Iii,[ sched_algo_twt.c : 534 ] twt_dbg: sched_algo_twt_sp_info_update peer_id=%u, is_announced=%d, is_ul_received=%d 
4888,I,[ sched_algo_twt.c : 559 ] twt_dbg: sched_algo_twt_sp_info_update_triggered_super_cycle peer_id=%u 
4887,IIIII,[ sched_algo_twt.c : 483 ] twt_dbg: twt_update_start_end_time peer_id=%u, start_time=%u, end_time=%u, flags=0x%x, valid=%u 
4911,IIIIIIIII,[ sched_algo_txbf.c : 819 ] SW Peer ID: %x cbf_mimo_ctrl VHT_HE: %x, NR: %x, NC: %x, FB: %x, BW: %x, NG: %x, CB: %x, ASNR: %x. 
4910,IIII,[ sched_algo_txbf.c : 843 ] cbf_mimo_ctrl NC index mismatch. SW_PEER_ID: %u, PEER_NC: %u, CV_NC: %u, Total Mismatch: %u. 
4909,IIII,[ sched_algo_txbf.c : 1828 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
4908,IIII,[ sched_algo_txbf.c : 1837 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
4907,IIII,[ sched_algo_txbf.c : 1872 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
4906,IIII,[ sched_algo_txbf.c : 1881 ] tone out of index: is_he:%x,cbf_bw:%x,pkt_bw:%x, ng:%x 
4905,II,[ sched_algo_txbf.c : 2648 ] cbf asnr mis-match asnr0=%u asnr1=%u
 
4904,iiii,[ sched_algo_txbf.c : 2974 ] snd_start: sucess to reserve %d cv_bufs, and %d cv_bufs remaining, and intotal %d cv_bufs in cv_ring  pdev_txbf_cnt %d 
4903,iiii,[ sched_algo_txbf.c : 3002 ] snd_start: fail to reserve %d cv_bufs, only %d cv_bufs remaining, and intotal %d cv_bufs in cv_ring  pdev_txbf_cnt %d 
4902,i,[ sched_algo_txbf.c : 1340 ] snd_failure update cv_buf num  %d 
4901,i,[ sched_algo_txbf.c : 1421 ] snd_success remaining cv_buf num  %d 
4900,Ii,[ sched_algo_txbf.c : 3435 ] cv_upload_dma invalid SW peer ID cv_buf->sw_peer_id 0x%x pdev_id %d 
4899,I,[ sched_algo_txbf.c : 3474 ] snd_cv_upload success buf 0x%0x 
4938,III,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 319 ] DFS_DUMPS Rejecting Radar since delta peak values are invalid : dl_delta_peak_match_count=%lu, dl_psidx_diff_match_count=%lu, rf_threshold=%lu
 
4937,IIi,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 324 ] DFS_DUMPS %s: Rejecting Radar since duration diff %ld is more than %d
 
4936,i,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 464 ] [%d]: dfs is NULL 
4935,i,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 561 ] [%d]: event is NULL  
4934,iiIIII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 794 ] 
[%d]:PHYERR# = %d ts = %u  diff_ts = %u ppdu_rssi = %u dur = %u
 
4933,iiiiii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 798 ] 
[%d]: is_hw_chirp = %d segid = %d sidx = %d peak_mag = %d delta_peak = %d 
 
4932,iiiiIi,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 802 ] 
[%d]: delta_diff = %d agc_total_gain = %d agc_mb_gain = %d radar_subchan_mask = 0x%x pulse_height = %d 
 
4931,iiiii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 807 ] 
[%d]: triggering_agc_event = %d rs_pulse_rssi = %d pri80_inband_power = %d ext80_inband_power = %d 
 
4930,iIIIII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 811 ] [%d]:xxxxx ts =%u re.re_dur=%u re.re_rssi =%u diff =%u pl->pl_lastelem.p_time=%llu xxxxx 
4929,Ii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 890 ] :chan->ic_flags=0x%x, MHz separation=%d
 
4928,iii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 894 ] : Peak Idx =%d,re.re_dur =%d,diff_ts =%d
 
4927,,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 897 ] 
: Modify pulse dur to fit valid range 
 
4926,Ii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 926 ] 
:chan->ic_flags=0x%x,MHz Separation=%d
 
4925,iii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 930 ] :Peak Index =%d,re.re_dur =%d,diff_ts =%d
 
4924,,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 933 ] :Modify ETSI pulse dur to valid range 
 
4923,,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 994 ] DFS_DUMPS found bin5 radar
 
4922,iII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1034 ] [%d]: Rejecting on rssi rssi=%u thresh=%u 
4921,ii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1035 ] DFS_DUMPS Rejecting pulses on rssi rssi=%d, thresh=%d
 
4920,iII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1066 ] [%d]:Rejecting on pri pri=%lld minpri=%u 
4919,iiII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1100 ] [%d]:filterID= %d::Rejecting on individual filter min PRI deltaT=%lld rf->rf_minpri=%u 
4918,iiII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1123 ] [%d]:filterID= %d :: Rejecting on individual filter max PRI deltaT=%lld rf->rf_minpri=%u 
4917,iiII,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1168 ] [%d]:filterID= %d :: Rejecting on individual filter max PRI deltaT=%lld rf->rf_minpri=%u 
4916,iiii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1242 ] [%d]:### Found on channel minDur = %d, filterId = %d  seg_id = %d ### 
4915,iiii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1290 ] DFS_DUMPS Radar Found with Filter Id = %d min dur=%d sidx=%d freq_offset=%d
 
4914,ii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1297 ] CHANNEL_CLOSE radarevent g_dfs_test_mode=%d  event_data.detection_mode=%d
 
4913,iiii,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1328 ] [%d]:### RADAR FOUND ON CHANNEL %d (%d MHz),seg_id=%d ### 
4912,i,[ hca_HwComponentBbLithium_dfs_process_radarevent.cpp : 1398 ] DFS_DEBUGS false_radar dfs->dfs_seq_num =%d
 
4940,,[ hca_HwComponentBbLithium_debug.cpp : 931 ] PHYDBG DISABLE: HcaHwComponentBbLithium_debug::PHYDBG_disable 
4939,,[ hca_HwComponentBbLithium_debug.cpp : 933 ] PHYDBG disabled
 
4950,ii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 479 ] DFS_DUMP Dfs0Sighandler pHandle=%d ipc_ring_id=%d
 
4949,ii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 487 ] DFS_DUMP Dfs1Sighandler pHandle=%d ipc_ring_id=%d
 
4948,ii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 497 ] DFS_DUMP Dfs2Sighandler pHandle=%d ipc_ring_id=%d
 
4947,,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 270 ] FFT_RAW START 
 
4946,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 274 ] FFT_RAW %p 0x%x 
 
4945,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 278 ] FFT_RAW %p 0x%x 
 
4944,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 280 ] FFT_RAW %p 0x%x 
 
4943,II,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 281 ] FFT_RAW %p 0x%x 
 
4942,,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 286 ] FFT_RAW END 
 
4941,iii,[ hca_HwComponentBbLithium_dfs_process_phyerr.cpp : 460 ] DFS_DUMP pcss_ipc_sig_handler_process_multiple_ring_element pHandle=%d ipc_ring_id=%d num_bufs=%d
 
4964,I,[ hca_HwComponentBbLithium_debug_core.cpp : 510 ] PHYDBG LWod 0x%lx
 
4963,I,[ hca_HwComponentBbLithium_debug_core.cpp : 511 ] PHYDBG UWod 0x%lx
 
4962,Ii,[ hca_HwComponentBbLithium_debug_core.cpp : 271 ] %s skipping bank %d
 
4961,I,[ hca_HwComponentBbLithium_debug_core.cpp : 461 ] PHYDBG_CAPTURE_U 0x%lx
 
4960,I,[ hca_HwComponentBbLithium_debug_core.cpp : 462 ] PHYDBG_CAPTURE_L 0x%lx
 
4959,I,[ hca_HwComponentBbLithium_debug_core.cpp : 463 ] PHYDBG_PLAYBACK_U 0x%lx
 
4958,I,[ hca_HwComponentBbLithium_debug_core.cpp : 464 ] PHYDBG_PLAYBACK_L 0x%lx
 
4957,I,[ hca_HwComponentBbLithium_debug_core.cpp : 465 ] PHYDBG_PHYRF_TX_PRE_DESC_WR_1_L 0x%lx
 
4956,I,[ hca_HwComponentBbLithium_debug_core.cpp : 466 ] PHYDBG_WFAX_PHYRF_PHYRF_ACTIVATION_CTRL_L 0x%lx
 
4955,I,[ hca_HwComponentBbLithium_debug_core.cpp : 467 ] PHYDBG_MODE_L 0x%lx
 
4954,I,[ hca_HwComponentBbLithium_debug_core.cpp : 468 ] PHYDBG_TRIGGER_0_L 0x%lx
 
4953,I,[ hca_HwComponentBbLithium_debug_core.cpp : 469 ] PHYDBG_TRIGGER_0_U 0x%lx
 
4952,I,[ hca_HwComponentBbLithium_debug_core.cpp : 470 ] PHYDBG_TRIGGER_1_L 0x%lx
 
4951,Ii,[ hca_HwComponentBbLithium_debug_core.cpp : 371 ] %s skipping bank %d
 
4968,iiIiiiiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 294 ] DFS_DUMPS ts=%d diff_ts=%d sidx=%i dur=%d chirp=%d det=%d radar_check=%d agc_event=%d rssi=%d  
4967,iiiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 300 ] DFS_DUMPS ts=%d delta_peak=%d delta_diff=%d total_gain=%d is_max_pw=%d  
4966,iiiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 324 ] DFS_DUMP radar summary detection_mode=%d  timestamp=%d pulse_rssi=%d is_chirp=%d sidx=%d
 
4965,iiiiiIiii,[ hca_HwComponentBbLithium_dfs_phyerr_tlv.cpp : 191 ] DFS_DUMPS ts=%d fft_num=%d radar_check=%d total_gain=%d base_pwr=%d peak_sidx=%i relpwr=%d peak_mag=%d num_str_bins_ib=%d
 
4969,I,[ hca_HwComponentBbLithium_phy.cpp : 139 ] %s
 
4970,i,[ hca_HwComponentBbLithium_pcss.cpp : 313 ] PcssIpcIRQHandler: PS Mode, ignoring IPC IRQ! phyId:%d 
4971,i,[ hca_HwComponentBbLithium_pcss_ipc.cpp : 530 ] PcssIpcRingIRQHandler: PS Mode, ignoring IPC Ring IRQ! phyId:%d 
4985,i,[ hca_HwComponentBbQca649x_pcss.cpp : 107 ] PHY M3 Assert for PHY : %d
 
4984,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 111 ] %c%c%c%c 
4983,I,[ hca_HwComponentBbQca649x_pcss.cpp : 279 ] PAPRD: UCODE VREG WAR enabled , vReg %x 
4982,ii,[ hca_HwComponentBbQca649x_pcss.cpp : 212 ] PCSS Version : Branch = %d, Build ID = %d  
4981,i,[ hca_HwComponentBbQca649x_pcss.cpp : 64 ] PHY M3 Assert for PHY : %d
 
4980,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 66 ] %c%c%c%c 
4979,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 68 ] %c%c%c%c 
4978,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 70 ] %c%c%c%c 
4977,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 72 ] %c%c%c%c 
4976,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 74 ] %c%c%c%c 
4975,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 76 ] %c%c%c%c 
4974,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 78 ] %c%c%c%c 
4973,IIII,[ hca_HwComponentBbQca649x_pcss.cpp : 80 ] %c%c%c%c 
4972,,[ hca_HwComponentBbQca649x_pcss.cpp : 295 ] Qca649x_pcss::WriteBeaconRssiValueToVreg: Error Cannot Access Register in Sleep, return 
5011,i,[ hca_HwComponentBbQca649x_reset.cpp : 1497 ] DssControl: Return with no-effect. synth_control=%d 
5010,ii,[ hca_HwComponentBbQca649x_reset.cpp : 1501 ] DssControl: phyId %d, enable %d 
5009,iiii,[ hca_HwComponentBbQca649x_reset.cpp : 1538 ] EnableOCL: enable=%d listen_chain=%d backoff=%d FOR PHYID %d 
5008,,[ hca_HwComponentBbQca649x_reset.cpp : 2149 ] Error Cannot Access RO_PLL_LOCK Register in Sleep, return 
5007,i,[ hca_HwComponentBbQca649x_reset.cpp : 2163 ] g_consecutive_ro_pll_unlock=%d 
5006,,[ hca_HwComponentBbQca649x_reset.cpp : 2171 ] R0 PLL got unlocked for 4 consecutive time 
5005,iIi,[ hca_HwComponentBbQca649x_reset.cpp : 305 ] PostProgInit: phyID %d, resetCause 0x%x, homeChan %d
 
5004,Ii,[ hca_HwComponentBbQca649x_reset.cpp : 1401 ] PerformPhyOff: q6_to_m3_ipc_address=%x q6_to_m3_ipc=%d 
5003,Ii,[ hca_HwComponentBbQca649x_reset.cpp : 1407 ] PerformPhyOff: isNotDone=%x, loopCount=%d 
5002,ii,[ hca_HwComponentBbQca649x_reset.cpp : 1414 ] PerformPhyOff: MAC|PHYID=%d WFAX_PCSS_VR_Q6_TO_M3_10_L=%d 
5001,Ii,[ hca_HwComponentBbQca649x_reset.cpp : 1553 ] SetPowerFeatMask: Set Power Mask to %x FOR PHYID %d 
 
5000,iiiiiiiii,[ hca_HwComponentBbQca649x_reset.cpp : 657 ] SetXOPowerMode phyId %d, valid=%d, wakeup=%d, imps=%d, valid_1=%d, wakeup_1=%d, imps_1=%d, ignore_other_phy=%d, ignore_this_phy=%d 
4999,iii,[ hca_HwComponentBbQca649x_reset.cpp : 690 ] SetXOPowerMode Done: phyId %d, lp_xo=%d, curr_xo_state_lp=%d 
4998,i,[ hca_HwComponentBbQca649x_reset.cpp : 1423 ] ANI_DUMP_PHYID%d SAVE ANI DEFAULTS 
 
4997,IIII,[ hca_HwComponentBbQca649x_reset.cpp : 2033 ] ###2G VCM_TRACK_Q_EVEN:%x %x, Q_ODD:%x %x 
4996,IIII,[ hca_HwComponentBbQca649x_reset.cpp : 2077 ] ###5G VCM_TRACK_Q_EVEN:%x %x, Q_ODD:%x %x 
4995,iiiiiiII,[ hca_HwComponentBbQca649x_reset.cpp : 1275 ] ResetPhyInputCommon: phyId %d bw %d mhz %d freq %d/%d dynPriChan %d txCM 0x%x rxCM 0x%x 
4994,iiiII,[ hca_HwComponentBbQca649x_reset.cpp : 1283 ] ResetPhyInputCommon: conc %d isSBS %d NF %d pwrMask 0x%x loadIniMask 0x%x 
4993,iIIiiiii,[ hca_HwComponentBbQca649x_reset.cpp : 753 ] RetentionSetChannel: phyId %d txCM 0x%x rxCM 0x%x wakeup %d imps %d fullsave %d homechan %d  cur_tbl_idx %d 
4992,iiiiI,[ hca_HwComponentBbQca649x_reset.cpp : 754 ] RetentionSetChannel: chan %d freq1 %d freq2 %d phy_mode %d flags 0x%x 
4991,iii,[ hca_HwComponentBbQca649x_reset.cpp : 782 ] RetentionSetChannel: phyId %d, IMPS %d, Sleep %d, is ignored by debug knob 
4990,iiiiiiiii,[ hca_HwComponentBbQca649x_reset.cpp : 1148 ] RetentionSetChannel: Profile PHYID=%d SLEEP=%d IMPS=%d, RETINI=%d RESET=%d CAL=%d TPC=%d TOT=%d PF=%d 
4989,iiI,[ hca_HwComponentBbQca649x_reset.cpp : 1706 ] WritePcssM3Register: phyId: %d pcssM3reg: %d pcssM3RegValue: 0x%x 
4988,,[ hca_HwComponentBbQca649x_reset.cpp : 1710 ] Error Cannot Access Register in Sleep, return 
4987,ii,[ hca_HwComponentBbQca649x_reset.cpp : 1349 ] WarmReset MAC|PHYID=%d CF_ACTIVE=%d 
4986,iiiiI,[ hca_HwComponentBbQca649x_reset.cpp : 1367 ] doing WarmReset | phyid=%d | ind_bitmap=%d | reason=%d | CF_ACTIVE=%d | WarmReset Cause = 0x%x 
5030,,[ hca_HwComponentBbQca649x_debug.cpp : 243 ] ERROR: Received Null Pointer buffer argument in ANI Reg Dump. Returning without filling buffer with the dump 
5029,,[ hca_HwComponentBbQca649x_debug.cpp : 671 ] ERROR: Received Null Pointer buffer argument in DPD Reg Dump. Returning without filling buffer with the dump 
5028,,[ hca_HwComponentBbQca649x_debug.cpp : 172 ] ERROR: Received Null Pointer buffer argument in TPC Reg Dump. Returning without filling buffer with the dump 
5027,,[ hca_HwComponentBbQca649x_debug.cpp : 597 ] ERROR: Received Null Pointer buffer argument in RXIQ Reg Dump. Returning without filling buffer with the dump 
5026,,[ hca_HwComponentBbQca649x_debug.cpp : 442 ] ERROR: Received Null Pointer buffer argument in RXTD Reg Dump. Returning without filling buffer with the dump 
5025,,[ hca_HwComponentBbQca649x_debug.cpp : 524 ] ERROR: Received Null Pointer buffer argument in TXIQ Reg Dump. Returning without filling buffer with the dump 
5024,,[ hca_HwComponentBbQca649x_debug.cpp : 744 ] ERROR: Received Null Pointer buffer argument in PKDET Reg Dump. Returning without filling buffer with the dump 
5023,,[ hca_HwComponentBbQca649x_debug.cpp : 491 ] ERROR: Received Null Pointer buffer argument in RXDCO Reg Dump. Returning without filling buffer with the dump 
5022,,[ hca_HwComponentBbQca649x_debug.cpp : 332 ] ERROR: Received Null Pointer buffer argument in Radar Reg Dump. Returning without filling buffer with the dump 
5021,,[ hca_HwComponentBbQca649x_debug.cpp : 285 ] ERROR: Received Null Pointer buffer argument in NF Reg Dump. Returning without filling buffer with the dump 
5020,,[ hca_HwComponentBbQca649x_debug.cpp : 393 ] ERROR: Received Null Pointer buffer argument in SS Reg Dump. Returning without filling buffer with the dump 
5019,,[ hca_HwComponentBbQca649x_debug.cpp : 816 ] ERROR: Received Null Pointer arguments 
5018,I,[ hca_HwComponentBbQca649x_debug.cpp : 822 ] REG DUMP: Started Selective PHY REGs store to buffer: 0x%08x 
5017,i,[ hca_HwComponentBbQca649x_debug.cpp : 838 ]  length of the reg dump= %d 
5016,I,[ hca_HwComponentBbQca649x_debug.cpp : 129 ] ###### CW Tone RSSI: before start SSCAN regVal2 %x
 
5015,iiiI,[ hca_HwComponentBbQca649x_debug.cpp : 157 ] ###### FTM CW Tone RSSI: rssi %d rssiPri20 %d rssi_dbm_offset %d ,regVal2 %x
 
5014,iII,[ hca_HwComponentBbQca649x_debug.cpp : 83 ] PHYDBG: PHYID = %d DBG_CLK_EN = %x in WFAX_PCSS_M3_CTRL_L and CSR_PHYDBG_CLOCKON = %x in WFAX_PHYRF_PHYDBG_MODE_L 
 
5013,,[ hca_HwComponentBbQca649x_debug.cpp : 84 ] PHYDBG: Disabled DBG_CLK_EN in WFAX_PCSS_M3_CTRL_L and CSR_PHYDBG_CLOCKON in WFAX_PHYRF_PHYDBG_MODE_L 
 
5012,,[ hca_HwComponentBbQca649x_debug.cpp : 108 ] PHYDBG: PHYDBG is Fully Disabled!
 
5031,iii,[ hca_HwComponentBbQca649x_spectral.cpp : 387 ] SSCAN: BinIndices scanMode %d isChan165 %d, pCfg.ScanRptMode: %d 
5033,I,[ hca_HwComponentBbQca649x_phy.cpp : 230 ] EnableDssWarCFO: enable 0x%x
 
5032,I,[ hca_HwComponentBbQca649x_phy.cpp : 224 ] SetDssWarCFODeltaThreshold: threshold 0x%x
 
5038,i,[ phyDevLibCommon.c : 71 ] Error: Invalid PHY ID [=%d] 
5037,II,[ phyDevLibCommon.c : 129 ] Dumping PDMEM: [0x%08lx : 0x%08lx] 
5036,,[ phyDevLibCommon.c : 134 ] Dumping PDMEM Done 
5035,I,[ phyDevLibCommon.c : 92 ] Switch WCSS ENV to %s 
5034,,[ phyDevLibCommon.c : 46 ] register polling disabled 
5040,,[ phyIniAg.c : 411 ] Error: cannot commit NULL table! 
5039,iI,[ phyIniAg.c : 437 ] Note: table filtered out. table[%d].filter = %c 
5044,i,[ phy_dev_init.c : 176 ] ERROR: get parameter ID %d not yet implemented 
5043,I,[ phy_dev_init.c : 92 ] wlan base: 0x%x 
5042,i,[ phy_dev_init.c : 118 ] ERROR: set parameter ID %d not yet implemented 
5041,III,[ phy_dev_init.c : 102 ] CHIP: %s ENV: %s VER: %s 
5060,i,[ m3_init.c : 112 ] phyM3Boot: phyId = %d 
5059,i,[ m3_init.c : 127 ] Polling for boot completion ... [max_poll_count = %d] 
5058,,[ m3_init.c : 143 ] Warning: Max Poll Count Exceeded 
5057,,[ m3_init.c : 150 ] M3 is idle 
5056,,[ m3_init.c : 155 ] Alert: M3 has reported boot failure 
5055,,[ m3_init.c : 160 ] Error: Could not detect M3 Boot completion 
5054,,[ m3_init.c : 115 ] M3 is already Running. Asserting Reset 
5053,,[ m3_init.c : 126 ] M3 Reset de-asserted [Running @640MHz] 
5052,,[ m3_init.c : 308 ] Recipe Complete 
5051,,[ m3_init.c : 262 ] invalid phym3 binary, skip loading 
5050,,[ m3_init.c : 266 ] Loading PDMEM (may take few minutes)... 
5049,iIIII,[ m3_init.c : 273 ] seg%d: buf: %p dsize: %x msize: %x offset: %x 
5048,I,[ m3_init.c : 288 ] Loading PDMEM %s 
5047,,[ m3_init.c : 172 ] Using Direct IO!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!! 
5046,III,[ m3_init.c : 200 ] dma: virt: %p phys: 0x%08x size: %x 
5045,Iii,[ m3_init.c : 84 ] m3ctrl: %x boot done/fail: %d/%d 
5067,,[ m3Config.c : 104 ] PHYB+80M 
5066,I,[ m3Config.c : 118 ] Error: Invalid PHYID [=%u]! 
5065,ii,[ m3Config.c : 336 ] BRANCH = %d BUILD = %d 
5064,i,[ m3Config.c : 84 ] Fatal Error: Invalid PHYID[=%d] 
5063,,[ m3Config.c : 287 ] M3 DFS INI programmed 
5062,ii,[ m3Config.c : 126 ] phy %d full %d 
5061,iiiii,[ m3Config.c : 389 ] phySetTempCompensation PHYID[=%d], channel[=%d], temp[=%d], ppmOffset[=%d], delta_sfo[=%d] 
5069,i,[ phy_dev_setChainMask.c : 72 ] phySetChainMask: setting chain mask for phyId = %d ... 
5068,i,[ phy_dev_setChainMask.c : 137 ] phySetChainMask: chain mask for phyId = %d completed 
5071,i,[ phy_dev_setXbar.c : 62 ] phySetXbar: setting xbar for phyId = %d ... 
5070,i,[ phy_dev_setXbar.c : 99 ] phySetXbar: xbar for phyId = %d completed 
5074,iii,[ phyInitCfoCsr.c : 96 ] regVal=%d freqOffset=%d fcPri20=%d 
5073,iiiiii,[ phyInitCfoCsr.c : 228 ] phyMode=%d dpc_idx=%d centerFreqPri20=%d pri20Offset=%d fc_pri80=%d fc_sec80=%d 
5072,iii,[ phyInitCfoCsr.c : 252 ] fcPri20=%dMHz band_center_freq1=%d  band_center_freq2=%d 
5079,,[ phyRegIni.c : 86 ] DFS INI programmed 
5078,iii,[ phyRegIni.c : 224 ] phyRegIni::phyLoadIni: bandcode = %d (1:2G;0:5G), enableDisableBits1= %d, spectralShapingEn = %d
 
5077,i,[ phyRegIni.c : 262 ] Unsupportd phyMode=%d 
5076,IIIIIII,[ phyRegIni.c : 166 ] band: %u regular: %u lg: %u vlg: %u coex: %u dpd: %u dco: %u 
5075,i,[ phyRegIni.c : 55 ] Fatal Error! Invalid PHY ID[=%d]. 
5093,,[ phyReset.c : 1088 ] Enter phyChannelSwitch() 
5092,iIiiiiiii,[ phyReset.c : 1099 ] phyId %d/%x band %d bw %d phyMode %d homeCh %d mhz %d freq %d/%d 
5091,IIiiIII,[ phyReset.c : 1108 ] rxMask %x txMask %x conc %d dynPri %d iniMask %x skipMask %x pwrMask %x 
5090,,[ phyReset.c : 1114 ] <PHY BB CONFIG> 
5089,,[ phyReset.c : 1124 ] <RFA CONFIG> 
5088,,[ phyReset.c : 1145 ] <PCSS & M3 CONFIG> 
5087,,[ phyReset.c : 1157 ] phyChannelSwitch() complete 
5086,,[ phyReset.c : 931 ] Enter phyReset() 
5085,,[ phyReset.c : 983 ] <PHY BB CONFIG> 
5084,,[ phyReset.c : 993 ] <RFA CONFIG> 
5083,,[ phyReset.c : 1018 ] <PCSS & M3 CONFIG> 
5082,,[ phyReset.c : 1076 ] phyReset() complete 
5081,iIiiiiiii,[ phyReset.c : 947 ] phyId %d/%x band %d bw %d phyMode %d homeCh %d mhz %d freq %d/%d 
5080,IIiiIII,[ phyReset.c : 956 ] rxMask %x txMask %x conc %d dynPri %d iniMask %x skipMask %x pwrMask %x 
5094,,[ phySetRx11bDetThr.c : 70 ] Recipe Complete 
5098,,[ phySetRxfePerNrx.c : 413 ] OCL need at least two chains so unflag OCL! 
5097,I,[ phySetRxfePerNrx.c : 468 ] 160M/165M RSSI_THR1A_DB 0x%02x 
5096,iiiii,[ phySetRxfePerNrx.c : 509 ] BypassxLNA %d, OCL %d, selColumn,OCL_On,OCL_Off = [%d %d %d] 
5095,I,[ phySetRxfePerNrx.c : 161 ] numChains = %u 
5099,I,[ wsiconfig.c : 41 ] Invalid chain idx: %x ... 
5100,iiii,[ getCoefficients.c : 9 ] 30KB version: bwPerSegment %d numberOfSpurs %d spur1Offset %d spur2Offset %d 
5108,Iiiiiii,[ phySpurMitigation.c : 41 ] phyBase 0x%x chainIdx %d band_center_freq1 %d bwPerSegment %d numberOfSpurs %d spur1Offset %d spur2Offset %d 
5107,,[ phySpurMitigation.c : 103 ] Error: chainmask is 0! 
5106,,[ phySpurMitigation.c : 105 ] Using default coeff 
5105,iii,[ phySpurMitigation.c : 188 ] Enabling dynamic spur notch feature numberOfSpurs %d, spurLevel %d rssiThrDb %d 
5104,,[ phySpurMitigation.c : 199 ] Disabling dynamic spur notch feature 
5103,I,[ phySpurMitigation.c : 214 ] WFAX_RXTD_NOTCH_CNTL_1_L = 0x%lx 
5102,iiiiiiiii,[ phySpurMitigation.c : 55 ] notch_corr_dc_i %d, notch_corr_dc_q %d, notch_corr_spur1_i %d, notch_corr_spur1_q %d, notch_corr_spur2_i %d, notch_corr_spur2_q %d, notch_corr_agg_i %d, spur_delta_phase_spur1 %d, spur_delta_phase_spur2 %d 
5101,I,[ phySpurMitigation.c : 83 ] bwPerSegment is %u 
5109,,[ phyWarmRst.c : 72 ] WarmReset RECIPE COMPLETE 
5110,I,[ phyRssiDbToDbmOffset.c : 52 ] Offset: 0x%x 
5111,i,[ phySbsModeConfig.c : 43 ] isSBSMode=%d 
5112,I,[ phySetOCL.c : 86 ] OCL_CONFIG = 0x%x 
5114,ii,[ phyXoOtp.c : 177 ] phySetXoCdacin_qca649x %d, %d 
5113,ii,[ phyXoOtp.c : 289 ] phySetXoCdacout_qca649x %d, %d 
5115,I,[ phyPSMask.c : 32 ] Set powerSavingMask to 0x%x 
5117,,[ phySetRxDeaf.c : 55 ] rxDeaf done! 
5116,,[ phySetRxDeaf.c : 75 ] rxDeaf cleared! 
5119,i,[ phyRtt.c : 42 ] RTT per busrt ini programming phyId=%d 
5118,i,[ phyRtt.c : 66 ] Restoring RTT per burst ini programed phyId=%d 
5123,i,[ phyCfrCirCap.c : 42 ] Enable CFR ini programming phyId=%d 
5122,i,[ phyCfrCirCap.c : 54 ] Restoring Enable CFR ini programed phyId=%d 
5121,i,[ phyCfrCirCap.c : 66 ] Enable CFR ini programming phyId=%d 
5120,i,[ phyCfrCirCap.c : 78 ] Restoring Enable CFR ini programed phyId=%d 
5125,,[ phyRetention.c : 49 ] Enter retention save 
5124,,[ phyRetention.c : 58 ] Enter retention restore 
5162,iiiiii,[ phyrf_ani.c : 102 ] NFREAD%d PHYID=%d NFInDBr=%d NFToDBm=%d maxNumChain=%d maxNFInDBm=%d 
 
5161,iiii,[ phyrf_ani.c : 145 ] ANI_EDCCA_PHYID%d CHAIN%d NFBDF=%d NFRUNTIME=%d 
5160,iiiiii,[ phyrf_ani.c : 152 ] ANI_EDCCA_PHYID%d NFBDF=%d NFRUNTIME=%d DELTA=%d txChainMask=%d rxChainMask=%d 
5159,i,[ phyrf_ani.c : 158 ] ANI_API_PHYID%d API: ANI CONFIGURE 
 
5158,iiii,[ phyrf_ani.c : 226 ] ANI_DUMP_PHYID%d DL_OFDM %d DL_MIN %d DL_MAX %d 
 
5157,iiiii,[ phyrf_ani.c : 223 ] ANI_DUMP_PHYID%d DL_OFDM %d DL_CCK %d DL_MIN %d DL_MAX %d 
 
5156,i,[ phyrf_ani.c : 355 ] ANI_LOG PHY%d ANI_RESET 
 
5155,i,[ phyrf_ani.c : 357 ] ANI_LOG PHY%d ANI_RESET 
 
5154,iiiii,[ phyrf_ani.c : 417 ] ANI_DUMP_PHYID%d ofdmPhyErrCnt %d lsigPhyErrCnt %d cckPhyErrCnt %d sizing1 %d 
 
5153,iiii,[ phyrf_ani.c : 423 ] ANI_LOW_POWER_CNTR_PHYID%d rxClearCnt %d ccaCntr0 %d time %d 
 
5152,iii,[ phyrf_ani.c : 424 ] ANI_DUMP_PHYID%d CYCLE_CNT %d time %d 
 
5151,iiiiii,[ phyrf_ani.c : 462 ] ANI_LOW_POWER_CNTR_PHYID%d cycleCnt %d txFrameCnt %d rxframecnt %d rxClearCnt %d time %d 
 
5150,iii,[ phyrf_ani.c : 464 ] ANI_EDCCA_PHYID%d raw_nfdelta=%d pedccaParam->curr_delta=%d 
 
5149,iiiiiiii,[ phyrf_ani.c : 516 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL -%d 
 
5148,iiiiiiii,[ phyrf_ani.c : 518 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL %d 
 
5147,iiiiiiii,[ phyrf_ani.c : 520 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL -%d 
 
5146,iiiiiiii,[ phyrf_ani.c : 522 ] ANI_LOG PHYB POLL %dms LISTEN %dms: OFDM %d LSIG %d CCK %d SIZ1 %d M %d OFDM_DL %d 
 
5145,iiiiiii,[ phyrf_ani.c : 532 ] ANI_LOG PHYA1 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL -%d
 
5144,iiiiiii,[ phyrf_ani.c : 534 ] ANI_LOG PHYA1 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL %d
 
5143,iiiiiii,[ phyrf_ani.c : 539 ] ANI_LOG PHYA0 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL -%d
 
5142,iiiiiii,[ phyrf_ani.c : 541 ] ANI_LOG PHYA0 POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL %d
 
5141,iiiiiii,[ phyrf_ani.c : 547 ] ANI_LOG PHYA POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL -%d
 
5140,iiiiiii,[ phyrf_ani.c : 549 ] ANI_LOG PHYA POLL %dms LISTEN %dms: OFDM %d LSIG %d SIZ1 %d M %d OFDM_DL %d
 
5139,ii,[ phyrf_ani.c : 558 ] ANI_DUMP_PHYID%d ERROR RATE < %d PERCENT 
 
5138,ii,[ phyrf_ani.c : 573 ] ANI_DUMP_PHYID%d ERROR RATE > %d PERCENT 
 
5137,i,[ phyrf_ani.c : 595 ] ANI_DUMP_PHYID%d CONSECUTIVE ERROR, INCREMENTING DESENSE LEVEL 
 
5136,i,[ phyrf_ani.c : 613 ] ANI_DUMP_PHYID%d CONSECUTIVE LESS ERROR, DECREMENTING DESENSE LEVEL 
 
5135,ii,[ phyrf_ani.c : 650 ] ANI_DUMP PHYID%d ramp_up_time %dms
 
5134,ii,[ phyrf_ani.c : 666 ] ANI_DUMP PHYID%d ramp_down_time %dms
 
5133,ii,[ phyrf_ani.c : 749 ] ANI_DUMP_PHYID%d ANI API ENABLED %d 
 
5132,ii,[ phyrf_ani.c : 775 ] ANI_DUMP_PHYID%d ENABLED %d 
 
5131,ii,[ phyrf_ani.c : 788 ] ANI_DUMP_PHYID%d DISABLED %d 
 
5130,ii,[ phyrf_ani.c : 878 ] ANI_DUMP_PHYID%d GET ANI STATE %d 
 
5129,ii,[ phyrf_ani.c : 872 ] ANI_LOG PHYID%d SetAniListenPeriod %d 
 
5128,ii,[ phyrf_ani.c : 865 ] ANI_LOG PHYID%d SetAniPollPeriod %d 
 
5127,i,[ phyrf_ani.c : 365 ] ANI_DUMP_PHYID%d READ AND CACHE VREG VALUES 
 
5126,i,[ phyrf_ani.c : 256 ] ANI_DUMP_PHYID%d RESTORE DL 
 
5213,,[ phyrf_bdf.c : 5011 ] phyrf_Set_BDFVersion: Feature support unavailable 
5212,,[ phyrf_bdf.c : 4964 ] phyrf_Set_BDFVersion: Feature support unavailable 
5211,iiiiiii,[ phyrf_bdf.c : 5194 ] iwconfig_logs:: REG TPC: bHomeChan=%d regTxPower=%d twiceAntennaReduction=%d twiceAntennaGain=%d twiceLargestAntenna=%d maxRegAllowedPower=%d power_type_6ghz = %d 
5210,iii,[ phyrf_bdf.c : 2505 ] phyrf_bdf_ActivateSARLimitSet  enable = %d, Index = %d, chainNum = %d
  
5209,ii,[ phyrf_bdf.c : 1194 ] DumpTpcPerPacket: Get Rate target pwr TPC pwr SAR ch0=%d, ch1=%d
 
5208,iiiiii,[ phyrf_bdf.c : 5258 ] iwconfig_logs:: TPC WMI:: Compute6GRegpwr: bHomeChan %d Eirp %d psd %d chan->mhz %d chan->band_center_freq1 %d chan->band_center_freq2 %d 
5207,ii,[ phyrf_bdf.c : 5261 ] iwconfig_logs:: TPC WMI:: power Compute: tx_pwr[%d] : %d 
5206,i,[ phyrf_bdf.c : 5263 ] iwconfig_logs:: TPC WMI:: power Compute: antGainOffset6GReg %d 
5205,ii,[ phyrf_bdf.c : 5284 ] iwconfig_logs:: REG TPC:: power Compute: final_psd_power=%d eirp_power=%d 
5204,i,[ phyrf_bdf.c : 5291 ] iwconfig_logs:: TPC WMI:: power Compute: Final Reg Tx pwr %d 
5203,,[ phyrf_bdf.c : 2890 ] VK_TPC!!! isFbin is TRUE 
5202,i,[ phyrf_bdf.c : 2904 ] VK_TPC!!! pTpcCalFreq=%d 
5201,i,[ phyrf_bdf.c : 2912 ] VK_TPC!!! chans5G=%d 
5200,iii,[ phyrf_bdf.c : 5662 ] phyrf_bdf_GetDisableCSDFlag powerMode %d, is2GHz %d, isG %d 
5199,iiii,[ phyrf_bdf.c : 1651 ] DumpTpcPerPacket: rtIdx = %d numStreams %d numChains %d rateCode %d
 
5198,iii,[ phyrf_bdf.c : 1773 ] DumpTpcPerPacket: Get Rate regulatory pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
5197,iii,[ phyrf_bdf.c : 1817 ] DumpTpcPerPacket: Get Rate regulatory pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
5196,iiii,[ phyrf_bdf.c : 1831 ] DumpTpcPerPacket: Get Rate ioctl pwr TPC pwr = ch0=%d ch1=%d phy: %d ioctl power %d
 
5195,iii,[ phyrf_bdf.c : 1867 ] DumpTpcPerPacket: Get Rate regulatory pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
5194,iii,[ phyrf_bdf.c : 1711 ] DumpTpcPerPacket: Get Rate target pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
5193,iii,[ phyrf_bdf.c : 1721 ] DumpTpcPerPacket: Get Rate CTL pwr TPC pwr = ch0=%d ch1=%d phy: %d
 
5192,i,[ phyrf_bdf.c : 5449 ] DumpTpcPerPacket: maxRegAllowedPower:%d
 
5191,i,[ phyrf_bdf.c : 5451 ] DumpTpcPerPacket: maxRegAllowedPower:%d
 
5190,i,[ phyrf_bdf.c : 5462 ] DumpTpcPerPacket: maxRegAllowedPower:%d
 
5189,iii,[ phyrf_bdf.c : 5492 ] DumpTpcPerPacket: Get max tx pwr from regulatory Info Hal-phy call BW:%d , Max_tx_pwr: %d, tx_power:%d 
 
5188,iii,[ phyrf_bdf.c : 5503 ] DumpTpcPerPacket: Get max tx pwr from regulatory Info Hal-phy call BW:%d , Max_tx_pwr: %d, tx_power:%d 
 
5187,iii,[ phyrf_bdf.c : 5514 ] DumpTpcPerPacket: Get max tx pwr from regulatory Info Hal-phy call BW:%d , Max_tx_pwr: %d, tx_power:%d 
 
5186,iii,[ phyrf_bdf.c : 5525 ] DumpTpcPerPacket: Get max tx pwr from regulatory Info Hal-phy call BW:%d , Max_tx_pwr: %d, tx_power:%d 
 
5185,iiiii,[ phyrf_bdf.c : 5556 ] DumpTpcPerPacket: Get max tx pwr from regulatory Info Hal-phy call %d , isPSD:%d, Max_tx_pwr: %d, curr_BW: %d, adj_BW:%d
 
5184,,[ phyrf_bdf.c : 2105 ] phyrf_bdf_GetTpcMaxTxPwr :: Invalid Channel Frequency 
5183,iiIi,[ phyrf_bdf.c : 2126 ] GetTpcMaxTxPwr: phyId %d txCM %d rcFlags 0x%x tpc_max_tx_power %d 
5182,i,[ phyrf_bdf.c : 2413 ] Invalid SAR Version set : %d  
5181,i,[ phyrf_bdf.c : 2418 ] Invalid SAR Index set  Index: %d  
5180,i,[ phyrf_bdf.c : 2424 ] Invalid SAR Index Index: %d  
5179,i,[ phyrf_bdf.c : 2432 ] Invalid SAR Index set Index: %d  
5178,i,[ phyrf_bdf.c : 2438 ] Invalid SAR Index Index: %d  
5177,I,[ phyrf_bdf.c : 1008 ] phyrf_bdf_SetCtlRegDomain g_6g_ctl = %x
  
5176,iiii,[ phyrf_bdf.c : 4346 ] phyrf_bdf_SetRegulatoryDomain_Subband mhz %d, channel %d, ctlSubbandFlag %d ctrlFlag %d 
 
5175,iiii,[ phyrf_bdf.c : 4349 ] phyrf_bdf_SetRegulatoryDomain_Subband Disable sub band CTL by cmd!!! mhz %d, channel %d ctlSubbandFlag %d ctrlFlag %d 
 
5174,,[ phyrf_bdf.c : 4370 ] phyrf_bdf_SetRegulatoryDomain_5G_Subband channel in not in all subband 
 
5173,ii,[ phyrf_bdf.c : 4382 ] phyrf_bdf_SetRegulatoryDomain_Subband cfgCtl[0] %d, phy %d 
 
5172,iiiiiiii,[ phyrf_bdf.c : 4398 ] phyrf_bdf_SetRegulatoryDomain_Subband pwrType6G %d, g_phyrf_power_type6G %d, devRole6G %d, isSap%d, phyId %d, homeChanflag %d, foundHomeIdx %d, freq6G %d
 
5171,iIIi,[ phyrf_bdf.c : 4485 ] phyrf_bdf_SetRegulatoryDomain_Subband isSap %d, cfgCtl_6G 0x%x g_6g_ctl 0x%x, phy %d 
 
5170,ii,[ phyrf_bdf.c : 5143 ] iwconfig_logs: Home->Scan->Home:: Restore reg pwr pTpcConfig->maxRegAllowedPower[%d] = %d
 
5169,i,[ phyrf_bdf.c : 5146 ] iwconfig_logs: Home->Scan->Home:: Restore  %d
 
5168,,[ phyrf_bdf.c : 5330 ] DumpTpcPerPacket: Set regulatory Info Hal-phy call 
 
5167,ii,[ phyrf_bdf.c : 5341 ] iwconfig_logs:: Store Home channel maxRegAllowedPower6GEIRP in g_6G_chan_txpower[%d] = %d
 
5166,i,[ phyrf_bdf.c : 5350 ] iwconfig_logs:: Store Home channel g_home_max_reg_power_6G %d
 
5165,iiI,[ phyrf_bdf.c : 5382 ] phyrf_bdf_setRegPwrInfo  1 => g_tpc_change[%d][%d] = [%08x] 
5164,iiI,[ phyrf_bdf.c : 5387 ] phyrf_bdf_setRegPwrInfo  2 => g_tpc_change[%d][%d] = [%08x] 
5163,i,[ phyrf_bdf.c : 5332 ] DumpTpcPerPacket phyrf_bdf_setRegPwrInfo tx_power = %d 
 
5222,IIIIIII,[ phyrf_cal.c : 767 ] phyid %u, mhz %4u, f1 %4u, f2 %4u, phyMode %2u, calType %2u, calResult %3u 
5221,i,[ phyrf_cal.c : 787 ] WAL_CHAN_CHANGE PAPRD 10ms timer expired for channel %d 
5220,iiiiii,[ phyrf_cal.c : 822 ] WAL_CHAN_CHANGE PAPRD RunCal: bHomeChan %d channel %d calChannel %d timerActive %d dpd cal State %d valid %d 
5219,IIi,[ phyrf_cal.c : 859 ] WAL_CHAN_CHANGE DPDCAL timer stopped for phyId %u at time(ms) : %u, channel %d 
5218,IIii,[ phyrf_cal.c : 879 ] WAL_CHAN_CHANGE DPDCAL timer started for phyId %u at time(ms) : %u cal channel %d, tot time by Timer API %d 
5217,i,[ phyrf_cal.c : 728 ] phyrf_cal_PmLockDispatch : lock %d 
5216,,[ phyrf_cal.c : 731 ] phyrf_cal_PmLockDispatch : LOCKED 
5215,,[ phyrf_cal.c : 735 ] phyrf_cal_PmLockDispatch : UNLOCKED 
5214,i,[ phyrf_cal.c : 689 ] in phyrf_cal_RunDPDCalibration : %d
 
5237,IIII,[ phyrf_cal_sm.c : 900 ] CC::: inside cal_SM_Main, 0x%x, (pHandle=0x%x, smInput=0x%x, pCalSmTable=0x%x) 
5236,iIII,[ phyrf_cal_sm.c : 980 ] CAL SM::: cal type idx=%d, ptrStandalone=%x, pIn=%x, pOut=%x  
5235,Iii,[ phyrf_cal_sm.c : 564 ] CC::: generateCalSmTable=0x%x, callingContext=%d, curCalTypeIdx=%d 
5234,iiiiiIIi,[ phyrf_cal_sm.c : 611 ] CALSM: globalCallingContext[%d]=%d, mhz=%d, freq1=%d, freq2=%d, phy_mode=%3d, txCM=%2X, Total_cal_time=%d us 
5233,ii,[ phyrf_cal_sm.c : 613 ] Summary starts: calibration with globalCallingContext[%d]=%d 
5232,iiiii,[ phyrf_cal_sm.c : 629 ] :::::::: %d	%d	%d	%d	%d 
5231,iI,[ phyrf_cal_sm.c : 677 ] CAL SM::: genCalTable calType=%d hwCalMask 0x%x 
5230,iii,[ phyrf_cal_sm.c : 719 ] ADC=%d: calType=%d, ptr_phyrf_cal_sm_table->calTypeVarianceId=%d 
5229,iii,[ phyrf_cal_sm.c : 730 ] TIADC_80=%d: calType=%d, ptr_phyrf_cal_sm_table->calTypeVarianceId=%d 
5228,iii,[ phyrf_cal_sm.c : 1074 ] CAL SM::: Phy mode=%d, IsTrue160supported=%d, bwcode=%d 
5227,Iiii,[ phyrf_cal_sm.c : 176 ] CALSM: %x,  callingContext=%d, masterCalDbExist()=%d, isSBS=%d 
5226,iIIiii,[ phyrf_cal_sm.c : 358 ] Previous: PhyId=%d, rCM=%x, tCM=%x, TalIdx=%d, PwrMask=%d, RFmode=%d 
5225,iiiiii,[ phyrf_cal_sm.c : 458 ] :::: doCalFlag = %d, doCalFlagCombIQ = %d, doCalFlagRxDCO = %d, preProfileExcludeScan = %d, txloCorrupted = %d, currentRFmode = %d 
5224,iiii,[ phyrf_cal_sm.c : 183 ] CALSM:  final 	calDBEnableSetting=%d, 	final CalTimeOutSetting = %d, 	final PersistentEnable = %d, ColdBootDfsCalEnable=%d 
5223,iIIiii,[ phyrf_cal_sm.c : 356 ] current : PhyId=%d, rCM=%x, tCM=%x, TalIdx=%d, PwrMask=%d, RFmode=%d 
5280,iiiiii,[ phyrf_caldb.c : 4556 ] CheckDpdMemForFCS() : maxChainIdx %d rfChainMask %d cur_tbl_idx %d subModeIndxFor80p80 %d phyId %d, chainIdx %d  
5279,IIii,[ phyrf_caldb.c : 4561 ]  previous hw tracking table %x , curremt tracking table %x tableValid %d CALDB_STATUS_VALID %d 
5278,I,[ phyrf_caldb.c : 4573 ] CB::: CheckDpdMemForFCS() : %x,   
5277,iiiiiIii,[ phyrf_caldb.c : 5926 ] TEMPSEN:::   phyId = %d, chainIdx = %d, CBNormalizedOffset=%d, CBTempInC=%d, LastTempInC=%d, getTime=%u, curTempID=%d, CBtempeID=%d 
5276,iiii,[ phyrf_caldb.c : 7108 ]  chain %d MemDPDValidateCurChSwForFCS %d channel %d rssult %d 
5275,iiiiii,[ phyrf_caldb.c : 2484 ] TEMPSEN:::  phyId=%d, calType=%d rfChainMask = %d, chainIdx=%d, globalCallingContext=%d, UseAltTableAllowed=%d  
5274,I,[ phyrf_caldb.c : 4616 ] CB::: IS_FTM_MODE() : %x, DISALBE_RESTORE_FOR_FTM is defined 
5273,i,[ phyrf_caldb.c : 6604 ] dualband_enable_phyb = %d 
 
5272,i,[ phyrf_caldb.c : 1362 ] dual_lo_needed = %d 
 
5271,IIIII,[ phyrf_caldb.c : 6583 ] CALDB_DEBUG: Frequency table dump  Start Freq %u | End freq %u | Sequential Index %u | Master Index %u | TPC mapped freq %u 
5270,,[ phyrf_caldb.c : 275 ] Secondary effrfchnmask: Invalid chainmask config!!! 
5269,,[ phyrf_caldb.c : 313 ] Listen effrfchnmask-  Invalid chainmask config!!! 
5268,i,[ phyrf_caldb.c : 1885 ] ERROR: invalid band of %d
 
5267,iiiiii,[ phyrf_caldb.c : 2046 ] :::: frequency=%d, bandw:%d calTypeIdx=%d,  *mapToCalGroupIdx=%d, *rfsub =%d, *sequentialSubBandIdx=%d 
5266,II,[ phyrf_caldb.c : 3603 ] CC::: rxiqGainMapStart: %x, rxiqDpdStart: %x 
5265,III,[ phyrf_caldb.c : 3548 ] CC::: rxiqStart: %x, txiqStart: %x, txloStart: %x 
5264,iiIi,[ phyrf_caldb.c : 3729 ] dpdStart address for cur_tbl_idx [%d] chainIdx %d is 0x%x channel %d 
5263,,[ phyrf_caldb.c : 3307 ] error: phyId not matched to system supported number of PHYs. 
5262,I,[ phyrf_caldb.c : 7322 ] Error: %s Invalid halphy_update_caldb_cal_channel DPD table address 
5261,iiii,[ phyrf_caldb.c : 7403 ]  caldb_DpdNonMemory is NULL :  get calTemp chain index %d table index %d freq %d cur_tbl_idx %d 
5260,iii,[ phyrf_caldb.c : 7409 ]  get paprdType %d calTemp %d caldb temperatureInC %d 
5259,iiii,[ phyrf_caldb.c : 7414 ]  caldb_DpdMemory is NULL :  get calTemp chain index %d table index %d freq %d cur_tbl_idx %d 
5258,iiiiii,[ phyrf_caldb.c : 7418 ]  get paprdType %d calTemp %d chain index %d freq %d cur_tbl_idx %d table_index %d 
5257,iii,[ phyrf_caldb.c : 6994 ]  halphy_get_caldb_dpd_mem_calValidBit  Cal Valid bits %d chain index %d freq %d 
5256,ii,[ phyrf_caldb.c : 6998 ]  cal_context is NULL : halphy_get_caldb_dpd_mem_calValidBit  chain index %d freq %d 
5255,iii,[ phyrf_caldb.c : 6864 ]  get  Cal attemps %d chain index %d freq %d 
5254,iii,[ phyrf_caldb.c : 6739 ]  invalid  Cal attemps %d chain index %d freq %d 
5253,I,[ phyrf_caldb.c : 7291 ] Error: %s Invalid halphy_update_caldb_cal_channel DPD table address 
5252,iiii,[ phyrf_caldb.c : 7356 ]  caldb_DpdNonMemory is NULL :  upadate calTemp chain index %d table index %d freq %d cur_tbl_idx %d 
5251,iii,[ phyrf_caldb.c : 7362 ]  get paprdType %d calTemp %d caldb temperatureInC %d 
5250,iiii,[ phyrf_caldb.c : 7367 ]  caldb_DpdMemory is NULL :  upadate calTemp chain index %d table index %d freq %d cur_tbl_idx %d 
5249,iiiiii,[ phyrf_caldb.c : 7371 ]  upadate paprdType %d calTemp %d chain index %d freq %d cur_tbl_idx %d table_index %d 
5248,iii,[ phyrf_caldb.c : 6709 ]  update  Cal attemps %d chain index %d freq %d 
5247,iiI,[ phyrf_caldb.c : 6930 ]  Conetxt is NULL :  upadate  chain index %d freq %d cur_tbl_idx %s 
5246,iii,[ phyrf_caldb.c : 6770 ]  update  Cal attemps %d chain index %d freq %d 
5245,,[ phyrf_caldb.c : 2292 ] error: phyId not matched to system supported number of PHYs. 
5244,iii,[ phyrf_caldb.c : 1504 ] Wow mode status operation : %d wow_mode_status (0: master calDB can be access) %d, wow entry cnt=%d  
5243,,[ phyrf_caldb.c : 5395 ] ERROR: CalDB checksum failure 
5242,,[ phyrf_caldb.c : 5203 ] error: phyId not matched to system supported number of PHYs. 
5241,ii,[ phyrf_caldb.c : 7447 ] chain%d minimum temperature is: %d 
5240,I,[ phyrf_caldb.c : 6569 ] eDPD ptr %p 
5239,iiiii,[ phyrf_caldb.c : 461 ] Search: rfsub=%d, cacheMasterInfo[shortenPhyId=%d][curRow=%d].masterCalDbRfSubIdx  = %d, cacheMasterInfo[shortenPhyId][curRow].masterCalDbGroupIndx = %d
 
5238,,[ phyrf_caldb.c : 3422 ] error: phyId not matched to system supported number of PHYs. 
5282,i,[ phyrf_cbc.c : 866 ] cbc: ENABLE_CHANNEL_LIST_IN_BDF not defined: repeatLimit=%d 
5281,i,[ phyrf_cbc.c : 879 ] MINI_CBC skip %d 
5285,i,[ phyrf_debug.c : 577 ] HALPHY DUMP: WIFITOOL issued with subcommand ID %d 
5284,i,[ phyrf_debug.c : 594 ] Unsupported, halphy debug func is null %d 
5283,i,[ phyrf_debug.c : 588 ] Invalid or Unsupported halphy debug sub command: %d 
5296,ii,[ phyrf_debug_prdd.c : 559 ] PRDD - Invalid number of args (should be %d..%d) 
5295,i,[ phyrf_debug_prdd.c : 730 ] PRDD - Invalid PRDD command (should be 0..%d) 
5294,,[ phyrf_debug_prdd.c : 735 ] PRDD - Invalid number of args in PRDD command (should be >= 2 args) 
5293,I,[ phyrf_debug_prdd.c : 742 ] PRDD - Invalid phyId - should be 0..%lu 
5292,,[ phyrf_debug_prdd.c : 701 ] PRDD - Not enough memory to support fixed mode 
5291,II,[ phyrf_debug_prdd.c : 454 ] PRDD - No report for phy%u at %u MHz 
5290,iii,[ phyrf_debug_prdd.c : 311 ] PRDD - %d MHz, phy%d, 1swT %d ms 
5289,iI,[ phyrf_debug_prdd.c : 400 ] PRDD -   module%d 0x%08lx 
5288,,[ phyrf_debug_prdd.c : 469 ] No PRDD report 
5287,i,[ phyrf_debug_prdd.c : 121 ] PRDD - Could not find idx for freq %d 
5286,ii,[ phyrf_debug_prdd.c : 964 ] PRDD - channel %d is not found in phy%d 
5472,,[ phyrf_debug_cmd.c : 862 ] WIFITOOL: PHYID is not active 
 
5471,iiii,[ phyrf_debug_cmd.c : 904 ] ANI_LOG PHYID%d ani_dl_min %d, ani_dl_max %d, error_threshold %d 
5470,ii,[ phyrf_debug_cmd.c : 916 ] ANI_LOG PHYID%d ani_ramp_down %d 
 
5469,i,[ phyrf_debug_cmd.c : 2058 ] BT_CLOCK_ENABLE: %d 
5468,iii,[ phyrf_debug_cmd.c : 2767 ] MMHostCmdCTLSetting::num_args=%d, args[%d]=%d 
5467,,[ phyrf_debug_cmd.c : 2774 ] CTL_SETTING::6G CTL POWER MODE::Invalid test arguments 
5466,iiI,[ phyrf_debug_cmd.c : 2785 ] phyId=%d, ctl6g_pwermode=%d, debugFlag0=0x%x 
5465,,[ phyrf_debug_cmd.c : 2550 ] Coldboot Calibration Feature Not Supported 
5464,,[ phyrf_debug_cmd.c : 2555 ] Coldboot Calibration Feature: Invalid test arguments 
5463,i,[ phyrf_debug_cmd.c : 1628 ] WIFITOOL: PHYID %d is not active 
 
5462,ii,[ phyrf_debug_cmd.c : 1633 ] EnableDssWarCFO: enable=%d FOR PHYID %d 
 
5461,iiII,[ phyrf_debug_cmd.c : 2121 ] CHAINMASKOVERRIDE %d - phy[%d]: txChMask 0x%x; rxChMask 0x%x 
5460,,[ phyrf_debug_cmd.c : 538 ] CTL_DISABLE: Invalid test arguments 
5459,,[ phyrf_debug_cmd.c : 556 ] CTL_DISABLE: Disabling CTL power limits! 
5458,,[ phyrf_debug_cmd.c : 561 ] CTL_DISABLE: Enabling back CTL power limits! 
5457,,[ phyrf_debug_cmd.c : 544 ] CTL_DISABLE: Invalid phyId 
5456,,[ phyrf_debug_cmd.c : 2277 ] DFS_ENABLE: Invalid test arguments  
5455,,[ phyrf_debug_cmd.c : 2283 ] DFS_ENABLE: Invalid phyId 
5454,,[ phyrf_debug_cmd.c : 2493 ] PHYRF_DEBUG_MM_HOST_CMD_SET_DPD_EDPD_ENABLE Invalid Command 
5453,Ii,[ phyrf_debug_cmd.c : 2500 ] PHYRF_DEBUG_MM_HOST_CMD_SET_DPD_EDPD_ENABLE: Invalid PHY ID = %u, phyrf_init_GetNumPhys()=%d 
5452,i,[ phyrf_debug_cmd.c : 2508 ] PHYRF_DEBUG_MM_HOST_CMD_SET_DPD_EDPD_ENABLE: Invalid pHandle for phyId=%d 
5451,iI,[ phyrf_debug_cmd.c : 2515 ] Set g_halphy_dpd_enable[%d] =0x%x
 
5450,,[ phyrf_debug_cmd.c : 1851 ] DDSS: PHYID 0 is not active 
 
5449,i,[ phyrf_debug_cmd.c : 1858 ] DDSS: ENABLE/DISABLE all DDSS: %d 
5448,i,[ phyrf_debug_cmd.c : 1867 ] DDSS: ENABLE/DISABLE CFO DSS: g_cfodss_enable=%d 
5447,i,[ phyrf_debug_cmd.c : 1871 ] DDSS: ENABLE/DISABLE CU DSS: g_cudss_enable=%d 
5446,i,[ phyrf_debug_cmd.c : 1875 ] CUDSS: ENABLE CU DSS: g_cudss_metric=%d 
5445,,[ phyrf_debug_cmd.c : 779 ] DO_NFCAL_ACTION Invalid Command 
5444,I,[ phyrf_debug_cmd.c : 786 ] DO_NFCAL_ACTION: Invalid PHY ID = %u 
5443,II,[ phyrf_debug_cmd.c : 805 ] DO_NFCAL_ACTION: Setting NF home channl IterCount to %u for phyId = %u 
5442,II,[ phyrf_debug_cmd.c : 812 ] DO_NFCAL_ACTION: Setting pResetStruct->nfPeriodicCalControl to %u for phyId %u 
5441,II,[ phyrf_debug_cmd.c : 819 ] DO_NFCAL_ACTION: Setting pResetStruct->nfPeriodicCalWithPhyOffPhyOnControl to %u for phyId %u 
5440,II,[ phyrf_debug_cmd.c : 826 ] DO_NFCAL_ACTION: Setting pResetStruct->nfResetCalControl to %u for phyId %u 
5439,II,[ phyrf_debug_cmd.c : 836 ] DO_NFCAL_ACTION: Triggering NFCAL with flags %x for phyId %u 
5438,i,[ phyrf_debug_cmd.c : 1395 ] DSS: WIFITOOL ISSUED TO ENABLE/DISABLE DSS %d
 
5437,i,[ phyrf_debug_cmd.c : 1406 ] DSS: G_SYNTH_CONTROL_FTM=%d FOR PHYID 0 
 
5436,i,[ phyrf_debug_cmd.c : 1418 ] DSS: G_SYNTH_CONTROL=%d FOR PHYID 0 
 
5435,i,[ phyrf_debug_cmd.c : 1608 ] WIFITOOL: PHYID %d is not active 
 
5434,ii,[ phyrf_debug_cmd.c : 1613 ] SetDssWarCFODeltaThreshold: cfo_threshold=%d FOR PHYID %d 
 
5433,i,[ phyrf_debug_cmd.c : 2590 ] DUMP_TPC_GLUT_WAKEUP_SLEEP: WIFITOOL ISSUED TO ENABLE TPC GLUT DUMP %d
 
5432,,[ phyrf_debug_cmd.c : 2594 ] DUMP_TPC_GLUT_WAKEUP_SLEEP: wifitool : Invalid test arguments 
5431,i,[ phyrf_debug_cmd.c : 2599 ] DUMP_TPC_GLUT_WAKEUP_SLEEP: WIFITOOL ISSUED TO DISABLE TPC GLUT DUMP %d
 
5430,i,[ phyrf_debug_cmd.c : 2573 ] DUMP_TPC_REGS_ENABLE: WIFITOOL ISSUED TO ENABLE TPC REG DUMP %d
 
5429,,[ phyrf_debug_cmd.c : 2577 ] DUMP_TPC_REGS_ENABLE: wifitool : Invalid test arguments 
5428,i,[ phyrf_debug_cmd.c : 2740 ] ENABLE_CHAN_CHANGE_BREAKDOWN: WIFITOOL ISSUED TO ENABLE CHAN CHANGE BREAKDOWN %d
 
5427,,[ phyrf_debug_cmd.c : 2744 ] ENABLE_CHAN_CHANGE_BREAKDOWN: wifitool : Invalid test arguments 
5426,i,[ phyrf_debug_cmd.c : 2749 ] ENABLE_CHAN_CHANGE_BREAKDOWN: WIFITOOL ISSUED TO DISABLE CHAN CHANGE BREAKDOWN %d
 
5425,I,[ phyrf_debug_cmd.c : 970 ] pResetStruct->enable_ldocal_otp = %u 
5424,i,[ phyrf_debug_cmd.c : 1057 ] PAPRD: Invalid PHY ID = %d 
5423,ii,[ phyrf_debug_cmd.c : 1061 ] PAPRD: Phy ID %d | Enable for MM = %d 
5422,ii,[ phyrf_debug_cmd.c : 1044 ] ANI_LOG PHYID%d error_threshold %d 
 
5421,ii,[ phyrf_debug_cmd.c : 1775 ] DSS: WIFITOOL ISSUED TO FORCED SYNTH phyId %d, Synth %d
 
5420,i,[ phyrf_debug_cmd.c : 1778 ] FORCED_SYNTH: Invalid PHY ID = %d 
5419,ii,[ phyrf_debug_cmd.c : 1794 ] FORCED SYNTH: G_SYNTH_CONTROL=%d FOR PHYID %d 
 
5418,ii,[ phyrf_debug_cmd.c : 1799 ] FORCED SYNTH: G_SYNTH_CONTROL=%d FOR PHYID %d 
 
5417,,[ phyrf_debug_cmd.c : 2625 ] GET BOARD CAL DETAILS : wifitool : Command unsupported !  
5416,II,[ phyrf_debug_cmd.c : 1207 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( Internal Error ) 
5415,II,[ phyrf_debug_cmd.c : 1211 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( No Entry ) 
5414,II,[ phyrf_debug_cmd.c : 1215 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( No Memory) 
5413,III,[ phyrf_debug_cmd.c : 1219 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( Success ), chanGradeInfoCount %u 
5412,IIIi,[ phyrf_debug_cmd.c : 1228 ] %u. Freq %u, BW %u, ChanPerfMetric %d 
5411,II,[ phyrf_debug_cmd.c : 1233 ] Unit Test ID %u :: phyrf_bdf_GetAllChanGradeInfo returns A_STATUS :: %u ( Unknown Error ) 
5410,i,[ phyrf_debug_cmd.c : 1154 ] PCSS: Invalid PHY ID = %d 
5409,iiii,[ phyrf_debug_cmd.c : 1141 ] PDL Version : %d.%d - RDL Version : %d.%d 
5408,,[ phyrf_debug_cmd.c : 1245 ] GetSignalLevel : Invalid test arguments  
5407,,[ phyrf_debug_cmd.c : 1261 ] GetSignalLevel : pHandle not found 
5406,IIIII,[ phyrf_debug_cmd.c : 1269 ] GetSignalLevel phyId %u, snrInput %u, chainMask %x, bandwidth %u, combRssi %u 
5405,I,[ phyrf_debug_cmd.c : 1273 ] GetSignalLevel : SNR Input %u 
5404,III,[ phyrf_debug_cmd.c : 1288 ] GetSignalLevel : SNR BW Segment Input %8x%8x for Chain %u 
5403,I,[ phyrf_debug_cmd.c : 1296 ] GetSignalLevel : Returns %u (WHAL_EINVAL) 
5402,Ii,[ phyrf_debug_cmd.c : 1305 ] GetSignalLevel : SNR=%u RSSI=%d 
5401,IIIIIi,[ phyrf_debug_cmd.c : 1319 ] GetSignalLevel : SNR[%u][%u]=%u RSSI[%u][%u]=%d 
5400,i,[ phyrf_debug_cmd.c : 2195 ] GTXENABLE: Invalid PHY ID = %d 
5399,ii,[ phyrf_debug_cmd.c : 2201 ] GreenTx Enable[%d]=%d 
5398,i,[ phyrf_debug_cmd.c : 2214 ] ImpsBmpsControl: Invalid PHY ID = %d 
5397,ii,[ phyrf_debug_cmd.c : 2225 ] ImpsBmpsControl: enable=%d, phyId=%d 
5396,iii,[ phyrf_debug_cmd.c : 2239 ] ImpsBmpsControl: imps=%d, enable=%d, phyId=%d 
5395,iiii,[ phyrf_debug_cmd.c : 2258 ] ImpsBmpsControl: imps=%d, w2s=%d, enable=%d, phyId=%d 
5394,,[ phyrf_debug_cmd.c : 2027 ] LP_SYNTH: Invalid test arguments  
5393,ii,[ phyrf_debug_cmd.c : 2044 ] LPSYNTHFORLEGACY: WIFITOOL ISSUED TO ENABLE LP SYNTH: legacy rate: %d, dtim: %d
 
5392,I,[ phyrf_debug_cmd.c : 989 ] ANI_LOG g_max_edcca=%x 
5391,ii,[ phyrf_debug_cmd.c : 1003 ] ANI_LOG PHYID%d g_ani_cca %d 
 
5390,iii,[ phyrf_debug_cmd.c : 1023 ] ANI_LOG PHYID%d ani_dl_min %d, ani_dl_max %d 
 
5389,I,[ phyrf_debug_cmd.c : 1731 ] NFCAL_READ_TEST : phyId %u not available for test 
5388,IIIIIi,[ phyrf_debug_cmd.c : 1749 ] NFCAL_READ_TEST : phyId %u, nfType 0x%x, bufferSize %u, validBuffer %u, bufferPointer 0x%x, returns %d 
5387,IIIi,[ phyrf_debug_cmd.c : 1757 ] NFCAL_READ_TEST : phyId %u, nfType 0x%x, Chain %u, NFValue %d 
5386,i,[ phyrf_debug_cmd.c : 1674 ] WIFITOOL: PHYID %d is not active 
 
5385,iii,[ phyrf_debug_cmd.c : 1686 ] Enable S-OCL: enable=%d listen_chain=%d FOR PHYID %d 
 
5384,,[ phyrf_debug_cmd.c : 1689 ] Invalid argument 
5383,Ii,[ phyrf_debug_cmd.c : 1696 ] Enable D-OCL: OCLFlag 0x%x FOR PHYID %d 
 
5382,,[ phyrf_debug_cmd.c : 2323 ] IpcHandler_Enable: Invalid test arguments  
5381,,[ phyrf_debug_cmd.c : 2329 ] IpcHandler_Enable: Invalid phyId 
5380,ii,[ phyrf_debug_cmd.c : 2336 ] IpcHandler_Enable: enable=%d, phyId=%d 
5379,i,[ phyrf_debug_cmd.c : 1352 ] PHYDBG: g_phydbg_disable = %d 
5378,,[ phyrf_debug_cmd.c : 1363 ] phydbg_reconfigure : Invalid test arguments  
5377,i,[ phyrf_debug_cmd.c : 1371 ] phydbg_reconfigure : Invalid PHY ID = %d
 
5376,ii,[ phyrf_debug_cmd.c : 1375 ] phydbg_reconfigure : PHYID = %d ,Event = %d
 
5375,,[ phyrf_debug_cmd.c : 2638 ] DebugCmdPhyOnOffSeq : Invalid test arguments 
5374,I,[ phyrf_debug_cmd.c : 2645 ] DebugCmdPhyOnOffSeq : Invalid phyId %u 
5373,I,[ phyrf_debug_cmd.c : 2653 ] DebugCmdPhyOnOffSeq : Invalid pHandle for phyId %u 
5372,I,[ phyrf_debug_cmd.c : 2661 ] DebugCmdPhyOnOffSeq : Invalid pResetStruct for phyId %u 
5371,IIII,[ phyrf_debug_cmd.c : 2670 ] DebugCmdPhyOnOffSeq : Pretest Counter phyId %u, cfActiveLow_Fail_cnt %04u, cfActiveLow_Pass_cnt %04u, phyOffThroughVregCnt %04u 
5370,I,[ phyrf_debug_cmd.c : 2681 ] DebugCmdPhyOnOffSeq : Validating vreg based phyOff for phyId %u 
5369,I,[ phyrf_debug_cmd.c : 2685 ] DebugCmdPhyOnOffSeq : Validating tlv based phyOff followed by vreg based phyOff for phyId %u 
5368,I,[ phyrf_debug_cmd.c : 2690 ] DebugCmdPhyOnOffSeq : Validating calling vreg based phyOff twice for phyId %u 
5367,I,[ phyrf_debug_cmd.c : 2696 ] DebugCmdPhyOnOffSeq : Validating tlv based phyOff for phyId %u 
5366,IIII,[ phyrf_debug_cmd.c : 2709 ] DebugCmdPhyOnOffSeq : Posttest Counter phyId %u, cfActiveLow_Fail_cnt %04u, cfActiveLow_Pass_cnt %04u, phyOffThroughVregCnt %04u 
5365,i,[ phyrf_debug_cmd.c : 609 ] BDF DUMP: Invalid NV Section  %d 
5364,i,[ phyrf_debug_cmd.c : 614 ] BDF DUMP: NV Section Size: %d 
5363,ii,[ phyrf_debug_cmd.c : 625 ] BDF DUMP: sub-section size: %d sub-section id: 0x%d 
5362,iI,[ phyrf_debug_cmd.c : 631 ] BDF DUMP: index: %d d: 0x%x 
5361,iI,[ phyrf_debug_cmd.c : 640 ] BDF DUMP: index: %d d:0x%x 
5360,I,[ phyrf_debug_cmd.c : 208 ] RegDumpId %u :: NFCAL_BDF_PER_CHAIN :: Exceptions :: Value = 1 : Chain Unsupported 
5359,IIIii,[ phyrf_debug_cmd.c : 244 ] RegDumpId %u :: NFCAL_RUNTIME_PER_CHAIN :: phyId %u :: Chain %u :: %d dBr :: %d dBm 
5358,III,[ phyrf_debug_cmd.c : 254 ] RegDumpId %u :: XTAL CAPIN=%u 	 CAPOUT=%u
 
5357,IIi,[ phyrf_debug_cmd.c : 258 ] BdfDump :: XTAL CAPIN=%u 	 CAPOUT=%u 	 PPM=%d 
 
5356,IIi,[ phyrf_debug_cmd.c : 261 ] BdfDump :: XTAL CAPIN=%u 	 CAPOUT=%u 	 PPM=-%d 
 
5355,II,[ phyrf_debug_cmd.c : 281 ] RegDumpId %u :: TPC_DUMP MASK %u 
5354,iii,[ phyrf_debug_cmd.c : 304 ] RxGainCalResult phyId:%d channel_idx:%d, channel_freq:%d 
5353,iiiii,[ phyrf_debug_cmd.c : 310 ] RxGainCalResult phyId:%d channel_idx:%d, chain_idx:%d, DBr_value:%d, DBm_value:%d 
5352,IIIii,[ phyrf_debug_cmd.c : 215 ] RegDumpId %u :: NFCAL_BDF_PER_CHAIN :: phyId %u :: Chain %u :: %d dBr :: %d dBm 
5351,iI,[ phyrf_debug_cmd.c : 328 ] FTM_DEBUG: g_ftm_ctxt[%d] addr = %p 
5350,iIIII,[ phyrf_debug_cmd.c : 339 ] FTM_DEBUG: g_ftm_ctxt[%d]: pdev = %p, vdev = %p, peer = %p, ftm_mode = 0x%x 
5349,iIIII,[ phyrf_debug_cmd.c : 341 ] FTM_DEBUG: g_ftm_ctxt[%d]: send_mgmt = 0x%x, send_data = 0x%x, encap_cfg = %p, ctrl = %p 
5348,,[ phyrf_debug_cmd.c : 345 ] FTM_DEBUG: encap_cfg pointer is NULL in g_ftm_ctxt !!  
5347,iiiI,[ phyrf_debug_cmd.c : 353 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg: pkt_len = %d, pkt_type = %d, vdev = %p 
5346,iIIIIII,[ phyrf_debug_cmd.c : 360 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg->sa_addr = 0x%02x:%02x:%02x:%02x:%02x:%02x 
5345,iIIIIII,[ phyrf_debug_cmd.c : 368 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg->da_addr = 0x%02x:%02x:%02x:%02x:%02x:%02x 
5344,iIIIIII,[ phyrf_debug_cmd.c : 376 ] FTM_DEBUG: g_ftm_ctxt[%d].encap_cfg->bss_addr = 0x%02x:%02x:%02x:%02x:%02x:%02x 
5343,,[ phyrf_debug_cmd.c : 381 ] FTM_DEBUG: ctrl pointer is NULL in g_ftm_ctxt !! 
5342,iii,[ phyrf_debug_cmd.c : 388 ] FTM_DEBUG: g_ftm_ctxt[%d].ctrl: num_pkts_to_send = %d, is_aggr_ok = %d 
5341,I,[ phyrf_debug_cmd.c : 237 ] RegDumpId %u :: NFCAL_RUNTIME_PER_CHAIN :: Exceptions :: Value = 1 : Chain Unsupported, Value = 0 : NFCAL Convergence Failed 
5340,iii,[ phyrf_debug_cmd.c : 395 ] FTM_DEBUG: g_dbg_overwrite_ppdu_dur_us = %d, g_dbg_gi_override = %d, g_dbg_he_ltf_override = %d 
5339,iiii,[ phyrf_debug_cmd.c : 426 ] CALDB_DEBUG:   	calDBEnableSetting=%d, 	 CalTimeOutSetting = %d, 	PersistentEnable = %d, 	masterCalDbExist()=%d 
5338,Ii,[ phyrf_debug_cmd.c : 427 ] CALDB_DEBUG: CALDB_ADDRE= %x dB size = %d 
5337,,[ phyrf_debug_cmd.c : 428 ] CALDB_DEBUG: Version info and CALDB Synopsis follows: 
5336,iIIi,[ phyrf_debug_cmd.c : 1099 ] ADDRVAL: indx = %d addr = 0x%X val = 0x%X en=%d 
5335,iIIi,[ phyrf_debug_cmd.c : 1109 ] ADDRVAL: indx = %d addr = 0x%X val = 0x%X en=%d 
5334,iIIi,[ phyrf_debug_cmd.c : 1115 ] ADDRVAL: indx = %d addr = 0x%X val = 0x%X en=%d 
5333,ii,[ phyrf_debug_cmd.c : 2891 ] Unit test, SAR Active enable %d dsi %d! 
5332,,[ phyrf_debug_cmd.c : 2897 ] BIOS Unit test 
5331,i,[ phyrf_debug_cmd.c : 2913 ]  ERR BIOS Unit test %d 
5330,,[ phyrf_debug_cmd.c : 2458 ] phyrf_debug_MMHostCmdSetCalMask Invalid Command 
5329,Ii,[ phyrf_debug_cmd.c : 2465 ] phyrf_debug_MMHostCmdSetCalMask: Invalid PHY ID = %u, phyrf_init_GetNumPhys()=%d 
5328,i,[ phyrf_debug_cmd.c : 2473 ] phyrf_debug_MMHostCmdSetCalMask: Invalid pHandle for phyId=%d 
5327,I,[ phyrf_debug_cmd.c : 2480 ] Set g_halphy_debug_cal_mask =0x%x
 
5326,,[ phyrf_debug_cmd.c : 2344 ] SetCcaThreshold: Invalid test arguments  
5325,,[ phyrf_debug_cmd.c : 2350 ] SetCcaThreshold: Invalid phyId 
5324,I,[ phyrf_debug_cmd.c : 2005 ] Set g_halphy_debug_mask =0x%x
 
5323,I,[ phyrf_debug_cmd.c : 2011 ] Set phyDebugMask =0x%x
 
5322,,[ phyrf_debug_cmd.c : 1812 ] PAPRD: Invalid test arguments  
5321,i,[ phyrf_debug_cmd.c : 1820 ] PAPRD: Invalid PHY ID = %d
 
5320,ii,[ phyrf_debug_cmd.c : 1824 ] PAPRD: PHYID = %d ,Event = %d
 
5319,i,[ phyrf_debug_cmd.c : 1650 ] WIFITOOL: PHYID %d is not active 
 
5318,i,[ phyrf_debug_cmd.c : 1657 ] Setting PBS Mode to %d
 
5317,i,[ phyrf_debug_cmd.c : 1935 ] Setting PBS Mode to %d
 
5316,,[ phyrf_debug_cmd.c : 2728 ] FUSE BOARD ID VALUE TO OTP : wifitool : Command unsupported !  
5315,,[ phyrf_debug_cmd.c : 2145 ] SPECTRAL_ENABLE: Invalid test arguments  
5314,,[ phyrf_debug_cmd.c : 2151 ] SPECTRAL_ENABLE: Invalid phyId 
5313,,[ phyrf_debug_cmd.c : 2157 ] SPECTRAL_ENABLE: Invalid scanMode 
5312,i,[ phyrf_debug_cmd.c : 947 ] THERMAL: Invalid PHY ID = %d 
5311,ii,[ phyrf_debug_cmd.c : 954 ] g_ThermalEnable[%d]=%d 
5310,,[ phyrf_debug_cmd.c : 2429 ] TPC CLPC SWITCH: Invalid test arguments  
5309,,[ phyrf_debug_cmd.c : 2435 ] TPC CLPC: Invalid phyId 
5308,,[ phyrf_debug_cmd.c : 2442 ] TPC CLPC: TO BE IMPLEMENTED 
5307,,[ phyrf_debug_cmd.c : 2382 ] TpcPowerOverride: Invalid test arguments  
5306,,[ phyrf_debug_cmd.c : 2388 ] TpcPowerOverride: Invalid phy ID 
5305,,[ phyrf_debug_cmd.c : 2406 ] TpcPowerOverride: Invalid test arguments  
5304,ii,[ phyrf_debug_cmd.c : 2414 ] TpcPowerOverride: chain %d: power: %d 
5303,i,[ phyrf_debug_cmd.c : 2807 ] TASSetting: Updating reserve_margin dB to %d
 
5302,i,[ phyrf_debug_cmd.c : 2812 ] TASSetting: Updating Peak Limit to %d
 
5301,,[ phyrf_debug_cmd.c : 2819 ] TAS_OL_TEST : Iwpriv cmd to TEST TAS OL issued. Commencing Test 
5300,,[ phyrf_debug_cmd.c : 2825 ] TAS_OL_TEST : Iwpriv cmd to Stop Testing TAS OL issued. Stopping Test 
5299,,[ phyrf_debug_cmd.c : 2833 ] TASSetting: wifitool : Invalid test arguments 
5298,i,[ phyrf_debug_cmd.c : 928 ] XTAL: Invalid PHY ID = %d 
5297,ii,[ phyrf_debug_cmd.c : 933 ] g_XtalCalPPM[%d]=%d 
5473,i,[ dfs_fcc_bin5.c : 110 ] DFS_DUMPS Rejecting pulses as they are not chirp %d
 
5500,iii,[ phyrf_dfs.c : 398 ] DFS_DUMPS regdomain %d phyId=%d g_DfsConfiguration=%d
 
5499,,[ phyrf_dfs.c : 227 ] DFS_DUMPS set 0x8000 
 
5498,,[ phyrf_dfs.c : 249 ] DFS_DUMP set g_dfs_test_mode 
 
5497,,[ phyrf_dfs.c : 254 ] DFS_DUMP clear g_dfs_test_mode 
 
5496,,[ phyrf_dfs.c : 259 ] DFS_DUMP Send Radar summary pulse to host 
 
5495,,[ phyrf_dfs.c : 263 ] DFS_DUMP stop Sending Radar summary pulse to host 
 
5494,,[ phyrf_dfs.c : 268 ] DFS_DUMPS Print all the pulse information
 
5493,,[ phyrf_dfs.c : 273 ] DFS_DUMPS Stop printing pulse information
 
5492,i,[ phyrf_dfs.c : 278 ] DFS_DUMPS RAW_FFT Data Dump set to %d
 
5491,iiiiiiiii,[ phyrf_dfs.c : 240 ] DFS_DUMPS timestamp=%d diff_ts=%d pulse_rssi=%d pulse_duration=%d is_chirp=%d sidx=%d detector_id=%d
 false_radar=%d radar_check=%d 
5490,,[ phyrf_dfs.c : 244 ] DFS_DUMPS set 0x8001 
 
5489,II,[ phyrf_dfs.c : 943 ] %s:Allocation of g_dfs_ic[dfs_detector_id] failed %zu 
5488,I,[ phyrf_dfs.c : 516 ] %s: DFS ic is Invalid 
5487,I,[ phyrf_dfs.c : 532 ] %s: DFS-FCC domain 
5486,I,[ phyrf_dfs.c : 540 ] %s: DFS-ETSI domain 
5485,I,[ phyrf_dfs.c : 555 ] %s:DFS-MKKN domain 
5484,I,[ phyrf_dfs.c : 573 ] %s: DFS-MKK domain 
5483,I,[ phyrf_dfs.c : 589 ] %s:  DFS_CN_DOMAIN 
5482,I,[ phyrf_dfs.c : 603 ] %s:  DFS_KR_DOMAIN 
5481,I,[ phyrf_dfs.c : 621 ] %s: DFS-UNINT domain 
5480,,[ phyrf_dfs.c : 644 ] PRDD_Test_Radar_Enable 
5479,Ii,[ phyrf_dfs.c : 647 ] %s[%d]: DFS- Radar Detection Enabling Failed 
5478,I,[ phyrf_dfs.c : 820 ] %s: DFS ic is Invalid 
5477,II,[ phyrf_dfs.c : 831 ] %s: allocation of dfs_ic->ic_curchan failed %zu 
5476,iiiii,[ phyrf_dfs.c : 853 ] DFS_DUMPS : req_chan=%d, ic_ieee_chan=%d, center_freq1=%d, center_freq2=%d, chan_wodth=%d
 
5475,Ii,[ phyrf_dfs.c : 903 ] %s: Recieved a wrong channel width %d 
5474,I,[ phyrf_dfs.c : 924 ] %s: DFS- CHANNEL CONFIGURED 
5501,III,[ wma_dfs_interface.c : 63 ] %s: called; ptr=%p, radar_info=%p
 
5503,,[ hca_rf_ftmIf_api.cpp : 140 ] ftmIf_SetRxDeaf 
5502,,[ hca_rf_ftmIf_api.cpp : 154 ] ftmIf_SetRxListen 
5504,i,[ hca_HwComponentTrx.cpp : 78 ] Error: processCmd ID of %d, unknown state. 
5505,i,[ hca_config.cpp : 85 ] Invalid HW component type %d
 
5588,i,[ phyrf_mc_paprd.c : 1950 ] PAPRD:Tx stats : hw_queued %d 
5587,i,[ phyrf_mc_paprd.c : 1951 ] PAPRD:Tx stats : hw_reaped %d 
5586,i,[ phyrf_mc_paprd.c : 1952 ] PAPRD:Tx stats : tx_done %d 
5585,i,[ phyrf_mc_paprd.c : 1953 ] PAPRD:Tx stats : tx_abort %d 
5584,i,[ phyrf_mc_paprd.c : 1954 ] PAPRD:Tx stats : tx_abort_compl_err_status %d 
5583,i,[ phyrf_mc_paprd.c : 1955 ] PAPRD:Tx stats : tx_abort_pdev_suspend %d 
5582,i,[ phyrf_mc_paprd.c : 1956 ] PAPRD:Tx stats : tx_async_enqueue %d 
5581,i,[ phyrf_mc_paprd.c : 1957 ] PAPRD:Tx stats : tx_async_dequeue %d 
5580,i,[ phyrf_mc_paprd.c : 1958 ] PAPRD:Tx stats : tx_fail %d 
5579,,[ phyrf_mc_paprd.c : 681 ] PAPRD: dpd_cal_start_timer_handler_0 : pHandle NULL 
5578,i,[ phyrf_mc_paprd.c : 691 ] PAPRD: PhyId %d Inactive, returning without CAL 
5577,i,[ phyrf_mc_paprd.c : 698 ] PAPRD: Start Calibration : %d ms Timer expired  
5576,i,[ phyrf_mc_paprd.c : 721 ] PAPRD: Timer Handler %d  current channel conntext is different from timer channel context 
5575,,[ phyrf_mc_paprd.c : 2483 ] PAPRD: dpd_cal_sync_handler_0 pHandle NULL 
5574,i,[ phyrf_mc_paprd.c : 2490 ] PAPRD: PhyId %d dpd_cal_sync_timer_handler_0, releasing the wal_lock 
5573,i,[ phyrf_mc_paprd.c : 1758 ] Calibration is in progress on other phy, cur phyId %d 
5572,iiiiii,[ phyrf_mc_paprd.c : 1797 ] PAPRD: Abort TempRecal phy %d, curr time %d, currTemp %d, last calTemp  %d curr Channel %d thermal channel %d 
5571,iiii,[ phyrf_mc_paprd.c : 1826 ] PAPRD : FTM PHY id %d currTemp %d cal temp %d tempDiff_scale %d 
5570,iiiii,[ phyrf_mc_paprd.c : 1837 ] PAPRD : TempRecal triggered phy %d, curr time %d, currTemp %d, last calTemp  %d channel %d 
5569,iiiii,[ phyrf_mc_paprd.c : 1841 ] PAPRD : Per chain TempRecal phy %d, chain_index %d, currTemp %d, last calTemp  %d channel %d 
5568,iiii,[ phyrf_mc_paprd.c : 1850 ] PAPRD : PHY id %d currTemp %d cal temp %d tempDiff_scale %d 
5567,iiiiii,[ phyrf_mc_paprd.c : 2312 ]  (chan %d ,cm %d halphyMemDPDValidateCalDB , result [%d %d], cal_attempts[%d %d] 
5566,iiiii,[ phyrf_mc_paprd.c : 2316 ]  (chan %d ,cm %d halphyMemDPDValidateCalDB , max attemps %d temp [%d %d] 
5565,iiii,[ phyrf_mc_paprd.c : 2282 ]  halphyPaprdValidateMemCalibration calattempts %d %d, validBits %d %d 
5564,,[ phyrf_mc_paprd.c : 2287 ]  CALIBRATION COMPLETE  chain 0, result 1 
5563,,[ phyrf_mc_paprd.c : 2291 ]  CALIBRATION COMPLETE  chain 1, result 1 
5562,,[ phyrf_mc_paprd.c : 2389 ] Do not have access to masterCalDb or localCalDb, failed to restore DPD 
5561,ii,[ phyrf_mc_paprd.c : 2393 ] DPD Memory : paprd_restore : finalCase %d channel %d 
5560,iiii,[ phyrf_mc_paprd.c : 1458 ] PAPRD: cur_channel %d, wal_channel %d, scan_channel %d, phyReset %d 
5559,iiiii,[ phyrf_mc_paprd.c : 1017 ] PAPRD: DPD calibration aborted on chain %d, tableIdx %d, channel %d, state %d, new_channel_change_request %d 
5558,i,[ phyrf_mc_paprd.c : 1032 ] PAPRD: DPD calibration aborted on channel %d 
5557,i,[ phyrf_mc_paprd.c : 209 ] PAPRD:SM state %d 
5556,iii,[ phyrf_mc_paprd.c : 286 ] PAPRD: Aborting Excess Retries. retry_dpd %d, Tx_Err %d, WoW Status %d 
5555,iiiii,[ phyrf_mc_paprd.c : 299 ] PAPRD: Tx chainmask Status FALSE m/c : channel %d, txchain %d, table %d, txChainMask %d, state %d 
5554,iii,[ phyrf_mc_paprd.c : 355 ] PAPRD:warmUpPktSupport %d (%d %d) 
5553,i,[ phyrf_mc_paprd.c : 361 ] PAPRD: eDPD MISSION MODE dpd continue state %d 
5552,i,[ phyrf_mc_paprd.c : 389 ] PAPRD: PAPRD_CAL_SM_DPD_TRAINING_PROCESS_DATA hwPaPrdStatus(fail) retry_dpd %d 
5551,iii,[ phyrf_mc_paprd.c : 421 ] PAPRD: TRAINING_PROCESS_DATA chain %d tableIdx %d processing_time %d 
5550,i,[ phyrf_mc_paprd.c : 447 ]  DPD Aborted due to BG thread activated in FTM mode : smState %d 
5549,,[ phyrf_mc_paprd.c : 243 ] PAPRD: UCODE VREG WAR enabled 
5548,,[ phyrf_mc_paprd.c : 508 ] PAPRD: PAPRD_CAL_SM_TEARDOWN_TRAINING : DPD ABORT 
5547,iii,[ phyrf_mc_paprd.c : 529 ] PAPRD: is160mode %d secondary %d primary_done %d 
5546,iii,[ phyrf_mc_paprd.c : 547 ] PAPRD: phy_a0_done %d phy_a1_done %d phy_a1_secondary_done %d 
5545,ii,[ phyrf_mc_paprd.c : 556 ] PAPRD: PAPRDTUNING DONE. total_caltime  %d, phyOff_cnt  %d 
5544,,[ phyrf_mc_paprd.c : 566 ] ----- PAPRDTUNING SECONDARY started----- 
5543,ii,[ phyrf_mc_paprd.c : 576 ] PAPRD: PAPRDTUNING DONE. total_caltime %d, phyOff_cnt %d 
5542,iii,[ phyrf_mc_paprd.c : 581 ] PAPRD: is160mode %d, secondary %d, isExtn %d 
5541,ii,[ phyrf_mc_paprd.c : 582 ] PAPRD: lastcalTime %d, current_time %d 
5540,ii,[ phyrf_mc_paprd.c : 591 ] PAPRD State %d,DPD cal type %d 
5539,i,[ phyrf_mc_paprd.c : 621 ] PAPRD PAPRD_CAL_SM_MEM_DPD_POST_PROC_DATA. thread status %d 
5538,iiii,[ phyrf_mc_paprd.c : 255 ] PAPRD: State m/c : channel %d, txchain %d, table %d, state %d 
5537,i,[ phyrf_mc_paprd.c : 630 ] PAPRD mem dpd retry count %d  
5536,ii,[ phyrf_mc_paprd.c : 975 ] PAPRD: Channel = %d, dpd_enable = %d 
5535,iii,[ phyrf_mc_paprd.c : 988 ] PAPRD: Chain = %d, txgainIdx = %d, dacgain = %d 
5534,,[ phyrf_mc_paprd.c : 2015 ] ******** PAPRD: PHY is not active 
5533,ii,[ phyrf_mc_paprd.c : 2021 ] PAPRD: phyrf_mc_PaprdMemDPD_post_proc_complete. PHY id %d SM state %d 
5532,ii,[ phyrf_mc_paprd.c : 790 ] PAPRD: Start Timer  %d  same  channel conntext as the timer channel context (%d) : do nothing 
5531,,[ phyrf_mc_paprd.c : 807 ] PAPRD : WOW Entered, return from DPD CAL 
5530,,[ phyrf_mc_paprd.c : 815 ] PAPRD : phyrf_mc_PaprdStartTimer: 
5529,i,[ phyrf_mc_paprd.c : 796 ] PAPRD: Cancel Timer  %d  current channel conntext is different from timer channel context 
5528,iiiiiii,[ phyrf_mc_paprd.c : 1565 ] PAPRD: phyrf_mc_SendTxCompletion : channel %d, txchain %d, table %d, new_channel_change_request %d, cal abort_ppdu %d, status %d, retry_cnt %d 
5527,iiiiiii,[ phyrf_mc_paprd.c : 1586 ] PAPRD: new_channel_change_request : channel %d, txchain %d, table %d, new_channel_change_request %d, cal abort_ppdu %d, status %d, retry_cnt %d 
5526,iiiii,[ phyrf_mc_paprd.c : 1604 ] PAPRD: Status %d, whal_tx_err_status_t %d, Flush_req_reason %d, tx_ctxt_flags %d, pdev_paused %d 
5525,i,[ phyrf_mc_paprd.c : 1626 ] PAPRD: TBTT Flush condition hit , flush_req_reason = %d 
5524,iiii,[ phyrf_mc_paprd.c : 1639 ] PAPRD: Tx Completion Status %d, whal_tx_err_status_t = %d , retrying (chain %d table %d) 
5523,iiiiii,[ phyrf_mc_paprd.c : 1497 ] PAPRD: TxChain %d, tableIdx %d, channel %d, state %d, new_channel_change_request %d, startEvtLatency %d 
5522,,[ phyrf_mc_paprd.c : 1506 ] PAPRD: PPDU Start Event Delayed - skip further processing and retry DPD 
5521,iii,[ phyrf_mc_paprd.c : 1517 ] PAPRD :  Start EVT captured SCAN: Aborted. Status %d abort_ppdu %d cur_tbl_idx %d 
5520,,[ phyrf_mc_paprd.c : 1523 ]  PAPRD: phyrf_paprd_TrainingStatus success 
5519,,[ phyrf_mc_paprd.c : 1528 ]  PAPRD: phyrf_paprd_TrainingStatus fail 
5518,i,[ phyrf_mc_paprd.c : 136 ] PAPRD: Paprd Done status is %d
 
5517,iiii,[ phyrf_mc_paprd.c : 1691 ]  PAPRD: phyId %d, txchainmask %d chain %d, degC %d 
5516,iiii,[ phyrf_mc_paprd.c : 1696 ]  PAPRD: phyId %d, txchainmask %d currtime %d, degC %d 
5515,iiii,[ phyrf_mc_paprd.c : 1980 ] PAPRD ApplyTempScaling: PhyId %d slope %d temp delta %d scaling %d 
5514,,[ phyrf_mc_paprd.c : 2459 ] PAPRD: pHandle NULL 
5513,i,[ phyrf_mc_paprd.c : 1736 ] Calibration is in progress on phyId %d 
5512,iiiiiii,[ phyrf_mc_paprd.c : 2232 ]  phyId %d thread context : workingChannel %d txChainMask  %d bHomeChan %d phyrfMode %d  WoW Mode %d curr Channel %d 
5511,ii,[ phyrf_mc_paprd.c : 2250 ]  MEM_DPD THREAD (START the new table) : UPDATING CALDB POST PROCESSING DATA :  %d %d 
5510,iiii,[ phyrf_mc_paprd.c : 2263 ]  BG THREAD CONTEXT is DIFFERENT :  %d %d, curr channel %d  bChannelContext %d 
5509,ii,[ phyrf_mc_paprd.c : 1922 ] thermal scaling value is %d and thermal slope is %d 
5508,iiiii,[ phyrf_mc_paprd.c : 1938 ] PAPRD: temp_recal_timer started. tempRecalcount %d, phyId %d, calTemp %d, calDb temp chain0 %d, calDb temp chain1 %d 
5507,iii,[ phyrf_mc_paprd.c : 2598 ] PAPRD: Calibration triggered for a pending request on PhyId %d Channel %d , home %d 
5506,iiiiii,[ phyrf_mc_paprd.c : 2447 ]  phyId %d  thread context : workingChannel %d txChainMask  %d bHomeChan %d phyrfMode %d  WoW Mode %d 
5589,I,[ phyrf_phy.c : 79 ] MAC FW Vreg update RU26 Tx disable = %x 
5651,ii,[ phyrf_regulatory.c : 271 ] RegDB Channel Prioritity Supported, Frequency Index value=%d Priority Frequency=%d
 
5650,,[ phyrf_regulatory.c : 280 ] RegDB Channel Prioritity Not Supported 
 
5649,i,[ phyrf_regulatory.c : 275 ] RegDB Channel Prioritity Supported but Country Not Supported, Frequency Index value=%d
 
5648,iii,[ phyrf_regulatory.c : 292 ] RegDB-6G MaxBW AP SP - %d, LPI - %d, VLP - %d
 
5647,iii,[ phyrf_regulatory.c : 298 ] RegDB-6G MaxBW CLIENT SP - %d, LPI - %d, VLP - %d
 
5646,,[ phyrf_regulatory.c : 305 ] RegDB - phyrf_regulatory_FillMinBW_6g
 
5645,iii,[ phyrf_regulatory.c : 309 ] RegDB-6G MinBW AP SP - %d, LPI - %d, VLP - %d
 
5644,iii,[ phyrf_regulatory.c : 315 ] RegDB-6G MinBW CLIENT SP - %d, LPI - %d, VLP - %d
 
5643,iii,[ phyrf_regulatory.c : 325 ] RegDB-6G NumRules AP SP - %d, LPI - %d, VLP - %d
 
5642,iii,[ phyrf_regulatory.c : 331 ] RegDB-6G NumRules CLIENT SP - %d, LPI - %d, VLP - %d
 
5641,Ii,[ phyrf_regulatory.c : 2025 ] RegDB-Test_Super Domain 6G %x %d
 
5640,i,[ phyrf_regulatory.c : 971 ] get valid country_code/domain_code from OTP %d. 
5639,iii,[ phyrf_regulatory.c : 1007 ] RegDB-BDF CC %d BDF RD %d CC Type %d
 
5638,i,[ phyrf_regulatory.c : 1039 ] RegDB-No Reg_Dmn diff with BDF %d
 
5637,,[ phyrf_regulatory.c : 1045 ] RegDB-Has a 6G domain ID
 
5636,,[ phyrf_regulatory.c : 1050 ] RegDB-Valid 6G super dmn and 5G2G reg pair Combo
 
5635,,[ phyrf_regulatory.c : 1059 ] RegDB-Invlid Combo
 
5634,ii,[ phyrf_regulatory.c : 1097 ] RegDB-6G Super Dmn %d Max BW %d
 
5633,i,[ phyrf_regulatory.c : 1116 ] super_dmn_6g  %d 
5632,ii,[ phyrf_regulatory.c : 1174 ] RegDB-6G Super Dmn %d Max BW %d
 
5631,ii,[ phyrf_regulatory.c : 1179 ] RegDB-Valid country ID %d Correspondig RegDmn %d
 
5630,ii,[ phyrf_regulatory.c : 1211 ] RegDB-6G Super Dmn %d Max BW %d
 
5629,ii,[ phyrf_regulatory.c : 1241 ] RegDB-6G Super Dmn %d Max BW %d
 
5628,ii,[ phyrf_regulatory.c : 1254 ] RegDB Channel Prioritity Supported, Frequency Index value=%d Priority Frequency=%d
 
5627,i,[ phyrf_regulatory.c : 1258 ] RegDB Channel Prioritity Supported but Country Not Supported, Frequency Index value=%d
 
5626,,[ phyrf_regulatory.c : 1263 ] RegDB Channel Prioritity Not Supported 
 
5625,ii,[ phyrf_regulatory.c : 1266 ] RegDB-Valid country ID %d Correspondig RegDmn %d
 
5624,i,[ phyrf_regulatory.c : 1277 ] RegDB-Status %d
 
5623,iiiiiiii,[ phyrf_regulatory.c : 1278 ] RegDB-Final Result alpha0 %d alpha1 %d alpha_size %d max_rules %d get_type %d cc_type %d ctryID %d dmnCode %d
 
5622,iiiiiiiii,[ phyrf_regulatory.c : 1279 ] RegDB-Final Result num_2g_rules %d num_5g_rules %d phybitmap %d dfsregion %d min_bw_2g %d min_bw_5g %d max_bw_2g %d max_bw_5g %d vlp_priority_freq %d
 
5621,i,[ phyrf_regulatory.c : 981 ] get valid country_code/domain_code from BDF %d. 
5620,,[ phyrf_regulatory.c : 984 ] neither OTP nor BDF valid value for country_code/domain_code. 
5619,iii,[ phyrf_regulatory.c : 1005 ] RegDB-BDF CC %d OTP RD %d CC Type %d
 
5618,,[ phyrf_regulatory.c : 675 ] RegDB-New Extended Event Invoked
 
5617,iii,[ phyrf_regulatory.c : 693 ] RegDB-Super Dmn Id %d validity %d Idx %d
 
5616,ii,[ phyrf_regulatory.c : 708 ] super_dmn_id_6g=%d, domain_code=%d 
5615,iii,[ phyrf_regulatory.c : 744 ] RegDB-Super Dmn Id %d validity %d Idx %d
 
5614,iii,[ phyrf_regulatory.c : 797 ] RegDB - Ext Event Status - 2G5G %d 6G %d Overall %d
 
5613,iiiiiiii,[ phyrf_regulatory.c : 798 ] RegDB-Final Result_Ext alpha0 %d alpha1 %d alpha_size %d max_rules %d get_type %d cc_type %d ctryID %d dmnCode %d
 
5612,iiiiiiii,[ phyrf_regulatory.c : 799 ] RegDB-Final Result_Ext num_2g_rules %d num_5g_rules %d phybitmap %d dfsregion %d min_bw_2g %d min_bw_5g %d max_bw_2g %d max_bw_5g %d
 
5611,Ii,[ phyrf_regulatory.c : 1874 ] RegDB-Test_Super Domain 6G %x %d
 
5610,i,[ phyrf_regulatory.c : 1374 ] get valid country_code/domain_code from OTP %d. 
5609,i,[ phyrf_regulatory.c : 1386 ] get valid country_code/domain_code from BDF %d. 
5608,,[ phyrf_regulatory.c : 1389 ] neither OTP nor BDF valid value for country_code/domain_code. 
5607,i,[ phyrf_regulatory.c : 582 ] get valid country_code/domain_code from OTP %d. 
5606,i,[ phyrf_regulatory.c : 594 ] get valid country_code/domain_code from BDF %d. 
5605,,[ phyrf_regulatory.c : 597 ] neither OTP nor BDF valid value for country_code/domain_code. 
5604,ii,[ phyrf_regulatory.c : 484 ] RegDB-Getting 6G_AP_LPI Rules dmn_id %d num_rules %d
 
5603,ii,[ phyrf_regulatory.c : 487 ] RegDB-Getting 6G_AP_SP Rules dmn_id %d num_rules %d
 
5602,ii,[ phyrf_regulatory.c : 490 ] RegDB-Getting 6G_AP_VLP Rules dmn_id %d num_rules %d
 
5601,ii,[ phyrf_regulatory.c : 501 ] RegDB-Getting 6G_CLIENT_LPI Rules dmn_id %d num_rules %d
 
5600,ii,[ phyrf_regulatory.c : 507 ] RegDB-Getting 6G_CLIENT_SP Rules dmn_id %d num_rules %d
 
5599,ii,[ phyrf_regulatory.c : 513 ] RegDB-Getting 6G_CLIENT_VLP Rules dmn_id %d num_rules %d
 
5598,i,[ phyrf_regulatory.c : 1303 ] RegDB-Valid reg dmn pair id %d
 
5597,ii,[ phyrf_regulatory.c : 1317 ] RegDB-Valid domain 2g rules %d 5g rules %d
  
5596,,[ phyrf_regulatory.c : 1443 ] Invalid country code. Setting to "US". 
5595,,[ phyrf_regulatory.c : 1528 ] Invalid country_code/domain_code. No currentRD or ctl value change. 
5594,,[ phyrf_regulatory.c : 1551 ] neither OTP nor BDF valid value for country_code/domain_code. 
5593,iiiiii,[ phyrf_regulatory.c : 215 ] RegDB 2G-Rule%d start %d end %d max_bw %d reg_power %d flags %d
 
5592,iiiiii,[ phyrf_regulatory.c : 243 ] RegDB 5G-Rule%d start %d end %d max_bw %d reg_power %d flags %d
 
5591,ii,[ phyrf_regulatory.c : 338 ] RegDB 6G Getting Rules dmn_id %d num_rules %d
 
5590,iiiiiii,[ phyrf_regulatory.c : 349 ] RegDB 6G-Rule%d start %d end %d max_bw %d tx_power_eirp %d max_psd_eirp %d flags %d
 
5663,ii,[ phyrf_reset.c : 2665 ] phyrf_reset_EnableCUDss: Enable DSS always... g_cudss_enable %d wlan driver mode %d 
5662,iiii,[ phyrf_reset.c : 2678 ] phyrf_reset_EnableCUDss: enable %d g_cudss_enable %d wlan driver mode %d isHomeChan %d 
5661,iI,[ phyrf_reset.c : 2821 ] phyrf_reset_EnableOCL_on_Flag: phyId=%d, ocl_flag = 0x%x 
5660,iii,[ phyrf_reset.c : 606 ] DumpTpc-3: set trasmit chan power: %d, forced: %d, max tx: %d 
5659,iIii,[ phyrf_reset.c : 1137 ] [phyId=%d]HALPHY_RESET_SETUP: Reset cause is 0x%x, bHomeChan=%d, ScanTPC channel=%d 
5658,i,[ phyrf_reset.c : 1154 ] [phyId=%d]HALPHY_RESET_SETUP 6G tx power update for home channel
 
5657,iiiii,[ phyrf_reset.c : 1210 ] DumpTpc-5: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d, curChan->max_tx_power: %d 
5656,II,[ phyrf_reset.c : 3102 ] PowerMode setting for phyId : 0x%x, value : 0x%x 
5655,,[ phyrf_reset.c : 741 ] phyrf_reset_SetHomeChannel: wrong channel context received and cannot be recovered from known failing patterns.. 
5654,iiiii,[ phyrf_reset.c : 440 ] DumpTpc-1: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d, limit: %d 
5653,iiii,[ phyrf_reset.c : 406 ] DumpTpc-4: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d 
5652,iiii,[ phyrf_reset.c : 864 ] DumpTpc-4: set trasmit chan power: %d, 2g limit: %d, 5g limit: %d, max tx: %d 
5667,,[ phyrf_spectral.c : 305 ] SSCAN: Activating spectral scan  
5666,,[ phyrf_spectral.c : 325 ] SSCAN: Deactivating spectral scan  
5665,,[ phyrf_spectral.c : 226 ] SSCAN: Enabling spectral scan  
5664,,[ phyrf_spectral.c : 349 ] SSCAN: Resetting spectral scan  
5751,,[ phyrf_tpc.c : 1100 ] TAS OL 500ms Timer handler 
5750,IiII,[ phyrf_tpc.c : 1710 ] addr %p len %d addr[0] %02x, addr[1] %02x 
5749,,[ phyrf_tpc.c : 1722 ] AAA 
5748,iiII,[ phyrf_tpc.c : 1724 ] iAG %d binIndex %d First %lld, ReserveLinear %lld 
5747,ii,[ phyrf_tpc.c : 1470 ] TAS OL phyrf_tpc_GetExposureBinSize: country_code=%d, isWorldMode=%d 
5746,i,[ phyrf_tpc.c : 1642 ] Get From BDF Reserve Margin %d 
5745,iiiiiiii,[ phyrf_tpc.c : 1604 ] TAS OL INIT reservemargindB %d numOfAGs %d exposureBinSize %d toleranceX100 %d peak_exposure_mode %d OLperiod %d capLimit %d peakLimit %d 
5744,iii,[ phyrf_tpc.c : 1605 ] TAS OL INIT Current Index %d CurrentOccupancy %d isBufferFull %d 
5743,iiiiiiii,[ phyrf_tpc.c : 1606 ] TAS OL INIT Current State %d Next State %d LastOLRunTime %d lastOLSleepTime %d lastReportUpdate %d numSleepCycles %d isTimerActive %d lastOlTimerExpiry %d 
5742,i,[ phyrf_tpc.c : 2329 ] phyrf_tpc_NormCombPwrReport, x_ms %d 
5741,,[ phyrf_tpc.c : 2356 ] error, sar_table is NULL 
5740,iiii,[ phyrf_tpc.c : 2360 ] DSI %d,sar_table %d %d %d 
5739,IIii,[ phyrf_tpc.c : 2392 ] accDuration %lu accMimoDuration %lu, AG chain0 %d chain1 %d 
5738,iiiIIIII,[ phyrf_tpc.c : 2393 ] band_%d_chain_%d is AG%d,(A_UINT32)watt %ld accEnergy %llu accMimoEnergy %llu chain_temp %llu chain_mimo_temp %llu 
5737,iii,[ phyrf_tpc.c : 2408 ] phyrf_tpc_NormCombPwrReport: totalAG %d %d %d 
5736,i,[ phyrf_tpc.c : 2449 ] SmartTxClearDcf:%d 
5735,i,[ phyrf_tpc.c : 1658 ] phyrf_tpc_SetPeakLimit Peak Limit %d 
5734,III,[ phyrf_tpc.c : 366 ] %s:chan 0x%x  flag:0x%x
 
5733,ii,[ phyrf_tpc.c : 1633 ] phyrf_tpc_SetReserveMarginDb Reserve Margin %d reserveMarginLinear %d 
5732,,[ phyrf_tpc.c : 1120 ] TAS OL phyrf_tpc_TASOLNonWOWAwake 
5731,,[ phyrf_tpc.c : 1148 ] TAS OL phyrf_tpc_TASOLNonWOWSleep 
5730,i,[ phyrf_tpc.c : 1159 ] TAS OL NonWOWSleep currentTime %d  
5729,,[ phyrf_tpc.c : 1167 ] TAS OL phyrf_tpc_TASOLNonWOWWakeup 
5728,iiiii,[ phyrf_tpc.c : 1207 ] TAS OL remainingTimeInCurrentBin %d currentTime %d currentBinStartingTime %d numSleepCycles %d numCyclesAfterOLRun %d 
5727,iiii,[ phyrf_tpc.c : 879 ] TAS OL latestAGkReport[%d] %d  gPhyRfTASOLBufferStruct.currentIndex %d Buffer %d  
5726,iiiiii,[ phyrf_tpc.c : 902 ] TAS OL currentTime %d isPartialReport %d CurrentIndex %d CurrentOccupancy %d isBufferFull %d isFirstReportInBin %d 
5725,ii,[ phyrf_tpc.c : 1430 ] phyrf_tpc_TASOLProcessSleepWakeup Updating sleepstate for PHY %d sleepState %d 
5724,,[ phyrf_tpc.c : 1461 ] phyrf_tpc_TASOLProcessSleepWakeup Triggering the temp timer 
5723,,[ phyrf_tpc.c : 1433 ] phyrf_tpc_TASOLProcessSleepWakeup DUT in WOW mode. not processing sleep/wake 
5722,iii,[ phyrf_tpc.c : 1439 ] Temp timer handler PhyId %d sleep %d numPhy %d  
5721,i,[ phyrf_tpc.c : 1441 ] Temp timer handler Sleepstate %d 
5720,,[ phyrf_tpc.c : 1400 ] phyrf_tpc_TASOLProcessWOWState DUT is already in WOW mode 
5719,ii,[ phyrf_tpc.c : 1416 ] phyrf_tpc_TASOLProcessWOWState WowState : %d gPhyrfTASOLState.nextState : %d 
5718,,[ phyrf_tpc.c : 1683 ] phyrf_tpc_TASOLRegisterTimer : Timer is Armed 
5717,,[ phyrf_tpc.c : 1687 ] phyrf_tpc_TASOLRegisterTimer : Timer is NULL 
5716,iiiiii,[ phyrf_tpc.c : 1512 ] phyrf_tpc_TASOLReset gPhyRfTASOLBufferStruct Current Index %d CurrentOccupancy %d isBufferFull %d, gPhyRfTASOLParams.numOfAGs %d, peak_exposure_mode %d, exposureBinSize %d 
5715,,[ phyrf_tpc.c : 1549 ] phyrf_tpc_TASOLReset : Timer is Armed 
5714,,[ phyrf_tpc.c : 1554 ] phyrf_tpc_TASOLReset : Timer is NULL 
5713,iiiiiiii,[ phyrf_tpc.c : 1557 ] TAS OL RESET reservemargindB %d numOfAGs %d exposureBinSize %d toleranceX100 %d peak_exposure_mode %d OLperiod %d capLimit %d peakLimit %d 
5712,iii,[ phyrf_tpc.c : 1558 ] TAS OL RESET Current Index %d CurrentOccupancy %d isBufferFull %d 
5711,iiiiiiii,[ phyrf_tpc.c : 1559 ] TAS OL RESET Current State %d Next State %d LastOLRunTime %d lastOLSleepTime %d lastReportUpdate %d numSleepCycles %d isTimerActive %d lastOlTimerExpiry %d 
5710,i,[ phyrf_tpc.c : 1776 ] phyrf_tpc_TASOLRestorePowerHistory, timeDiff %d 
5709,,[ phyrf_tpc.c : 1778 ] TAS not enable 
5708,Ii,[ phyrf_tpc.c : 1784 ] Get Memory Fail. addr %p len %d 
5707,ii,[ phyrf_tpc.c : 1789 ] phyrf_tpc_TASOLRestorePowerHistory, timeDiff %d offset %d 
5706,i,[ phyrf_tpc.c : 1794 ] offset > gPhyRfTASOLParams.exposureBinSize %d 
5705,iiii,[ phyrf_tpc.c : 1799 ] Before restore power history: gPhyRfTASOLBufferStruct Current Index %d CurrentOccupancy %d isBufferFull %d, gPhyRfTASOLParams.numOfAGs %d 
5704,iiii,[ phyrf_tpc.c : 1810 ] After restore power histroy: gPhyRfTASOLBufferStruct Current Index %d CurrentOccupancy %d isBufferFull %d, gPhyRfTASOLParams.numOfAGs %d,  
5703,ii,[ phyrf_tpc.c : 1811 ] exposureBinSize %d gPhyRfTASOLParams.exposureBinSize %d 
5702,iiii,[ phyrf_tpc.c : 1844 ] After Clear some Power History for offset: gPhyRfTASOLBufferStruct Current Index %d CurrentOccupancy %d isBufferFull %d, gPhyRfTASOLParams.numOfAGs %d 
5701,Iii,[ phyrf_tpc.c : 944 ] TAS OL Read Buffer idx %u AG 0 : %d AG 1 : %d 
5700,,[ phyrf_tpc.c : 955 ] Sum Above Reserve is negative 
5699,IIIIIIII,[ phyrf_tpc.c : 982 ] TAS OL Before calculation sumAboveReserve[0] : lsb 0x%x msb 0x%x sumAboveReserve[1] : lsb 0x%x msb 0x%x sumExposureBin[0] : lsb 0x%x msb 0x%x sumExposureBin[1] : lsb 0x%x msb 0x%x 
5698,II,[ phyrf_tpc.c : 991 ] TAS OL Before calculation allowedMarginAboveReserve[iAG] : lsb 0x%x msb 0x%x 
5697,iI,[ phyrf_tpc.c : 997 ] Original smartTxILParams->norm_total_expo_AGk_limit[%d] :%u 
5696,ii,[ phyrf_tpc.c : 1002 ] Peak Limit smartTxILParams->norm_total_expo_AGk_limit[%d] :%d 
5695,ii,[ phyrf_tpc.c : 1015 ] Cap Limit smartTxILParams->norm_total_expo_AGk_limit[%d] :%d 
5694,iiII,[ phyrf_tpc.c : 1028 ] Compliance failed norm_total_expo_AGk_limit[%d] : %d temp : lsb0 0x%x msb0 0x%x 
5693,iiIIIIi,[ phyrf_tpc.c : 1040 ] AG %d TAS OL Final norm_total_expo_AGk_limit[iAG] : %d sumAboveReserve[iAG] : lsb 0x%x msb 0x%x allowedMarginAboveReserve[iAG] : lsb 0x%x msb 0x%x currentTime : %d 
5692,iII,[ phyrf_tpc.c : 951 ] Sum Above Reserve iAG %d  First %lld, Second %lld 
5691,,[ phyrf_tpc.c : 1736 ] TAS not enable 
5690,Ii,[ phyrf_tpc.c : 1743 ] Get Memory Fail. addr %p len %d 
5689,i,[ phyrf_tpc.c : 1747 ] phyrf_tpc_TASOLSavePowerHistory remote addr length %d 
5688,iiiiiiiii,[ phyrf_tpc.c : 1056 ] TAS OL Before Current State %d Next State %d LastOLRunTime %d lastOLSleepTime %d lastReportUpdate %d numSleepCycles %d numCyclesAfterOlrun %d isTimerActive %d lastOlTimerExpiry %d 
5687,iiiiiiii,[ phyrf_tpc.c : 1057 ] TAS OL Before reservemargin %d numOfAGs %d exposureBinSize %d toleranceX100 %d peak_exposure_mode %d OLperiod %d capLimit %d peakLimit %d 
5686,iii,[ phyrf_tpc.c : 1058 ] TAS OL Before CurrentIndex %d CurrentOccupancy %d isBufferFull %d 
5685,iiiiiiiii,[ phyrf_tpc.c : 1088 ] TAS OL After Current State %d Next State %d LastOLRunTime %d lastOLSleepTime %d lastReportUpdate %d numSleepCycles %d numCyclesAfterOlrun %d isTimerActive %d lastOlTimerExpiry %d 
5684,iiiiiiii,[ phyrf_tpc.c : 1089 ] TAS OL After reservemargin %d numOfAGs %d exposureBinSize %d toleranceX100 %d peak_exposure_mode %d OLperiod %d capLimit %d peakLimit %d 
5683,iii,[ phyrf_tpc.c : 1090 ] TAS OL After CurrentIndex %d CurrentOccupancy %d isBufferFull %d 
5682,,[ phyrf_tpc.c : 1236 ] TAS OL phyrf_tpc_TASOLWOWEntry 
5681,iiii,[ phyrf_tpc.c : 1269 ] TAS OL phyrf_tpc_TASOLWOWEntry Entering WOW mode when TAS OL is in sleep sleepingPhys %d currentTime %d lastOlTimerExpiry %d numCyclesAfterOLRun %d 
5680,,[ phyrf_tpc.c : 1296 ] TAS OL phyrf_tpc_TASOLWOWExit 
5679,iiiii,[ phyrf_tpc.c : 1324 ] TAS OL remainingTimeInCurrentBin %d currentTime %d currentBinStartingTime %d numSleepCycles %d numCyclesAfterOLRun %d  
5678,iiii,[ phyrf_tpc.c : 1353 ] TAS OL TASOL WOW Exit. Setting the current state to TAS_OL_NON_WOW_SLEEP as all PHYs are in sleep sleepingPhys %d nextState %d currentState %d isOlTimerActive %d 
5677,,[ phyrf_tpc.c : 1380 ] TAS OL phyrf_tpc_TASOLWlanOff 
5676,II,[ phyrf_tpc.c : 2428 ] accDuration %lu accMimoDuration %lu 
5675,iiiIIiii,[ phyrf_tpc.c : 2429 ] phyrf_tpc_UpdateDutyCyclePower band %d/chain %d: dc %d%% last_dcf %d, dcf %d Pdc %d 
5674,ii,[ phyrf_tpc.c : 2072 ] ##Chan %d CalDB Ferq%d
 
5673,i,[ phyrf_tpc.c : 2109 ] clpcError got negative value %d, need to covent it to int value. 
5672,iii,[ phyrf_tpc.c : 2113 ] phyId %d chain %d: got clpcError %d  
5671,iiiii,[ phyrf_tpc.c : 2127 ] txGainIdx = %d, measPwr =%d, dacGain = %d, minDacGain = %d, numGlutEntries = %d 
5670,ii,[ phyrf_tpc.c : 2131 ] nextMeasPwr = %d, minDacgainMargin= %d 
5669,iiiIiiiii,[ phyrf_tpc.c : 2139 ] ch %d, pwr %d, dGain %d, gIdx %x, minDG %d maxDG %d tpcError %d minTxPwr[%d] %d 
5668,,[ phyrf_tpc.c : 1111 ] TAS OL temp Timer handler 
5761,iii,[ phyrf_bdf_tpc.c : 1219 ]  phyrf_tpc_device_ClpcPlutAlutUpdate tpcPowerOffset[%d] %d twoPtOffset[cmask] %d 
5760,ii,[ phyrf_bdf_tpc.c : 1531 ] Copy FCS0 GLUT to FCS1 GLUT. cur_tbl_idx=%d bHomeChan=%d 
5759,iiiii,[ phyrf_bdf_tpc.c : 221 ] return from phyrf_tpc_device_AlutGeneration as pdadc meas seems to be zero %d %d %d %d %d 
5758,ii,[ phyrf_bdf_tpc.c : 388 ] : tmp_32thdB = %d tmp_32thdB = %d 
5757,iiiiiii,[ phyrf_bdf_tpc.c : 326 ] calPerPointClpc[0].meas_pwr %d measPwrDelta %d pdadcTargetHiBackOff %d targetIdxLo_1dB %d targetIdxHi_1dB %d target_lo_8thdB_atMinPdadc %d target_hi_8thdB %d 
5756,iiiiiiii,[ phyrf_bdf_tpc.c : 328 ] pout_lo %d pout_hi %d tbl_10log10[%d] %d tbl_10log10[%d] %d tbl_10log10[%d] %d 
5755,ii,[ phyrf_bdf_tpc.c : 843 ] ##TPC_DBG: GVC Chan %d CalDB %d
 
5754,ii,[ phyrf_bdf_tpc.c : 848 ] ##TPC_DBG: sec80 Chan %d sec80 CalDB %d
 
5753,i,[ phyrf_bdf_tpc.c : 936 ] GLUT_PROG_ERROR: pRawCalPerPointOlpcGtxExt was unexpectedly NULL, last 2 entries of GLUT NOT BEING PROGRAMMED maxGlutIdx = %d 
5752,Iiiiii,[ phyrf_bdf_tpc.c : 1040 ] ##GVC0 chIDX %lu, pwr %d, dGain %d, gIdx %d, paCfg %d, maxGlutIdx %d 
 
5869,I,[ hca_HwComponentRf_bdf_v1.cpp : 88 ] %s NOT available
 
5868,I,[ hca_HwComponentRf_bdf_v1.cpp : 38 ] %s NOT available
 
5867,I,[ hca_HwComponentRf_bdf_v1.cpp : 96 ] %s NOT available
 
5866,I,[ hca_HwComponentRf_bdf_v1.cpp : 79 ] %s NOT available
 
5865,I,[ hca_HwComponentRf_bdf_v1.cpp : 115 ] %s NOT available
 
5864,I,[ hca_HwComponentRf_bdf_v1.cpp : 70 ] %s NOT available
 
5863,I,[ hca_HwComponentRf_bdf_v1.cpp : 60 ] %s NOT available
 
5862,I,[ hca_HwComponentRf_bdf_v1.cpp : 77 ] %s NOT available
 
5861,I,[ hca_HwComponentRf_bdf_v1.cpp : 64 ] %s NOT available
 
5860,I,[ hca_HwComponentRf_bdf_v1.cpp : 71 ] %s NOT available
 
5859,I,[ hca_HwComponentRf_bdf_v1.cpp : 89 ] %s NOT available
 
5858,I,[ hca_HwComponentRf_bdf_v1.cpp : 76 ] %s NOT available
 
5857,I,[ hca_HwComponentRf_bdf_v1.cpp : 105 ] %s NOT available
 
5856,I,[ hca_HwComponentRf_bdf_v1.cpp : 133 ] %s NOT available
 
5855,I,[ hca_HwComponentRf_bdf_v1.cpp : 91 ] %s NOT available
 
5854,I,[ hca_HwComponentRf_bdf_v1.cpp : 75 ] %s NOT available
 
5853,I,[ hca_HwComponentRf_bdf_v1.cpp : 45 ] %s NOT available
 
5852,I,[ hca_HwComponentRf_bdf_v1.cpp : 95 ] %s NOT available
 
5851,I,[ hca_HwComponentRf_bdf_v1.cpp : 51 ] %s NOT available
 
5850,I,[ hca_HwComponentRf_bdf_v1.cpp : 40 ] %s NOT available
 
5849,I,[ hca_HwComponentRf_bdf_v1.cpp : 65 ] %s NOT available
 
5848,I,[ hca_HwComponentRf_bdf_v1.cpp : 81 ] %s NOT available
 
5847,I,[ hca_HwComponentRf_bdf_v1.cpp : 78 ] %s NOT available
 
5846,I,[ hca_HwComponentRf_bdf_v1.cpp : 92 ] %s NOT available
 
5845,I,[ hca_HwComponentRf_bdf_v1.cpp : 101 ] %s NOT available
 
5844,I,[ hca_HwComponentRf_bdf_v1.cpp : 69 ] %s NOT available
 
5843,I,[ hca_HwComponentRf_bdf_v1.cpp : 100 ] %s NOT available
 
5842,I,[ hca_HwComponentRf_bdf_v1.cpp : 99 ] %s NOT available
 
5841,I,[ hca_HwComponentRf_bdf_v1.cpp : 116 ] %s NOT available
 
5840,I,[ hca_HwComponentRf_bdf_v1.cpp : 132 ] %s NOT available
 
5839,I,[ hca_HwComponentRf_bdf_v1.cpp : 73 ] %s NOT available
 
5838,I,[ hca_HwComponentRf_bdf_v1.cpp : 39 ] %s NOT available
 
5837,I,[ hca_HwComponentRf_bdf_v1.cpp : 50 ] %s NOT available
 
5836,I,[ hca_HwComponentRf_bdf_v1.cpp : 80 ] %s NOT available
 
5835,I,[ hca_HwComponentRf_bdf_v1.cpp : 63 ] %s NOT available
 
5834,I,[ hca_HwComponentRf_bdf_v1.cpp : 55 ] %s NOT available
 
5833,I,[ hca_HwComponentRf_bdf_v1.cpp : 46 ] %s NOT available
 
5832,I,[ hca_HwComponentRf_bdf_v1.cpp : 67 ] %s NOT available
 
5831,I,[ hca_HwComponentRf_bdf_v1.cpp : 74 ] %s NOT available
 
5830,I,[ hca_HwComponentRf_bdf_v1.cpp : 44 ] %s NOT available
 
5829,I,[ hca_HwComponentRf_bdf_v1.cpp : 68 ] %s NOT available
 
5828,I,[ hca_HwComponentRf_bdf_v1.cpp : 42 ] %s NOT available
 
5827,I,[ hca_HwComponentRf_bdf_v1.cpp : 58 ] %s NOT available
 
5826,I,[ hca_HwComponentRf_bdf_v1.cpp : 102 ] %s NOT available
 
5825,I,[ hca_HwComponentRf_bdf_v1.cpp : 41 ] %s NOT available
 
5824,I,[ hca_HwComponentRf_bdf_v1.cpp : 90 ] %s NOT available
 
5823,I,[ hca_HwComponentRf_bdf_v1.cpp : 57 ] %s NOT available
 
5822,I,[ hca_HwComponentRf_bdf_v1.cpp : 56 ] %s NOT available
 
5821,I,[ hca_HwComponentRf_bdf_v1.cpp : 110 ] %s NOT available
 
5820,I,[ hca_HwComponentRf_bdf_v1.cpp : 103 ] %s NOT available
 
5819,I,[ hca_HwComponentRf_bdf_v1.cpp : 61 ] %s NOT available
 
5818,I,[ hca_HwComponentRf_bdf_v1.cpp : 93 ] %s NOT available
 
5817,I,[ hca_HwComponentRf_bdf_v1.cpp : 43 ] %s NOT available
 
5816,I,[ hca_HwComponentRf_bdf_v1.cpp : 107 ] %s NOT available
 
5815,I,[ hca_HwComponentRf_bdf_v1.cpp : 114 ] %s NOT available
 
5814,I,[ hca_HwComponentRf_bdf_v1.cpp : 111 ] %s NOT available
 
5813,I,[ hca_HwComponentRf_bdf_v1.cpp : 106 ] %s NOT available
 
5812,I,[ hca_HwComponentRf_bdf_v1.cpp : 47 ] %s NOT available
 
5811,I,[ hca_HwComponentRf_bdf_v1.cpp : 48 ] %s NOT available
 
5810,I,[ hca_HwComponentRf_bdf_v1.cpp : 109 ] %s NOT available
 
5809,I,[ hca_HwComponentRf_bdf_v1.cpp : 82 ] %s NOT available
 
5808,I,[ hca_HwComponentRf_bdf_v1.cpp : 83 ] %s NOT available
 
5807,I,[ hca_HwComponentRf_bdf_v1.cpp : 122 ] %s NOT available
 
5806,I,[ hca_HwComponentRf_bdf_v1.cpp : 130 ] %s NOT available
 
5805,I,[ hca_HwComponentRf_bdf_v1.cpp : 72 ] %s NOT available
 
5804,I,[ hca_HwComponentRf_bdf_v1.cpp : 104 ] %s NOT available
 
5803,I,[ hca_HwComponentRf_bdf_v1.cpp : 123 ] %s NOT available
 
5802,I,[ hca_HwComponentRf_bdf_v1.cpp : 85 ] %s NOT available
 
5801,I,[ hca_HwComponentRf_bdf_v1.cpp : 112 ] %s NOT available
 
5800,I,[ hca_HwComponentRf_bdf_v1.cpp : 113 ] %s NOT available
 
5799,I,[ hca_HwComponentRf_bdf_v1.cpp : 66 ] %s NOT available
 
5798,I,[ hca_HwComponentRf_bdf_v1.cpp : 62 ] %s NOT available
 
5797,I,[ hca_HwComponentRf_bdf_v1.cpp : 84 ] %s NOT available
 
5796,I,[ hca_HwComponentRf_bdf_v1.cpp : 94 ] %s NOT available
 
5795,I,[ hca_HwComponentRf_bdf_v1.cpp : 108 ] %s NOT available
 
5794,I,[ hca_HwComponentRf_bdf_v1.cpp : 52 ] %s NOT available
 
5793,I,[ hca_HwComponentRf_bdf_v1.cpp : 86 ] %s NOT available
 
5792,I,[ hca_HwComponentRf_bdf_v1.cpp : 59 ] %s NOT available
 
5791,I,[ hca_HwComponentRf_bdf_v1.cpp : 37 ] %s NOT available
 
5787,i,[ hca_HwComponentRf_bdf_v1.cpp : 2541 ] RTT - Invalid preamble: %d; return 0 delays 
5786,iiiiiiii,[ hca_HwComponentRf_bdf_v1.cpp : 2554 ] RTT - phy%d chainNum: %d txRxIdx: %d, dynBw: %d, preamble: %d, heLtf: %d, pktBw: %d, whalRate: %d 
5785,i,[ hca_HwComponentRf_bdf_v1.cpp : 2565 ] RTT - base=%d 
5784,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2569 ] RTT - freq %d, delta=%d 
5783,i,[ hca_HwComponentRf_bdf_v1.cpp : 2575 ] RTT - pri20, delta=%d 
5782,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2583 ] RTT - chain %d delta=%d 
5781,i,[ hca_HwComponentRf_bdf_v1.cpp : 2590 ] RTT - IQ, delta=%d 
5780,i,[ hca_HwComponentRf_bdf_v1.cpp : 2595 ] RTT - LCP, delta=%d 
5779,i,[ hca_HwComponentRf_bdf_v1.cpp : 2606 ] RTT - heavyclip, delta=%d 
5778,i,[ hca_HwComponentRf_bdf_v1.cpp : 2611 ] RTT - DPD PEF, delta=%d 
5777,i,[ hca_HwComponentRf_bdf_v1.cpp : 2616 ] RTT - Tx DAC, delta=%d 
5776,i,[ hca_HwComponentRf_bdf_v1.cpp : 2625 ] RTT - Ti ADC, delta=%d 
5775,i,[ hca_HwComponentRf_bdf_v1.cpp : 2630 ] RTT - VSRC, delta=%d 
5774,i,[ hca_HwComponentRf_bdf_v1.cpp : 2635 ] RTT - spur mit, delta=%d 
5773,,[ hca_HwComponentRf_bdf_v1.cpp : 2644 ] RTT - apply 2G 6us offset
 
5772,i,[ hca_HwComponentRf_bdf_v1.cpp : 2649 ] RTT - delayPs=%d ps 
5771,,[ hca_HwComponentRf_bdf_v1.cpp : 2730 ] NEED to implement GetTpcCalFreq in chip specific class 
5770,,[ hca_HwComponentRf_bdf_v1.cpp : 3456 ] FTM CALDB: Skipping regeneration of CALDB:
 
5769,,[ hca_HwComponentRf_bdf_v1.cpp : 3458 ] FTM CALDB: NOT Skipping regeneration of CALDB:
 
5768,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2512 ] RTT - pktBw %d is not valid in dynamicBw %d 
5767,III,[ hca_HwComponentRf_bdf_v1.cpp : 1912 ] sticky - add 0x%08lx, flag 0x%08lx, val 0x%08lx 
5766,i,[ hca_HwComponentRf_bdf_v1.cpp : 2100 ] returning from phyrf_bdf_GetRxGainCalCfgLocalByBand: %d
 
5765,I,[ hca_HwComponentRf_bdf_v1.cpp : 345 ] WHAL_ERROR_EEPROM_MACADDR - sum = %lx
 
5764,iiii,[ hca_HwComponentRf_bdf_v1.cpp : 2485 ] tempCode ch%d = %d, calTemp %d, tempSlope %d
 
5763,ii,[ hca_HwComponentRf_bdf_v1.cpp : 2489 ] ##########bdf thermCode %d, calTemp %d
 
5762,i,[ hca_HwComponentRf_bdf_v1.cpp : 2493 ] ##########bdf temp slope %d
 
5790,I,[ hca_HwComponentRf_bdf_v1.cpp : 120 ] %s NOT available
 
5789,I,[ hca_HwComponentRf_bdf_v1.cpp : 119 ] %s NOT available
 
5788,I,[ hca_HwComponentRf_bdf_v1.cpp : 146 ] %s NOT available
 
5877,,[ phy_dev_calUtils.c : 273 ] QfpromRead 
5876,IiiI,[ phy_dev_calUtils.c : 286 ] Qfprom_base= 0x%8x row %d isMSB %d addr 0x%8x 
5875,i,[ phy_dev_calUtils.c : 280 ] Invalid QFPROM_ROW[=%d]. 
5874,I,[ phy_dev_calUtils.c : 711 ] before cal, AON_COEX_COEX value is 0x%08x 
5873,I,[ phy_dev_calUtils.c : 254 ] otpRead: otp_read_en = 0x%08x 
5872,i,[ phy_dev_calUtils.c : 259 ] Invalid OTP_WORD[=%d]. 
5871,,[ phy_dev_calUtils.c : 430 ] Recipe failure 
5870,I,[ phy_dev_calUtils.c : 431 ] [trigger_cal Recipe failure=%x] 
5878,iiiiiiii,[ phy_dev_fdmtCombCal.c : 2099 ] Q5_FDMT: eng%d, numTxGains = %d ,numNormRxGains = %d, calRxGainOft = %d, numCalRxGains = %d, freq = %d, bwCode = %d, pwrMask = %d 
5880,i,[ phy_dev_fdmtCore.c : 2489 ] useSingleTap = %d 
5879,ii,[ phy_dev_fdmtCore.c : 1360 ] Q5_FDMT: eng%dRun%d fail !!!
 
5892,,[ phy_dev_NFCal.c : 517 ] phyDevLib_NFCal_enterNFCalMode 
5891,,[ phy_dev_NFCal.c : 531 ] phyDevLib_NFCal_exitNFCalMode 
5890,Ii,[ phy_dev_NFCal.c : 490 ] BW code = %u, NF compensation = %d 
5889,iiii,[ phy_dev_NFCal.c : 498 ] nfCalInput->fixedNFCalPrimary[%d] = %d, nfCalInput->fixedNFCalSecondary[%d] = %d 
5888,iiii,[ phy_dev_NFCal.c : 499 ] phyDevLib_NFCal_forceFixedNFCal priNFCalValDb2[%d] = %d secNFCalValDb2[%d] = %d 
5887,Ii,[ phy_dev_NFCal.c : 354 ] NFCal: pNFCalValues[0] result = %x, ch0_NF=%d 
5886,Ii,[ phy_dev_NFCal.c : 355 ] NFCal: pNFCalValues[1] result = %x, ch1_NF=%d 
5885,,[ phy_dev_NFCal.c : 69 ] ======================phyForceFixedNFCal_qca649x starts here=================== 
5884,,[ phy_dev_NFCal.c : 43 ] ======================phyNFCal_qca649x=================== 
5883,i,[ phy_dev_NFCal.c : 60 ] phyNFCal: Noise Floor CAL phyId = %d completed 
5882,,[ phy_dev_NFCal.c : 48 ] ======================Entering Force fixed values=================== 
5881,i,[ phy_dev_NFCal.c : 56 ] phyNFCal: Running Noise Floor CAL phyId = %d ... 
6315,i,[ phy_dev_paprd_device.c : 4618 ] -Q5-PAPRD-:channel freq %d 
6314,ii,[ phy_dev_paprd_device.c : 4619 ] -Q5-PAPRD-:txChain %d tableIndex %d 
6313,i,[ phy_dev_paprd_device.c : 4620 ] -Q5-PAPRD-:forced_sq_idx %d 
6312,ii,[ phy_dev_paprd_device.c : 4621 ] -Q5-PAPRD-:sq_idx_sw %d sq_idx_hw %d 
6311,iiiii,[ phy_dev_paprd_device.c : 536 ] Agc2atten phyId %d is2GHz %d txChainMask %d reference Power %d ipa_xcoupler %d  
6310,iiiiii,[ phy_dev_paprd_device.c : 554 ] Agc2atten phyId %d is2GHz %d chainNum %d tx_gain_index %d MeasuredPower %d actual atten %d 
6309,i,[ phy_dev_paprd_device.c : 4895 ] -Q5-PAPRDTUNING-: max_bin  %d 
6308,i,[ phy_dev_paprd_device.c : 4896 ] -Q5-PAPRDTUNING-: base_bin %d 
6307,ii,[ phy_dev_paprd_device.c : 4937 ] -Q5-PAPRDTUNING-: WARMUP: dpdDynDacgain %d, max_dac_gain %d  
6306,ii,[ phy_dev_paprd_device.c : 4945 ] -Q5-PAPRDTUNING-: WARMUP: compression %d/64, new upbound dacgain %d  
6305,,[ phy_dev_paprd_device.c : 4949 ] -Q5-PAPRDTUNING-: WARMUP greater than max_dac_gain 
6304,ii,[ phy_dev_paprd_device.c : 4958 ] -Q5-PAPRDTUNING-: WARMUP: old rxgain %d, new rxgain %d  
6303,iiii,[ phy_dev_paprd_device.c : 4996 ] x_base_bin:%d y_base_bin:%d x_max_bin:%d y_max_bin:%d 
6302,ii,[ phy_dev_paprd_device.c : 4997 ] -Q5-PAPRDTUNING-: bin_idx %d compression %d/64 
6301,ii,[ phy_dev_paprd_device.c : 5020 ] -Q5-PAPRDTUNING-:DPD FAIL. Improper compression. dacgain decrease %d to  %d 
6300,i,[ phy_dev_paprd_device.c : 4778 ] PAPRD: ConfigTempScaling() scaling factor %d 
6299,I,[ phy_dev_paprd_device.c : 4816 ] PHYRF_EDPD_CTRL_6_L_B0 = 0x%x 
6298,I,[ phy_dev_paprd_device.c : 4817 ] PHYRF_EDPD_CTRL_7_L_B0 = 0x%x 
6297,I,[ phy_dev_paprd_device.c : 4818 ] PHYRF_EDPD_CTRL_6_L_B1 = 0x%x 
6296,I,[ phy_dev_paprd_device.c : 4819 ] PHYRF_EDPD_CTRL_7_L_B1 = 0x%x 
6295,I,[ phy_dev_paprd_device.c : 1765 ] -Q5-PAPRDTUNING-:DPD training AGC2 size %x 
6294,I,[ phy_dev_paprd_device.c : 1768 ] -Q5-PAPRDTUNING-:DPD training AGC2 pwr 0x%8x 
6293,I,[ phy_dev_paprd_device.c : 1772 ] -Q5-PAPRDTUNING-:DPD training rx gain idx 0x%x 
6292,I,[ phy_dev_paprd_device.c : 1776 ] -Q5-PAPRDTUNING-:SQ index HW is %u 
6291,iiiii,[ phy_dev_paprd_device.c : 4637 ] phy_paprd_device_GetComplete: phyId %d channel %d, enable %d phyInput CM %d  validmask %d 
6290,II,[ phy_dev_paprd_device.c : 4686 ] --Q5--PAPRD: dpdComplete validmask 0x%lx phyInput->validChainMask 0x%x 
6289,,[ phy_dev_paprd_device.c : 666 ] PAPRD: HWDISABLE ALL 
6288,i,[ phy_dev_paprd_device.c : 647 ] PAPRD: HWDISABLE CHAIN : %d 
6287,I,[ phy_dev_paprd_device.c : 1475 ] PAPRD_CTRL_L_B0 = 0x%x 
6286,I,[ phy_dev_paprd_device.c : 1477 ] PAPRD_VALID_GAIN_L_B0 = 0x%x 
6285,I,[ phy_dev_paprd_device.c : 1479 ] PHYRF_PAPRD_TABLE_TYPE_L_B0 = 0x%x 
6284,I,[ phy_dev_paprd_device.c : 1481 ] PAPRD_CTRL_L_B1 = 0x%x 
6283,I,[ phy_dev_paprd_device.c : 1483 ] PAPRD_VALID_GAIN_L_B1 = 0x%x 
6282,I,[ phy_dev_paprd_device.c : 1485 ] PHYRF_PAPRD_TABLE_TYPE_L_B1 = 0x%x 
6281,I,[ phy_dev_paprd_device.c : 1489 ] CUREENT HW TABLE  = 0x%x 
6280,,[ phy_dev_paprd_device.c : 728 ] MM_PAPRD: HWReset ALL 
6279,i,[ phy_dev_paprd_device.c : 299 ] eDPD SendDpdTrainPkt: %d 
6278,,[ phy_dev_paprd_device.c : 303 ] -Q5-PAPRD-: phy_paprd_device_InitStaticSettings 
6277,i,[ phy_dev_paprd_device.c : 1193 ] -Q5-PAPRDTUNING-:DynBW = %d 
6276,i,[ phy_dev_paprd_device.c : 1216 ] -Q5 - PAPRDTUNING - :min loopback delay = %d 
6275,i,[ phy_dev_paprd_device.c : 1227 ] ADC OVRD VAL : %d 
6274,,[ phy_dev_paprd_device.c : 1289 ] force SQ 
6273,,[ phy_dev_paprd_device.c : 1295 ] NOT force SQ 
6272,I,[ phy_dev_paprd_device.c : 1323 ] -edpdRawData DDR address before alignment = 0x%x 
6271,I,[ phy_dev_paprd_device.c : 1325 ] -edpdRawData DDR address after  alignment = 0x%x 
6270,I,[ phy_dev_paprd_device.c : 1329 ] -edpdRawData DDR address = 0x%x 
6269,I,[ phy_dev_paprd_device.c : 1334 ] -edpdRawData.edpdTrainData = 0x%x 
6268,i,[ phy_dev_paprd_device.c : 1338 ] -edpdRawData.fw_ucode_chunks = %d 
6267,i,[ phy_dev_paprd_device.c : 812 ] ipa_xcoupler=%d 
6266,,[ phy_dev_paprd_device.c : 834 ] ******xPA recipe 
6265,iiI,[ phy_dev_paprd_device.c : 838 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
6264,I,[ phy_dev_paprd_device.c : 847 ] -Q5-PAPRD-: PHYA 5G xPA chain0 gc = 0x%x 
6263,I,[ phy_dev_paprd_device.c : 849 ] -Q5-PAPRD-: PHYA_5G xPA chain1 gc = 0x%x 
6262,,[ phy_dev_paprd_device.c : 858 ] ******iPA_xcoupler recipe 
6261,iiI,[ phy_dev_paprd_device.c : 862 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
6260,I,[ phy_dev_paprd_device.c : 872 ] -Q5-PAPRD-: PHYB_2G xPA chain0 gc = 0x%x 
6259,I,[ phy_dev_paprd_device.c : 874 ] -Q5-PAPRD-: PHYB_2G xPA chain1 gc = 0x%x 
6258,,[ phy_dev_paprd_device.c : 879 ] ******iPA_icoupler recipe 
6257,iiI,[ phy_dev_paprd_device.c : 883 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
6256,I,[ phy_dev_paprd_device.c : 893 ] -Q5-PAPRD-: PHYA 5G iPA chain0 gc = 0x%x 
6255,I,[ phy_dev_paprd_device.c : 895 ] -Q5-PAPRD-: PHYA_5G iPA chain1 gc = 0x%x 
6254,I,[ phy_dev_paprd_device.c : 903 ] -Q5-PAPRD-: chain0 gpo_cfg_per_chain = 0x%x 
6253,I,[ phy_dev_paprd_device.c : 912 ] -Q5-PAPRD-: chain1 gpo_cfg_per_chain = 0x%x 
6252,I,[ phy_dev_paprd_device.c : 921 ] -Q5-PAPRD-: chain3 gpo_cfg_per_chain = 0x%x 
6251,I,[ phy_dev_paprd_device.c : 930 ] PHYA_XFEM_PIN_CFG0-prgm = 0x%x 
6250,I,[ phy_dev_paprd_device.c : 932 ] PHYA_XFEM_GPO_CFG -prgm = 0x%x 
6249,iI,[ phy_dev_paprd_device.c : 937 ] -Q5-PAPRD-: Chain%d Cal Mode = %lu 
6248,iI,[ phy_dev_paprd_device.c : 940 ] -Q5-PAPRD-: Chain%d Cal Mode = %lu 
6247,iiI,[ phy_dev_paprd_device.c : 943 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d DPD_xPA_en = %lu 
6246,,[ phy_dev_paprd_device.c : 959 ] ******xPA recipe 
6245,iiI,[ phy_dev_paprd_device.c : 964 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
6244,I,[ phy_dev_paprd_device.c : 974 ] -Q5-PAPRD-: PHYB_2G xPA chain0 gc = 0x%x 
6243,I,[ phy_dev_paprd_device.c : 976 ] -Q5-PAPRD-: PHYB_2G xPA chain1 gc = 0x%x 
6242,,[ phy_dev_paprd_device.c : 985 ] ******iPA_xcoupler recipe 
6241,iiI,[ phy_dev_paprd_device.c : 989 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
6240,I,[ phy_dev_paprd_device.c : 999 ] -Q5-PAPRD-: PHYB_2G xPA chain0 gc = 0x%x 
6239,I,[ phy_dev_paprd_device.c : 1001 ] -Q5-PAPRD-: PHYB_2G xPA chain1 gc = 0x%x 
6238,,[ phy_dev_paprd_device.c : 1006 ] ******iPA_icoupler recipe 
6237,iiI,[ phy_dev_paprd_device.c : 1010 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d Rx Cal Sub Mode = %lu 
6236,I,[ phy_dev_paprd_device.c : 1020 ] -Q5-PAPRD-: PHYB 2G iPA chain0 gc = 0x%x 
6235,I,[ phy_dev_paprd_device.c : 1022 ] -Q5-PAPRD-: PHYB_2G iPA chain1 gc = 0x%x 
6234,I,[ phy_dev_paprd_device.c : 1030 ] -Q5-PAPRD-: chain0 gpo_cfg_per_chain = 0x%x 
6233,I,[ phy_dev_paprd_device.c : 1039 ] -Q5-PAPRD-: chain1 gpo_cfg_per_chain = 0x%x 
6232,I,[ phy_dev_paprd_device.c : 1061 ] PHYB_XFEM_PIN_CFG0-prgm = 0x%x 
6231,I,[ phy_dev_paprd_device.c : 1063 ] PHYB_XFEM_GPO_CFG -prgm = 0x%x 
6230,iI,[ phy_dev_paprd_device.c : 1079 ] -Q5-PAPRD-: Chain%d Cal Mode = %lu 
6229,iI,[ phy_dev_paprd_device.c : 1082 ] -Q5-PAPRD-: Chain%d Cal Mode = %lu 
6228,iiI,[ phy_dev_paprd_device.c : 1085 ] -Q5-PAPRD-:Chain = %d, dpd Rx loop chain %d DPD_xPA_en = %lu 
6227,,[ phy_dev_paprd_device.c : 1094 ] -Q5-PAPRD-: phy_paprd_device_Iron_programming 
6226,I,[ phy_dev_paprd_device.c : 815 ] icoupler_femCtrl5g_enable = 0x%x 
6225,I,[ phy_dev_paprd_device.c : 816 ] icoupler_femCtrl2g_enable = 0x%x 
6224,I,[ phy_dev_paprd_device.c : 818 ] gpo_cfg = 0x%x 
6223,i,[ phy_dev_paprd_device.c : 820 ] attenBypass %d 
6222,iii,[ phy_dev_paprd_device.c : 3965 ] Populate DPD LUT of Chain %d at table_idx %d paprdType %d 
6221,,[ phy_dev_paprd_device.c : 4018 ] Invalid tableOffset 
6220,,[ phy_dev_paprd_device.c : 4071 ] Invalid tableOffset 
6219,,[ phy_dev_paprd_device.c : 4077 ] Invalid tableType 
6218,iiII,[ phy_dev_paprd_device.c : 4090 ]  populate-PAPRD:tableType: %d tableIdx: %d at even entry: %2d from is : %x 
6217,iiII,[ phy_dev_paprd_device.c : 4092 ]  populate-PAPRD:tableType: %d tableIdx: %d at  odd entry: %2d from is : %x 
6216,,[ phy_dev_paprd_device.c : 4099 ] Start Populated MemoryDPD Table! 
6215,i,[ phy_dev_paprd_device.c : 4103 ] int delay ddr x1 = %d 
6214,i,[ phy_dev_paprd_device.c : 4104 ] int delay ddr x2 = %d 
6213,i,[ phy_dev_paprd_device.c : 4105 ] int delay ddr x3 = %d 
6212,i,[ phy_dev_paprd_device.c : 4106 ] int delay ddr x4 = %d 
6211,i,[ phy_dev_paprd_device.c : 4107 ] int delay ddr x5 = %d 
6210,i,[ phy_dev_paprd_device.c : 4108 ] int delay ddr x6 = %d 
6209,i,[ phy_dev_paprd_device.c : 4111 ]  PAPRD: packed delay_ddr1: %d 
6208,i,[ phy_dev_paprd_device.c : 4115 ]  PAPRD: packed delay_ddr1: %d 
6207,iIi,[ phy_dev_paprd_device.c : 4167 ] Memlut x0_abs_x1 Q base low [%d], address %X, value %d 
6206,iIi,[ phy_dev_paprd_device.c : 4170 ] Memlut x0_abs_x1 Q high [%d], address %X, value %d 
6205,iIi,[ phy_dev_paprd_device.c : 4174 ] Memlut x0_abs_x1 I base low [%d], address %X, value %d 
6204,iIi,[ phy_dev_paprd_device.c : 4177 ] Memlut x0_abs_x1 I high [%d], address %X, value %d 
6203,iIi,[ phy_dev_paprd_device.c : 4182 ] Memlut x1_abs_x1 Q base low [%d], address %X, value %d 
6202,iIi,[ phy_dev_paprd_device.c : 4185 ] Memlut x1_abs_x1 Q high [%d], address %X, value %d 
6201,iIi,[ phy_dev_paprd_device.c : 4189 ] Memlut x1_abs_x1 I base low [%d], address %X, value %d 
6200,iIi,[ phy_dev_paprd_device.c : 4192 ] Memlut x1_abs_x1 I high [%d], address %X, value %d 
6199,iIi,[ phy_dev_paprd_device.c : 4197 ] Memlut x0_abs_x2 Q base low [%d], address %X, value %d 
6198,iIi,[ phy_dev_paprd_device.c : 4200 ] Memlut x0_abs_x2 Q high [%d], address %X, value %d 
6197,iIi,[ phy_dev_paprd_device.c : 4204 ] Memlut x0_abs_x2 I base low [%d], address %X, value %d 
6196,iIi,[ phy_dev_paprd_device.c : 4207 ] Memlut x0_abs_x2 I high [%d], address %X, value %d 
6195,iIi,[ phy_dev_paprd_device.c : 4212 ] Memlut x2_abs_x2 Q base low [%d], address %X, value %d 
6194,iIi,[ phy_dev_paprd_device.c : 4215 ] Memlut x2_abs_x2 Q high [%d], address %X, value %d 
6193,iIi,[ phy_dev_paprd_device.c : 4219 ] Memlut x2_abs_x2 I base low [%d], address %X, value %d 
6192,iIi,[ phy_dev_paprd_device.c : 4222 ] Memlut x2_abs_x2 I high [%d], address %X, value %d 
6191,iIi,[ phy_dev_paprd_device.c : 4227 ] Memlut x0_abs_x3 Q base low [%d], address %X, value %d 
6190,iIi,[ phy_dev_paprd_device.c : 4230 ] Memlut x0_abs_x3 Q high [%d], address %X, value %d 
6189,iIi,[ phy_dev_paprd_device.c : 4234 ] Memlut x0_abs_x3 I base low [%d], address %X, value %d 
6188,iIi,[ phy_dev_paprd_device.c : 4237 ] Memlut x0_abs_x3 I high [%d], address %X, value %d 
6187,iIi,[ phy_dev_paprd_device.c : 4242 ] Memlut x0_abs_x4 Q base low [%d], address %X, value %d 
6186,iIi,[ phy_dev_paprd_device.c : 4245 ] Memlut x0_abs_x4 Q high [%d], address %X, value %d 
6185,iIi,[ phy_dev_paprd_device.c : 4249 ] Memlut x0_abs_x4 I base low [%d], address %X, value %d 
6184,iIi,[ phy_dev_paprd_device.c : 4252 ] Memlut x0_abs_x4 I high [%d], address %X, value %d 
6183,iIi,[ phy_dev_paprd_device.c : 4257 ] Memlut xq0_abs_xq1 Q base low [%d], address %X, value %d 
6182,iIi,[ phy_dev_paprd_device.c : 4260 ] Memlut xq0_abs_xq1 Q high [%d], address %X, value %d 
6181,iIi,[ phy_dev_paprd_device.c : 4264 ] Memlut xq0_abs_xq1 I base low [%d], address %X, value %d 
6180,iIi,[ phy_dev_paprd_device.c : 4267 ] Memlut xq0_abs_xq1 I high [%d], address %X, value %d 
6179,iIi,[ phy_dev_paprd_device.c : 4272 ] Memlut xq2_abs_xq3 Q base low [%d], address %X, value %d 
6178,iIi,[ phy_dev_paprd_device.c : 4275 ] Memlut xq2_abs_xq3 Q high [%d], address %X, value %d 
6177,iIi,[ phy_dev_paprd_device.c : 4279 ] Memlut xq2_abs_xq3 I base low [%d], address %X, value %d 
6176,iIi,[ phy_dev_paprd_device.c : 4282 ] Memlut xq2_abs_xq3 I high [%d], address %X, value %d 
6175,iIi,[ phy_dev_paprd_device.c : 4287 ] Memlut xq4_abs_xq5 Q base low [%d], address %X, value %d 
6174,iIi,[ phy_dev_paprd_device.c : 4290 ] Memlut xq4_abs_xq5 Q high [%d], address %X, value %d 
6173,iIi,[ phy_dev_paprd_device.c : 4294 ] Memlut xq4_abs_xq5 I base low [%d], address %X, value %d 
6172,iIi,[ phy_dev_paprd_device.c : 4297 ] Memlut xq4_abs_xq5 I high [%d], address %X, value %d 
6171,iIi,[ phy_dev_paprd_device.c : 4302 ] Memlut xq6_abs_xq7 Q base low [%d], address %X, value %d 
6170,iIi,[ phy_dev_paprd_device.c : 4305 ] Memlut xq6_abs_xq7 Q high [%d], address %X, value %d 
6169,iIi,[ phy_dev_paprd_device.c : 4309 ] Memlut xq6_abs_xq7 Q base low [%d], address %X, value %d 
6168,iIi,[ phy_dev_paprd_device.c : 4312 ] Memlut xq6_abs_xq7 Q high [%d], address %X, value %d 
6167,,[ phy_dev_paprd_device.c : 4340 ] Invalid tableOffset 
6166,,[ phy_dev_paprd_device.c : 4369 ] Invalid tableOffset 
6165,,[ phy_dev_paprd_device.c : 4379 ] Finished populating DPD LUT into memory! 
6164,,[ phy_dev_paprd_device.c : 1993 ] -Q5-PAPRD-:Read back DPD training data from memory: 
6163,ii,[ phy_dev_paprd_device.c : 1994 ] -Q5-PAPRD-:Raw Data: chain %d table %d 
6162,,[ phy_dev_paprd_device.c : 1995 ] -Q5-PAPRD-:DpdTrainData0	  DpdTrainData1	 DpdTrainData2	 DpdTrainData3 
6161,IIIII,[ phy_dev_paprd_device.c : 1998 ] -Q5-PAPRD-[%2u]:%8u	 %8u	 %8u	 %8u 
6160,iiiiii,[ phy_dev_paprd_device.c : 616 ] ReadGlut table_offset %d tpc_index %d TPC_GLUT_INIT/LAST_IDX_DPDTRAIN %d dpd_glut_end_idx %d fcs_sec_offset %d, tx_gain_idx %d 
6159,i,[ phy_dev_paprd_device.c : 622 ] Invalid txgain_idx_cal value = %d (expect 0..63) 
6158,ii,[ phy_dev_paprd_device.c : 625 ] phy_paprd_device_ReadGlut. glutIndx %d, powerMeasured get from glut: %d 
6157,iiIIi,[ phy_dev_paprd_device.c : 632 ] MM_PAPRD:Chain = %d, tpc_index = %d, table_offset = %lu, glut_idx_offset = %lx, txgain_index = %d 
6156,,[ phy_dev_paprd_device.c : 1403 ] -Q5-PAPRD-: phy_paprd_device_ResetPaprdTraining 
6155,I,[ phy_dev_paprd_device.c : 4510 ] PHYA_XFEM_PIN_CFG0-restore = 0x%x 
6154,I,[ phy_dev_paprd_device.c : 4512 ] PHYA_XFEM_GPO_CFG -restore = 0x%x 
6153,I,[ phy_dev_paprd_device.c : 4521 ] PHYB_XFEM_PIN_CFG0-restore = 0x%x 
6152,I,[ phy_dev_paprd_device.c : 4523 ] PHYB_XFEM_GPO_CFG -restore = 0x%x 
6151,I,[ phy_dev_paprd_device.c : 4551 ] PHYB_IRON2G_RFA_WL_TXFE_2G_CH0_WL_TXFE_OV2-restore = 0x%x 
6150,I,[ phy_dev_paprd_device.c : 4555 ] PHYB_IRON2G_RFA_WL_TXFE_2G_CH1_WL_TXFE_OV2-restore = 0x%x 
6149,I,[ phy_dev_paprd_device.c : 4565 ] Restore-GCC_EDPD_AXI_CBCR=0x%x 
6148,I,[ phy_dev_paprd_device.c : 4567 ] Restore-GCC_PCNOC_EDPD_AHB_CBCR=0x%x 
6147,i,[ phy_dev_paprd_device.c : 1507 ] -Q5-PAPRD : StopTraining for Chain = %d 
6146,I,[ phy_dev_paprd_device.c : 1868 ] -Q5-PAPRD-:Dispersion value at SQ Stage2 (minimum index - 1) = %u 
6145,I,[ phy_dev_paprd_device.c : 1869 ] -Q5-PAPRD-:Dispersion value at SQ Stage2 (minimum index + 1) = %u 
6144,iiii,[ phy_dev_paprd_device.c : 1918 ] -Q5-PAPRD-: In training signal quality --- Bin idx %d -- accum count = %d, X value = %d, Average X = %d 
6143,i,[ phy_dev_paprd_device.c : 1926 ] -Q5-PAPRD-:Max value of Averaged X = %d 
6142,iiii,[ phy_dev_paprd_device.c : 1946 ] -Q5-PAPRD-:Bin %d chk_acc = %d, cnt = %d, diffn = %d 
6141,i,[ phy_dev_paprd_device.c : 1951 ] -Q5-PAPRD-: Averaged SQ value is %d 
6140,i,[ phy_dev_paprd_device.c : 1599 ] PAPRD:paprdpaprd_done time %d 
6139,iIi,[ phy_dev_paprd_device.c : 1633 ] -Q5-PAPRDTUNING-:sq PASS: sq_idx_sw %d sq_idx_hw %ld force_sq_idx %d 
6138,iiIi,[ phy_dev_paprd_device.c : 1639 ] -Q5-PAPRDTUNING-:sq FAIL : %d sq_idx_sw %d sq_idx_hw %ld force_sq_idx %d 
6137,,[ phy_dev_paprd_device.c : 1646 ] -Q5-PAPRD-:DPD training Failed. Paprd Done bit is not set in HW! 
6136,,[ phy_dev_paprd_device.c : 1420 ] -Q5-PAPRD-: phy_paprd_device_XmitTrainningFrame 
6135,i,[ phy_dev_paprd_device.c : 3595 ] paprdType %d 
6134,,[ phy_dev_paprd_device.c : 3665 ] Invalid tableOffset 
6133,,[ phy_dev_paprd_device.c : 3718 ] Invalid tableOffset 
6132,,[ phy_dev_paprd_device.c : 3724 ] Invalid tableType 
6131,iIIII,[ phy_dev_paprd_device.c : 3728 ] MM_ctrl_restore_FCS: %d paprdCtrl_0: 0x%x paprdCtrl_1: 0x%x paprdCtrl_2: 0x%x paprdCtrl_3: 0x%x 
6130,,[ phy_dev_paprd_device.c : 3491 ] Invalid tableOffset 
6129,,[ phy_dev_paprd_device.c : 3534 ] Invalid tableOffset 
6128,,[ phy_dev_paprd_device.c : 3540 ] Invalid tableType 
6127,iIIII,[ phy_dev_paprd_device.c : 3543 ] MM_ctrl_save_FCS: %d paprdCtrl_0: 0x%x paprdCtrl_1: 0x%x paprdCtrl_2: 0x%x paprdCtrl_3: 0x%x 
6126,iI,[ phy_dev_paprd_device.c : 2872 ] Populate DPD LUT of Chain %d at table_idx %hhu 
6125,i,[ phy_dev_paprd_device.c : 2874 ]  phy_paprd_device_dpd_restore : fcsEnabled %d 
6124,i,[ phy_dev_paprd_device.c : 2875 ]  paprdType %d 
6123,ii,[ phy_dev_paprd_device.c : 2914 ] dump previous version for paprdType logic: suspectpardtype=%d, system paprdType=%d 
6122,iiII,[ phy_dev_paprd_device.c : 2932 ]  restore-PAPRD_register_update:FCS: %d tableIdx: %d at even entry: %2d from is : %x 
6121,iiII,[ phy_dev_paprd_device.c : 2934 ]  restore-PAPRD_register_update:FCS: %d tableIdx: %d at  odd entry: %2d from is : %x 
6120,iiIii,[ phy_dev_paprd_device.c : 2947 ]  restore-PAPRD_from_input_buffer: FCS: %d tableIdx: %d at even entry:  %2d :*((uint32_t *) (tmpDpdStart) + 2 * i )=%d is : %d 
6119,iiIii,[ phy_dev_paprd_device.c : 2949 ]  restore-PAPRD_from_input_buffer: FCS: %d tableIdx: %d at even entry:  %2d :*((uint32_t *) (tmpDpdStart) + 2 * i )=%d is : %d 
6118,i,[ phy_dev_paprd_device.c : 2965 ] phy_dev_MemDPDTrain: hstp_chip_ID: %d 
6117,iiii,[ phy_dev_paprd_device.c : 2974 ]  valid_gain_idx0: %d   gsmall: %d   adaptive_table_valid: %d   paprdType: %d 
6116,I,[ phy_dev_paprd_device.c : 2997 ]  restore-tableOffset: 0x%x 
6115,IIII,[ phy_dev_paprd_device.c : 2998 ]  paprdCtrl_0: 0x%x paprdCtrl_1: 0x%x paprdCtrl_2: 0x%x paprdCtrl_3: 0x%x 
6114,iiii,[ phy_dev_paprd_device.c : 2999 ]  valid_gain_idx0: %d   gsmall: %d   adaptive_table_valid: %d   paprdType: %d 
6113,,[ phy_dev_paprd_device.c : 3052 ] Invalid tableOffset 
6112,,[ phy_dev_paprd_device.c : 3105 ] Invalid tableOffset 
6111,,[ phy_dev_paprd_device.c : 3111 ] Invalid tableType 
6110,iIIII,[ phy_dev_paprd_device.c : 3115 ] MM_restore_FCS: %d paprdCtrl_0: 0x%x paprdCtrl_1: 0x%x paprdCtrl_2: 0x%x paprdCtrl_3: 0x%x 
6109,,[ phy_dev_paprd_device.c : 2213 ] Start Save MemlessDPD Table! 
6108,iII,[ phy_dev_paprd_device.c : 2228 ]  save-PAPRD_coefficient:tableIdx: %d at even entry: %2d from is : %x 
6107,iII,[ phy_dev_paprd_device.c : 2230 ]  save-PAPRD_coefficient:tableIdx: %d at  odd entry: %2d from is : %x 
6106,iiII,[ phy_dev_paprd_device.c : 2234 ]  save_memory-PAPRD:FCS: %d tableIdx: %d at entry: %2d from is : %x 
6105,,[ phy_dev_paprd_device.c : 2240 ] Start Save eDPD Table! 
6104,III,[ phy_dev_paprd_device.c : 2256 ] mem_coef[%ld].real/imag is %f / %f
 
6103,III,[ phy_dev_paprd_device.c : 2257 ] mem_coef[%ld].real/imag is %f / %f
 
6102,,[ phy_dev_paprd_device.c : 2310 ] Invalid tableOffset 
6101,,[ phy_dev_paprd_device.c : 2354 ] Invalid tableOffset 
6100,,[ phy_dev_paprd_device.c : 2360 ] Invalid tableType 
6099,iIIII,[ phy_dev_paprd_device.c : 2363 ] MM_save_FCS: %d paprdCtrl_0: 0x%x paprdCtrl_1: 0x%x paprdCtrl_2: 0x%x paprdCtrl_3: 0x%x 
6098,IIII,[ phy_dev_paprd_device.c : 2366 ]  paprdCtrl_0: 0x%x paprdCtrl_1: 0x%x paprdCtrl_2: 0x%x paprdCtrl_3: 0x%x 
6097,i,[ phy_dev_paprd_device.c : 5941 ]  phy_paprd_device_edpd_coef : cmd %d 
6096,i,[ phy_dev_paprd_device.c : 5947 ]  START EDPD_LUT_TABLES : chain %d 
6095,ii,[ phy_dev_paprd_device.c : 5976 ]  START EDPD_LUT : table %d , iter %d 
6094,,[ phy_dev_paprd_device.c : 5980 ]  0: lut x0_abs_x1 
6093,I,[ phy_dev_paprd_device.c : 5981 ]  0x%x  
6092,I,[ phy_dev_paprd_device.c : 5983 ]  0x%x  
6091,I,[ phy_dev_paprd_device.c : 5985 ]  0x%x  
6090,I,[ phy_dev_paprd_device.c : 5987 ]  0x%x  
6089,,[ phy_dev_paprd_device.c : 5990 ]  1: lut x1_abs_x1 
6088,I,[ phy_dev_paprd_device.c : 5992 ]  0x%x  
6087,I,[ phy_dev_paprd_device.c : 5994 ]  0x%x  
6086,I,[ phy_dev_paprd_device.c : 5996 ]  0x%x  
6085,I,[ phy_dev_paprd_device.c : 5998 ]  0x%x  
6084,,[ phy_dev_paprd_device.c : 6001 ]  2: lut x0_abs_x2 
6083,I,[ phy_dev_paprd_device.c : 6003 ]  0x%x  
6082,I,[ phy_dev_paprd_device.c : 6005 ]  0x%x  
6081,I,[ phy_dev_paprd_device.c : 6007 ]  0x%x  
6080,I,[ phy_dev_paprd_device.c : 6009 ]  0x%x  
6079,,[ phy_dev_paprd_device.c : 6012 ]  3: lut x2_abs_x2 
6078,I,[ phy_dev_paprd_device.c : 6014 ]  0x%x  
6077,I,[ phy_dev_paprd_device.c : 6016 ]  0x%x  
6076,I,[ phy_dev_paprd_device.c : 6018 ]  0x%x  
6075,I,[ phy_dev_paprd_device.c : 6020 ]  0x%x  
6074,,[ phy_dev_paprd_device.c : 6023 ]  4: lut x0_abs_x3 
6073,I,[ phy_dev_paprd_device.c : 6025 ]  0x%x  
6072,I,[ phy_dev_paprd_device.c : 6027 ]  0x%x  
6071,I,[ phy_dev_paprd_device.c : 6029 ]  0x%x  
6070,I,[ phy_dev_paprd_device.c : 6031 ]  0x%x  
6069,,[ phy_dev_paprd_device.c : 6034 ]  5: lut x0_abs_x4 
6068,I,[ phy_dev_paprd_device.c : 6036 ]  0x%x  
6067,I,[ phy_dev_paprd_device.c : 6038 ]  0x%x  
6066,I,[ phy_dev_paprd_device.c : 6040 ]  0x%x  
6065,I,[ phy_dev_paprd_device.c : 6042 ]  0x%x  
6064,,[ phy_dev_paprd_device.c : 6045 ] 6: lut xq0_abs_xq1 
6063,I,[ phy_dev_paprd_device.c : 6047 ]  0x%x  
6062,I,[ phy_dev_paprd_device.c : 6049 ]  0x%x  
6061,I,[ phy_dev_paprd_device.c : 6051 ]  0x%x  
6060,I,[ phy_dev_paprd_device.c : 6053 ]  0x%x  
6059,,[ phy_dev_paprd_device.c : 6056 ] 7: lut xq2_abs_xq3 
6058,I,[ phy_dev_paprd_device.c : 6058 ]  0x%x  
6057,I,[ phy_dev_paprd_device.c : 6060 ]  0x%x  
6056,I,[ phy_dev_paprd_device.c : 6062 ]  0x%x  
6055,I,[ phy_dev_paprd_device.c : 6064 ]  0x%x  
6054,,[ phy_dev_paprd_device.c : 6067 ] 8: lut xq4_abs_xq5 
6053,I,[ phy_dev_paprd_device.c : 6069 ]  0x%x  
6052,I,[ phy_dev_paprd_device.c : 6071 ]  0x%x  
6051,I,[ phy_dev_paprd_device.c : 6073 ]  0x%x  
6050,I,[ phy_dev_paprd_device.c : 6075 ]  0x%x  
6049,,[ phy_dev_paprd_device.c : 6078 ] 9: lut xq6_abs_xq7 
6048,I,[ phy_dev_paprd_device.c : 6080 ]  0x%x  
6047,I,[ phy_dev_paprd_device.c : 6082 ]  0x%x  
6046,I,[ phy_dev_paprd_device.c : 6084 ]  0x%x  
6045,I,[ phy_dev_paprd_device.c : 6086 ]  0x%x  
6044,ii,[ phy_dev_paprd_device.c : 6088 ]  END EDPD_LUT : table %d , iter %d 
6043,i,[ phy_dev_paprd_device.c : 6092 ]  END EDPD_LUT_TABLE : chain %d 
6042,ii,[ phy_dev_paprd_device.c : 5334 ] EDPD NEW CTRL REGISTERS   SAVE(1) : RESTORE(2) : PRINT(3)  (phyId= %d), cmd %d 
6041,II,[ phy_dev_paprd_device.c : 5417 ] PHYRF_EDPD_CTRL_2_L_B1 = 0x%x addr = 0x%x 
6040,II,[ phy_dev_paprd_device.c : 5420 ] PHYRF_EDPD_CTRL_2_U_B1 = 0x%x addr = 0x%x 
6039,II,[ phy_dev_paprd_device.c : 5423 ] PHYRF_EDPD_CTRL_3_L_B1 = 0x%x addr = 0x%x 
6038,II,[ phy_dev_paprd_device.c : 5431 ] PHYRF_EDPD_CTRL_4_L_B1 = 0x%x addr = 0x%x 
6037,II,[ phy_dev_paprd_device.c : 5434 ] PHYRF_EDPD_CTRL_4_U_B1 = 0x%x addr = 0x%x 
6036,II,[ phy_dev_paprd_device.c : 5437 ] PHYRF_EDPD_CTRL_5_L_B1 = 0x%x addr = 0x%x 
6035,II,[ phy_dev_paprd_device.c : 5440 ] PHYRF_EDPD_CTRL_5_U_B1 = 0x%x addr = 0x%x 
6034,II,[ phy_dev_paprd_device.c : 5443 ] PHYRF_EDPD_CTRL_6_L_B1 = 0x%x addr = 0x%x 
6033,II,[ phy_dev_paprd_device.c : 5446 ] PHYRF_EDPD_CTRL_6_U_B1 = 0x%x addr = 0x%x 
6032,II,[ phy_dev_paprd_device.c : 5449 ] PHYRF_EDPD_CTRL_7_L_B1 = 0x%x addr = 0x%x 
6031,II,[ phy_dev_paprd_device.c : 5452 ] PHYRF_EDPD_CTRL_7_U_B1 = 0x%x addr = 0x%x 
6030,II,[ phy_dev_paprd_device.c : 5455 ] PHYRF_EDPD_CTRL_8_L_B1 = 0x%x addr = 0x%x 
6029,II,[ phy_dev_paprd_device.c : 5472 ] PHYRF_EDPD_CTRL_0_L_B0 = 0x%x edpd_ctrl = 0x%x 
6028,II,[ phy_dev_paprd_device.c : 5477 ] PHYRF_EDPD_CTRL_0_U_B0 = 0x%x edpd_ctrl = 0x%x 
6027,II,[ phy_dev_paprd_device.c : 5482 ] PHYRF_EDPD_CTRL_1_L_B0 = 0x%x edpd_ctrl = 0x%x 
6026,II,[ phy_dev_paprd_device.c : 5487 ] PHYRF_EDPD_CTRL_1_U_B0 = 0x%x edpd_ctrl = 0x%x 
6025,II,[ phy_dev_paprd_device.c : 5492 ] PHYRF_EDPD_CTRL_2_L_B0 = 0x%x edpd_ctrl = 0x%x 
6024,II,[ phy_dev_paprd_device.c : 5497 ] PHYRF_EDPD_CTRL_2_U_B0 = 0x%x edpd_ctrl = 0x%x 
6023,II,[ phy_dev_paprd_device.c : 5502 ] PHYRF_EDPD_CTRL_3_L_B0 = 0x%x edpd_ctrl = 0x%x 
6022,II,[ phy_dev_paprd_device.c : 5507 ] PHYRF_EDPD_CTRL_4_L_B0 = 0x%x edpd_ctrl = 0x%x 
6021,II,[ phy_dev_paprd_device.c : 5512 ] PHYRF_EDPD_CTRL_4_U_B0 = 0x%x edpd_ctrl = 0x%x 
6020,II,[ phy_dev_paprd_device.c : 5517 ] PHYRF_EDPD_CTRL_5_L_B0 = 0x%x edpd_ctrl = 0x%x 
6019,II,[ phy_dev_paprd_device.c : 5522 ] PHYRF_EDPD_CTRL_5_U_B0 = 0x%x edpd_ctrl = 0x%x 
6018,II,[ phy_dev_paprd_device.c : 5527 ] PHYRF_EDPD_CTRL_6_L_B0 = 0x%x edpd_ctrl = 0x%x 
6017,II,[ phy_dev_paprd_device.c : 5532 ] PHYRF_EDPD_CTRL_6_U_B0 = 0x%x edpd_ctrl = 0x%x 
6016,II,[ phy_dev_paprd_device.c : 5537 ] PHYRF_EDPD_CTRL_7_L_B0 = 0x%x edpd_ctrl = 0x%x 
6015,II,[ phy_dev_paprd_device.c : 5542 ] PHYRF_EDPD_CTRL_7_U_B0 = 0x%x edpd_ctrl = 0x%x 
6014,II,[ phy_dev_paprd_device.c : 5547 ] PHYRF_EDPD_CTRL_8_L_B0 = 0x%x edpd_ctrl = 0x%x 
6013,II,[ phy_dev_paprd_device.c : 5556 ] PHYRF_EDPD_CTRL_0_L_B1 = 0x%x edpd_ctrl = 0x%x 
6012,II,[ phy_dev_paprd_device.c : 5561 ] PHYRF_EDPD_CTRL_0_U_B1 = 0x%x edpd_ctrl = 0x%x 
6011,II,[ phy_dev_paprd_device.c : 5566 ] PHYRF_EDPD_CTRL_1_L_B1 = 0x%x edpd_ctrl = 0x%x 
6010,II,[ phy_dev_paprd_device.c : 5571 ] PHYRF_EDPD_CTRL_1_U_B1 = 0x%x edpd_ctrl = 0x%x 
6009,II,[ phy_dev_paprd_device.c : 5576 ] PHYRF_EDPD_CTRL_2_L_B1 = 0x%x edpd_ctrl = 0x%x 
6008,II,[ phy_dev_paprd_device.c : 5581 ] PHYRF_EDPD_CTRL_2_U_B1 = 0x%x edpd_ctrl = 0x%x 
6007,II,[ phy_dev_paprd_device.c : 5586 ] PHYRF_EDPD_CTRL_3_L_B1 = 0x%x edpd_ctrl = 0x%x 
6006,II,[ phy_dev_paprd_device.c : 5597 ] PHYRF_EDPD_CTRL_4_L_B1 = 0x%x edpd_ctrl = 0x%x 
6005,II,[ phy_dev_paprd_device.c : 5602 ] PHYRF_EDPD_CTRL_4_U_B1 = 0x%x edpd_ctrl = 0x%x 
6004,II,[ phy_dev_paprd_device.c : 5607 ] PHYRF_EDPD_CTRL_5_L_B1 = 0x%x edpd_ctrl = 0x%x 
6003,II,[ phy_dev_paprd_device.c : 5612 ] PHYRF_EDPD_CTRL_5_U_B1 = 0x%x edpd_ctrl = 0x%x 
6002,II,[ phy_dev_paprd_device.c : 5617 ] PHYRF_EDPD_CTRL_6_L_B1 = 0x%x edpd_ctrl = 0x%x 
6001,II,[ phy_dev_paprd_device.c : 5622 ] PHYRF_EDPD_CTRL_6_U_B1 = 0x%x edpd_ctrl = 0x%x 
6000,II,[ phy_dev_paprd_device.c : 5627 ] PHYRF_EDPD_CTRL_7_L_B1 = 0x%x edpd_ctrl = 0x%x 
5999,II,[ phy_dev_paprd_device.c : 5632 ] PHYRF_EDPD_CTRL_7_U_B1 = 0x%x edpd_ctrl = 0x%x 
5998,II,[ phy_dev_paprd_device.c : 5637 ] PHYRF_EDPD_CTRL_8_L_B1 = 0x%x edpd_ctrl = 0x%x 
5997,II,[ phy_dev_paprd_device.c : 5655 ] PHYRF_EDPD_CTRL_0_L_B0 = 0x%x edpd_ctrl = 0x%x 
5996,II,[ phy_dev_paprd_device.c : 5660 ] PHYRF_EDPD_CTRL_0_U_B0 = 0x%x edpd_ctrl = 0x%x 
5995,II,[ phy_dev_paprd_device.c : 5665 ] PHYRF_EDPD_CTRL_1_L_B0 = 0x%x edpd_ctrl = 0x%x 
5994,II,[ phy_dev_paprd_device.c : 5670 ] PHYRF_EDPD_CTRL_1_U_B0 = 0x%x edpd_ctrl = 0x%x 
5993,II,[ phy_dev_paprd_device.c : 5675 ] PHYRF_EDPD_CTRL_2_L_B0 = 0x%x edpd_ctrl = 0x%x 
5992,II,[ phy_dev_paprd_device.c : 5680 ] PHYRF_EDPD_CTRL_2_U_B0 = 0x%x edpd_ctrl = 0x%x 
5991,II,[ phy_dev_paprd_device.c : 5685 ] PHYRF_EDPD_CTRL_3_L_B0 = 0x%x edpd_ctrl = 0x%x 
5990,II,[ phy_dev_paprd_device.c : 5690 ] PHYRF_EDPD_CTRL_4_L_B0 = 0x%x edpd_ctrl = 0x%x 
5989,II,[ phy_dev_paprd_device.c : 5695 ] PHYRF_EDPD_CTRL_4_U_B0 = 0x%x edpd_ctrl = 0x%x 
5988,II,[ phy_dev_paprd_device.c : 5700 ] PHYRF_EDPD_CTRL_5_L_B0 = 0x%x edpd_ctrl = 0x%x 
5987,II,[ phy_dev_paprd_device.c : 5705 ] PHYRF_EDPD_CTRL_5_U_B0 = 0x%x edpd_ctrl = 0x%x 
5986,II,[ phy_dev_paprd_device.c : 5710 ] PHYRF_EDPD_CTRL_6_L_B0 = 0x%x edpd_ctrl = 0x%x 
5985,II,[ phy_dev_paprd_device.c : 5715 ] PHYRF_EDPD_CTRL_6_U_B0 = 0x%x edpd_ctrl = 0x%x 
5984,II,[ phy_dev_paprd_device.c : 5720 ] PHYRF_EDPD_CTRL_7_L_B0 = 0x%x edpd_ctrl = 0x%x 
5983,II,[ phy_dev_paprd_device.c : 5725 ] PHYRF_EDPD_CTRL_7_U_B0 = 0x%x edpd_ctrl = 0x%x 
5982,II,[ phy_dev_paprd_device.c : 5730 ] PHYRF_EDPD_CTRL_8_L_B0 = 0x%x edpd_ctrl = 0x%x 
5981,II,[ phy_dev_paprd_device.c : 5739 ] PHYRF_EDPD_CTRL_0_L_B1 = 0x%x edpd_ctrl = 0x%x 
5980,II,[ phy_dev_paprd_device.c : 5744 ] PHYRF_EDPD_CTRL_0_U_B1 = 0x%x edpd_ctrl = 0x%x 
5979,II,[ phy_dev_paprd_device.c : 5749 ] PHYRF_EDPD_CTRL_1_L_B1 = 0x%x edpd_ctrl = 0x%x 
5978,II,[ phy_dev_paprd_device.c : 5754 ] PHYRF_EDPD_CTRL_1_U_B1 = 0x%x edpd_ctrl = 0x%x 
5977,II,[ phy_dev_paprd_device.c : 5759 ] PHYRF_EDPD_CTRL_2_L_B1 = 0x%x edpd_ctrl = 0x%x 
5976,II,[ phy_dev_paprd_device.c : 5764 ] PHYRF_EDPD_CTRL_2_U_B1 = 0x%x edpd_ctrl = 0x%x 
5975,II,[ phy_dev_paprd_device.c : 5769 ] PHYRF_EDPD_CTRL_3_L_B1 = 0x%x edpd_ctrl = 0x%x 
5974,II,[ phy_dev_paprd_device.c : 5780 ] PHYRF_EDPD_CTRL_4_L_B1 = 0x%x edpd_ctrl = 0x%x 
5973,II,[ phy_dev_paprd_device.c : 5785 ] PHYRF_EDPD_CTRL_4_U_B1 = 0x%x edpd_ctrl = 0x%x 
5972,II,[ phy_dev_paprd_device.c : 5790 ] PHYRF_EDPD_CTRL_5_L_B1 = 0x%x edpd_ctrl = 0x%x 
5971,II,[ phy_dev_paprd_device.c : 5795 ] PHYRF_EDPD_CTRL_5_U_B1 = 0x%x edpd_ctrl = 0x%x 
5970,II,[ phy_dev_paprd_device.c : 5800 ] PHYRF_EDPD_CTRL_6_L_B1 = 0x%x edpd_ctrl = 0x%x 
5969,II,[ phy_dev_paprd_device.c : 5805 ] PHYRF_EDPD_CTRL_6_U_B1 = 0x%x edpd_ctrl = 0x%x 
5968,II,[ phy_dev_paprd_device.c : 5810 ] PHYRF_EDPD_CTRL_7_L_B1 = 0x%x edpd_ctrl = 0x%x 
5967,II,[ phy_dev_paprd_device.c : 5815 ] PHYRF_EDPD_CTRL_7_U_B1 = 0x%x edpd_ctrl = 0x%x 
5966,II,[ phy_dev_paprd_device.c : 5820 ] PHYRF_EDPD_CTRL_8_L_B1 = 0x%x edpd_ctrl = 0x%x 
5965,I,[ phy_dev_paprd_device.c : 5348 ] PHYRF_EDPD_CTRL_0_L_B0 = 0x%x 
5964,I,[ phy_dev_paprd_device.c : 5351 ] PHYRF_EDPD_CTRL_0_U_B0 = 0x%x 
5963,I,[ phy_dev_paprd_device.c : 5354 ] PHYRF_EDPD_CTRL_1_L_B0 = 0x%x 
5962,I,[ phy_dev_paprd_device.c : 5357 ] PHYRF_EDPD_CTRL_1_U_B0 = 0x%x 
5961,I,[ phy_dev_paprd_device.c : 5360 ] PHYRF_EDPD_CTRL_2_L_B0 = 0x%x 
5960,I,[ phy_dev_paprd_device.c : 5363 ] PHYRF_EDPD_CTRL_2_U_B0 = 0x%x 
5959,I,[ phy_dev_paprd_device.c : 5366 ] PHYRF_EDPD_CTRL_3_L_B0 = 0x%x 
5958,I,[ phy_dev_paprd_device.c : 5374 ] PHYRF_EDPD_CTRL_4_L_B0 = 0x%x 
5957,I,[ phy_dev_paprd_device.c : 5377 ] PHYRF_EDPD_CTRL_4_U_B0 = 0x%x 
5956,I,[ phy_dev_paprd_device.c : 5380 ] PHYRF_EDPD_CTRL_5_L_B0 = 0x%x 
5955,I,[ phy_dev_paprd_device.c : 5383 ] PHYRF_EDPD_CTRL_5_U_B0 = 0x%x 
5954,I,[ phy_dev_paprd_device.c : 5386 ] PHYRF_EDPD_CTRL_6_L_B0 = 0x%x 
5953,I,[ phy_dev_paprd_device.c : 5389 ] PHYRF_EDPD_CTRL_6_U_B0 = 0x%x 
5952,I,[ phy_dev_paprd_device.c : 5392 ] PHYRF_EDPD_CTRL_7_L_B0 = 0x%x 
5951,I,[ phy_dev_paprd_device.c : 5395 ] PHYRF_EDPD_CTRL_7_U_B0 = 0x%x 
5950,I,[ phy_dev_paprd_device.c : 5398 ] PHYRF_EDPD_CTRL_8_L_B0 = 0x%x 
5949,II,[ phy_dev_paprd_device.c : 5405 ] PHYRF_EDPD_CTRL_0_L_B1 = 0x%x addr = 0x%x 
5948,II,[ phy_dev_paprd_device.c : 5408 ] PHYRF_EDPD_CTRL_0_U_B1 = 0x%x addr = 0x%x 
5947,II,[ phy_dev_paprd_device.c : 5411 ] PHYRF_EDPD_CTRL_1_L_B1 = 0x%x addr = 0x%x 
5946,II,[ phy_dev_paprd_device.c : 5414 ] PHYRF_EDPD_CTRL_1_U_B1 = 0x%x addr = 0x%x 
5945,ii,[ phy_dev_paprd_device.c : 5106 ] PAPRD SAVE(1) : RESTORE(2) : PRINT(3)  (phyId= %d), cmd %d 
5944,I,[ phy_dev_paprd_device.c : 5117 ] PAPRD_CTRL_L_B0 = 0x%x 
5943,I,[ phy_dev_paprd_device.c : 5119 ] PAPRD_VALID_GAIN_L_B0 = 0x%x 
5942,I,[ phy_dev_paprd_device.c : 5121 ] PHYRF_PAPRD_TABLE_TYPE_L_B0 = 0x%x 
5941,I,[ phy_dev_paprd_device.c : 5126 ] PAPRD_CTRL_L_B1 = 0x%x 
5940,I,[ phy_dev_paprd_device.c : 5128 ] PAPRD_VALID_GAIN_L_B1 = 0x%x 
5939,I,[ phy_dev_paprd_device.c : 5130 ] PHYRF_PAPRD_TABLE_TYPE_L_B1 = 0x%x 
5938,II,[ phy_dev_paprd_device.c : 5148 ] PAPRD_CTRL_L_B0 = 0x%x paprd_ctrl = 0x%x 
5937,II,[ phy_dev_paprd_device.c : 5153 ] PAPRD_VALID_GAIN_L_B0 = 0x%x paprd_ctrl = 0x%x 
5936,II,[ phy_dev_paprd_device.c : 5158 ] PHYRF_PAPRD_TABLE_TYPE_L_B0 = 0x%x paprd_ctrl = 0x%x 
5935,II,[ phy_dev_paprd_device.c : 5165 ] PAPRD_CTRL_L_B1 = 0x%x paprd_ctrl_1 = 0x%x 
5934,II,[ phy_dev_paprd_device.c : 5170 ] PAPRD_VALID_GAIN_L_B1 = 0x%x paprd_ctrl_1 = 0x%x 
5933,II,[ phy_dev_paprd_device.c : 5175 ] PHYRF_PAPRD_TABLE_TYPE_L_B1 = 0x%x paprd_ctrl_1 = 0x%x 
5932,II,[ phy_dev_paprd_device.c : 5194 ] PAPRD_CTRL_L_B0 = 0x%x paprd_ctrl = 0x%x 
5931,II,[ phy_dev_paprd_device.c : 5199 ] PAPRD_VALID_GAIN_L_B0 = 0x%x paprd_ctrl = 0x%x 
5930,II,[ phy_dev_paprd_device.c : 5204 ] PHYRF_PAPRD_TABLE_TYPE_L_B0 = 0x%x paprd_ctrl = 0x%x 
5929,II,[ phy_dev_paprd_device.c : 5211 ] PAPRD_CTRL_L_B1 = 0x%x paprd_ctrl_1 = 0x%x 
5928,II,[ phy_dev_paprd_device.c : 5216 ] PAPRD_VALID_GAIN_L_B1 = 0x%x paprd_ctrl_1 = 0x%x 
5927,II,[ phy_dev_paprd_device.c : 5221 ] PHYRF_PAPRD_TABLE_TYPE_L_B1 = 0x%x paprd_ctrl_1 = 0x%x 
5926,I,[ phy_dev_paprd_device.c : 5229 ] CUREENT HW TABLE  = 0x%x 
5925,iii,[ phy_dev_paprd_device.c : 1165 ] MM_PAPRD: txgain_index = %d phyId %d dpdDacGain %d 
5924,i,[ phy_dev_paprd_device.c : 419 ] -Q5-PAPRD-: write_Agc2atten, atten = %d 
5923,I,[ phy_dev_paprd_device.c : 434 ] -Q5-PAPRD-: PHYA 5G xPA chain0 gc = 0x%x 
5922,I,[ phy_dev_paprd_device.c : 436 ] -Q5-PAPRD-: PHYA_5G xPA chain1 gc = 0x%x 
5921,,[ phy_dev_paprd_device.c : 440 ] ******iPA 5G recipe 
5920,I,[ phy_dev_paprd_device.c : 448 ] -Q5-PAPRD-: PHYA 5G iPA chain0 gc = 0x%x 
5919,I,[ phy_dev_paprd_device.c : 450 ] -Q5-PAPRD-: PHYA_5G iPA chain1 gc = 0x%x 
5918,,[ phy_dev_paprd_device.c : 459 ] ******xPA recipe 
5917,I,[ phy_dev_paprd_device.c : 467 ] -Q5-PAPRD-: PHYB_2G xPA chain0 gc = 0x%x 
5916,I,[ phy_dev_paprd_device.c : 469 ] -Q5-PAPRD-: PHYB_2G xPA chain1 gc = 0x%x 
5915,,[ phy_dev_paprd_device.c : 476 ] ******iPA_xcoupler recipe 
5914,I,[ phy_dev_paprd_device.c : 485 ] -Q5-PAPRD-: PHYB_2G iPA chain0 gc = 0x%x 
5913,I,[ phy_dev_paprd_device.c : 487 ] -Q5-PAPRD-: PHYB_2G iPA chain1 gc = 0x%x 
5912,,[ phy_dev_paprd_device.c : 492 ] ******iPA_icoupler recipe 
5911,I,[ phy_dev_paprd_device.c : 499 ] -Q5-PAPRD-: PHYB 2G iPA chain0 gc = 0x%x 
5910,I,[ phy_dev_paprd_device.c : 501 ] -Q5-PAPRD-: PHYB 2G iPA chain1 gc = 0x%x 
5909,,[ phy_dev_paprd_device.c : 426 ] ******xPA 5G recipe 
5908,ii,[ phy_dev_paprd_device.c : 393 ] phy_paprd_getGlutindexFromTgtPwr maxTxPowerMCS9 %d last_dpd_glut_idx %d 
5907,,[ phy_dev_paprd_device.c : 6102 ] ******Memory DPD 
5906,I,[ phy_dev_paprd_device.c : 6105 ] Read-GCC_EDPD_AXI_CBCR=0x%x 
5905,I,[ phy_dev_paprd_device.c : 6106 ] Read-GCC_PCNOC_EDPD_AHB_CBCR=0x%x 
5904,I,[ phy_dev_paprd_device.c : 6111 ] Set-GCC_EDPD_AXI_CBCR=0x%x 
5903,I,[ phy_dev_paprd_device.c : 6116 ] Set-GCC_PCNOC_EDPD_AHB_CBCR=0x%x 
5902,I,[ phy_dev_paprd_device.c : 6273 ] PHYRF_PHYDBG_CAPTURE_L-enable = 0x%x 
5901,I,[ phy_dev_paprd_device.c : 6275 ] PHYRF_PHYDBG_CAPTURE_U-enable = 0x%x 
5900,I,[ phy_dev_paprd_device.c : 6277 ] PHYRF_PHYDBG_MODE_L   -enable = 0x%x 
5899,I,[ phy_dev_paprd_device.c : 6279 ] PHYRF_PHYDBG_TRIGGER_0_L -enable = 0x%x 
5898,I,[ phy_dev_paprd_device.c : 6281 ] WFAX_PHYRF_PHYDBG_TRIGGER_1_L -enable = 0x%x 
5897,I,[ phy_dev_paprd_device.c : 6283 ] PHYDBG_BANK3_EVENT_MASK = 0x%x 
5896,I,[ phy_dev_paprd_device.c : 1522 ] PHYRF_PHYDBG_CAPTURE_L-readPhyDbgCapMem = 0x%x 
5895,I,[ phy_dev_paprd_device.c : 1524 ] PHYRF_PHYDBG_CAPTURE_U-readPhyDbgCapMem = 0x%x 
5894,I,[ phy_dev_paprd_device.c : 1526 ] PHYRF_PHYDBG_MODE_L   -readPhyDbgCapMem = 0x%x 
5893,IIIIII,[ phy_dev_paprd_device.c : 1559 ] --Q5--PAPRDPHYDBG %lu Bank%lu %5d %5d %5d %5d 
6343,iI,[ phy_dev_paprd_core.c : 729 ] phy_core_PaprdCalcGainFxp : max bins %d X[GfxpIdx] %lu 
6342,Ii,[ phy_dev_paprd_core.c : 739 ] small signal gain is %ld, max_bins %d 
6341,ii,[ phy_dev_paprd_core.c : 51 ] phy_core_PaprdChangeTrainingIndex(): Change training position to chain index %d and dpd table index %d 
6340,I,[ phy_dev_paprd_core.c : 699 ] small signal gain is %ld 
6339,II,[ phy_dev_paprd_core.c : 706 ] PA_in[%2d] = 0x%lx 
6338,i,[ phy_dev_paprd_core.c : 70 ] Invalid channel %d 
6337,ii,[ phy_dev_paprd_core.c : 133 ] pPaprdStruct->tableIndex = %d, pPaprdStruct->txChain = %d 
6336,i,[ phy_dev_paprd_core.c : 144 ] warmpacket_cnt: %d 
6335,,[ phy_dev_paprd_core.c : 190 ] ******Memless DPD_curve fitting on 
6334,,[ phy_dev_paprd_core.c : 195 ] ******Memless DPD_curve fitting off 
6333,,[ phy_dev_paprd_core.c : 203 ] ******Memory DPD 
6332,I,[ phy_dev_paprd_core.c : 209 ] Set-GCC_EDPD_AXI_CBCR=0x%x 
6331,I,[ phy_dev_paprd_core.c : 214 ] Set-GCC_PCNOC_EDPD_AHB_CBCR=0x%x 
6330,IIIII,[ phy_dev_paprd_core.c : 261 ] -Q5-PAPRD-: EDPD data tx_i/q, rx_i/q[%5d]:%5ld %5ld %5ld %5ld 
6329,i,[ phy_dev_paprd_core.c : 136 ] training_done_for_curr_table_idx %d 
6328,ii,[ phy_dev_paprd_core.c : 274 ] DPD NMSE check fail : nmsex10 = %d nmselimitx10 = %d 
6327,I,[ phy_dev_paprd_core.c : 282 ] SQ is %lu and update DPD table 
6326,ii,[ phy_dev_paprd_core.c : 290 ]  SQ > SQ limit, DPD cal failed at chain %d and table index %d 
6325,I,[ phy_dev_paprd_core.c : 291 ]  SQ = %lu 
6324,iiii,[ phy_dev_paprd_core.c : 137 ] paprdType %d ldpdAdapDacGainEnable %d edpdAdapDacGainEnable %d dpdAdapDacPktCnt %d 
6323,i,[ phy_dev_paprd_core.c : 466 ] -Q5-PAPRD-:max_idx = %d (before adding bin#1) 
6322,,[ phy_dev_paprd_core.c : 471 ] -Q5-PAPRD-:		X	Y	theta 
6321,IIII,[ phy_dev_paprd_core.c : 475 ] -Q5-PAPRD-[%2u]:%4lu	%4lu	%4d 
6320,I,[ phy_dev_paprd_core.c : 362 ] --Q5-PAPRD-: Board id is 0%x 
6319,I,[ phy_dev_paprd_core.c : 363 ] --Q5-PAPRD-: Phy Id is 0%x 
6318,I,[ phy_dev_paprd_core.c : 364 ] --Q5-PAPRD-: SBS Mode  0%x 
6317,I,[ phy_dev_paprd_core.c : 366 ] --Q5-PAPRD-: Bw Idx is  0%x 
6316,iiiiIi,[ phy_dev_paprd_core.c : 809 ] warmpacketsupport %d: warmpacket_cnt %d max_warmpackets %d tlbidx %d s:%x ch:%d 
6351,iIii,[ phy_dev_DPDCal.c : 80 ] phyId : %d phyBase = 0x%lx txmask = %d rxmask = %d 
6350,,[ phy_dev_DPDCal.c : 125 ] Start post-processing 
6349,,[ phy_dev_DPDCal.c : 132 ] Finished post-processing and population of one DPD LUT 
6348,,[ phy_dev_DPDCal.c : 137 ] Training data not valid poor SQ 
6347,,[ phy_dev_DPDCal.c : 142 ] train_done flag cannot be set by HW, DPD Cal hits an critical error and abort 
6346,ii,[ phy_dev_DPDCal.c : 105 ] Start to setup DPD cal: phy_DPDCal_InitTrainingData() phyId = %d txmask = %d 
6345,,[ phy_dev_DPDCal.c : 115 ] Start to transmit training packet: phy_paprd_device_TransmitTrainingPacket() 
6344,,[ phy_dev_DPDCal.c : 321 ] DPDCal Recipe Start!!! 
6363,I,[ phy_dev_PkDetCal.c : 150 ] before cal, AON_COEX_COEX value = 0x%08x 
6362,Iii,[ phy_dev_PkDetCal.c : 255 ] calStatus check failed,  remainingChains = %x chain = %d calStatus=%d 
6361,I,[ phy_dev_PkDetCal.c : 277 ] D_AGC_PKDET_GAIN is set to %x 
6360,iiii,[ phy_dev_PkDetCal.c : 279 ] PKDET_DCOC_RES_OVD for chain %d  is = 'd%d is_sbs=%d PKDET_THRES_5G = %d 
6359,I,[ phy_dev_PkDetCal.c : 289 ] IWL_AGC_PKDET_GAIN is set to %x 
6358,iiii,[ phy_dev_PkDetCal.c : 291 ] PKDET_DCOC_RES_OVD for chain %d  is = 'd%d is_sbs=%d PKDET_THRES_2G = %d 
6357,I,[ phy_dev_PkDetCal.c : 298 ] D_AGC_PKDET_GAIN is set to %x 
6356,iii,[ phy_dev_PkDetCal.c : 300 ] PKDET_DCOC_RES_OVD for chain %d  is = 'd%d is_sbs=%d 
6355,IIII,[ phy_dev_PkDetCal.c : 244 ] PKdet cal check result, RO_AGC_CAL=%x , current chain=%x , remain chain=%x , counter=%x 
6354,Iii,[ phy_dev_PkDetCal.c : 251 ] remainingChains = %x DCOC_RES_Chain%d= 'd%d  
6353,IIIii,[ phy_dev_PkDetCal.c : 461 ] pkdet_restore :: regCalResult = 0x%x regParameters[0] = 0x%x regParameters[1] = 0x%x chain = %d is_sbs=%d 
6352,IIIii,[ phy_dev_PkDetCal.c : 416 ] pkdet_save :: regCalResult = 0x%x regParameters[0] = 0x%x regParameters[1] = 0x%x chain = %d is_sbs=%d 
6394,i,[ phy_dev_RxDCOCal.c : 1871 ] RxDCO: Cal failed on chain%d! Writing zeros to DCO LUT... 
6393,iii,[ phy_dev_RxDCOCal.c : 1877 ] RXDCO: Using forced value:Ch[%d] (I,Q)=(%d, %d) 
6392,,[ phy_dev_RxDCOCal.c : 2114 ] phyRxDCOCal_qca649x 
6391,,[ phy_dev_RxDCOCal.c : 1901 ] restore_rxdco_calResult 
6390,I,[ phy_dev_RxDCOCal.c : 1984 ] restore_rxdco_calResult:::Override mode is not restored for table mode: Value = %x 
6389,I,[ phy_dev_RxDCOCal.c : 1412 ] RXDCO: A_DELAY_USECS cal_done time out calDoneCount=%u 
6388,i,[ phy_dev_RxDCOCal.c : 1416 ] RXDCO: A_DELAY_USECS cal_done early calDoneCount=%d 
6387,,[ phy_dev_RxDCOCal.c : 1423 ] RXDCO: cal_done failure and reset DO_CALIBRATE bit and CF_RESET_CORE !!!!! 
6386,I,[ phy_dev_RxDCOCal.c : 1426 ] WFAX_PHYRF_CAL_SEQ_CTRL_16_L.DO_CALIBRATE= %lu 
6385,,[ phy_dev_RxDCOCal.c : 2083 ] rxdco_disable 
6384,,[ phy_dev_RxDCOCal.c : 144 ] rxdco_docal 
6383,i,[ phy_dev_RxDCOCal.c : 286 ] rxdco_docal, RXDCO TIMER2: %d 
6382,,[ phy_dev_RxDCOCal.c : 294 ] RXDCO: Allocating memory for CalResult 
6381,i,[ phy_dev_RxDCOCal.c : 255 ] rxdco_docal, RXDCO TIMER0: %d 
6380,i,[ phy_dev_RxDCOCal.c : 274 ] rxdco_docal, RXDCO TIMER1: %d 
6379,,[ phy_dev_RxDCOCal.c : 2073 ] rxdco_enable 
6378,,[ phy_dev_RxDCOCal.c : 1581 ] index out of range 
6377,I,[ phy_dev_RxDCOCal.c : 1289 ] xfem_gpo_cfg= 0x%x 
6376,,[ phy_dev_RxDCOCal.c : 2050 ] rxdco_restore 
6375,i,[ phy_dev_RxDCOCal.c : 574 ] RxDCO: Cal failed on chain%d! Writing zeros to DCO LUT... 
6374,iii,[ phy_dev_RxDCOCal.c : 580 ] RXDCO: Using forced value:Ch[%d] (I,Q)=(%d, %d) 
6373,,[ phy_dev_RxDCOCal.c : 368 ] RXDCO: *************************************** HW cal timeout 
6372,i,[ phy_dev_RxDCOCal.c : 377 ] RXDCO: cal done successful, range_iter=%d 
6371,i,[ phy_dev_RxDCOCal.c : 402 ] rxdco_run_rxdco_hw_cal: range_iter= %d 
6370,,[ phy_dev_RxDCOCal.c : 459 ] RXDCO: Failed in all tries! 
6369,,[ phy_dev_RxDCOCal.c : 2028 ] rxdco_save 
6368,,[ phy_dev_RxDCOCal.c : 2041 ] RxDCO: Invalid selection. CAL_SAVE is not supported for raw Cal Results 
6367,i,[ phy_dev_RxDCOCal.c : 1243 ] skip_forceTRSW= %d 
6366,i,[ phy_dev_RxDCOCal.c : 1257 ] forceTRSW= %d 
6365,,[ phy_dev_RxDCOCal.c : 1626 ] save_restore_rxdco_DcoLut 
6364,I,[ phy_dev_RxDCOCal.c : 1708 ] save_restore_rxdco_DcoLut:::Override mode is not restored for table mode: Value = %x 
6536,I,[ phy_dev_TPCcal.c : 1101 ] GLUT - Chain %u 
6535,I,[ phy_dev_TPCcal.c : 3728 ] In CLPCModeICOUPLER_IS: txChainMask = 0x%x 
6534,IIii,[ phy_dev_TPCcal.c : 3783 ]  CLPCModeICOUPLER_IS chmask %x WL_TPC_5G_CH0_TPC_OVERRIDE_3: %x input->pdetcalInput->PdetHighGain[idx]: %d input->pdetcalInput->PdetLowGain[idx]:%d 
 
6533,I,[ phy_dev_TPCcal.c : 3812 ] WL_TPC_5G_CH0_TPC_OVERRIDE_3: 0x%x 
6532,i,[ phy_dev_TPCcal.c : 3844 ] forcing PDET_GAIN_IDX_OVS %d 
6531,I,[ phy_dev_TPCcal.c : 3890 ] In CLPCModeICOUPLER_PO: txChainMask = 0x%x 
6530,I,[ phy_dev_TPCcal.c : 3974 ] In CLPCModePdet: txChainMask = 0x%x 
6529,IIii,[ phy_dev_TPCcal.c : 4029 ] CLPCModePdet chmask %x WL_TPC_5G_CH0_TPC_OVERRIDE_3: %x input->pdetcalInput->PdetHighGain[idx]: %d input->pdetcalInput->PdetLowGain[idx]:%d 
6528,ii,[ phy_dev_TPCcal.c : 4059 ] PDL_TPC_DBG: chain %d resDCLo %d 
6527,ii,[ phy_dev_TPCcal.c : 4079 ] PDL_TPC_DBG:: chain %d resDCHi %d 
6526,I,[ phy_dev_TPCcal.c : 4130 ] WL_TPC_5G_CH0_TPC_OVERRIDE_3: 0x%x 
6525,I,[ phy_dev_TPCcal.c : 4133 ] SD1: override_1 0x%x 
6524,I,[ phy_dev_TPCcal.c : 4135 ] SD1: override_4 0x%x 
6523,i,[ phy_dev_TPCcal.c : 4164 ] forcing PDET_GAIN_IDX_OVS %d 
6522,I,[ phy_dev_TPCcal.c : 4186 ] SD2: override_1 0x%x 
6521,I,[ phy_dev_TPCcal.c : 4188 ] SD2: override_4 0x%x 
6520,I,[ phy_dev_TPCcal.c : 3939 ] In CLPCModeVdet: txChainMask = 0x%x 
6519,,[ phy_dev_TPCcal.c : 1051 ] In clearalut routine, Clearing ALUT indices 
6518,I,[ phy_dev_TPCcal.c : 2699 ] SD: override_1 = 0x%x 
6517,iI,[ phy_dev_TPCcal.c : 2715 ] PDL_TPC_DBG EnableHwPdetCal checking LOW GAIN done chain %d cal_done %x 
6516,i,[ phy_dev_TPCcal.c : 2721 ] EnableHwPdetCal FAILED (TIA LOW GAIN) for chain %d!!! 
6515,ii,[ phy_dev_TPCcal.c : 2727 ] EnableHwPdetCal for good value (TIA LOW GAIN) for chain %d temp %d !!! 
6514,ii,[ phy_dev_TPCcal.c : 2734 ] EnableHwPdetCal PASSED (TIA LOW GAIN) for chain %d temp %d !!! 
6513,I,[ phy_dev_TPCcal.c : 2760 ] SD: override_1 = 0x%x 
6512,iI,[ phy_dev_TPCcal.c : 2775 ] PDL_TPC_DBG EnableHwPdetCal checking HIGH GAIN done chain %d cal_done %x 
6511,i,[ phy_dev_TPCcal.c : 2781 ] EnableHwPdetCal FAILED (TIA HIGH GAIN) for chain %d!!! 
6510,ii,[ phy_dev_TPCcal.c : 2788 ] EnableHwPdetCal for good value (TIA HIGH GAIN) for chain %d temp %d!!! 
6509,,[ phy_dev_TPCcal.c : 2795 ] EnableHwPdetCal PASSED (TIA HIGH GAIN) !!! 
6508,I,[ phy_dev_TPCcal.c : 2807 ] SD: override_1 = 0x%x 
6507,i,[ phy_dev_TPCcal.c : 2810 ] EnableHwPdetCal: calFailed = %d 
6506,I,[ phy_dev_TPCcal.c : 2899 ] SD: WL_TPC_2G_CH0_TPC_OVERRIDE_1 = 0x%x 
6505,iI,[ phy_dev_TPCcal.c : 2919 ] PDL_TPC_DBG EnableHwPdetCal checking LOW GAIN done chain %d cal_done %x 
6504,i,[ phy_dev_TPCcal.c : 2925 ] EnableHwPdetCal FAILED (TIA LOW GAIN) for chain %d!!! 
6503,ii,[ phy_dev_TPCcal.c : 2931 ] EnableHwPdetCal for good value (TIA LOW GAIN) for chain %d temp %d !!! 
6502,ii,[ phy_dev_TPCcal.c : 2938 ] EnableHwPdetCal PASSED (TIA LOW GAIN) for chain %d temp %d !!! 
6501,iI,[ phy_dev_TPCcal.c : 2985 ] PDL_TPC_DBG EnableHwPdetCal checking HIGH GAIN done chain %d cal_done %x 
6500,i,[ phy_dev_TPCcal.c : 2991 ] EnableHwPdetCal FAILED (TIA HIGH GAIN) for chain %d!!! 
6499,ii,[ phy_dev_TPCcal.c : 2998 ] EnableHwPdetCal for good value (TIA HIGH GAIN) for chain %d temp %d!!! 
6498,,[ phy_dev_TPCcal.c : 3005 ] EnableHwPdetCal PASSED (TIA HIGH GAIN) !!! 
6497,i,[ phy_dev_TPCcal.c : 3019 ] EnableHwPdetCal: calFailed = %d 
6496,II,[ phy_dev_TPCcal.c : 763 ] PDL_TPC:5G EnableTPCMode input->tgtPwrClpcThrDb4 %x with shift %x 
6495,IIIII,[ phy_dev_TPCcal.c : 3497 ] PDL_TPC_DBG: phyBase = %x SEQ_WCSS_PHYA_OFFSET %x pdadc reg %x valid_pwr %x wl_tpc_ch_offset %x 
6494,,[ phy_dev_TPCcal.c : 1325 ] Invalid GLUT numEntries! 
6493,I,[ phy_dev_TPCcal.c : 1356 ] GLUT - Chain %u 
6492,II,[ phy_dev_TPCcal.c : 4300 ] OtpExtract_Ko_Kg: otpRev 0x%x, chipId 0x%x 
6491,IIII,[ phy_dev_TPCcal.c : 4347 ] read OTP r100m %x r101l %x r101m %x r102l %x 
6490,II,[ phy_dev_TPCcal.c : 4372 ] kg ch0, ch1: 0x%x, 0x%x 
6489,II,[ phy_dev_TPCcal.c : 4373 ] ko ch0, ch1: 0x%x, 0x%x 
6488,II,[ phy_dev_TPCcal.c : 4228 ] OtpExtract_Rterm: otpRev 0x%x, chipId 0x%x 
6487,II,[ phy_dev_TPCcal.c : 4264 ] read OTP r100l %x r100m %x  
6486,II,[ phy_dev_TPCcal.c : 4277 ] Rterm ch0, ch1: 0x%x, 0x%x 
6485,,[ phy_dev_TPCcal.c : 3386 ] OverrideHwPdetCalValues 
6484,,[ phy_dev_TPCcal.c : 3564 ] OverridePdetAttn 
6483,ii,[ phy_dev_TPCcal.c : 3607 ] SD: attn %d PDET_GAIN_IDX_OVS %d 
6482,iII,[ phy_dev_TPCcal.c : 2033 ] chain idx %d Programming ko = 0x%x kg = 0x%x 
6481,iI,[ phy_dev_TPCcal.c : 2248 ] chain idx = %d programming rterm = 0x%x 
6480,iI,[ phy_dev_TPCcal.c : 2265 ] chain idx = %d programming rterm = 0x%x 
6479,,[ phy_dev_TPCcal.c : 2291 ] PDL_TPC_DBG: Setting WL_TPC_2G_CH0_TPC_CFG_1 for phyA ipdet_vdet PDets 
6478,,[ phy_dev_TPCcal.c : 2311 ] PDL_TPC_DBG: Setting WL_TPC_2G_CH0_TPC_CFG_1 for phyB ipdet_vdet PDets 
6477,,[ phy_dev_TPCcal.c : 2335 ] PDL_TPC_DBG: Setting WL_TPC_2G_CH0_TPC_CFG_1 for phyA ipdet_vdet PDets 
6476,,[ phy_dev_TPCcal.c : 2362 ] PDL_TPC_DBG: Setting WL_TPC_2G_CH0_TPC_CFG_1 for phyB ipdet_vdet PDets 
6475,,[ phy_dev_TPCcal.c : 2405 ] PDL_TPC_DBG: Setting WL_TPC_2G_CH0_TPC_CFG_1 for all other PDets 
6474,I,[ phy_dev_TPCcal.c : 1183 ] PLUT - Chain %u 
6473,IIIII,[ phy_dev_TPCcal.c : 461 ] TPC_PHYDEVLIB dacBOFlags %x, maxCCK %x, minCCK %x, maxSglRU %x minSglRU %x 
6472,IIIIIII,[ phy_dev_TPCcal.c : 463 ] TPC_PHYDEVLIB maxQAM[0..5] %x %x %x %x %x %x %x 
6471,IIIIIII,[ phy_dev_TPCcal.c : 465 ] TPC_PHYDEVLIB minQAM[0..5] %x %x %x %x %x %x %x 
6470,IIIIIII,[ phy_dev_TPCcal.c : 467 ] TPC_PHYDEVLIB maxQAM MU[0..5] %x %x %x %x %x %x %x 
6469,IIIIIII,[ phy_dev_TPCcal.c : 469 ] TPC_PHYDEVLIB minQAM MU[0..5] %x %x %x %x %x %x %x 
6468,i,[ phy_dev_TPCcal.c : 329 ] In ProgramGLUTIndicesByRange: powerRange = %d 
6467,,[ phy_dev_TPCcal.c : 333 ] Programming GLUT Indices Range 0 
6466,,[ phy_dev_TPCcal.c : 351 ] Programming GLUT Indices Range 1 
6465,,[ phy_dev_TPCcal.c : 364 ] Programming GLUT Indices Range 2 
6464,,[ phy_dev_TPCcal.c : 377 ] Programming GLUT Indices Range 3 
6463,i,[ phy_dev_TPCcal.c : 266 ] pktMCSType = %d 
6462,IiI,[ phy_dev_TPCcal.c : 980 ] programGLUT: Address of the GLUt base  = 0x%x: GLUT_Idx = %d; Measured power = %hx 
6461,,[ phy_dev_TPCcal.c : 3658 ] ReleasePdetAttn 
6460,IIII,[ phy_dev_TPCcal.c : 4656 ] tpcOnepointCal:: thermCalValue %u alphaTherm %u thermGainErrMax %u for chain %u 
6459,ii,[ phy_dev_TPCcal.c : 1701 ] TX_CONV: Invalid chain_idx:%d for phy_idx:%d 
6458,iii,[ phy_dev_TPCcal.c : 1705 ] TX_CONV: TxConvergenceRegRead phy_idx:%d for chain_idx:%d state:%d 
6457,i,[ phy_dev_TPCcal.c : 1706 ] TX_CONV: txgain_count:%d 
6456,i,[ phy_dev_TPCcal.c : 1707 ] TX_CONV: stat_latest_fwd:%d 
6455,i,[ phy_dev_TPCcal.c : 1708 ] TX_CONV: stat_latest_lb:%d 
6454,iii,[ phy_dev_TPCcal.c : 1751 ] TX_CONV: TX_CONVERGENCE_VALIDATION_RETRY_SUCCESS  phy_idx:%d chain_idx:%d retry_cnt:%d 
6453,iii,[ phy_dev_TPCcal.c : 1756 ] TX_CONV: TX_CONVERGENCE_VALIDATION_RETRY  phy_idx:%d chain_idx:%d retry_cnt:%d 
6452,iii,[ phy_dev_TPCcal.c : 1759 ] TX_CONV: TX_CONVERGENCE_VALIDATION_FAILURE  phy_idx:%d chain_idx:%d retry_cnt:%d 
6451,iiii,[ phy_dev_TPCcal.c : 1768 ] TX_CONV: mhz:%d phy_idx:%d chain_idx:%d state:%d 
6450,,[ phy_dev_TPCcal.c : 1773 ] TX_CONV: TX_CONVERGENCE_CLEAR 
6449,,[ phy_dev_TPCcal.c : 1779 ] TX_CONV: TX_CONVERGENCE_INIT 
6448,,[ phy_dev_TPCcal.c : 1784 ] TX_CONV: TX_CONVERGENCE_UPDATE 
6447,,[ phy_dev_TPCcal.c : 1792 ] TX_CONV: TX_CONVERGENCE_UPDATE_RETRY 
6446,i,[ phy_dev_TPCcal.c : 1805 ] TX_CONV: Invalid state: %d 
6445,iiii,[ phy_dev_TPCcal.c : 1730 ] TX_CONV: phy_idx:%d chain_idx:%d txgain_count_delta:%d latest_pwr_delta:%d 
6444,,[ phy_dev_TPCcal.c : 1734 ] TX_CONV: TX_CONVERGENCE_VALIDATION_SUCCESS 
6443,iiii,[ phy_dev_TPCcal.c : 3046 ] PDL_TPC_DBG EnableHwPdetCal BE_CAL_RESULT: hi_valid %d dac1_hi %d lo_valid %d dac1_lo %d 
6442,ii,[ phy_dev_TPCcal.c : 3083 ] PDL_TPC_DBG: in cal chain %d resDCLo %d 
6441,ii,[ phy_dev_TPCcal.c : 3131 ] PDL_TPC_DBG:: in cal chain %d resDCHi %d 
6440,iiii,[ phy_dev_TPCcal.c : 3172 ] PDL_TPC_DBG EnableHwPdetCal BE_CAL_RESULT: hi_valid %d dac1_hi %d lo_valid %d dac1_lo %d 
6439,ii,[ phy_dev_TPCcal.c : 3209 ] PDL_TPC_DBG: in cal chain %d resDCLo %d 
6438,ii,[ phy_dev_TPCcal.c : 3257 ] PDL_TPC_DBG:: in cal chain %d resDCHi %d 
6437,i,[ phy_dev_TPCcal.c : 819 ] WriteDacGainSettings GLUT_DAC_GAIN_CAL = %d 
6436,,[ phy_dev_TPCcal.c : 3614 ] apiOverrideReleasePdetAttn 
6435,i,[ phy_dev_TPCcal.c : 3640 ] apiOverrideReleasePdetAttn: pdetDcWarEn %d 
6434,i,[ phy_dev_TPCcal.c : 3642 ] ov_rel1:%d 
6433,,[ phy_dev_TPCcal.c : 1548 ] Printing all the input paramters 
6432,I,[ phy_dev_TPCcal.c : 1551 ] ForceDacGain - 0x%x 
6431,I,[ phy_dev_TPCcal.c : 1552 ] ForceTxGainIdx - 0x%x 
6430,iI,[ phy_dev_TPCcal.c : 1556 ] ForcedDacGain[%d] = 0x%x 
6429,iI,[ phy_dev_TPCcal.c : 1560 ] ForcedTxGainIdx[%d] = 0x%x 
6428,i,[ phy_dev_TPCcal.c : 1549 ] phyId - %d 
6427,I,[ phy_dev_TPCcal.c : 1550 ] ForcedTargetPower - 0x%x 
6426,,[ phy_dev_TPCcal.c : 1874 ] phyLatestAccumulatedCLPCError_qca649x was passed NULL Ptr 
6425,iII,[ phy_dev_TPCcal.c : 1897 ] tpcOnepointCal::phyId %d Chain %u latestAccumulatedClpcError %u 
6424,i,[ phy_dev_TPCcal.c : 1918 ] max_temp= %d 
6423,,[ phy_dev_TPCcal.c : 1934 ] phyLatestThermValue_qca649x was passed NULL Ptr 
6422,iII,[ phy_dev_TPCcal.c : 1941 ] tpcOnepointCal::phyId %d Chain %u thermalVal %u 
6421,,[ phy_dev_TPCcal.c : 4673 ] phyOLPCTempComp_qca649x 
6420,i,[ phy_dev_TPCcal.c : 4685 ] latest_therm_value_output.latestThermValue= %d 
6419,I,[ phy_dev_TPCcal.c : 606 ] TPC_PHYDEVLIB: TPC_GLUT_TARGET_PWR_LEVEL %x 
6418,I,[ phy_dev_TPCcal.c : 614 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_4_L %x 
6417,I,[ phy_dev_TPCcal.c : 622 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_5_L %x 
6416,I,[ phy_dev_TPCcal.c : 630 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_2_L %x 
6415,I,[ phy_dev_TPCcal.c : 638 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_3_L %x 
6414,I,[ phy_dev_TPCcal.c : 646 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_0_L %x 
6413,I,[ phy_dev_TPCcal.c : 654 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_1_L %x 
6412,I,[ phy_dev_TPCcal.c : 662 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_6_L %x 
6411,I,[ phy_dev_TPCcal.c : 670 ] TPC_PHYDEVLIB: TPC_GLUT_IDX_7_L %x 
6410,iii,[ phy_dev_TPCcal.c : 4755 ] Scan TPC: alphaThermSigned %d, scanThermOffset %d temp_code_cal %d 
6409,ii,[ phy_dev_TPCcal.c : 4763 ] Scan TPC: final temp_code_cal [0] [1] %d %d 
6408,iii,[ phy_dev_TPCcal.c : 4784 ] Scan TPC: isScanCh %d, OLPC_MODE %d FORCE_CLPC_ENABL %d 
6407,i,[ phy_dev_TPCcal.c : 117 ] pdetDcWarEn %d 
6406,II,[ phy_dev_TPCcal.c : 179 ] set ch %x WL_TPC_5G_CH0_TPC_OVERRIDE_3 to %x 
6405,IIII,[ phy_dev_TPCcal.c : 119 ] Get the Modes - CLPCMode - 0x%x readTPCStatus - 0x%x Force Mode - 0x%x Forced gain - 0x%x 
6404,,[ phy_dev_TPCcal.c : 151 ] Incorrect Test Selection ... 
6403,i,[ phy_dev_TPCcal.c : 1826 ] TX_CONV: TX_CONVERGENCE_VALIDATION_FAILURE invalid phyInput->phyId:%d 
6402,i,[ phy_dev_TPCcal.c : 1830 ] TX_CONV: Start: tx_converged:%d 
6401,iii,[ phy_dev_TPCcal.c : 1842 ] TX_CONV: TX_CONVERGENCE_VALIDATION_FAILURE invalid phy_base_addr:%d phy_idx:%d chain_idx:%d 
6400,iii,[ phy_dev_TPCcal.c : 1847 ] TX_CONV: phyInput->phyId:%d, phyInput->txChMask:%d, tx_active_chain_mask:%d 
6399,i,[ phy_dev_TPCcal.c : 1859 ] TX_CONV: End: tx_converged:%d 
6398,i,[ phy_dev_TPCcal.c : 194 ] FCS is enabled - setting the SEL_ALT_TABLES bit to %d 
6397,,[ phy_dev_TPCcal.c : 199 ] PHYA/B Configuration 
6396,,[ phy_dev_TPCcal.c : 234 ] Completed the OLPC settings... 
6395,iiii,[ phy_dev_TPCcal.c : 3557 ] PDL_TPC_DBG: pdadc[0] %d dcVal[0] %d pdadc[1] %d dcVal[1] %d 
6539,,[ phy_dev_TxBBFCal.c : 309 ] Beol and/or pw came back as zero - OTP is likely not programmed 
6538,II,[ phy_dev_TxBBFCal.c : 141 ] TxBBFCal restore. bandcode: %u txChMask %u 
6537,II,[ phy_dev_TxBBFCal.c : 46 ] TxBBF save. bandcode: %u txChMask %u 
6546,II,[ phy_dev_RxBBFCal.c : 190 ] [MY]    Channel = %u, phyinput chain mask = %u 
6545,,[ phy_dev_RxBBFCal.c : 234 ] [MY]    TOP_PRCM_qmom_rcx_rf_BEOL_shield__1 = 0. Beol came back as Zero - OTP is likely not programmed. No action taken. 
6544,,[ phy_dev_RxBBFCal.c : 282 ] RXBBFCAL: bw code too large!!! Defaulting to 0 
6543,II,[ phy_dev_RxBBFCal.c : 124 ] RxBBF restore. bandcode: %u rxChMask %u 
6542,,[ phy_dev_RxBBFCal.c : 128 ] Error: phyInput->rxChMask > 2 or NULL input. Return RECIPE_FAILURE! 
6541,II,[ phy_dev_RxBBFCal.c : 55 ] RxBBF save. bandcode: %u rxChMask %u 
6540,,[ phy_dev_RxBBFCal.c : 59 ] Error: phyInput->rxChMask > 2 or NULL input. Return RECIPE_FAILURE! 
6550,i,[ phy_dev_paprd_curve_fit_on_binning.c : 124 ] max_bin = %d 
6549,iii,[ phy_dev_paprd_curve_fit_on_binning.c : 211 ] tbl[%d] = %d / %d 
6548,iiii,[ phy_dev_paprd_curve_fit_on_binning.c : 125 ] curve_fit_noise_bin[%d] = %d, curve_fit_sm_sgi_gain[%d] = %d 
6547,iII,[ phy_dev_paprd_curve_fit_on_binning.c : 196 ] curvefit_coef(%d) = %f + j*%f 
6692,II,[ phy_dev_mem_paprd.c : 1598 ] DCEst done with dco = %ld/%ld  
6691,I,[ phy_dev_mem_paprd.c : 1541 ] rxiq done! sample_cnt = %ld  
6690,iiiiii,[ phy_dev_mem_paprd.c : 1543 ] rxiq_mask = %d/%d/%d/%d/%d/%d  
6689,II,[ phy_dev_mem_paprd.c : 1546 ] rxiq_coef.x0 = %ld/%ld  
6688,II,[ phy_dev_mem_paprd.c : 1551 ] rxiq_coef.conj_x0  = %ld/%ld  
6687,II,[ phy_dev_mem_paprd.c : 1556 ] rxiq_coef.conj_x1_minus_conj_xm1= %ld/%ld  
6686,II,[ phy_dev_mem_paprd.c : 1561 ] rxiq_coef.conj_x0_3rd= %ld/%ld  
6685,II,[ phy_dev_mem_paprd.c : 1566 ] rxiq_coef.x0_x0= %ld/%ld  
6684,II,[ phy_dev_mem_paprd.c : 1571 ] rxiq_coef.conj_x0_2nd= %ld/%ld  
6683,I,[ phy_dev_mem_paprd.c : 2465 ] EDPD_CAL_ACC_TXRX_SAMPLE_MEM_START_ADDR_val physical address=0x%x 
6682,I,[ phy_dev_mem_paprd.c : 2497 ] EDPD_CAL_ACC_CTRL_L = 0x%lx  
6681,I,[ phy_dev_mem_paprd.c : 2498 ] EDPD_CAL_ACC_CTRL_U = 0x%lx  
6680,I,[ phy_dev_mem_paprd.c : 2518 ] before Disable DCD TLMM_DBG_BUS_Read %x 
6679,,[ phy_dev_mem_paprd.c : 2525 ] TLMM_DBG_BUS_Read status done 
6678,I,[ phy_dev_mem_paprd.c : 2531 ] before Disable DCD TLMM_DBG_BUS_Read %x 
6677,I,[ phy_dev_mem_paprd.c : 2548 ] Read-GCC_SNOC_DCD_CONFIG: 0x%x 
6676,I,[ phy_dev_mem_paprd.c : 2549 ] Read-GCC_SNOC_DCD_HYSTERESIS_CNT: 0x%x 
6675,I,[ phy_dev_mem_paprd.c : 2550 ] Read-GCC_PCNOC_DCD_CONFIG: 0x%x 
6674,I,[ phy_dev_mem_paprd.c : 2551 ] Read-GCC_PCNOC_DCD_HYSTERESIS_CNT: 0x%x 
6673,I,[ phy_dev_mem_paprd.c : 2558 ] Set-GCC_SNOC_DCD_CONFIG: 0x%x 
6672,I,[ phy_dev_mem_paprd.c : 2559 ] Set-GCC_SNOC_DCD_HYSTERESIS_CNT: 0x%x 
6671,I,[ phy_dev_mem_paprd.c : 2560 ] Set-GCC_PCNOC_DCD_CONFIG: 0x%x 
6670,I,[ phy_dev_mem_paprd.c : 2561 ] Set-GCC_PCNOC_DCD_HYSTERESIS_CNT: 0x%x 
6669,I,[ phy_dev_mem_paprd.c : 2566 ] EDPD_CAL_ACC_CTRL_U = 0x%x 
6668,I,[ phy_dev_mem_paprd.c : 2569 ] EDPD_CAL_ACC_CTRL_U = 0x%x 
6667,I,[ phy_dev_mem_paprd.c : 2572 ] eDPD HW ACC activated, time stamp: %ld 
6666,i,[ phy_dev_mem_paprd.c : 2585 ] EDPD_CAL_ACC_DONE_INTERRUPT_val: %d 
6665,i,[ phy_dev_mem_paprd.c : 2586 ] EDPD_CAL_ACC_DDR_READTIME_GT_THR: %d 
6664,I,[ phy_dev_mem_paprd.c : 2597 ] eDPD HW ACC done, time stamp: %ld 
6663,,[ phy_dev_mem_paprd.c : 739 ] enable self eql training and status_ starts with MEMLESS_EST_FOR_SELF_EQL 
6662,,[ phy_dev_mem_paprd.c : 760 ] eDPD - BUFrefill_ON 
6661,,[ phy_dev_mem_paprd.c : 769 ] eDPD - BUFrefill_OFF 
6660,I,[ phy_dev_mem_paprd.c : 905 ] rxiq with taps = %ld 
6659,i,[ phy_dev_mem_paprd.c : 1753 ] delay_ddr = %d  
6658,II,[ phy_dev_mem_paprd.c : 1770 ] eDPD mem start_pt/stop_pt = %ld / %ld  
6657,I,[ phy_dev_mem_paprd.c : 1771 ] eDPD taps = %ld  
6656,IIII,[ phy_dev_mem_paprd.c : 1669 ] SQTiming done with offset = %ld and SQAvg=%ld/%ld/%ld 
6655,I,[ phy_dev_mem_paprd.c : 2421 ] EDPD_CAL_ACC_DC_CTRL_L = 0x%lx  
6654,I,[ phy_dev_mem_paprd.c : 2422 ] EDPD_CAL_ACC_RXIQ_CTRL0_L = 0x%lx  
6653,I,[ phy_dev_mem_paprd.c : 2423 ] EDPD_CAL_ACC_RXIQ_CTRL0_U = 0x%lx  
6652,I,[ phy_dev_mem_paprd.c : 2424 ] EDPD_CAL_ACC_RXIQ_CTRL1_L = 0x%lx  
6651,I,[ phy_dev_mem_paprd.c : 2425 ] EDPD_CAL_ACC_RXIQ_CTRL1_U = 0x%lx  
6650,I,[ phy_dev_mem_paprd.c : 2265 ] EDPD_CAL_ACC_BASE_DLY_CTRL_L  = 0x%lx  
6649,I,[ phy_dev_mem_paprd.c : 2266 ] EDPD_CAL_ACC_BASE_DLY_CTRL_U  = 0x%lx  
6648,iiI,[ phy_dev_mem_paprd.c : 2318 ] EDPD_CAL_ACC_KERNEL%d%d_ACT_L = 0x%lx  
6647,iiI,[ phy_dev_mem_paprd.c : 2319 ] EDPD_CAL_ACC_KERNEL%d%d_ACT_U = 0x%lx  
6646,I,[ phy_dev_mem_paprd.c : 2341 ] EDPD_CAL_ACC_KERNEL3031_ACT_L = 0x%lx  
6645,iiI,[ phy_dev_mem_paprd.c : 2377 ] EDPD_CAL_ACC_KERNEL%d%d_IDX_L = 0x%lx  
6644,iiI,[ phy_dev_mem_paprd.c : 2378 ] EDPD_CAL_ACC_KERNEL%d%d_IDX_U = 0x%lx  
6643,IIII,[ phy_dev_mem_paprd.c : 2977 ] txiq rxiq=(%ld, %ld, %ld, %ld) 
6642,III,[ phy_dev_mem_paprd.c : 1021 ] memless_coef_for_self_eql[%ld] = %f/%f 
 
6641,I,[ phy_dev_mem_paprd.c : 1218 ] restore DCD TLMM_DBG_BUS_Read %x 
6640,,[ phy_dev_mem_paprd.c : 1224 ] TLMM_DBG_BUS_Read status done 
6639,I,[ phy_dev_mem_paprd.c : 1230 ] restore DCD TLMM_DBG_BUS_Read %x 
6638,I,[ phy_dev_mem_paprd.c : 1238 ] GCC_WL_MEMSS_SW_RST_REG: 0x%x 
6637,I,[ phy_dev_mem_paprd.c : 1239 ] GCC_WL_CMN_IM_SW_RST_REG: 0x%x 
6636,,[ phy_dev_mem_paprd.c : 1023 ] memless_est_on_tx done and status_ goes to SELF_EQL_TRAINING
 
6635,I,[ phy_dev_mem_paprd.c : 1245 ] GCC_WL_MEMSS_SW_RST_REG: 0x%x 
6634,I,[ phy_dev_mem_paprd.c : 1246 ] GCC_WL_CMN_IM_SW_RST_REG: 0x%x 
6633,I,[ phy_dev_mem_paprd.c : 1252 ] GCC_WL_MEMSS_SW_RST_REG: 0x%x 
6632,I,[ phy_dev_mem_paprd.c : 1253 ] GCC_WL_CMN_IM_SW_RST_REG: 0x%x 
6631,,[ phy_dev_mem_paprd.c : 1262 ] after edpd restore 
6630,I,[ phy_dev_mem_paprd.c : 1263 ] Restore-GCC_SNOC_DCD_CONFIG: 0x%x 
6629,I,[ phy_dev_mem_paprd.c : 1264 ] Restore-GCC_SNOC_DCD_HYSTERESIS_CNT: 0x%x 
6628,I,[ phy_dev_mem_paprd.c : 1265 ] Restore-GCC_PCNOC_DCD_CONFIG: 0x%x 
6627,I,[ phy_dev_mem_paprd.c : 1266 ] Restore-GCC_PCNOC_DCD_HYSTERESIS_CNT: 0x%x 
6626,I,[ phy_dev_mem_paprd.c : 1271 ] Disable-GCC_EDPD_AXI_CBCR=0x%x 
6625,,[ phy_dev_mem_paprd.c : 1045 ] status_ goes to SELF_EQL_TRAINING  
6624,I,[ phy_dev_mem_paprd.c : 1275 ] Disable-GCC_PCNOC_EDPD_AHB_CBCR=0x%x 
6623,I,[ phy_dev_mem_paprd.c : 1285 ] status_ goes to MEM_COEFF_TRAINING, dpdmemtrain_[thread_id].sample_cnt = %ld  
6622,I,[ phy_dev_mem_paprd.c : 1327 ] SW before Rxx Rxy, time stamp: %ld 
6621,III,[ phy_dev_mem_paprd.c : 1335 ] mem_coef[%ld].real/imag is %ld / %ld 
6620,I,[ phy_dev_mem_paprd.c : 1344 ] SW before enter WAIT_FOR_SETTLE_NMSE, time stamp: %ld 
6619,I,[ phy_dev_mem_paprd.c : 1358 ] WAIT_FOR_SETTLE_NMSE, time stamp: %ld 
6618,I,[ phy_dev_mem_paprd.c : 1360 ] status_ goes to NMSE calc, dpdmemtrain_[thread_id].sample_cnt = %ld  
6617,i,[ phy_dev_mem_paprd.c : 1395 ] NMSE_acc is %d  
6616,i,[ phy_dev_mem_paprd.c : 1396 ] tx_acc is %d  
6615,i,[ phy_dev_mem_paprd.c : 1404 ] nmsex10 is %d  
6614,I,[ phy_dev_mem_paprd.c : 1073 ] coef_max_val = %ld   
6613,i,[ phy_dev_mem_paprd.c : 1405 ] PHYDEVLIB_DPD_DATA size %d  
6612,I,[ phy_dev_mem_paprd.c : 1077 ] eql_nshift = %ld 
6611,III,[ phy_dev_mem_paprd.c : 1082 ] self_eql_coef[%ld] = %f/%f 
 
6610,III,[ phy_dev_mem_paprd.c : 1088 ] self_eql_coef[%ld] = %f/%f 
 
6609,,[ phy_dev_mem_paprd.c : 1093 ] SELF_EQL_TRAINING done and status_ goes to LB_IMPAIR_EST 
6608,I,[ phy_dev_mem_paprd.c : 1121 ] status_ goes to RXIQ_TRAINING, dpdmemtrain_[thread_id].sample_cnt = %ld  
6607,I,[ phy_dev_mem_paprd.c : 1149 ] RXIQ_TRAINING done, time stamp: %ld 
6606,,[ phy_dev_mem_paprd.c : 1152 ] RXIQ done and status_ goes to HW_ACC 
6605,,[ phy_dev_mem_paprd.c : 1158 ] RXIQ done and status_ goes to WAIT_FOR_SETTLE 
6604,,[ phy_dev_mem_paprd.c : 1175 ] HW ACCELERATOR complete! perform LDL to get mem_coef:  
6603,I,[ phy_dev_mem_paprd.c : 1179 ] HW ACC before Rxx Rxy, time stamp: %ld 
6602,III,[ phy_dev_mem_paprd.c : 1187 ] mem_coef[%ld].real/imag is %ld / %ld 
6601,I,[ phy_dev_mem_paprd.c : 1196 ] HW ACC before enter WAIT_FOR_SETTLE_NMSE, time stamp: %ld 
6600,,[ phy_dev_mem_paprd.c : 1199 ] HW ACCELERATOR TIME OUT! TRY pure SW post processing 
6599,,[ phy_dev_mem_paprd.c : 1200 ] status_ goes to WAIT_FOR_SETTLE 
6598,,[ phy_dev_mem_paprd.c : 1209 ] before edpd reset 
6597,I,[ phy_dev_mem_paprd.c : 1210 ] Restore-GCC_SNOC_DCD_CONFIG: 0x%x 
6596,I,[ phy_dev_mem_paprd.c : 1211 ] Restore-GCC_SNOC_DCD_HYSTERESIS_CNT: 0x%x 
6595,I,[ phy_dev_mem_paprd.c : 1212 ] Restore-GCC_PCNOC_DCD_CONFIG: 0x%x 
6594,I,[ phy_dev_mem_paprd.c : 1213 ] Restore-GCC_PCNOC_DCD_HYSTERESIS_CNT: 0x%x 
6593,I,[ phy_dev_mem_paprd.c : 3278 ] buff refill start, time stamp: %lld
 
6592,Iiiii,[ phy_dev_mem_paprd.c : 3354 ] -Q5-PAPRD-: EDPD data tx_i/q, rx_i/q[%5d]:%d %d %d %d 
6591,Iiiii,[ phy_dev_mem_paprd.c : 3362 ] -Q5-PAPRD-: EDPD data tx_i/q, rx_i/q[%5d]:%d %d %d %d 
6590,I,[ phy_dev_mem_paprd.c : 3371 ] buff refill end, time stamp: %lld
 
6589,IIIi,[ phy_dev_mem_paprd.c : 3455 ] enable_self_eql 0x%x postDpdScaling 0x%x  rxIQMask 0x%x is_bandedge %d 
6588,i,[ phy_dev_mem_paprd.c : 3670 ] phy_dev_MemDPDTrain: hstp_chip_ID: %d 
6587,i,[ phy_dev_mem_paprd.c : 3674 ] phy_dev_MemDPDTrain: phyInput->bwCode: %d 
6586,iiii,[ phy_dev_mem_paprd.c : 3700 ] min_loop_dly=%d sq_idx=%d sq_timing_offset=%d is_160_mode=%d
 
6585,I,[ phy_dev_mem_paprd.c : 3712 ] iq sample begins, time stamp: %ld 
6584,i,[ phy_dev_mem_paprd.c : 3713 ] WHAL_EDPD_NUM_SAMPLES_PER_CHUNK=%d 
6583,,[ phy_dev_mem_paprd.c : 3726 ] buff refill start for 160 mode
 
6582,,[ phy_dev_mem_paprd.c : 3729 ] buff refill done for 160 mode
 
6581,,[ phy_dev_mem_paprd.c : 3794 ] buff refill for selfeql
 
6580,I,[ phy_dev_mem_paprd.c : 3830 ] all eDPD post processing done, time stamp: %ld 
6579,,[ phy_dev_mem_paprd.c : 3558 ] portingMemDpdResult: hstp_chip_ID = 0 
6578,,[ phy_dev_mem_paprd.c : 3563 ] portingMemDpdResult: hstp_chip_ID = 1 
6577,,[ phy_dev_mem_paprd.c : 3586 ] ddr*1
 
6576,,[ phy_dev_mem_paprd.c : 3594 ] ddr*2
 
6575,,[ phy_dev_mem_paprd.c : 3617 ] eDPD OUTPUT-------------------------> 
6574,i,[ phy_dev_mem_paprd.c : 3618 ] int memDpd_bin_size_sel = %d 
6573,i,[ phy_dev_mem_paprd.c : 3619 ] int q0_for_lut_xq0_abs_xq1 = %d 
6572,i,[ phy_dev_mem_paprd.c : 3620 ] int q1_for_lut_xq0_abs_xq1 = %d 
6571,i,[ phy_dev_mem_paprd.c : 3621 ] int q2_for_lut_xq2_abs_xq3 = %d 
6570,i,[ phy_dev_mem_paprd.c : 3622 ] int q3_for_lut_xq2_abs_xq3 = %d 
6569,i,[ phy_dev_mem_paprd.c : 3623 ] int q4_for_lut_xq4_abs_xq5 = %d 
6568,i,[ phy_dev_mem_paprd.c : 3624 ] int q5_for_lut_xq4_abs_xq5 = %d 
6567,i,[ phy_dev_mem_paprd.c : 3625 ] int q6_for_lut_xq6_abs_xq7 = %d 
6566,i,[ phy_dev_mem_paprd.c : 3626 ] int q7_for_lut_xq6_abs_xq7 = %d 
6565,i,[ phy_dev_mem_paprd.c : 3627 ] int q_for_Xq = %d 
6564,i,[ phy_dev_mem_paprd.c : 3628 ] int q1_for_X0X0ConjXq1 = %d 
6563,i,[ phy_dev_mem_paprd.c : 3629 ] int q2_for_X0X0ConjXq2 = %d 
6562,i,[ phy_dev_mem_paprd.c : 3630 ] int q1_for_Xq1Xq2 = %d 
6561,i,[ phy_dev_mem_paprd.c : 3631 ] int q2_for_Xq1Xq2 = %d 
6560,i,[ phy_dev_mem_paprd.c : 3632 ] int q3_for_Xq3Xq4 = %d 
6559,i,[ phy_dev_mem_paprd.c : 3633 ] int q4_for_Xq3Xq4 = %d 
6558,i,[ phy_dev_mem_paprd.c : 3634 ] int q1_for_Xq1AbsXq2AbsXq3 = %d 
6557,i,[ phy_dev_mem_paprd.c : 3635 ] int q2_for_Xq1AbsXq2AbsXq3 = %d 
6556,i,[ phy_dev_mem_paprd.c : 3636 ] int q3_for_Xq1AbsXq2AbsXq3 = %d 
6555,ii,[ phy_dev_mem_paprd.c : 3638 ] int memDpd_standalone_coef_I[%d] = %d
 
6554,ii,[ phy_dev_mem_paprd.c : 3639 ] int memDpd_standalone_coef_Q[%d] = %d
 
6553,ii,[ phy_dev_mem_paprd.c : 3642 ] int memDpd_paprd_memless_table_I[%d] = %d
 
6552,ii,[ phy_dev_mem_paprd.c : 3643 ] int memDpd_paprd_memless_table_Q[%d] = %d
 
6551,i,[ phy_dev_mem_paprd.c : 3645 ] int memDpd_standalone_coefShift = %d 
6693,,[ phy_dev_ADCCal.c : 83 ] ADC Cal Done! 
6700,III,[ phy_dev_DACCal.c : 499 ] phyId: %u, bandCode: %u, chMask: %u 
6699,III,[ phy_dev_DACCal.c : 545 ] DACCAL docal Setting Enable bit phyId: %u, bandCode: %u, chMask: %u 
6698,III,[ phy_dev_DACCal.c : 564 ] DACCAL docal Setting Enable bit. phyId: %u, bandCode: %u, chMask: %u 
6697,I,[ phy_dev_DACCal.c : 667 ] Starting Dac CalCmd: %u 
6696,II,[ phy_dev_DACCal.c : 628 ] DACCal restore. bandcode: %u txChMask %u 
6695,II,[ phy_dev_DACCal.c : 647 ] DACCal restore Setting Enable bit. bandcode: %u txChMask %u 
6694,II,[ phy_dev_DACCal.c : 586 ] DACCal save. bandcode: %u txChMask %u 
6729,,[ phy_dev_rstCal.c : 559 ] Q5_RST: CAL_DOCAL
 
6728,IIII,[ phy_dev_rstCal.c : 235 ] 0L_corr_mean_i_L=%u, 1U_corr_mean_i_U=%u, 2L_abs_adc_mean=%u, 3U_tone_gen_phs_step=%u
 
6727,iIIII,[ phy_dev_rstCal.c : 236 ] gain_num(%d, :) = [0L_corr_mean_i_L=%u, 1U_corr_mean_i_U=%u, 2L_abs_adc_mean=%u, 3U_tone_gen_phs_step=%u] 
6726,IIII,[ phy_dev_rstCal.c : 237 ] CIM[0]=0x%x, CIM[1]=0x%x, CIM[2]=0x%x, CIM[3]=0x%x

 
6725,iiiii,[ phy_dev_rstCal.c : 238 ] RSSI=%d, adc_BO=%d, meanAbs_log=%d, meanAbs=%d, RxGainDB=%d
 
6724,i,[ phy_dev_rstCal.c : 243 ] RSSI_value=%d 
6723,iiiiiii,[ phy_dev_rstCal.c : 474 ] # chain%d: txGain=(%d, %d), rxGainIdx=(%d, %d) dacScaleDb=(%d, %d)
 
6722,iiiiiii,[ phy_dev_rstCal.c : 476 ] # chain%d: calTxGain=%d, latestTxGainIdx=%d, calRxGain=%d, calRxGainIdx=%d, calDacGainDb=%d, latestDacGain=%d
 
6721,,[ phy_dev_rstCal.c : 139 ] call ch0tx/ch1rx step1 
 
6720,,[ phy_dev_rstCal.c : 146 ] call ch1rx/ch0tx step2 
 
6719,,[ phy_dev_rstCal.c : 150 ] 
 ERROR! Incorrect rstDir setting!!! 
 
6718,,[ phy_dev_rstCal.c : 363 ] call ch0tx/ch1rx step1 
 
6717,,[ phy_dev_rstCal.c : 368 ] call ch1rx/ch0tx step2 
 
6716,,[ phy_dev_rstCal.c : 372 ] 
 ERROR! Incorrect rstDir setting!!! 
 
6715,I,[ phy_dev_rstCal.c : 376 ] call: rstInput->cal_chain_mask = 0x%x
 
6714,,[ phy_dev_rstCal.c : 488 ] call
 
6713,,[ phy_dev_rstCal.c : 300 ] call ch0tx/ch1rx step1 
 
6712,,[ phy_dev_rstCal.c : 306 ] call ch1rx/ch0tx step2 
 
6711,,[ phy_dev_rstCal.c : 310 ] 
 ERROR! Incorrect rstDir setting!!! 
 
6710,i,[ phy_dev_rstCal.c : 595 ] rxTd chn0: TOTAL_GAIN_DB=%d 
 
6709,i,[ phy_dev_rstCal.c : 597 ] rxTd chn1: TOTAL_GAIN_DB=%d 

 
6708,i,[ phy_dev_rstCal.c : 602 ] phyB, Dtop ch0: RO_RX_IDX=%d 
 
6707,i,[ phy_dev_rstCal.c : 604 ] phyB, Dtop ch1: RO_RX_IDX=%d 

 
6706,iiiiii,[ phy_dev_rstCal.c : 612 ] phyB, Dtop ch0: RO_RX_GAIN_ADDR=%d, Gw=[%d, %d, %d, %d, %d]
 
6705,iiiiii,[ phy_dev_rstCal.c : 620 ] phyB, Dtop ch1: RO_RX_GAIN_ADDR=%d, Gw=[%d, %d, %d, %d, %d]
 
6704,i,[ phy_dev_rstCal.c : 625 ] phyA, Dtop ch0: RO_RX_IDX=%d 
 
6703,i,[ phy_dev_rstCal.c : 627 ] phyA, Dtop ch1: RO_RX_IDX=%d 

 
6702,iiiiii,[ phy_dev_rstCal.c : 635 ] phyA, Dtop ch0: RO_RX_GAIN_ADDR=%d, Gw=[%d, %d, %d, %d, %d]
 
6701,iiiiii,[ phy_dev_rstCal.c : 643 ] phyA, Dtop ch1: RO_RX_GAIN_ADDR=%d, Gw=[%d, %d, %d, %d, %d]
 
6751,IIIIIII,[ rfaConfig.c : 1606 ] band: %u regular: %u lg: %u vlg: %u coex: %u dpd: %u dco: %u 
6750,i,[ rfaConfig.c : 627 ] tx gain table size (%d) is not correct. So don't change TX_PWR_LV_LAA_0 and TX_PWR_LV_N79_0. 
6749,,[ rfaConfig.c : 634 ] TX_PWR_LV_LAA_0 and TX_PWR_LV_LAA_0 are 0. So use INI default setting 
6748,,[ rfaConfig.c : 696 ] phyRfaIni 
6747,II,[ rfaConfig.c : 721 ] major version: %u, minor version: %u 
6746,I,[ rfaConfig.c : 722 ] psMask = 0x%x 
6745,,[ rfaConfig.c : 1321 ] RfaIni Done 
6744,,[ rfaConfig.c : 719 ] ERROR! UNKNOWN WCSS ENVIRONMENT 
6743,iiii,[ rfaConfig.c : 4604 ] phyRfaSetAltTblIdx: rxGain_tbl_info[%d] freq = %d bwCode = %d rxGainLutSel = %d 
6742,,[ rfaConfig.c : 4628 ] set channel Recipe Start 
6741,,[ rfaConfig.c : 4672 ] set channel Recipe Complete 
6740,,[ rfaConfig.c : 4695 ] Turning 2G Off 
6739,,[ rfaConfig.c : 4713 ] Turning 5G Off 
6738,,[ rfaConfig.c : 3994 ] ERROR! UNKNOWN WCSS ENVIRONMENT 
6737,,[ rfaConfig.c : 4013 ] phyMode Incompatible with 165 Mhz! 
6736,i,[ rfaConfig.c : 4058 ] Warning: INVALID PwrMask = %d 
6735,I,[ rfaConfig.c : 4179 ] INVALID FREQUENCY1 %u 
6734,,[ rfaConfig.c : 4185 ] This is in DBS or SBS mode 
6733,,[ rfaConfig.c : 4204 ] Turning 5G Off 
6732,,[ rfaConfig.c : 4216 ] Turning 2G Off 
6731,II,[ rfaConfig.c : 4231 ]  pwrMask: %u DFSMASK: %u 
6730,ii,[ rfaConfig.c : 4501 ] set_synth_channel, chidx = %d, freq = %d 
6752,iii,[ hca_HwComponentTrxHastingsPrime_config.cpp : 89 ] EnableHwDtimSlna: phyId = %d, chain = %d, SLNA_CTRL = %d 
6770,I,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 186 ] XTAL CAL_SetXtalCalCWTone: enableFlag = %x 
6769,i,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 199 ] XTAL_CAL - CWgain_index = %d 
6768,i,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 203 ] XTAL_CAL clear - gainIdx4XtalCal = %d 
6767,iiI,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 235 ] XTAL_CAL: SET - Reg_values, chain = %d, idx = %d, value = 0x%x
 
6766,iiI,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 305 ] XTAL_CAL: Restore - Reg_values, chain = %d, idx = %d, value = 0x%x
 
6765,iiI,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 320 ] XTAL_CAL_MAP: Clear - Reg_values, chain = %d, idx = %d, value = 0x%x
 
6764,iII,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 478 ] XtalCal::sign_flag=%d,  ppm(0.5 unit) = %x value = %x 
 
6763,iii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 486 ] PPM WAR: halphy_bdf_GetXtalCalValue: capin=%d, capout=%d offsetPPM = %d 
6762,ii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 489 ] PPM WAR:: Entering AdjustXtalForLongPkt: capin=%d, capout=%d 
6761,iiii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 499 ] PPM WAR:: delta = %d, loop %d,  residue=%d, STEPSIZE=%d 
6760,ii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 529 ] XtalCal:: CAPIN %d CAPOUT %d
 
6759,ii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 577 ] PPM WAR : CAPIN %d CAPOUT %d 
6758,iii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 590 ] PPM WAR:: AdjustXtalCAPValue -> bdf::: CAPIN %d CAPOUT %d, offsetPPM %d 
6757,i,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 596 ] PPM WAR:: AdjustXtalCAPValue::: deltaTime in MS = %d 
6756,i,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 600 ] PPM WAR:: AdjustXtalCAPValue::: deltaTime in MS = %d 
6755,iii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 608 ] PPM WAR :: %d us used for updating CAPIN %d CAPOUT %d
 
6754,iii,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 613 ] PPM WAR:: AdjustXtalCAPValue::: incoming adjusted ppm X = %d real adjusted ppm Y = %d, (X - Y) = %d 
6753,,[ hca_HwComponentTrxHastingsPrime_xtalCal.cpp : 446 ] OTPPatch failed!!! 
6777,ii,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 449 ] HcaHwComponentTrxHastingsPrime_efuse::ReadPerRfa %d, %d 
6776,II,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 422 ] HcaHwComponentTrxHastingsPrime_efuse::WritePerRfa 0x%x, 0x%x 
6775,ii,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 428 ] HcaHwComponentTrxHastingsPrime_efuse::WritePerRfa::XO cdacin %d, cdacout %d 
6774,i,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 563 ] HcaHwComponentTrxHastingsPrime_efuse::GetOTPRegDomain domain_code2, otpRegDomain %d 
6773,i,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 567 ] HcaHwComponentTrxHastingsPrime_efuse::GetOTPRegDomain domain_code1, otpRegDomain %d 
6772,i,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 571 ] HcaHwComponentTrxHastingsPrime_efuse::GetOTPRegDomain domain_code0, otpRegDomain %d 
6771,,[ hca_HwComponentTrxHastingsPrime_efuse.cpp : 575 ] HcaHwComponentTrxHastingsPrime_efuse::GetOTPRegDomain Null of regDomain in OTP, return 0 
6857,iiiiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9878 ] version %d isPairWith3rdPartyWwan %d AGE %d %d %d %d %d %d  
6856,iIII,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9883 ] index %d, peakModeIndicator 0x%08x domainIndicator 0x%08x, powerLimitIndicator 0x%08x 
6855,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9886 ] reserverMarginDb %d 
6854,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4565 ] tpcOnepointCal:: GetAlphaTherm cEeprom->baseBdfHeader.commonBoardFlags = %d chainIdx = %d channel = %d 
6853,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4595 ] tpcOnepointCal:: GetAlphaTherm channel %d alphaThermFreq[iAlphaThermFreq] %d chosenChannelIdx %d 
6852,IIIIIII,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4635 ] tpcOnepointCal:: chosen phyId %u alphaThermFreq[%u] %u curChan %u curChain %u tempIdx %u alphaThermValue %u 
6851,iIIiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5684 ] AmapCalulation bandSel %d AGk_lim %lu %lu,numActiveBands %d,numActiveRadios %d/%d,AmapPower[0] %d,CM %d 
6850,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9914 ] SetBiosTASData len is wrong, len=%d 
6849,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9922 ] call phyrf_tpc_TASOLReset by SetBiosTASData for BOIS SAR enable 
6848,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9929 ] call phyrf_tpc_TASOLReset by SetBiosTASData for BOIS SAR enable 
6847,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9934 ] EnableFlag %d PowerTableIndex(DSI) %d 
6846,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5413 ] BIOS Antenna Group 
6845,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5418 ] BDF Antenna Group 
6844,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 1754 ] CTL disalbe by debug command! 
6843,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 1771 ] 6G CTL powerMode = %d 
6842,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 2394 ] CTL_DEBUG: Update chanListIdx = %d 
6841,iiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 2463 ] Testing current j=%d, CTL=%d, max pwr=%d, minPwr=%d, mode=%d 
6840,iiiiiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 2486 ] GetMaxEdgePower: channel=%d, mode=%d, regdmn=%d, beamform=%d, chainmask=%d, nssmask=%d, power=%d, cost time=%d us, isWorldMode=%d 
6839,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5456 ] TAS OL GetTASPeakExposureMode BitMapArrayIndex %d BitMapArrayBit %d SARDomain %d 
6838,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4884 ] BIOS GEO DATA push failed. 
6837,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4853 ] BIOS SAR DATA push failed 
6836,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9898 ] SetBiosTASConfig len is wrong, len=%d 
6835,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7667 ] DumpTpcPerPacket: Get CTL pwr = good chain: %d sec chain: %d 
 
6834,I,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9102 ] halphy_bdf_ModifyBdfOtpFlags: disableOTPOnePtCal 0x%x 
6833,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5743 ] get5GSubBandIndex Error chan freq %d subBand %d 
6832,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5746 ] chan freq %d subBand %d 
6831,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5779 ] get6GSubBandIndex Error chan freq %d subBand %d 
6830,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5782 ] chan freq %d subBand %d 
6829,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5992 ] AddSAR1LimitTPCTAS BIOS TAS ENTRY 
6828,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5997 ] AddSAR1LimitTPCTAS BDF TAS ENTRY 
6827,Iiiiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 6131 ] DumpTpcPerPacket: Get Rate target pwr TPC pwr Bios SAR regDmn 0x%x, chainMask %d, freq %d, isDbsMode %d, SubBandIndex %d, GeoIndex=%d, ch0=%d, ch1=%d
 
6826,iiiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4966 ] GetSAR1TableValues chan=%d, sarversion=%d, sarFlag=%d, regDmn=%d, regDmnIdx=%d, numSARValidSets=%d, isWorldMode=%d 
6825,iiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5004 ] GetSAR1TableValues is2G %d chan %d chan_bin_2G %d regDmn %d regDmnIdx %d numSARValidSets%d 
6824,iiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5130 ] GetSAR1TableValues is2G %d chan %d chan_bin_5G %d regDmn %d regDmnIdx %d numSARValidSets%d 
6823,iiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5261 ] GetSAR1TableValues is2G %d chan %d chan_bin_6G %d regDmn %d regDmnIdx %d numSARValidSets%d 
6822,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 10013 ] Error parameter is NULL 
6821,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4932 ] Bios Cca Threshold configure success  
6820,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4935 ] FW ignore Bios Cca Threshold, use BDF agcEnergyDetThr parameters 
6819,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 2785 ] CTL6G Value %d
 
6818,iIii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 2790 ] CTL_ENGINE: chan = %d, pEepromStruct->cfgCtl[is2GHz]is 0x%x, is2GHz is %d, g_6g_ctl is %d 
 
6817,I,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 2802 ] CTL_ENGINE: ignore CTL, regDmn = NEW_CTL_IGNORE or NEW_NO_CTL, regDmn = 0x%x
 
6816,iiiiiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5932 ] SAR1PwrTbl2G %d %d %d,SAR1PwrTbl5G %d %d %d, SAR1PwrTbl6G %d, %d 
6815,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5975 ] Overwrite negative Psar to 0! 
6814,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5981 ] Overwrite negative Psar to 0! 
6813,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5558 ] Received NULL pointer for internal parameter. Please check 
6812,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5571 ] RFMode %d, chainMask %d Band %d MaxChain %d 
6811,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5644 ] numActiveBands %d,numActiveRadios %d/%d 
6810,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5853 ] AddSAR1LimitTPCTASBIOS band %d PwrTbl %d %d %d 
6809,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5872 ] Overwrite negative Psar to 0! 
6808,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5878 ] Overwrite negative Psar to 0! 
6807,IIIIIi,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4544 ] tpcOnepointCal:: chosen phyId %u calFreq[%u] %u curChan %u curChain %u onePointThermOffset %d 
6806,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5491 ] TAS OL GetTASPeakExposureMode BitMapArrayIndex %d BitMapArrayBit %d peakExposureMode %d 
6805,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 6787 ] DumpTpcPerPacket: target power: chain1: %d chain2: %d
 
6804,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7971 ] Received debug command 6G CTL powerMode = %d 
6803,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7975 ] ProgramAGCEnergyDetThr powerMode %d, cfgCtl %d, is2GHz %d, isG %d 
6802,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 8005 ] ProgramAGCEnergyDetThr 6G power mode error: powerMode %d cfgCtl %d 
6801,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 8034 ] ProgramAGCEnergyDetThr ETSI finnal threshold pri20 %d, Ext20 %d, Ext40 %d, Ext80 %d 
6800,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 8036 ] ProgramAGCEnergyDetThr FCC final threshold pri20 %d, Ext20 %d, Ext40 %d, Ext80 %d 
6799,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 10174 ] Error, len is wrong. 
6798,IIII,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 10180 ] %02x %02x %02x %02x 
6797,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 10183 ] SetBiosBandEdgeCtlData enable flag %d 
6796,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 3023 ] TPC: iwconfig_logs:: band=%d g_maxRDPower6G=%d homechan = %d 
6795,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 3090 ] DumpTpc: power_type_6ghz = %d twiceAntennaGain = %d
 
6794,iiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 3113 ] DumpTpc: before maxRegDef p1 bdf val: %d, user antenna gain: 2G: %d - 5G: %d, twiceAntennaGain (max of BDF and user): %d, twiceAntennaReduction: %d,  
6793,iiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 3127 ] DumpTpc: before maxRegDef powerLimit: %d, userMaxPowerx2: %d, twiceMaxRD: %d, twiceLargestAntenna %d, lowest power: %d 
6792,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 3141 ] DumpTpc: Reg Power update not supported as part of set Tx power as we have new WMI 
6791,iiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 3151 ] DumpTpc: after maxRegDef default reg pwr: %d pTpcConfig->maxRegAllowedPower[%d]: %d, twiceMultiChainGain[%d]: %d 
6790,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 10047 ] GetBiosBandEdgeCTLPower channelFreq %d bandWidth %d type %d 
6789,,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9396 ] Target pwr mode is invalid 
6788,IIIIIi,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4185 ] tpcOnepointCal:: chosen phyId %u calFreq[%u] %u curChan %u curChain %u onePointTpcGLUTOffset %d 
6787,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7745 ] DumpTpcPerPacket: Get regulatory pwr EIRP: %d, is PSD: %d, New regdb WMI call: %d, curr_BW:%d 
 
6786,iiiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7750 ] DumpTpcPerPacket: Get regulatory Final combined power : %d CurrBW: %d, isValidTxPwr: %d,  tx_power: %d , PSD_PWR: %d
 
6785,ii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7764 ] DumpTpcPerPacket: Get regulatory pwr = good chain: %d sec chain: %d 
 
6784,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7395 ] SetBiosBandEdgeCtlData DumpTpcPerPacket: Get CTL pwr =  chain 0 = %d, chain 1 = %d ctlPwr %d %d 
6783,iiii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 7416 ] DumpTpcPerPacket: Get CTL pwr =  chain 0 = %d, chain 1 = %d ctlPwr %d isGetBandEdgePower %d 
6782,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4806 ] cbc: chlist_flag: %d 
6781,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 5524 ] TAS OL GetTASPowerLimitIndicator BitMapArrayIndex %d BitMapArrayBit %d powerLimitIndicator %d 
6780,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9991 ] Error, band %d, retrun default value 
6779,iii,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 9481 ] rssiOffset=%d, bdf_rssiffset=%d, total rssi offset=%d 
6778,i,[ hca_HwComponentTrxHastingsPrime_bdf.cpp : 4815 ] cbc: chlist_repeat_count: %d 
6911,II,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 177 ] HcaHwComponentTrxHastingsPrime_tpc tpc_flag %x exouple = %x 
6910,II,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 199 ] TPC_DBG:EnableCLPC (hastingsPrime) clpc thresh in alutGen %x out %x 
6909,iii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 211 ] [TempComp]HcaHwComponentTrxHastingsPrime_tpc::chainIdx=%d, thermCalValue=%d, alphaTherm=%d 
6908,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 235 ] HcaHwComponentTrxHastingsPrime_tpc::EnableCLPC=%d 
6907,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 240 ] HcaHwComponentTrxHastingsPrime_tpc::EnableCLPC=%d 
6906,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 601 ] ov_rel0:%d 
6905,iIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1176 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId %d, PrimaryChan %u, SecondaryChan %u, txChainMask %u, rxChainMask %u 
6904,iiiiiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1178 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: Home Chan = %d, RF Mode = %d, Pwr Mask = %d, Phy Mode = %d, GLUT_DAC_GAIN_CAL = %d, CMD_COUNT_TXGAIN_COUNT_B0 = %d, CMD_COUNT_TXGAIN_COUNT_B1 =%d 
6903,iIiiiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1208 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, LATEST_FWD_L_B0 = 0x%0x, LATEST_TARGET_PWR_B0 = %d, LATEST_DAC_GAIN_B0 = %d, LATEST_TXGAIN_IDX_B0 = %d, LATEST_GLUT_IDX_B0 = %d, LATEST_TX_IQ_IDX_B0 = %d 
6902,iIiiiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1210 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, LATEST_FWD_L_B1 = 0x%0x, LATEST_TARGET_PWR_B1 = %d, LATEST_DAC_GAIN_B1 = %d, LATEST_TXGAIN_IDX_B1 = %d, LATEST_GLUT_IDX_B1 = %d, LATEST_TX_IQ_IDX_B1 = %d 
6901,iIiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1234 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, LATEST_LB_L_B0 = 0x%0x, LATEST_ACCUMULATED_CLPC_ERR_B0 = %d, LATEST_CLPC_ERR_B0 = %d, LATEST_MEAS_PWR_OUT_B0 = %d 
6900,iIiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1236 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, LATEST_LB_L_B1 = 0x%0x, LATEST_ACCUMULATED_CLPC_ERR_B1 = %d, LATEST_CLPC_ERR_B1 = %d, LATEST_MEAS_PWR_OUT_B1 = %d 
6899,iIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1253 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, 2G_TPC_FB_12_STAT_B0 = 0x%0x, 2G_TPC_FB_12_STAT_B1 = 0x%0x, 5G_TPC_FB_12_STAT_B0 = 0x%0x, 5G_TPC_FB_12_STAT_B1 = 0x%0x 
6898,iIiiIii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1272 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, TPC_GEN_CTRL_L = 0x%0x, OLPC_MODE = %d, TARGET_PWR_CLPC_THR_CORR = %d; TPC_CLPC_CTRL = 0x%0x, CLPC_ERR_UPDATE_DIS = %d, MASK_OUT_CLPC_ERR_UPDATE = %d 
6897,iIiiIii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1289 ] HcaHwComponentTrxHastingsPrime_tpc::DumpTpcRegisters: phyId = %d, TPC_CHN_STAT_LATEST_TXGAIN_L_B0 = 0x%0x, LATEST_WSI_TPC_PDET_GAIN_IDX_B0 = %d, LATEST_WSI_TPC_ATTEN_B0 = %d; TPC_CHN_STAT_LATEST_TXGAIN_L_B1 = 0x%0x, LATEST_WSI_TPC_PDET_GAIN_IDX_B1 = %d, LATEST_WSI_TPC_ATTEN_B1 = %d 
6896,,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1303 ] SmartTxClearVreg 
6895,iii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 515 ] force glut: chain%d, gainindex%d: dacgain=%d
 
6894,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 617 ] OPC: phyId:%d state 
6893,ii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 710 ] bHomeChan=%d, TPCisOLPC=%d, Need to re-program TPC registers 
6892,iii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 150 ] [TempComp]HcaHwComponentTrxHastingsPrime_tpc::chainIdx=%d, thermCalValue=%d, alphaTherm=%d 
6891,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1420 ] SmartTxQueryAccumulatedStats: phy %d is in sleep, VREG is not accessible 
6890,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1426 ] SmartTxQueryAccumulatedStats: phy %d be skipped as this is SBS mode 
6889,iiIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1458 ] SmartTxQuery: bandSelection %d--chainIdx %d: Energy %lu/%lu Duration %u/%u 
6888,iiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1464 ] band %d chainIdx %d enable %d %d 
6887,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 632 ]  GetLatestAccumulatedCLPCError :%d 
6886,,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1320 ] SmartTxClearFWAcc 
6885,iiiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1341 ] pResetStruct->curChan %d, pResetStruct->prevChan %d, newChan->band_center_freq1 %d, is6Gto5G %d,is5Gto6G %d 
6884,,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1345 ] HcaHwComponentTrxHastingsPrime_tpc No tracking required if no band change happens 
6883,iiIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1374 ] SmartTxBandChg: bandSelection %d--chainIdx %d: Energy %lu/%lu Duration %u/%u 
6882,iiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1380 ] band %d chainIdx %d enable %d %d 
6881,,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1387 ] HcaHwComponentTrxHastingsPrime_tpc No tracking required for PHY B 
6880,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 644 ]  GetLatestAccumulatedCLPCErrorPerChain :%d 
6879,iIIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 794 ] DumpTpcLuts: phyId %d, PrimaryChan %u, SecondaryChan %u, dumpMask=%u  txChainMask %u, rxChainMask %u 
6878,IIIIIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 830 ] DumpTpcLuts: GLUT: tpcTblIdx %3u |  tpcChainIdx %3u | tpcGainIdx %3u | pwrMeas %3d | minDacGain %3d | txGainIdx %3d | clpcError %3d | tpcClPktCnt %3d 
6877,IIIIIIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 857 ] DumpTpcLuts: tpcTblIdx %3u |  tpcChainIdx %3u | tpcPlutIdx %3u | pdadc[%3u-%3u] HEX:%8x | pdadc[%3u-%3u] HEX:%8x | 
6876,IIIIIIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 886 ] DumpTpcLuts: tpcTblIdx %3u |  tpcChainIdx %3u | tpcAlutIdx %3u | Alut tgtPwr Step [%3u-%3u] HEX:%8x | Alut tgtPwr Step [%3u-%3u]  HEX:%8x 
6875,IiIi,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 928 ] TPC_DUMP_CHAIN: tpcChainIdx %3u | CH%d_TPC_FB_1 (0x%08x) | PD_DC_SEL= %d 
6874,IiIii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 935 ] TPC_DUMP_CHAIN: tpcChainIdx %3u | CH%d_TPC_OVERRIDE_1 (0x%08x) | PDET_GAIN_IDX_OVS %d | FE_XPA_RF_DISCONNECT_OVS %d 
6873,IiII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 941 ] TPC_DUMP_CHAIN: tpcChainIdx %3u | CH%d_TPC_OVERRIDE_3 (0x%08x) 0x%08x 
6872,IiIi,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 947 ] TPC_DUMP_CHAIN: tpcChainIdx %3u | CH%d_TPC_FB_8_B0 (0x%08x) | PDADC_BIAS= %d 
6871,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 963 ] TPC_DUMP_BDF : DUMP BDF GLUT FOR FREQ=%d 
6870,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 970 ] TPC-DUMP_BDF calFreqPier2G=%d 
6869,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 976 ] TPC-DUMP_BDF calFreqPier5G=%d 
6868,IIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 999 ] TPC_DUMP_BDF : tpcchan %3u | tpcChainIdx %3u | gainIdx %3u | txgainIdx %3u | meas_pwr %3d | 
6867,IIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1024 ] TPC_DUMP_BDF : tpcchan %3u | tpcChainIdx %3u | gainIdx %3u | txgainIdx %3u | meas_pwr %3d | 
6866,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1033 ] TPC_DUMP_BDF_PLUT : DUMP BDF PLUT FOR FREQ=%d 
6865,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1039 ] TPC-DUMP_BDF calFreqPier2G=%d 
6864,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1045 ] TPC-DUMP_BDF calFreqPier5G=%d 
6863,i,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1050 ] TPC_DUMP_BDF : DUMP BDF CLPC FOR FREQ=%d 
6862,IIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1070 ] TPC_DUMP_BDF : tpcchan %3u | tpcChainIdx %3u | gainIdx %3u | pdadc_read %3u | meas_pwr %3d | 
6861,IIIII,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1095 ] TPC_DUMP_BDF : tpcchan %3u | tpcChainIdx %3u | gainIdx %3u | pdadc_read %3u | meas_pwr %3d | 
6860,II,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1113 ] TPC_DUMP_RATEARRAY : ratesArray[%u] = 0x%x 
6859,II,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 1120 ] TPC_DUMP_RATEARRAY : ratesArray2[%u] = 0x%x 
6858,iiiiiiii,[ hca_HwComponentTrxHastingsPrime_tpc.cpp : 435 ] [FCS%d] tpc glut chainIdx:%d channel:%d glutIdxEnd:%d i:%d txGainIdx:%d measPwr:%d minDacGain:%d 
6989,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1220 ] Do not have access to masterCalDb or localCalDb, failed to restore DPD 
6988,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1224 ] paprd_restore : finalCase %d, paprdType %d 
6987,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1244 ] Do not have access to masterCalDb or localCalDb, failed to restore DPD 
6986,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1248 ] DPD Memory : paprd_restore : finalCase %d 
6985,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 80 ]  ********* halphy_mem_paprd_edpd_ctrl paprdType%d  
6984,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 87 ]  WoW Entry mode, update caldb(return) chainmask %d  
6983,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 92 ] Error: %s Invalid DPD table address 
6982,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 99 ] Error: %s Invalid DPD table address 
6981,iiI,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 105 ]  Channel %d  chain (%d) caldb_addr dpdStart 0x%8x  Memory DPD  
6980,iiI,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 176 ] (1)paprdType %d Untrained tables: chain %d, training_done 0x%8x
 
6979,iiI,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 179 ] paprdType %d Untrained tables: chain %d, training_done_table 0x%8x
 
6978,iiiII,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 796 ] halphyPaprdCheckCalibrationFailure : chain %d training_done_table %d training_fail_table %d mask %0x%8x 
6977,iiiII,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 803 ] halphyPaprdCheckCalibrationFailure : chain %d training_done_table %d training_fail_table %d mask %0x%8x 
6976,iiii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 806 ] halphyPaprdCheckCalibrationFailure : chain %d training_done_table %d training_fail_table %d retry_dpd %d 
6975,iiIi,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 2187 ] (1)paprdType %d Untrained tables: chain %d, training_done_table 0x%8x alltablesDone %d 
6974,iI,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 2217 ] NEW VALID BITS Untrained tables: chain %d, training_done_table 0x%8x
 
6973,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1299 ]  WoW Entry mode, update caldb(return) chainmask %d  
6972,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1305 ] Error: %s Invalid DPD table address 
6971,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1316 ] Error: %s Invalid DPD table address 
6970,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1321 ] Error: %s Invalid DPD table address 
6969,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1332 ] Error: %s Invalid DPD table address 
6968,iiII,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1339 ]  Channel %d  chain (%d) caldb_addr dpdStart 0x%8x dpdCtrlStart 0x%8x  
6967,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1373 ]  ********* halphy_mem_paprd_device_update_caldb_addr paprdType%d  
6966,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1388 ]  WoW Entry mode, update caldb(return) chainmask %d  
6965,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1394 ] Error: %s Invalid DPD table address 
6964,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1405 ] Error: %s Invalid DPD table address 
6963,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1410 ] Error: %s Invalid DPD table address 
6962,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1419 ] Error: %s Invalid DPD table address 
6961,iiII,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1425 ]  Channel %d  chain (%d) caldb_addr dpdStart 0x%8x dpdCtrlStart 0x%8x  Memory DPD  
6960,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1087 ] HwComponentTrxHastingsPrime_paprd::FtmControl : channel %d dpd_enable %d 
 
6959,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1685 ]  StorePaprd paprdType %d chain %d table %d   
6958,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1699 ]  StorePaprd WoW Entry mode, StorePaprd (return) paprdType   
6957,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1730 ]  eDPD : StorePaprd WoW Entry mode, StorePaprd (return) paprdType   
6956,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1748 ] Memory DPD :  end of memeory StorePaprd  
6955,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1113 ] PAPRD ResetParams phyExtn = %d
 
6954,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 990 ] PHY INCATIVE : retrun 
6953,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1547 ] RestorePaprd : caltype %d  
6952,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1556 ]  ReStorePaprd WoW Entry mode, ValidateCALDB(return) paprdType %d   
6951,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1575 ] Cals cal valid bits chain(%d)  %d  
6950,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1583 ] *********** RestorePaprd : caltype %d  
6949,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 2005 ] PAPRD ProcessMemDPD 
6948,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1769 ] StoreMemPaprd Entry 
6947,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1786 ]  StoreMemPaprd WoW Entry mode, StorePaprd (return) paprdType   
6946,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 338 ]  chain %d dpdPostScalingValue %d 
6945,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 342 ]  chain %d table %d dpdWarmPktDacGain %d 
6944,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 343 ]  chain %d table %d dpdGMGlutIdx %d 
6943,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 400 ]  chain %d table %d ldpdTrainingDacGain %d 
6942,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1456 ] ValidateCalDb : Invalid caltype %d  
6941,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1461 ]  ValidateCalDb WoW Entry mode, ValidateCALDB(return) paprdType %d  chainmask %d  
6940,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1468 ]  halphyDPDValidateCalDB paprdType %d  chainmask %d,  
6939,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1478 ]  CALIBRATION COMPLETE  chain %d, result 1 
6938,iiii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1496 ]  halphyPaprdValidateCalibration calattempts %d %d, validBits %d %d 
6937,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1497 ]  halphyPaprdValidateCalibration results[0] %d [1] %d 
6936,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1072 ] PAPRD phy_core_set_paprd_enable : enable %d ldpd %d edpd %d
 
6935,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1616 ] RestoreMemPaprd : Invalid caltype %d  
6934,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1620 ] *********** RestoreMemPaprd : caltype %d channel %d paprdType %d 
6933,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1624 ]  RestoreMemPaprd WoW Entry mode, ValidateCALDB(return) paprdType %d   
6932,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1645 ] Cals cal valid bits chain(%d)  %d  
6931,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 2134 ]  NMSE Check failed %d %d 
6930,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 2142 ]  NMSE Check %d %d %d 
6929,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1992 ] PAPRD PHY ID %d GetDPDEnable() DPD enable (lDPD %d eDPD %d) 
6928,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 930 ] PAPRD Calibration complete %d 
6927,iiii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 2089 ] Channel Context :(before BG processing)  workingChannel %d txChainMask  %d  phyrfMode %d  WoW Mode %d 
6926,iiiii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1155 ] PAPRD PHY ID %d start %d end %d chan start %d chan end %d 
 
6925,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 526 ]  postProcessingConfig  %d, valid chain mask %d paprdType %d 
6924,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 276 ] PAPRDTUNING: SETTING - LoopBack Attn | Glut %d Value %d
 
6923,ii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 283 ] PAPRDTUNING: SETTING - Timing Delay | Glut %d Value %d
 
6922,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 865 ] PAPRD table index %d; skipping chain 
 
6921,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 882 ] ChangeTrainingIndex : paprdType %d 
6920,iiii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 898 ] PAPRDTUNING: Channel %d chainIdx %d glutIdx %d gainIdx %d
 
6919,,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 912 ] PAPRD Calibration complete 
6918,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1823 ]  Memory DPD Restore : Control  paprdType%d 
6917,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1844 ]  Memory DPD Restore : Control  paprdType%d 
6916,iii,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 728 ] phy_paprd_device_PopulatePaprdTables : chain %d tableIndex %d paprdType %d 
6915,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 639 ]  PAPRD: XmitTrainingFrame failed. Status %d 
 
6914,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 641 ]  PAPRD: XmitTrainingFrame tx_count %d
 
6913,i,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 1129 ] PAPRD ResetParams phyExtn = %d
 
6912,I,[ hca_HwComponentTrxHastingsPrime_paprd.cpp : 215 ] PAPRD:HcaHwComponentTrxHastingsPrime_paprd::HwDisable : PhyBase %8x 
 
6990,i,[ hca_HwComponentTrxHastingsPrime_cal.cpp : 491 ] TrxHastingPrime-RSSI:%d 
6992,,[ hca_HwComponentTrxHastingsPrime_btcoex.cpp : 211 ] TrxHastingsPrime_btcoex::SetOverrideGainSetting: Error Cannot Access Register in Sleep 
6991,iIii,[ hca_HwComponentTrxHastingsPrime_btcoex.cpp : 233 ] TrxHastingsPrime_btcoex::SetOverrideGainSetting: Read back value of PHYID = %d, ovsVal = 0x%02x WLAN_CONTROL_EN_CH0_OVS = %d, BT_CONTROL_SLNA_L_CH0_OVS = %d 
6993,,[ hca_HwComponentTrxHastingsPrime_calSmIm2.cpp : 117 ] IM2CAL:  completed 
7011,Ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 171 ] DPD Cal::: phyRfMode = %x, cannot do cal - BDF disabled for DPD(Memory), phy %d 
7010,iiiii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 188 ] PAPRD: already in progress -bHomeChan %d  home channel %d cal channel %d timerActive %d  dpd cal State %d, returning 
7009,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 192 ] PAPRD : Cancel timer Channel %d 
7008,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 198 ] Calibration is in progress on other phy cur phyId %d 
7007,,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 209 ] PAPRD: DPD disabled for this range of frequency 
7006,iii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 232 ] PAPRD: INVALIDATING CALDB caldb channel %d home channel %d cal channel %d 
7005,,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 244 ] Cant fo DPD Calibration , WoW mode is enabled 
7004,Iiiiii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 249 ] eDPD:::pHdl=%x, phyRfMode=%d, phyID=%d, txCM=%d, rxCM=%d finalCase %d 
7003,ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 256 ] Cals cal valid bits chain %d %d  
7002,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 259 ] Cals attempted(mem_dpd) chain 0 %d  
7001,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 262 ] Cals attempted(mem_dpd) chain 1 %d  
7000,ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 264 ] Cals cal valid bits chain %d %d  
6999,,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 270 ] PAPRD: DPD disabled for this range of frequency 
6998,I,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 310 ] PAPRD: Memory DPD , Resubmission Final Case0x%08x 
6997,Ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 336 ] DPD Cal::: phyRfMode = %x, cannot do cal - NAN vDev found , phy %d 
6996,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 358 ] PAPRD: Memory DPD , is temp recal? %d 
6995,ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 367 ]  new channel request %d channel %d 
6994,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemory.cpp : 118 ] Invalid channel %d
 
7027,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 159 ] Calibration is in progress on phyId %d 
7026,iii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 128 ] DPD Cal State m/c ::: new_channel_change_request(%d) on channel %d smState %d 
7025,,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 203 ] PAPRD: background thread is active(eDPD is running), calibration is in progress 
7024,Ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 208 ] DPD Cal::: phyRfMode = %x, cannot do cal - BDF disabled for DPD Type(MemLess), phy %d 
7023,iiiii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 216 ] PAPRD: already in progress - bHomeChan %d  channel %d calChannel %d timerActive %d  dpd cal State %d returning 
7022,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 220 ] PAPRD : Cancel timer: cur channel %d 
7021,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 231 ] Calibration is in progress on other phy cur phyId %d 
7020,Iiiii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 259 ] DPD:::pHdl=%x, phyRfMode=%d, phyID=%d, txCM=%d, rxCM=%d  
7019,Ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 263 ] DPD Cal::: phyRfMode = %x, cannot do cal - NAN vDev found , phy %d 
7018,,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 282 ] PAPRD: DPD disabled for this range of frequency 
7017,,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 304 ] Cant fo DPD Calibration , WoW mode is enabled 
7016,ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 308 ]  finalCase %d globalCallingContext %d 
7015,ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 317 ] Cals attempted chain %d  %d  
7014,ii,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 319 ] Cals cal valid bits chain %d %d  
7013,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 341 ] PAPRD: Memory DPD , is temp recal? %d 
7012,i,[ hca_HwComponentTrxHastingsPrime_calSmDpdMemoryLess.cpp : 110 ] Invalid channel %d
 
7029,i,[ hca_HwComponentTrxHastingsPrime_calSmAdc.cpp : 124 ] CalSM: ADC or TIADC starts: calTypeVarianceId=%d 
7028,iii,[ hca_HwComponentTrxHastingsPrime_calSmAdc.cpp : 153 ] CalSM: TIADC invoke recipe: calTypeVarianceId=%d, tIadcInput.calCmdId=%d, CAL_DOCAL=%d 
7034,,[ hca_HwComponentTrxHastingsPrime_calSmBwFilter.cpp : 146 ] calSmBwFilter: WARNING: pHandle is NULL: return without operation. 
7033,,[ hca_HwComponentTrxHastingsPrime_calSmBwFilter.cpp : 251 ] TXBwFilter: Restored now 
7032,,[ hca_HwComponentTrxHastingsPrime_calSmBwFilter.cpp : 262 ] TXBwFilter: Save now 
7031,,[ hca_HwComponentTrxHastingsPrime_calSmBwFilter.cpp : 291 ] RXBwFilter: Restored now 
7030,,[ hca_HwComponentTrxHastingsPrime_calSmBwFilter.cpp : 304 ] RXBwFilter: Save now 
7068,i,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1089 ] ITER2CMDIDX  iterIdx 		=%d 
7067,i,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 691 ] FC_HANDLE  finalCase 		=%d 
7066,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 843 ] RXDCO FC_HANDLE: BTC_CALLBACK_FALSE skip Cal in DTIM 
7065,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 848 ] RXDCO FC_HANDLE: BTC_CALLBACK_TRUE Doing CAL in DTIM 
7064,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 855 ] RXDCO FC_HANDLE: BTC_CALLBACK_FALSE skip Cal 
7063,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 860 ] RXDCO FC_HANDLE: BTC_CALLBACK_TRUE Doing CAL 
7062,ii,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 864 ] finalCase before switch statement=%d, localrxDcoValid=%d 
7061,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 937 ] RXDCO ::: CAL_RESTORE convertNewRxdcoLutfromCalDb failed
 
7060,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 948 ] RXDCO ::: CAL_RESTORE phyRxDCOCal_qca649x failed
 
7059,i,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 993 ] RXDCO FC_HANDLE: CALLING BTC CALLBACK to inform CAL has ended CAL done in %d 
7058,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1046 ] RXDCO ::: CAL_SAVE convertNewRxdcoLutfromCalDb failed
 
7057,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1051 ] RXDCO ::: condition for saving to calDB not met!!!
 
7056,I,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1262 ] read back pwrMask=%x at location A 
7055,iiIi,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1387 ] :::: Can't do rxdco calibration due to conditionally check fails: isSBS = %d, phyId=%d, pwrMask=%x, callingContext)=%d
 
7054,II,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1450 ] read back pwrMask=%x, phyInput->rxChMask=%x at location B 
7053,i,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1482 ] RXDCO Standalone:: time = %d 
7052,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1495 ] :::: phyrf_turn_off is called 
7051,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1497 ] :::: phyrf_turn_on is called 
7050,iiIIi,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1875 ] calSmRxDcoStandaloneWowDtim: Restore RXDCO LUT from DTIM cache for chainIdx = %d, synthidx = %d, LUT_Imag = 0x%x, LUT_Real = 0x%x, range = %d 
7049,iIIi,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1627 ] calSmRxDcoStandaloneWowScan: Restore RXDCO LUT from local scan cache with chainIdx = %d, LUT_Imag = 0x%x, LUT_Real = 0x%x, range = %d
 
7048,i,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 302 ] RXDCO ::SM::: convertNewRxdcoLutfromCalDb chainIdx = %d pStart= NULL!!!!
 
7047,iIIi,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 349 ] Restore Rxdco LUT OVD from caldb with chainIdx = %d, LUT_Imag = 0x%x, LUT_Real = 0x%x, range = %d
 
7046,iIIi,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 360 ] convertNewRxdcoLutfromCalDb:::Save Rxdco LUT to caldb with chainIdx = %d, LUT_Imag = 0x%x, LUT_Real = 0x%x, range = %d
 
7045,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 397 ] APPLICALBE_RESUBMISSION_ONLY:: failure on not getting pStart (= NULL) from caldb! 
7044,i,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 403 ] APPLICALBE_RESUBMISSION_ONLY:: failure on getting chainIdx:%d from pPhyRxdcoInput 
7043,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1706 ] calSmRxDcoStandaloneWowHomeOrWakeup: Setting table mode for RXDCO FCS 
7042,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1169 ] calling calSmRxDcoStandaloneWowScan 
7041,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1174 ] calling calSmRxDcoStandaloneWowHomeOrWakeup 
7040,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1179 ] calling calSmRxDcoStandaloneWowDtim 
7039,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1187 ] calling calSmRxDcoStandaloneWowScan to attempt to use wow scan cache 
7038,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1192 ] calling calSmRxDcoStandaloneWowHomeOrWakeup to attempt for FCS 
7037,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1197 ] calling calSmRxDcoStandaloneWowDtim to attempt for FCS 
7036,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1202 ] calling calSmRxDcoStandaloneNominal 
7035,,[ hca_HwComponentTrxHastingsPrime_calSmRxDco.cpp : 1212 ] calling calSmRxDcoStandaloneNominal, FCS check failed 
7071,,[ hca_HwComponentTrxHastingsPrime_calSmDac.cpp : 173 ] calSmDac: DOCAL invoked 
7070,,[ hca_HwComponentTrxHastingsPrime_calSmDac.cpp : 177 ] calSmDac: Save invoked 
7069,,[ hca_HwComponentTrxHastingsPrime_calSmDac.cpp : 203 ] calSmDac: Restore invoked 
7158,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 947 ] combCal_SM_save: RXIQ: chainIdx=%d,  pStartRxIq=%x 
7157,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 948 ] combCal_SM_save: RXIQ: chainIdx=%d,  pStartRxIqGainMap=%x 
7156,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 949 ] combCal_SM_save: RXIQ: chainIdx=%d,  pStartRxIqDpd=%x 
7155,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 950 ] combCal_SM_save: TXLO: chainIdx=%d,  pStartTxLo=%x 
7154,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 951 ] combCal_SM_save: TXIQ: chainIdx=%d,  pStartTxIq=%x 
7153,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1168 ] cannot update txiq table in caldb for chainIdx = %d! 
7152,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1302 ] cannot update txlo table in caldb for chainIdx = %d! 
7151,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1867 ] CAL_COMMON_PARAM pHandle 	=%x 
7150,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1868 ] CAL_COMMON_PARAM calType 	=%d 
7149,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1869 ] CAL_COMMON_PARAM cmdGroupId 	=%d 
7148,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1870 ] CAL_COMMON_PARAM isRestoreOnly 	=%d 
7147,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1871 ] CAL_COMMON_PARAM calTypeVarianceId 	=%d 
7146,iii,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1872 ] CAL_COMMON_PARAM reserved 	=%d %d %d 
7145,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1873 ] CAL_COMMON_PARAM (pIn->pHandle).phyId 	=%x 
7144,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1874 ] CAL_COMMON_PARAM halphyBW 	=%x 
7143,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1875 ] PHYDEVLIB_PHY_INPUT phyId 		=%d 
7142,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1876 ] PHYDEVLIB_PHY_INPUT bandCode	=%d 
7141,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1877 ] PHYDEVLIB_PHY_INPUT bwCode 	=%d 
7140,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1878 ] PHYDEVLIB_PHY_INPUT phyMode 	=%d 
7139,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1879 ] PHYDEVLIB_PHY_INPUT band_center_freq1 	=%d 
7138,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1880 ] PHYDEVLIB_PHY_INPUT band_center_freq2 	=%d 
7137,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1881 ] PHYDEVLIB_PHY_INPUT txChMask 	=%x 
7136,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1882 ] PHYDEVLIB_PHY_INPUT rxChMask 	=%x 
7135,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1883 ] PHYDEVLIB_PHY_INPUT phyBase 	=%x 
7134,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1884 ] PHYDEVLIB_PHY_INPUT phyBaseExt 	=%x 
7133,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1885 ] PHYDEVLIB_PHY_INPUT concMode 	=%d 
7132,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1886 ] PHYDEVLIB_PHY_INPUT dynPriChan 	=%d 
7131,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1887 ] PHYDEVLIB_PHY_INPUT homeCh		=%d 
7130,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1888 ] PHYDEVLIB_PHY_INPUT pwrMask 		=%d 
7129,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1889 ] PHYDEVLIB_PHY_INPUT extLNA 		=%d 
7128,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1890 ] PHYDEVLIB_PHY_INPUT extPA 		=%d 
7127,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1891 ] PHYDEVLIB_PHY_INPUT isSBSmode 	=%d 
7126,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1892 ] PHYDEVLIB_PHY_INPUT loType 		=%d 
7125,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1893 ] PHYDEVLIB_PHY_INPUT dpdMode 	=%d 
7124,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1894 ] PHYDEVLIB_PHY_INPUT loadIniMask 	=%d 
7123,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1895 ] PHYDEVLIB_PHY_INPUT calMask 	=%d 
7122,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1896 ] PHYDEVLIB_PHY_INPUT cal_mode_ctrl 	=%d 
7121,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1898 ] CCAL_INPUT calCmdId		=%d 
7120,I,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1899 ] CCAL_INPUT cal_chain_mask		=%x 
7119,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1900 ] CCAL_INPUT cal_mode		=%d 
7118,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1901 ] CCAL_INPUT mode (80p80 mode)		=%d 
7117,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1902 ] CCAL_INPUT fixed_gain		=%d 
7116,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1903 ] CCAL_INPUT engineSharing		=%d 
7115,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1904 ] CCAL_INPUT driveTxGLUTIdx		=%d 
7114,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1905 ] CCAL_INPUT enableBlockAccAvg		=%d 
7113,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1906 ] CCAL_INPUT blockSize[0]		=%d 
7112,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1907 ] CCAL_INPUT dcEstWindowSize		=%d 
7111,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1908 ] CCAL_INPUT numOfBlocks		=%d 
7110,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1909 ] CCAL_INPUT numSamplesToReadback[0]	=%d 
7109,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1910 ] CCAL_INPUT numSamplesToReadback[1]	=%d 
7108,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1911 ] CCAL_INPUT numSamplesToReadback[2]	=%d 
7107,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1912 ] CCAL_INPUT rxGainSettlingTime		=%d 
7106,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1913 ] CCAL_INPUT txGainSettlingTime		=%d 
7105,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1914 ] CCAL_INPUT txShiftSettlingTime		=%d 
7104,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1915 ] CCAL_INPUT calModeSettlingTime	=%d 
7103,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1916 ] CCAL_INPUT loopbackSettlingTime	=%d 
7102,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1917 ] CCAL_INPUT txResidueSettlingTime	=%d 
7101,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1918 ] CCAL_INPUT numTaps[0] 		=%d 
7100,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1919 ] CCAL_INPUT numTaps[1] 		=%d 
7099,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 535 ] combCal_SM_restore: RXIQ: chainIdx=%d,  pStartRxIq=%x 
7098,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 556 ] cannot update rxiq table in caldb for chainIdx = %d! 
7097,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 562 ] combCal_SM_restore: RXIQ: chainIdx=%d,  pStartRxIqGainMap=%x 
7096,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 563 ] combCal_SM_restore: RXIQ: chainIdx=%d,  pStartRxIqDpd=%x 
7095,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 700 ] combCal_SM_restore: TXIQ: chainIdx=%d,  pStartTxIq=%x 
7094,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 722 ] cannot update txiq table in caldb for chainIdx = %d! 
7093,iI,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 793 ] combCal_SM_restore: TXLO: chainIdx=%d,  pStartTxLo=%x 
7092,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 820 ] cannot update txlo table in caldb for chainIdx = %d! 
7091,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1683 ] COMBCAL FC_HANDLE: BTC_CALLBACK_FALSE skip Cal 
7090,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1688 ] COMBCAL FC_HANDLE: BTC_CALLBACK_TRUE Doing Cal 
7089,ii,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1698 ] FC_HANDLE  finalCase before switch statement		=%d, localtxloValid=%d 
7088,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1772 ] COMBCAL FC_HANDLE: CALLING BTC CALLBACK to inform CAL has ended CAL Done in %d 
7087,iiiii,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2184 ] CalSM: callingContext=%d, shortenPhyId=%d, pwrMaskRead=%d, illegalSbsLpCombo=%d, determineSBSMode(pHandle))=%d 
7086,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2191 ] :::: return upon illegal pwrMask/SBS input/onlyOne main synth supported: pwrMaskRead = %d 
7085,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2224 ] :::: return upon SCAN: disable 
7084,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2234 ] ::::return upon back to same home channel from scan or from previous home channel wakeup: enable only 
7083,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2239 ] :::: bypass FCS/PS wakeup check, continue use calDB to determine action 
7082,ii,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2262 ] CalSM: effective pwrMaskRead=%d, numSynForCal=%d 
7081,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2043 ] calSmCombStandaloneWowHome: ::::return upon back to same home channel from scan or from previous home channel wakeup: enable only 
7080,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 2095 ] calSmCombStandaloneWowScan: :::: return upon SCAN: disable 
7079,iiiIiIii,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1408 ] cur_tbl_idx=%d, hwsBw=%d, freq1=%d, tMask=%x, concMode=%d, pwrMask=%x, isSBSmode=%d, loadIniMask=%d 
7078,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1951 ] calling calSmCombStandaloneWowScan 
7077,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1956 ] calling calSmCombStandaloneWowHome 
7076,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1964 ] calling calSmCombStandaloneWowScan to attempt for FCS 
7075,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1971 ] calling calSmCombStandaloneWowHome to attempt for FCS 
7074,i,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1978 ] forcing cal for combcal, forceCombCalCounter = %d 
7073,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1983 ] calling calSmCombStandaloneNominal 
7072,,[ hca_HwComponentTrxHastingsPrime_calSmComb.cpp : 1993 ] calling calSmCombStandaloneNominal, FCS check failed 
7164,i,[ hca_HwComponentTrxHastingsPrime_calSmPdet.cpp : 152 ] calSmDET: PDET_Standalone callingContext = %d 
7163,ii,[ hca_HwComponentTrxHastingsPrime_calSmPdet.cpp : 159 ] calSmDET: PDET_Standalone by pass cal cal or restore: pHandle->phyId=%d, isSBSmode=%d 
7162,,[ hca_HwComponentTrxHastingsPrime_calSmPdet.cpp : 206 ] PDET: BTC_CALLBACK_FALSE skip Cal 
7161,i,[ hca_HwComponentTrxHastingsPrime_calSmPdet.cpp : 215 ] PDET: CALLING BTC CALLBACK to inform CAL has ended CAL Done in %d 
7160,i,[ hca_HwComponentTrxHastingsPrime_calSmPdet.cpp : 249 ] calSmPDET: restore invoked on chainIdx = %d 
7159,,[ hca_HwComponentTrxHastingsPrime_calSmPdet.cpp : 93 ] Welcome, cal SM for Pdet Cal will be created 
7167,i,[ wls_main.c : 195 ] wls_fw thread exists with %d! 
7166,i,[ wls_main.c : 197 ] wls_locsvr thread exists with %d! 
7165,i,[ wls_main.c : 199 ] wls_wlansvr thread exists with %d! 
7233,i,[ wls_loc_server.c : 203 ] qmi_csi_send_ind returns error %d 
7232,,[ wls_loc_server.c : 769 ] connected to location client! 
7231,i,[ wls_loc_server.c : 787 ] loc disconnected! clnt_num = %d 
7230,,[ wls_loc_server.c : 837 ] null parameters 
7229,i,[ wls_loc_server.c : 841 ] LOC_SVR_RECV msg id = %d! 
7228,i,[ wls_loc_server.c : 851 ] no function defined to handle request for message ID: %d 
7227,i,[ wls_loc_server.c : 854 ] message id: %d greater than maximum known message ID.
 
7226,,[ wls_loc_server.c : 590 ] discovery scan query received 
7225,,[ wls_loc_server.c : 594 ] empty discovery request 
7224,iiiiiiii,[ wls_loc_server.c : 601 ] scan id: %d, active: %d, dwell %d timeout %d freq_list_len: %d scan_type: %d dwell_mode: %d, radio_chain_pref: %d 
7223,,[ wls_loc_server.c : 607 ] Freq_list_length greater than max_size of freq_list 
7222,ii,[ wls_loc_server.c : 615 ] freq_list[%d]: %d 
7221,i,[ wls_loc_server.c : 624 ] qmi_csi_send_resp transmission fails %d! 
7220,i,[ wls_loc_server.c : 638 ] wls_fuse_req_id() fails %d 
7219,i,[ wls_loc_server.c : 665 ] wls_fw_issue_scan_cmd returns %d! 
7218,,[ wls_loc_server.c : 479 ] subscription received 
7217,,[ wls_loc_server.c : 483 ] empty subscription request 
7216,iiii,[ wls_loc_server.c : 489 ] sub req_id %d sub enable %d sub type %d snoop mode %d 
7215,ii,[ wls_loc_server.c : 500 ] invalid params: is_enable_valid %d sub_type_valid %d 
7214,i,[ wls_loc_server.c : 507 ] invalid sub type %d 
7213,i,[ wls_loc_server.c : 514 ] invalid intf type %d 
7212,,[ wls_loc_server.c : 538 ] invalid snoop_mode_valid 
7211,iiiii,[ wls_loc_server.c : 555 ] clnt_info: sub_intf_type %d subscription %d sub_snoop_scan_req_id %d sub_event_req_id %d snoop_mode %d 
7210,i,[ wls_loc_server.c : 562 ] qmi_csi_send_resp transmission fails %d! 
7209,,[ wls_loc_server.c : 872 ] null parameter 
7208,i,[ wls_loc_server.c : 885 ] qmi_csi_register_with_options failed %d 
7207,,[ wls_loc_server.c : 124 ] wls_clear_clntl, clear clients after unregister qmi 
7206,,[ wls_loc_server.c : 158 ] null pointer 
7205,,[ wls_loc_server.c : 171 ] clnt info lookup fails 
7204,,[ wls_loc_server.c : 955 ] WLS Location Server thread started! 
7203,,[ wls_loc_server.c : 967 ] wlan not ready to serve, exit loc_svc! 
7202,i,[ wls_loc_server.c : 974 ] wlan host ready to serve - %d 
7201,,[ wls_loc_server.c : 978 ] starting wlan fw intf 
7200,,[ wls_loc_server.c : 987 ] wlan not ready to serve, exit loc_svc! 
7199,,[ wls_loc_server.c : 1001 ] wlan fw is ready to serve 
7198,,[ wls_loc_server.c : 1004 ] starting location service... 
7197,,[ wls_loc_server.c : 1021 ] location service started 
7196,,[ wls_loc_server.c : 1025 ] waiting for locatoin request! 
7195,I,[ wls_loc_server.c : 1035 ] sig_val = %x 
7194,,[ wls_loc_server.c : 1038 ] WLS_WLIF_RX_SIG! 
7193,i,[ wls_loc_server.c : 1049 ] wlan not ready to serve, stop location service! - %d 
7192,i,[ wls_loc_server.c : 1052 ] qmi_csi_unregister() returns error %d 
7191,,[ wls_loc_server.c : 1057 ] return 
7190,,[ wls_loc_server.c : 1060 ] break 
7189,,[ wls_loc_server.c : 1068 ] event handled! 
7188,,[ wls_loc_server.c : 263 ] indication is NULL or has length 0 
7187,,[ wls_loc_server.c : 268 ] info: no location client is connected yet 
7186,,[ wls_loc_server.c : 279 ] no location client is connected yet 
7185,i,[ wls_loc_server.c : 691 ] wls_fw_issue_rtt_req returns %d! 
7184,i,[ wls_loc_server.c : 700 ] qmi_csi_send_resp transmission fails %d! 
7183,ii,[ wls_loc_server.c : 222 ] wls_send_indication: msg_id %d, len %d 
7182,i,[ wls_loc_server.c : 240 ] __wls_send_indication() returns %d 
7181,,[ wls_loc_server.c : 225 ] location client is not connected yet 
7180,,[ wls_loc_server.c : 235 ] qmi csi connection is Busy 
7179,i,[ wls_loc_server.c : 374 ] intf_type %d don't send status! 
7178,,[ wls_loc_server.c : 385 ] malloc fails for rtt_oem_channel_list! 
7177,i,[ wls_loc_server.c : 404 ] wls_send_indication transmission fails %d! 
7176,i,[ wls_loc_server.c : 407 ] status indication sent %d! 
7175,,[ wls_loc_server.c : 437 ] empty status request 
7174,i,[ wls_loc_server.c : 441 ] status req received %d! 
7173,i,[ wls_loc_server.c : 450 ] qmi_csi_send_resp transmission fails %d! 
7172,i,[ wls_loc_server.c : 453 ] status resp sent %d! 
7171,,[ wls_loc_server.c : 330 ] version query received 
7170,,[ wls_loc_server.c : 334 ] empty version request 
7169,,[ wls_loc_server.c : 340 ] version info unavailable 
7168,i,[ wls_loc_server.c : 347 ] qmi_csi_send_resp transmission fails %d! 
7252,,[ wls_wlan_service_server.c : 333 ] null parameter 
7251,i,[ wls_wlan_service_server.c : 344 ] qmi_csi_register_with_options failed %d 
7250,,[ wls_wlan_service_server.c : 132 ] wlan status request recieved 
7249,i,[ wls_wlan_service_server.c : 136 ] wls_save_status() returned error: %d 
7248,i,[ wls_wlan_service_server.c : 144 ] qmi_csi_send_resp returned error: %d 
7247,,[ wls_wlan_service_server.c : 150 ] wls_fetch_status returns NULL! 
7246,,[ wls_wlan_service_server.c : 155 ] malloc fails for rtt_oem_channel_list! 
7245,,[ wls_wlan_service_server.c : 163 ] wlan staus is ready 
7244,,[ wls_wlan_service_server.c : 169 ] wlan status changed to NOT ready 
7243,,[ wls_wlan_service_server.c : 94 ] wlan version request recieved 
7242,i,[ wls_wlan_service_server.c : 102 ] qmi_csi_send_resp returned error: %d 
7241,,[ wls_wlan_service_server.c : 237 ] connected to wlan cnss-daemon! 
7240,,[ wls_wlan_service_server.c : 258 ] disconnected! 
7239,i,[ wls_wlan_service_server.c : 300 ] WLAN_SVR_RECV msg id = %d! 
7238,i,[ wls_wlan_service_server.c : 312 ] No function defined to handle request for message ID: %d 
7237,i,[ wls_wlan_service_server.c : 315 ] Message ID: %d greater than maximum known message ID.
 
7236,,[ wls_wlan_service_server.c : 366 ] WLS APSS WLAN Server thread started! 
7235,,[ wls_wlan_service_server.c : 401 ] close wlan service! 
7234,,[ wls_wlan_service_server.c : 392 ] waiting for signal! 
7282,,[ wls_wlan_service_data.c : 38 ] rtt_oem_channel_list is NULL! 
7281,,[ wls_wlan_service_data.c : 140 ] event struct pointer is NULL 
7280,i,[ wls_wlan_service_data.c : 152 ] fw_adsp_support    : %d 
7279,i,[ wls_wlan_service_data.c : 153 ] is_on              : %d 
7278,i,[ wls_wlan_service_data.c : 154 ] vdev_id            : %d 
7277,i,[ wls_wlan_service_data.c : 155 ] vdev_mode          : %d 
7276,i,[ wls_wlan_service_data.c : 156 ] vdev_is_connected  : %d 
7275,I,[ wls_wlan_service_data.c : 157 ]   ap: country_code : %s 
7274,i,[ wls_wlan_service_data.c : 158 ]   ap: freq         : %d 
7273,i,[ wls_wlan_service_data.c : 159 ]   ap: rssi         : %d 
7272,i,[ wls_wlan_service_data.c : 160 ]   ap: ssid_len     : %d 
7271,IIIIII,[ wls_wlan_service_data.c : 162 ]   ap: bssid        : %x %x %x %x %x %x 
7270,i,[ wls_wlan_service_data.c : 163 ] channel_info_len   : %d 
7269,i,[ wls_wlan_service_data.c : 164 ] rtt_info_len       : %d 
7268,ii,[ wls_wlan_service_data.c : 169 ] Error: # of channel %d beyond max limit %d 
7267,ii,[ wls_wlan_service_data.c : 175 ] channel_info[%d]    : %d 
7266,ii,[ wls_wlan_service_data.c : 177 ] channel_info[%d]   : %d 
7265,i,[ wls_wlan_service_data.c : 183 ] Error: ssid length %d is beyond the limit 
7264,,[ wls_wlan_service_data.c : 292 ] null pointers 
7263,i,[ wls_wlan_service_data.c : 297 ] invalid intf type %d 
7262,,[ wls_wlan_service_data.c : 200 ] event struct pointer is null 
7261,i,[ wls_wlan_service_data.c : 210 ] invalid vdev type %d 
7260,,[ wls_wlan_service_data.c : 74 ] version struct pointer is null 
7259,I,[ wls_wlan_service_data.c : 90 ] chip name :      %s 
7258,I,[ wls_wlan_service_data.c : 91 ] chip from :      %s 
7257,I,[ wls_wlan_service_data.c : 92 ] host version :   %s 
7256,I,[ wls_wlan_service_data.c : 93 ] fw version :     %s 
7255,,[ wls_wlan_service_data.c : 88 ] saving version... 
7254,i,[ wls_wlan_service_data.c : 89 ] chip id :        %d 
7253,,[ wls_wlan_service_data.c : 403 ] Alloc RTT memory by using malloc 
7482,i,[ wls_fw.c : 1687 ] __wls_fw_scan_result_handler(): scan req id %d 
7481,ii,[ wls_fw.c : 1691 ] parse_scan_result() returns error %d on req_id %d 
7480,i,[ wls_fw.c : 1701 ] wls_fw_scan_complete_handler() returns %d 
7479,,[ wls_fw.c : 701 ] invalid param 
7478,,[ wls_fw.c : 706 ] invalid vdev_id 
7477,ii,[ wls_fw.c : 751 ] create_scan_cmd() radio_pref %d, scan_ctrl_flags_ext %d 
7476,i,[ wls_fw.c : 774 ] invalid ssid len %d 
7475,i,[ wls_fw.c : 1776 ] handoff vdev_id  %d 
7474,IIIIII,[ wls_fw.c : 1778 ] handoff bssid    %x %x %x %x %x %x 
7473,i,[ wls_fw.c : 1780 ] handoff ssid len %d 
7472,I,[ wls_fw.c : 1782 ] handoff ssid     %s 
7471,i,[ wls_fw.c : 1783 ] handoff freq     %d 
7470,i,[ wls_fw.c : 1784 ] handoff rssi     %d 
7469,ii,[ wls_fw.c : 94 ] find_scan_data(): req_id : %d, pending state: %d 
7468,i,[ wls_fw.c : 1218 ] validata_scan_result returns error %d 
7467,,[ wls_fw.c : 1223 ] null pointer 
7466,I,[ wls_fw.c : 1230 ] scanned result data TLV 0x%x 
7465,i,[ wls_fw.c : 1233 ] parsing scan result packet (with header) of %d bytes 
7464,i,[ wls_fw.c : 1234 ]   scan result data length %d bytes 
7463,ii,[ wls_fw.c : 1241 ] scan_data_alloc_buffer() returns error %d on req_id %d 
7462,ii,[ wls_fw.c : 1248 ] parse_scanned_chan() returns error %d on req_id %d 
7461,i,[ wls_fw.c : 1252 ] ap_data length %d 
7460,iI,[ wls_fw.c : 1258 ] parsing scan entry #%d from 0x%x 
7459,i,[ wls_fw.c : 1261 ] data_len_raw %d 
7458,iII,[ wls_fw.c : 1268 ] data_len_raw %d bssid 0x%x:0x%x 
7457,i,[ wls_fw.c : 1271 ] data_len_raw %d 
7456,ii,[ wls_fw.c : 1277 ] data_len_raw %d is_probe %d 
7455,i,[ wls_fw.c : 1281 ] data_len_raw %d 
7454,i,[ wls_fw.c : 1286 ] ssid_len %d 
7453,I,[ wls_fw.c : 1289 ] ssid %s 
7452,i,[ wls_fw.c : 1290 ] data_len_raw %d 
7451,ii,[ wls_fw.c : 1292 ] ssid_len %d > %d  
7450,i,[ wls_fw.c : 1298 ] data_len_raw %d 
7449,ii,[ wls_fw.c : 1304 ] data_len_raw %d rssi %d 
7448,i,[ wls_fw.c : 1307 ] data_len_raw %d 
7447,ii,[ wls_fw.c : 1313 ] data_len_raw %d freq %d 
7446,i,[ wls_fw.c : 1316 ] data_len_raw %d 
7445,ii,[ wls_fw.c : 1322 ] data_len_raw %d tx_power %d 
7444,i,[ wls_fw.c : 1325 ] data_len_raw %d 
7443,ii,[ wls_fw.c : 1331 ] data_len_raw %d tx_rate %d 
7442,i,[ wls_fw.c : 1334 ] data_len_raw %d 
7441,ii,[ wls_fw.c : 1340 ] data_len_raw %d mc_support %d 
7440,i,[ wls_fw.c : 1343 ] data_len_raw %d 
7439,iI,[ wls_fw.c : 1349 ] data_len_raw %d tsf_timer_value_lower 0x%x 
7438,i,[ wls_fw.c : 1352 ] data_len_raw %d 
7437,iI,[ wls_fw.c : 1358 ] data_len_raw %d tsf_timer_value_upper 0x%x 
7436,i,[ wls_fw.c : 1361 ] data_len_raw %d 
7435,iI,[ wls_fw.c : 1367 ] data_len_raw %d age_of_measurement 0x%x 
7434,i,[ wls_fw.c : 1370 ] data_len_raw %d 
7433,ii,[ wls_fw.c : 1376 ] data_len_raw %d connection_status %d 
7432,i,[ wls_fw.c : 1379 ] data_len_raw %d 
7431,i,[ wls_fw.c : 1385 ] msap_ie_len %d 
7430,i,[ wls_fw.c : 1386 ] data_len_raw %d 
7429,ii,[ wls_fw.c : 1388 ] msap_ie_len %d > %d  
7428,ii,[ wls_fw.c : 1395 ] data_len_raw %d, msap_ie_len %d 
7427,i,[ wls_fw.c : 1401 ] data_len_raw %d 
7426,i,[ wls_fw.c : 1404 ] data_len_raw %d 
7425,ii,[ wls_fw.c : 1410 ] data_len_raw %d security_enabled %d 
7424,i,[ wls_fw.c : 1413 ] data_len_raw %d 
7423,ii,[ wls_fw.c : 1419 ] data_len_raw %d device_type %d 
7422,i,[ wls_fw.c : 1422 ] data_len_raw %d 
7421,ii,[ wls_fw.c : 1428 ] data_len_raw %d channel_is_passive %d 
7420,i,[ wls_fw.c : 1431 ] data_len_raw %d 
7419,ii,[ wls_fw.c : 1437 ] data_len_raw %d dwell_time %d 
7418,i,[ wls_fw.c : 1440 ] data_len_raw %d 
7417,ii,[ wls_fw.c : 1446 ] data_len_raw %d band_center_freq_1 %d 
7416,i,[ wls_fw.c : 1449 ] data_len_raw %d 
7415,ii,[ wls_fw.c : 1455 ] data_len_raw %d band_center_freq_2 %d 
7414,i,[ wls_fw.c : 1458 ] data_len_raw %d 
7413,ii,[ wls_fw.c : 1464 ] data_len_raw %d phy_mode %d 
7412,i,[ wls_fw.c : 1467 ] data_len_raw %d 
7411,ii,[ wls_fw.c : 1473 ] data_len_raw %d scan_mod_id%d 
7410,i,[ wls_fw.c : 1476 ] data_len_raw %d 
7409,ii,[ wls_fw.c : 1482 ] data_len_raw %d scan_id%d 
7408,i,[ wls_fw.c : 1485 ] data_len_raw %d 
7407,ii,[ wls_fw.c : 1491 ] data_len_raw %d flags%d 
7406,i,[ wls_fw.c : 1494 ] data_len_raw %d 
7405,ii,[ wls_fw.c : 1500 ] data_len_raw %d scan_cache%d 
7404,i,[ wls_fw.c : 1503 ] data_len_raw %d 
7403,ii,[ wls_fw.c : 1509 ] data_len_raw %d report_context_hub%d 
7402,i,[ wls_fw.c : 1512 ] data_len_raw %d 
7401,ii,[ wls_fw.c : 1518 ] data_len_raw %d ess%d 
7400,i,[ wls_fw.c : 1521 ] data_len_raw %d 
7399,ii,[ wls_fw.c : 1527 ] data_len_raw %d sec_mode%d 
7398,i,[ wls_fw.c : 1530 ] data_len_raw %d 
7397,ii,[ wls_fw.c : 1536 ] data_len_raw %d tx_nss%d 
7396,i,[ wls_fw.c : 1539 ] data_len_raw %d 
7395,ii,[ wls_fw.c : 1545 ] data_len_raw %d tx_mcs%d 
7394,i,[ wls_fw.c : 1548 ] data_len_raw %d 
7393,ii,[ wls_fw.c : 1554 ] data_len_raw %d rx_nss%d 
7392,i,[ wls_fw.c : 1557 ] data_len_raw %d 
7391,ii,[ wls_fw.c : 1563 ] data_len_raw %d rx_mcs%d 
7390,i,[ wls_fw.c : 1566 ] data_len_raw %d 
7389,ii,[ wls_fw.c : 1573 ] data_len_raw %d radio_chain_mask %d 
7388,i,[ wls_fw.c : 1576 ] data_len_raw %d 
7387,ii,[ wls_fw.c : 1583 ] data_len_raw %d rssi_chain_0 %d 
7386,i,[ wls_fw.c : 1586 ] data_len_raw %d 
7385,ii,[ wls_fw.c : 1593 ] data_len_raw %d rssi_chain_1 %d 
7384,i,[ wls_fw.c : 1644 ] scan_data_append() returns error %d 
7383,i,[ wls_fw.c : 1648 ] scan_data_buf full (%d APs) 
7382,i,[ wls_fw.c : 1656 ]   scan result entry num %d 
7381,ii,[ wls_fw.c : 1662 ] %d APs beyond fullness threshold %d 
7380,i,[ wls_fw.c : 1667 ] partial ap data found! remain data length %d 
7379,,[ wls_fw.c : 1118 ] null data pointer 
7378,i,[ wls_fw.c : 1124 ] invalid req_id %d 
7377,i,[ wls_fw.c : 1131 ] num of channel scanned %d 
7376,i,[ wls_fw.c : 1139 ] parse_scanned_chan(): invalid chan_num %d 
7375,iii,[ wls_fw.c : 1152 ] data[%d] / freq[%d] %d 
7374,i,[ wls_fw.c : 1156 ] freq_list_len %d 
7373,,[ wls_fw.c : 110 ] scan data is null 
7372,i,[ wls_fw.c : 126 ] malloc(%d) failed 
7371,ii,[ wls_fw.c : 156 ] scan buf of len %d allocated for req_id %d 
7370,i,[ wls_fw.c : 115 ] scan with req_id %d is not pending 
7369,,[ wls_fw.c : 120 ] info: scan buffer not null 
7368,ii,[ wls_fw.c : 251 ] req_id %d len %d 
7367,,[ wls_fw.c : 254 ] scan data is null 
7366,i,[ wls_fw.c : 290 ] loc scan result entry length %d 
7365,,[ wls_fw.c : 218 ] scan data is null 
7364,,[ wls_fw.c : 317 ] scan_data_dump(): null pointer 
7363,i,[ wls_fw.c : 321 ] data.req_id %d 
7362,i,[ wls_fw.c : 322 ] data.pending %d 
7361,I,[ wls_fw.c : 323 ] data.head %p 
7360,i,[ wls_fw.c : 324 ] data.max_len %d 
7359,i,[ wls_fw.c : 325 ] data.len %d 
7358,I,[ wls_fw.c : 326 ] data.cur_pos %p 
7357,i,[ wls_fw.c : 327 ] data.len_chre %d 
7356,I,[ wls_fw.c : 328 ] data.cur_pos_chre %p 
7355,i,[ wls_fw.c : 329 ] data.len_chain %d 
7354,I,[ wls_fw.c : 330 ] data.cur_pos_chain %p 
7353,,[ wls_fw.c : 175 ] scan data is null 
7352,i,[ wls_fw.c : 180 ] entry for req_id %d not free 
7351,,[ wls_fw.c : 1067 ] null scan result pointer! 
7350,ii,[ wls_fw.c : 1074 ] empty scan result msg len %d scan_result->data_len %d 
7349,ii,[ wls_fw.c : 1082 ] scan result's tlv corrupted expected %d tlv.len %d 
7348,ii,[ wls_fw.c : 1092 ] corrupted scan result msg! len %d payload_len %d 
7347,I,[ wls_fw.c : 1099 ] corrupted scan result msg! ie_bitmap 0x%x 
7346,i,[ wls_fw.c : 444 ] timer_def_osal() returns error %d 
7345,,[ wls_fw.c : 1801 ] wls_fw_handoff_handler(): entered 
7344,,[ wls_fw.c : 1804 ] null handoff event 
7343,i,[ wls_fw.c : 1812 ] invalid vdev_id %d 
7342,i,[ wls_fw.c : 1817 ] invalid ssid_len %d 
7341,,[ wls_fw.c : 1829 ] null status pointer 
7340,,[ wls_fw.c : 1836 ] malloc fails for rtt_oem_channel_list! 
7339,,[ wls_fw.c : 1950 ] wls_fw_init entered 
7338,,[ wls_fw.c : 1969 ] wmi_save_rx_data(): inform loc server thread of fw intf readiness 
7337,,[ wls_fw.c : 499 ] rtt_req_blob_valid == 0 
7336,,[ wls_fw.c : 505 ] Invalid buf->rtt_req_blob_len 
7335,,[ wls_fw.c : 512 ] malloc failed 
7334,i,[ wls_fw.c : 528 ] wmi_unified_cmd_send returns %d 
7333,i,[ wls_fw.c : 536 ] wls_fw_issue_rtt_req: submitted successfully %d 
7332,i,[ wls_fw.c : 822 ] wls_fw_issue_scan_cmd(): scan req_id : %d 
7331,i,[ wls_fw.c : 831 ] invalid req_id : %d 
7330,i,[ wls_fw.c : 837 ] invalid freq_list_len : %d 
7329,i,[ wls_fw.c : 843 ] invalid ssid_list_len : %d 
7328,i,[ wls_fw.c : 851 ] invalid scan time out : %d 
7327,i,[ wls_fw.c : 858 ] scan data entry not found for req_id %d 
7326,i,[ wls_fw.c : 864 ] req_id is already pending: %d 
7325,iiii,[ wls_fw.c : 880 ] req_id %d time_out %d too short for dwell_time %d ms and freq_list_len %d 
7324,iii,[ wls_fw.c : 889 ] req_id %d radio_pref %d (> %d) -> use default 
7323,i,[ wls_fw.c : 903 ] malloc(scan_cmd) failed, size %d 
7322,i,[ wls_fw.c : 925 ] create_scan_cmd() failed %d 
7321,i,[ wls_fw.c : 933 ] scan_data_init() failed %d 
7320,i,[ wls_fw.c : 947 ] wmi_unified_cmd_send() failed %d 
7319,i,[ wls_fw.c : 825 ] another scan with req_id %d is being serviced! 
7318,,[ wls_fw.c : 2010 ] wls_fw_reinit entered 
7317,i,[ wls_fw.c : 1915 ] wls_fw_rtt_resp_handler() %d 
7316,i,[ wls_fw.c : 981 ] data entry not found for req_id %d 
7315,i,[ wls_fw.c : 987 ] wls_fw_scan_complete_handler(): req_id %d is not pending 
7314,i,[ wls_fw.c : 996 ] info: scan data buffer for req_id %d is null. empty scan result? 
7313,i,[ wls_fw.c : 1001 ] scan_data_alloc_buffer() returns error %d 
7312,i,[ wls_fw.c : 1023 ] ap array data size %d 
7311,i,[ wls_fw.c : 1024 ] sending scan data size %d 
7310,i,[ wls_fw.c : 1025 ] req_id %d 
7309,i,[ wls_fw.c : 1026 ] ap_array_len %d 
7308,i,[ wls_fw.c : 1027 ] ap_array_chre_len %d 
7307,i,[ wls_fw.c : 1028 ] ap_array_chain_len %d 
7306,i,[ wls_fw.c : 1029 ] extscan_is_completed %d 
7305,i,[ wls_fw.c : 1030 ] scan_type_performed %d 
7304,i,[ wls_fw.c : 1031 ] radio_chain_pref %d 
7303,iii,[ wls_fw.c : 1033 ] wls_fw_scan_complete_handler, scan_is_truly_complete %d, scan_type_performed %d, radio_chain_pref %d 
7302,ii,[ wls_fw.c : 1721 ] wls_fw_scan_result_handler(): rx_scan_data_pkt_num %d rx_data_pkt_len %d 
7301,i,[ wls_fw.c : 1724 ] __wls_fw_scan_result_handler() returns %d 
7300,i,[ wls_fw.c : 413 ] latest req id %d 
7299,i,[ wls_fw.c : 1864 ] wls_fw_status_handler(): data len %d 
7298,ii,[ wls_fw.c : 1871 ] wls_fw_status_handler(): scan completed on req_id %d and extscan_is_completed %d 
7297,i,[ wls_fw.c : 1875 ] wls_fw_status_handler(): fw scan timeout on req_id %d 
7296,i,[ wls_fw.c : 1879 ] wls_fw_status_handler(): medium busy on req_id %d 
7295,i,[ wls_fw.c : 1884 ] wls_fw_status_handler(): scan dropped or aborted on req_id %d 
7294,i,[ wls_fw.c : 1889 ] wls_fw_status_handler(): fw detected illegal scan params on req_id %d 
7293,ii,[ wls_fw.c : 1893 ] wls_fw_status_handler(): invalid scan status %d on req_id %d 
7292,,[ wls_fw.c : 2036 ] WLS FW thread started! 
7291,,[ wls_fw.c : 2047 ] close fw interface! 
7290,,[ wls_fw.c : 2055 ] waiting for fw signal! 
7289,i,[ wls_fw.c : 2057 ] signal received! signal value = %d 
7288,,[ wls_fw.c : 2062 ] close fw interface! 
7287,i,[ wls_fw.c : 2071 ] scan timeout detected from adsp on req_id %d! 
7286,,[ wls_fw.c : 2076 ] received fw rx signal! 
7285,,[ wls_fw.c : 557 ] malloc failed 
7284,i,[ wls_fw.c : 579 ] wmi_unified_cmd_send returns %d 
7283,iI,[ wls_fw.c : 591 ] snoop subscription: enable %d snoop_mode %x submitted successfully 
7499,,[ wmi_unified.c : 262 ] wmi_process_rx_data() entered 
7498,i,[ wmi_unified.c : 269 ] __wmi_dequeue_rx_data() processed %d wmi msgs in total in current round 
7497,I,[ wmi_unified.c : 279 ] wmi_process_rx_data(): cmd/event id = 0x%x 
7496,i,[ wmi_unified.c : 280 ] wmi_process_rx_data(): raw packet len = %d 
7495,i,[ wmi_unified.c : 291 ] idx %d 
7494,i,[ wmi_unified.c : 295 ] event handler is not registered: event id %d 
7493,i,[ wmi_unified.c : 298 ] event handler is null: event idx %d 
7492,i,[ wmi_unified.c : 374 ] wmi_save_rx_data(): RX dump start, size = %d 
7491,,[ wmi_unified.c : 376 ] wmi_save_rx_data(): RX dump done 
7490,,[ wmi_unified.c : 379 ] wmi_save_rx_data(): inform fw thread of scan result arrival 
7489,,[ wmi_unified.c : 381 ] wmi_save_rx_data(): RX signal sent 
7488,,[ wmi_unified.c : 343 ] wmi_tx_done_handler(): called 
7487,i,[ wmi_unified.c : 168 ] wlif_tx failed %d 
7486,i,[ wmi_unified.c : 205 ] event handler already registered %d 
7485,i,[ wmi_unified.c : 210 ] no more event handlers %d 
7484,i,[ wmi_unified.c : 219 ] wmi_unified_register_event_handler(): handler idx %d registered 
7483,i,[ wmi_unified.c : 237 ] event handler is not registered: event id %d 
7515,,[ wls_wlif.c : 152 ] wlif_init gets called 
7514,II,[ wls_wlif.c : 187 ] WLIF_RX_NOTIFY_CB:%x, WLIF_TX_DONE_CB:%x 
7513,,[ wls_wlif.c : 195 ] wlif_init is done! 
7512,,[ wls_wlif.c : 397 ] TX WLS -> WLAN: calling WLAN RX callback 
7511,,[ wls_wlif.c : 408 ] WLS RX done. calling WLAN TX done callback 
7510,i,[ wls_wlif.c : 414 ] %d: WLIF error! 
7509,,[ wls_wlif.c : 253 ] wlif_register_callback gets called 
7508,II,[ wls_wlif.c : 267 ] WLIF_RX_NOTIFY_CB:%x, WLIF_TX_DONE_CB:%x 
7507,,[ wls_wlif.c : 269 ] wlif_register_callback is done! 
7506,I,[ wls_wlif.c : 420 ] wlif_rx_done pBuf:%x 
7505,,[ wls_wlif.c : 424 ] WLAN RX done. Calling WLS TX done callback 
7504,,[ wls_wlif.c : 428 ] WLS RX done. siganlling it to WLAN thread 
7503,IiI,[ wls_wlif.c : 354 ] Requested TX %x with len-%d, %x 
7502,I,[ wls_wlif.c : 362 ] TX: WLAN -> WLS, calling WLS RX callback with %x 
7501,,[ wls_wlif.c : 371 ] Cannot find WLAN thread 
7500,I,[ wls_wlif.c : 376 ] TX: WLS -> WLAN, signal to WLAN thread with %x 
