1. Change the silk screen on the PCB to ROCK 5A V1.2
2. Modify schematic



3.Modify layout



1. Change BOM Package for R95239
2. Remove optional circuit for SPI FLASH



1. Increase the routing area for the VCC\_1V8\_S3 net

